# ECDSA Digital Signature Peripheral (ECDSA_DS)

[中文]

The ECDSA Digital Signature Peripheral (ECDSA_DS) implements the Elliptic Curve Digital Signature Algorithm (ECDSA), a variant of the Digital Signature Algorithm (DSA) that uses elliptic-curve cryptography.

ESP32-S31's ECDSA_DS peripheral provides a secure and efficient environment for computing ECDSA signatures. It offers fast computations while ensuring the confidentiality of the signing process to prevent information leakage. ECDSA private key used in the signing process is accessible only to the hardware peripheral, and it is not readable by software.

The ECDSA_DS peripheral can help to establish Secure Device Identity for TLS mutual authentication and similar use-cases.

## Supported Features

- ECDSA digital signature generation and verification

- Three different elliptic curves, namely P-192, P-256 and P-384 (FIPS 186-3 specification)

- Three hash algorithms for message hash in the ECDSA operation, namely SHA-224, SHA-256 and SHA-384 (FIPS PUB 180-4 specification)

## ECDSA_DS on ESP32-S31

On ESP32-S31, the ECDSA_DS module works with a secret key burnt into an eFuse block.

On ESP32-S31, the ECDSA_DS module also supports storing a secret key in the Key Manager. Refer to Key Manager for more details.

This key is made completely inaccessible (default mode) for any resources outside the cryptographic modules, thus avoiding key leakage.

### ECDSA Key Storage

ECDSA private keys are stored in eFuse key blocks. The number of key blocks required depends on the curve size:

- P-256 curve: Require one eFuse key block (256 bits)

- P-384 curve: Requires two eFuse key blocks (512 bits total)

For curves requiring two key blocks (like P-384), configure the following fields:

- Set `esp_tls_cfg_t::ecdsa_key_efuse_blk` to the low block number

- Set `esp_tls_cfg_t::ecdsa_key_efuse_blk_high` to the high block number

For single-block curves (like P-256), only set `esp_tls_cfg_t::ecdsa_key_efuse_blk` and leave `esp_tls_cfg_t::ecdsa_key_efuse_blk_high` as 0 or unassigned.

ECDSA key can be programmed externally through `idf.py` script. Here is an example of how to program the ECDSA key:

Using eFuses to store the ECDSA key:

    idf.py efuse-burn-key <BLOCK_NUM> </path/to/ecdsa_private_key.pem> ECDSA_KEY

Note

Six physical eFuse blocks can be used as keys for the ECDSA_DS module: block 4 ~ block 9. E.g., for block 4 (which is the first key block) , the argument should be `BLOCK_KEY0`.

Using the Key Manager to store the ECDSA key:

ECDSA private keys can be stored in the Key Manager. Refer to Key Manager for more details.

Deploy an ECDSA key into the Key Manager and store the generated Key Recovery info in the flash memory for persistent keys.

Alternatively the ECDSA key can also be programmed through the application running on the target.

Using eFuses to store the ECDSA key:

Following code snippet uses `esp_efuse_write_key()` to set physical key block 0 in the eFuse with key purpose as `esp_efuse_purpose_t::ESP_EFUSE_KEY_PURPOSE_ECDSA_KEY`:

    #include "esp_efuse.h"

    const uint8_t key_data[32] = { ... };

    esp_err_t status = esp_efuse_write_key(EFUSE_BLK_KEY0,
                        ESP_EFUSE_KEY_PURPOSE_ECDSA_KEY,
                        key_data, sizeof(key_data));

    if (status == ESP_OK) {
        // written key
    } else {
        // writing key failed, maybe written already
    }

## Deterministic Signature Generation

The ECDSA_DS peripheral of ESP32-S31 also supports generation of deterministic signatures using deterministic derivation of the parameter K as specified in the RFC 6979 section 3.2.

## Non-Determinisitic Signature Generation

### Dependency on TRNG

The ECDSA_DS peripheral relies on the hardware True Random Number Generator (TRNG) for its internal entropy requirement for generating non-deterministic signatures. During ECDSA signature creation, the algorithm requires a random integer to be generated as specified in the RFC 6090 section 5.3.2.

Please ensure that hardware RNG is enabled before starting ECDSA computations (primarily signing) in the application.

## Application Outline

Please refer to the ECDSA Digital Signature Peripheral (ECDSA_DS) with ESP-TLS guide for details on how-to use the ECDSA_DS peripheral for establishing a mutually authenticated TLS connection.

The ECDSA_DS peripheral in Mbed TLS stack is integrated by overriding the ECDSA signing and verifying APIs. Please note that, the ECDSA_DS peripheral does not support all curves or hash algorithms, and hence for cases where the hardware requirements are not met, the implementation falls back to the software.

For a particular TLS context, additional APIs have been supplied to populate certain fields (e.g., private key ctx) to differentiate routing to hardware. ESP-TLS layer integrates these APIs internally and hence no additional work is required at the application layer. However, for custom use-cases please refer to API details below.

## API Reference

### Header File

- components/mbedtls/port/psa_driver/include/psa_crypto_driver_esp_ecdsa_contexts.h

- This header file can be included with:

  >     #include "psa_crypto_driver_esp_ecdsa_contexts.h"

- This header file is a part of the API provided by the `mbedtls` component. To declare that your component depends on `mbedtls`, add the following to your CMakeLists.txt:

  >     REQUIRES mbedtls

  > or

  >     PRIV_REQUIRES mbedtls

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.