# SDMMC Host Driver

[中文]

## Overview

ESP32-P4's SDMMC host peripheral has two slots. Each slot can be used independently to connect to an SD card, SDIO device, or eMMC chip.

- `SDMMC_HOST_SLOT_1` is routed via GPIO Matrix. This means that any GPIO may be used for each of the SD card signals. It is for non UHS-I usage.

- `SDMMC_HOST_SLOT_0` is dedicated to UHS-I mode, which is not yet supported in the driver.

On ESP32-P4, SDMMC host requires an external power supply for the IO voltage. Please refer to Configuring Voltage Level for details.

## Supported Speed Modes

SDMMC Host driver supports the following speed modes:

- Default Speed (20 MHz): 1-line or 4-line with SD cards, and 1-line, 4-line, or 8-line with 3.3 V eMMC

- High Speed (40 MHz): 1-line or 4-line with SD cards, and 1-line, 4-line, or 8-line with 3.3 V eMMC

- UHS-I 1.8 V, SDR50 (100 MHz): 4-line with SD cards

- UHS-I 1.8 V, DDR50 (50 MHz): 4-line with SD cards

- High Speed DDR (40 MHz): 4-line with 3.3 V eMMC

Speed modes not supported at present:

- High Speed DDR mode: 8-line eMMC

## Using the SDMMC Host Driver

Of all the functions listed below, only the following ones will be used directly by most applications:

- `sdmmc_host_init()`

- `sdmmc_host_init_slot()`

- `sdmmc_host_deinit()`

Other functions, such as the ones given below, will be called by the SD/MMC protocol layer via function pointers in the `sdmmc_host_t` structure:

- `sdmmc_host_set_bus_width()`

- `sdmmc_host_set_card_clk()`

- `sdmmc_host_do_transaction()`

## Configuring Bus Width and Frequency

With the default initializers for `sdmmc_host_t` and `sdmmc_slot_config_t`, i.e., `SDMMC_HOST_DEFAULT` and `SDMMC_SLOT_CONFIG_DEFAULT`, SDMMC Host driver will attempt to use the widest bus supported by the card (4 lines for SD, 8 lines for eMMC) and the frequency of 20 MHz.

In the designs where communication at 40 MHz frequency can be achieved, it is possible to increase the bus frequency by changing the `max_freq_khz` field of `sdmmc_host_t`:

    sdmmc_host_t host = SDMMC_HOST_DEFAULT();
    host.max_freq_khz = SDMMC_FREQ_HIGHSPEED;

If you need a specific frequency other than standard speeds, you are free to use any value from within an appropriate range of the SD interface given (SDMMC or SDSPI). However, the real clock frequency shall be calculated by the underlying driver and the value can be different from the one required.

For the SDMMC, `max_freq_khz` works as the upper limit so the final frequency value shall be always lower or equal. For the SDSPI, the nearest fitting frequency is supplied and thus the value can be greater than/equal to/lower than `max_freq_khz`.

To configure the bus width, set the `width` field of `sdmmc_slot_config_t`. For example, to set 1-line mode:

    sdmmc_slot_config_t slot = SDMMC_SLOT_CONFIG_DEFAULT();
    slot.width = 1;

## Configuring GPIOs

ESP32-P4 SDMMC Host can be configured to use arbitrary GPIOs for each of the signals. Configuration is performed by setting members of `sdmmc_slot_config_t` structure.

For example, to use GPIOs 1-6 for CLK, CMD, and D0-D3 signals respectively:

    sdmmc_slot_config_t slot = SDMMC_SLOT_CONFIG_DEFAULT();
    slot.clk = GPIO_NUM_1;
    slot.cmd = GPIO_NUM_2;
    slot.d0 = GPIO_NUM_3;
    slot.d1 = GPIO_NUM_4;
    slot.d2 = GPIO_NUM_5;
    slot.d3 = GPIO_NUM_6;

It is also possible to configure Card Detect and Write Protect pins. Similar to other signals, set `cd` and `wp` members of the same structure:

    slot.cd = GPIO_NUM_7;
    slot.wp = GPIO_NUM_8;

`SDMMC_SLOT_CONFIG_DEFAULT` sets both to `GPIO_NUM_NC`, meaning that by default the signals are not used.

Once `sdmmc_slot_config_t` structure is initialized this way, you can use it when calling `sdmmc_host_init_slot()` or one of the higher level functions (such as `esp_vfs_fat_sdmmc_mount()`).

## Configuring Voltage Level

ESP32-P4 SDMMC Host requires the IO voltage to be supplied externally via the VDDPST_5 (SD_VREF) pin. If the design doesn't require the higher speed SD modes, this pin can be simply connected to the 3.3V supply.

If the design does require higher speed SD modes (which only work at 1.8V IO levels), there are two options available:

- Use the on-chip programmable LDO. In this case, connect the desired LDO output channel to VDDPST_5 (SD_VREF) pin. Call `sd_pwr_ctrl_new_on_chip_ldo()` to initialize the SD power control driver, then set `sdmmc_host_t::pwr_ctrl_handle` to the resulting handle.

- Use an external programmable LDO. Likewise, connect the LDO output to the VDDPST_5 (SD_VREF) pin. Then implement a custom sd_pwr_ctrl driver to control your LDO. Finally, assign `sdmmc_host_t::pwr_ctrl_handle` to the handle of your driver instance.

## DDR Mode for eMMC Chips

By default, DDR mode will be used if:

- SDMMC host frequency is set to `SDMMC_FREQ_HIGHSPEED` in `sdmmc_host_t` structure, and

- eMMC chip reports DDR mode support in its CSD register

DDR mode places higher requirements for signal integrity. To disable DDR mode while keeping the `SDMMC_FREQ_HIGHSPEED` frequency, clear the `SDMMC_HOST_FLAG_DDR` bit in `sdmmc_host_t::flags` field of the `sdmmc_host_t`:

    sdmmc_host_t host = SDMMC_HOST_DEFAULT();
    host.max_freq_khz = SDMMC_FREQ_HIGHSPEED;
    host.flags &= ~SDMMC_HOST_FLAG_DDR;

## See also

- SD/SDIO/MMC Driver: introduces the higher-level driver which implements the protocol layer.

- SD SPI Host Driver: introduces a similar driver that uses the SPI controller and is limited to SD protocol's SPI mode.

- SD Pull-up Requirements: introduces pull-up support and compatibility of modules and development kits.

## API Reference

### Header File

- components/esp_driver_sdmmc/include/driver/sdmmc_host.h

- This header file can be included with:

  >     #include "driver/sdmmc_host.h"

- This header file is a part of the API provided by the `esp_driver_sdmmc` component. To declare that your component depends on `esp_driver_sdmmc`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_driver_sdmmc

  > or

  >     PRIV_REQUIRES esp_driver_sdmmc

### Functions

esp_err_t sdmmc_host_init(void)

  Initialize SDMMC host peripheral.

  Note

  This function is not thread safe

  Returns:

    - ESP_OK on success or if sdmmc_host_init was already initialized with this function

    - ESP_ERR_NO_MEM if memory can not be allocated

esp_err_t sdmmc_host_init_slot(int slot, const sdmmc_slot_config_t *slot_config)

  Initialize given slot of SDMMC peripheral.

  On the ESP32, SDMMC peripheral has two slots:

  - Slot 0: 8-bit wide, maps to HS1_* signals in PIN MUX

  - Slot 1: 4-bit wide, maps to HS2_* signals in PIN MUX

  Card detect and write protect signals can be routed to arbitrary GPIOs using GPIO matrix.

  Note

  This function is not thread safe

  Parameters:

    - slot -- slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

    - slot_config -- additional configuration for the slot

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_STATE if host has not been initialized using sdmmc_host_init

    - ESP_ERR_INVALID_ARG if GPIO pins from slot_config are not valid

esp_err_t sdmmc_host_set_bus_width(int slot, size_t width)

  Select bus width to be used for data transfer.

  SD/MMC card must be initialized prior to this command, and a command to set bus width has to be sent to the card (e.g. SD_APP_SET_BUS_WIDTH)

  Note

  This function is not thread safe

  Parameters:

    - slot -- slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

    - width -- bus width (1, 4, or 8 for slot 0; 1 or 4 for slot 1)

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if slot number or width is not valid

size_t sdmmc_host_get_slot_width(int slot)

  Get bus width configured in `sdmmc_host_init_slot` to be used for data transfer.

  Parameters:

    slot -- slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

  Returns:

    configured bus width of the specified slot.

esp_err_t sdmmc_host_set_card_clk(int slot, uint32_t freq_khz)

  Set card clock frequency.

  Currently only integer fractions of 40MHz clock can be used. For High Speed cards, 40MHz can be used. For Default Speed cards, 20MHz can be used.

  Note

  This function is not thread safe

  Parameters:

    - slot -- slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

    - freq_khz -- card clock frequency, in kHz

  Returns:

    - ESP_OK on success

    - other error codes may be returned in the future

esp_err_t sdmmc_host_set_bus_ddr_mode(int slot, bool ddr_enabled)

  Enable or disable DDR mode of SD interface.

  Parameters:

    - slot -- slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

    - ddr_enabled -- enable or disable DDR mode

  Returns:

    - ESP_OK on success

    - ESP_ERR_NOT_SUPPORTED if DDR mode is not supported on this slot

esp_err_t sdmmc_host_set_cclk_always_on(int slot, bool cclk_always_on)

  Enable or disable always-on card clock When cclk_always_on is false, the host controller is allowed to shut down the card clock between the commands. When cclk_always_on is true, the clock is generated even if no command is in progress.

  Parameters:

    - slot -- slot number

    - cclk_always_on -- enable or disable always-on clock

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if the slot number is invalid

esp_err_t sdmmc_host_do_transaction(int slot, sdmmc_command_t *cmdinfo)

  Send command to the card and get response.

  This function returns when command is sent and response is received, or data is transferred, or timeout occurs.

  Attention

    Data buffer passed in cmdinfo->data must be in DMA capable memory and aligned to 4 byte boundary. If it's behind the cache, both cmdinfo->data and cmdinfo->buflen need to be aligned to cache line boundary.

  Note

  This function is not thread safe w.r.t. init/deinit functions, and bus width/clock speed configuration functions. Multiple tasks can call sdmmc_host_do_transaction as long as other sdmmc_host_* functions are not called.

  Parameters:

    - slot -- slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

    - cmdinfo -- pointer to structure describing command and data to transfer

  Returns:

    - ESP_OK on success

    - ESP_ERR_TIMEOUT if response or data transfer has timed out

    - ESP_ERR_INVALID_CRC if response or data transfer CRC check has failed

    - ESP_ERR_INVALID_RESPONSE if the card has sent an invalid response

    - ESP_ERR_INVALID_SIZE if the size of data transfer is not valid in SD protocol

    - ESP_ERR_INVALID_ARG if the data buffer is not in DMA capable memory

esp_err_t sdmmc_host_io_int_enable(int slot)

  Enable IO interrupts.

  This function configures the host to accept SDIO interrupts.

  Parameters:

    slot -- slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

  Returns:

    returns ESP_OK, other errors possible in the future

esp_err_t sdmmc_host_io_int_wait(int slot, TickType_t timeout_ticks)

  Block until an SDIO interrupt is received, or timeout occurs.

  Parameters:

    - slot -- slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

    - timeout_ticks -- number of RTOS ticks to wait for the interrupt

  Returns:

    - ESP_OK on success (interrupt received)

    - ESP_ERR_TIMEOUT if the interrupt did not occur within timeout_ticks

esp_err_t sdmmc_host_deinit_slot(int slot)

  Disable SDMMC host and release allocated resources gracefully.

  Note

  If there are more than 1 active slots, this function will just decrease the reference count and won't actually disable the host until the last slot is disabled

  Note

  This function is not thread safe

  Parameters:

    slot -- slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_STATE if SDMMC host has not been initialized

    - ESP_ERR_INVALID_ARG if invalid slot number is used

esp_err_t sdmmc_host_deinit(void)

  Disable SDMMC host and release allocated resources forcefully.

  Note

  This function will deinitialize the host immediately, regardless of the number of active slots

  Note

  This function is not thread safe

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_STATE if SDMMC host has not been initialized

esp_err_t sdmmc_host_get_real_freq(int slot, int *real_freq_khz)

  Provides a real frequency used for an SD card installed on specific slot of SD/MMC host controller.

  This function calculates real working frequency given by current SD/MMC host controller setup for required slot: it reads associated host and card dividers from corresponding SDMMC registers, calculates respective frequency and stores the value into the 'real_freq_khz' parameter

  Parameters:

    - slot -- slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

    - real_freq_khz -- [out] output parameter for the result frequency (in kHz)

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG on real_freq_khz == NULL or invalid slot number used

esp_err_t sdmmc_host_set_input_delay(int slot, sdmmc_delay_phase_t delay_phase)

  set input delay

  - This API sets delay when the SDMMC Host samples the signal from the SD Slave.

  - This API will check if the given `delay_phase` is valid or not.

  - This API will print out the delay time, in picosecond (ps)

  Note

  ESP32 doesn't support this feature, you will get an `ESP_ERR_NOT_SUPPORTED`

  Parameters:

    - slot -- slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

    - delay_phase -- delay phase, this API will convert the phase into picoseconds and print it out

  Returns:

    - ESP_OK: ON success.

    - ESP_ERR_INVALID_ARG: Invalid argument.

    - ESP_ERR_NOT_SUPPORTED: ESP32 doesn't support this feature.

esp_err_t sdmmc_host_get_dma_info(int slot, esp_dma_mem_info_t *dma_mem_info)

  Get the DMA memory information for the host driver.

  Deprecated:

    This API is deprecated

  Parameters:

    - slot -- [in] slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

    - dma_mem_info -- [out] DMA memory information structure

  Returns:

    - ESP_OK: ON success.

    - ESP_ERR_INVALID_ARG: Invalid argument.

bool sdmmc_host_check_buffer_alignment(int slot, const void *buf, size_t size)

  Check if the buffer meets the alignment requirements.

  Parameters:

    - slot -- [in] slot number (SDMMC_HOST_SLOT_0 or SDMMC_HOST_SLOT_1)

    - buf -- [in] buffer pointer

    - size -- [in] buffer size

  Returns:

    True for aligned buffer, false for not aligned buffer

esp_err_t sdmmc_host_is_slot_set_to_uhs1(int slot, bool *is_uhs1)

  Check if the slot is set to uhs1 or not.

  Parameters:

    - slot -- [in] Slot id

    - is_uhs1 -- [out] Is uhs1 or not

  Returns:

    - ESP_OK: on success

    - ESP_ERR_INVALID_STATE: driver not in correct state

esp_err_t sdmmc_host_get_state(sdmmc_host_state_t *state)

  Get the state of SDMMC host.

  Parameters:

    state -- [out] output parameter for SDMMC host state structure

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG on invalid argument

### Structures

struct sdmmc_slot_config_t

  Extra configuration for SDMMC peripheral slot

  Public Members

  gpio_num_t clk

    GPIO number of CLK signal.

  gpio_num_t cmd

    GPIO number of CMD signal.

  gpio_num_t d0

    GPIO number of D0 signal.

  gpio_num_t d1

    GPIO number of D1 signal.

  gpio_num_t d2

    GPIO number of D2 signal.

  gpio_num_t d3

    GPIO number of D3 signal.

  gpio_num_t d4

    GPIO number of D4 signal. Ignored in 1- or 4- line mode.

  gpio_num_t d5

    GPIO number of D5 signal. Ignored in 1- or 4- line mode.

  gpio_num_t d6

    GPIO number of D6 signal. Ignored in 1- or 4- line mode.

  gpio_num_t d7

    GPIO number of D7 signal. Ignored in 1- or 4- line mode.

  gpio_num_t gpio_cd

    GPIO number of card detect signal.

  gpio_num_t cd

    GPIO number of card detect signal; shorter name.

  gpio_num_t gpio_wp

    GPIO number of write protect signal.

  gpio_num_t wp

    GPIO number of write protect signal; shorter name.

  uint8_t width

    Bus width used by the slot (might be less than the max width supported)

  uint32_t flags

    Features used by this slot.

struct sdmmc_host_state_t

  SD/MMC host state structure

  Public Members

  bool host_initialized

    Whether the host is initialized.

  int num_of_init_slots

    Number of initialized slots.

### Macros

SDMMC_SLOT_FLAG_INTERNAL_PULLUP

  Enable internal pullups on enabled pins. The internal pullups are insufficient however, please make sure external pullups are connected on the bus. This is for debug / example purpose only.

SDMMC_SLOT_FLAG_WP_ACTIVE_HIGH

  GPIO write protect polarity. 0 means "active low", i.e. card is protected when the GPIO is low; 1 means "active high", i.e. card is protected when GPIO is high.

SDMMC_SLOT_FLAG_UHS1

  Enable UHS-I mode for this slot

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.