# Mbed TLS

[中文]

Mbed TLS is a C library that implements cryptographic primitives, X.509 certificate manipulation and the SSL/TLS and DTLS protocols. Its small code footprint makes it suitable for embedded systems.

Note

ESP-IDF uses a fork of Mbed TLS which includes a few patches (related to hardware routines of certain modules like `bignum (MPI)` and `ECC`) over vanilla Mbed TLS.

Mbed TLS supports TLS 1.2, TLS 1.3 and DTLS 1.2 communication by providing the following:

- TCP/IP communication functions: listen, connect, accept, read/write.

- SSL/TLS communication functions: init, handshake, read/write.

- X.509 functions: CRT, CRL and key handling

- Random number generation

- Hashing

- Encryption/decryption

Note

Mbed TLS v3.x.x series supports only TLS 1.2 and TLS 1.3 protocols. Support for SSL 3.0, TLS 1.0/1.1 and DTLS 1.0 has been removed (deprecated). TLS 1.3 is fully supported starting Mbed TLS v3.6.0 release, before this release some features were still in experimental state. Please refer to Mbed TLS ChangeLog for more details.

## Mbed TLS Documentation

For Mbed TLS documentation please refer to the following (upstream) pointers:

- API Reference

- Knowledge Base

## Mbed TLS Support in ESP-IDF

Please find the information about the Mbed TLS versions presented in different branches of ESP-IDF here.

Note

Please refer the Mbed TLS to migrate from Mbed TLS version 2.x to version 3.0 or greater.

### Configuration Presets

ESP-IDF provides a preset-based configuration system for Mbed TLS to simplify setup and provide optimized starting points for different use cases. This system works alongside the existing manual configuration system and provides baseline configurations that can be further customized through menuconfig or additional configuration files.

Preset | Use Case | Key Features
--- | --- | ---
Default | General purpose applications | TLS 1.2 & 1.3 support Certificate bundle enabled Hardware acceleration Full cipher suite support
Minimal | Resource-constrained applications | TLS 1.2 client only RSA & PSK key exchange AES-128 CBC/CTR modes Basic X.509 parsing
Bluetooth (BT) | Bluetooth applications | Optimized for BLE security ECC P-256 curve support Minimal TLS overhead Bluetooth-specific algorithms

### Using Configuration Presets

Presets serve as starting points for your mbedTLS configuration. You can use them as-is or customize them further using standard ESP-IDF configuration methods.

To use a preset configuration, add the following line to your project's `CMakeLists.txt` file before the `project()` call:

    # Include the default preset (recommended for most applications)
    list(APPEND sdkconfig_defaults $ENV{IDF_PATH}/components/mbedtls/config/mbedtls_preset_default.conf)

    # Or for resource-constrained applications
    list(APPEND sdkconfig_defaults $ENV{IDF_PATH}/components/mbedtls/config/mbedtls_preset_minimal.conf)

    # Or for Bluetooth applications
    list(APPEND sdkconfig_defaults $ENV{IDF_PATH}/components/mbedtls/config/mbedtls_preset_bt.conf)

    # Standard ESP-IDF project setup
    include($ENV{IDF_PATH}/tools/cmake/project.cmake)
    project(my_project)

Note

The preset configurations are located in `components/mbedtls/config/` and can be customized or used as a starting point for your own configurations.

### Customizing Preset Configurations

After applying a preset, you can further customize the configuration using any of these methods:

Method 1: Using menuconfig (Recommended)

    # After applying a preset in CMakeLists.txt
    idf.py menuconfig

Navigate to `Component Config` > `mbedTLS` to modify any settings. Your changes will override the preset defaults.

Method 2: Additional Configuration Files

You can combine a preset with your own custom configuration by creating an additional configuration file:

    # Use the minimal preset as a base, then add custom settings
    list(APPEND SDKCONFIG_DEFAULTS
        $ENV{IDF_PATH}/components/mbedtls/config/mbedtls_preset_minimal.conf
        ${CMAKE_CURRENT_SOURCE_DIR}/my_custom_mbedtls.conf
    )

### Migration from Manual Configuration

The preset system complements manual configuration. If you have an existing manually configured mbedTLS setup:

Option 1: Keep Your Existing Configuration

Your current manual configuration will continue to work without any changes.

Option 2: Migrate to Preset + Customization

1. Choose a base preset that's closest to your current configuration.

2. Apply the preset in your `CMakeLists.txt`.

3. Use menuconfig to adjust settings to match your requirements.

4. Test thoroughly to ensure functionality is maintained.

### Configuration Categories

The new mbedTLS configuration system is organized into logical categories for easier navigation:

Core Configuration

  Basic mbedTLS settings including memory allocation, threading, and debug options.

TLS Protocol Configuration

  TLS/DTLS protocol versions, modes (client/server), and protocol-specific features.

Symmetric Ciphers

  Block ciphers (AES, ARIA, etc.), cipher modes (CBC, GCM, etc.), and symmetric cryptography.

Asymmetric Ciphers

  RSA, ECC, and other public key cryptography algorithms.

Hash Functions

  Message digest algorithms (SHA-256, SHA-512, etc.) and HMAC.

Hardware Acceleration

  ESP32-specific hardware acceleration for cryptographic operations.

Certificate Support

  X.509 certificate parsing, validation, and certificate bundle management.

## Application Examples

Examples in ESP-IDF use ESP-TLS which provides a simplified API interface for accessing the commonly used TLS functionality.

Refer to the examples protocols/https_server/simple (simple HTTPS server) and protocols/https_request (make HTTPS requests) for more information.

If you plan to use the Mbed TLS API directly, refer to the example protocols/https_mbedtls. This example demonstrates how to establish an HTTPS connection using Mbed TLS by setting up a secure socket with a certificate bundle for verification.

## Alternatives

ESP-TLS acts as an abstraction layer over the underlying SSL/TLS library and thus has an option to use Mbed TLS or wolfSSL as the underlying library. By default, only Mbed TLS is available and used in ESP-IDF whereas wolfSSL is available publicly at https://github.com/espressif/esp-wolfSSL with the upstream submodule pointer.

Please refer to ESP-TLS: Underlying SSL/TLS Library Options documentation for more information on this and comparison of Mbed TLS and wolfSSL.

## Important Config Options

The Mbed TLS configuration system supports preset configurations. Following is a brief list of important config options accessible at `Component Config` > `mbedTLS`. The full list of config options can be found here.

Core Configuration:

- CONFIG_MBEDTLS_HARDWARE_SHA: Support for hardware SHA acceleration

- CONFIG_MBEDTLS_HARDWARE_AES: Support for hardware AES acceleration

- CONFIG_MBEDTLS_HARDWARE_MPI: Support for hardware MPI (bignum) acceleration

- CONFIG_MBEDTLS_MEM_ALLOC_MODE: Memory allocation strategy (Internal/External/Custom)

- CONFIG_MBEDTLS_ASYMMETRIC_CONTENT_LEN: Asymmetric in/out fragment length for memory optimization

- CONFIG_MBEDTLS_DYNAMIC_BUFFER: Enable dynamic TX/RX buffer allocation

- CONFIG_MBEDTLS_DEBUG: Enable mbedTLS debugging (useful for debugging)

TLS Protocol Configuration:

- CONFIG_MBEDTLS_TLS_ENABLED: Enable TLS protocol support

- CONFIG_MBEDTLS_SSL_PROTO_TLS1_2: Support for TLS 1.2 (recommended)

- CONFIG_MBEDTLS_SSL_PROTO_TLS1_3: Support for TLS 1.3 (latest standard)

- CONFIG_MBEDTLS_SSL_PROTO_DTLS: Support for DTLS (UDP-based TLS)

- CONFIG_MBEDTLS_CLIENT_SSL_SESSION_TICKETS: Support for TLS Session Resumption (client session tickets)

- CONFIG_MBEDTLS_SERVER_SSL_SESSION_TICKETS: Support for TLS Session Resumption Server session tickets

- CONFIG_MBEDTLS_SSL_ALPN: Support for Application Layer Protocol Negotiation

- CONFIG_MBEDTLS_SSL_SERVER_NAME_INDICATION: Support for Server Name Indication (SNI)

Certificate Support:

- CONFIG_MBEDTLS_CERTIFICATE_BUNDLE: Support for trusted root certificate bundle (more about this: ESP x509 Certificate Bundle)

- CONFIG_MBEDTLS_X509_USE_C: Enable X.509 certificate support

- CONFIG_MBEDTLS_PEM_PARSE_C: Read & Parse PEM formatted certificates

- CONFIG_MBEDTLS_PEM_WRITE_C: Write PEM formatted certificates

- CONFIG_MBEDTLS_X509_CRT_PARSE_C: Parse X.509 certificates

- CONFIG_MBEDTLS_X509_CRL_PARSE_C: Parse X.509 certificate revocation lists

Cryptographic Algorithms:

- CONFIG_MBEDTLS_AES_C: AES block cipher support

- CONFIG_MBEDTLS_RSA_C: RSA public key cryptosystem

- CONFIG_MBEDTLS_ECP_C: Elliptic Curve Cryptography support

- CONFIG_MBEDTLS_ECDSA_C: Elliptic Curve Digital Signature Algorithm

- CONFIG_MBEDTLS_ECDH_C: Elliptic Curve Diffie-Hellman key exchange

- CONFIG_MBEDTLS_SHA256_C: SHA-256 hash function

- CONFIG_MBEDTLS_SHA512_C: SHA-512 hash function

- CONFIG_MBEDTLS_GCM_C: Galois/Counter Mode for authenticated encryption

Note

The new configuration structure provides better organization with categories like "Core Configuration", "TLS Protocol Configuration", "Symmetric Ciphers", "Asymmetric Ciphers", "Hash Functions", and "Hardware Acceleration" for easier navigation and configuration management.

### Debugging mbedTLS

To enable debugging, add these configurations:

    CONFIG_MBEDTLS_DEBUG=y
    CONFIG_MBEDTLS_DEBUG_LEVEL=3
    CONFIG_LOG_DEFAULT_LEVEL_DEBUG=y

### Performance Optimization

For optimal performance, enable hardware acceleration when available:

    CONFIG_MBEDTLS_HARDWARE_AES=y
    CONFIG_MBEDTLS_HARDWARE_SHA=y
    CONFIG_MBEDTLS_HARDWARE_MPI=y
    CONFIG_MBEDTLS_HARDWARE_ECC=y

## Performance and Memory Tweaks

### Reducing Heap Usage

The following table shows typical memory usage with different configs when the protocols/https_request example (with Server Validation enabled) is run with Mbed TLS as the SSL/TLS library.

Mbed TLS Test | Related Configs | Heap Usage (approx.)
--- | --- | ---
Default | NA | 42196 B
Enable SSL Dynamic Buffer Length | CONFIG_MBEDTLS_SSL_VARIABLE_BUFFER_LENGTH | 42120 B
Disable Keep Peer Certificate | CONFIG_MBEDTLS_SSL_KEEP_PEER_CERTIFICATE | 38533 B
Enable Dynamic TX/RX Buffer | CONFIG_MBEDTLS_DYNAMIC_BUFFER CONFIG_MBEDTLS_DYNAMIC_FREE_CONFIG_DATA CONFIG_MBEDTLS_DYNAMIC_FREE_CA_CERT | 22013 B

Note

These values are subject to change with changes in configuration options and versions of Mbed TLS.

### Reducing Binary Size

Under `Component Config` > `mbedTLS`, several Mbed TLS features are enabled by default. These can be disabled if not needed to save code size. More information is available in the Minimizing Binary Size documentation.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.