# High Priority Interrupts

[中文]

The Xtensa architecture supports 32 interrupts, divided over 7 priority levels from level 1 to 7, with level 7 being an non-maskable interrupt (NMI), plus an assortment of exceptions. On the ESP32, the Interrupt Allocation can route most interrupt sources to these interrupts via the interrupt mux. Normally, interrupts are written in C, but ESP-IDF allows high-priority interrupts to be written in assembly as well, resulting in very low interrupt latencies.

## Interrupt Priorities

Priority Level | Symbol | Remark
--- | --- | ---
1 | N/A | Exception and low priority interrupts, handled by ESP-IDF.
2-3 | N/A | Medium priority interrupts, handled by ESP-IDF.
4 | xt_highint4 | High priority interrupt, free to use. [1]
5 | xt_highint5 | Normally used by ESP-IDF debug logic. [1]
NMI | xt_nmi | Non-maskable interrupt, free to use.
dbg | xt_debugexception | Debug exception. Called on e.g., a BREAK instruction. [2]

[1] (1,2)

ESP-IDF debug logic can be configured to run on `xt_highint4` or `xt_highint5` in CONFIG_ESP_SYSTEM_CHECK_INT_LEVEL. Bluetooth's interrupt can be configured to run on priority level 4 by enabling CONFIG_BTDM_CTRL_HLI. If CONFIG_BTDM_CTRL_HLI is enabled, ESP-IDF debug logic must be running on priority level 5 interrupt.

[2]

If CONFIG_BTDM_CTRL_HLI is enabled, `xt_debugexception` is used to fix the live lock issue in ESP32 ECO3.

Using these symbols is done by creating an assembly file with suffix `.S` and defining the named symbols, like this:

        .section .iram1,"ax"
        .global     xt_highint4
        .type       xt_highint4,@function
        .align      4
    xt_highint5:
        ... your code here
        rsr     a0, EXCSAVE_5
        rfi     5

For a real-life example, see the esp_system/port/soc/esp32/highint_hdl.S file; the panic handler interrupt is implemented there.

## Notes

- Do not call C code from a high-priority interrupt; as these interrupts are run from a critical section, this can cause the target to crash. Note that although the panic handler interrupt does call normal C code, this exception is allowed due to the fact that this handler never returns (i.e., the application does not continue to run after the panic handler), so breaking C code execution flow is not a problem.

When CONFIG_BTDM_CTRL_HLI is enabled, C code is also called from a high-priority interrupt, this is possible thanks to some additional protection added to it.

- Make sure your assembly code gets linked in. Indeed, as the free-to-use symbols are declared as weak, the linker may discard the file containing the symbol. This happens if the only symbol defined, or used from the user file is the `xt_*` free-to-use symbol. To avoid this, in the assembly file containing the `xt_*` symbol, define another symbol, like:

    .global ld_include_my_isr_file
    ld_include_my_isr_file:

Here it is called `ld_include_my_isr_file` but can have any name, as long as it is not defined anywhere else in the project.

Then, in the component `CMakeLists.txt`, add this name as an unresolved symbol to the ld command line arguments:

    target_link_libraries(${COMPONENT_TARGET} "-u ld_include_my_isr_file")

This will ensure the linker to always includes the file defining `ld_include_my_isr_file`, so that the ISR is always linked.

- High-priority interrupts can be routed and handled using `esp_intr_alloc()` and associated functions. However, the handler and handler arguments to `esp_intr_alloc()` must be NULL.

- In theory, medium priority interrupts could also be handled in this way. ESP-IDF does not support this yet.

- To check Xtensa instruction set architecture (ISA), please refer to Xtensa ISA Summary.

See system/nmi_isr for an example of how to implement a custom NMI handler on Xtensa-based targets.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.