# Elliptic Curve Digital Signature Algorithm (ECDSA)

[中文]

The Elliptic Curve Digital Signature Algorithm (ECDSA) offers a variant of the Digital Signature Algorithm (DSA) which uses elliptic-curve cryptography.

ESP32-C61's ECDSA peripheral provides a secure and efficient environment for computing ECDSA signatures. It offers fast computations while ensuring the confidentiality of the signing process to prevent information leakage. ECDSA private key used in the signing process is accessible only to the hardware peripheral, and it is not readable by software.

ECDSA peripheral can help to establish Secure Device Identity for TLS mutual authentication and similar use-cases.

## Supported Features

- ECDSA digital signature generation and verification

- Two different elliptic curves, namely P-192 and P-256 (FIPS 186-3 specification)

- Two hash algorithms for message hash in the ECDSA operation, namely SHA-224 and SHA-256 (FIPS PUB 180-4 specification)

## ECDSA on ESP32-C61

On ESP32-C61, the ECDSA module works with a secret key burnt into an eFuse block.

This key is made completely inaccessible (default mode) for any resources outside the cryptographic modules, thus avoiding key leakage.

### ECDSA Key Storage

ECDSA private keys are stored in eFuse key blocks. One eFuse key block (256 bits) is required for P-256 curve.

Configure the following field:

- Set `esp_tls_cfg_t::ecdsa_key_efuse_blk` to the block number and leave `esp_tls_cfg_t::ecdsa_key_efuse_blk_high` as 0 or unassigned.

ECDSA key can be programmed externally through `idf.py` script. Here is an example of how to program the ECDSA key:

Using eFuses to store the ECDSA key:

    idf.py efuse-burn-key <BLOCK_NUM> </path/to/ecdsa_private_key.pem> ECDSA_KEY

Note

Six physical eFuse blocks can be used as keys for the ECDSA module: block 4 ~ block 9. E.g., for block 4 (which is the first key block) , the argument should be `BLOCK_KEY0`.

Alternatively the ECDSA key can also be programmed through the application running on the target.

Using eFuses to store the ECDSA key:

Following code snippet uses `esp_efuse_write_key()` to set physical key block 0 in the eFuse with key purpose as `esp_efuse_purpose_t::ESP_EFUSE_KEY_PURPOSE_ECDSA_KEY`:

    #include "esp_efuse.h"

    const uint8_t key_data[32] = { ... };

    esp_err_t status = esp_efuse_write_key(EFUSE_BLK_KEY0,
                        ESP_EFUSE_KEY_PURPOSE_ECDSA_KEY,
                        key_data, sizeof(key_data));

    if (status == ESP_OK) {
        // written key
    } else {
        // writing key failed, maybe written already
    }

## Deterministic Signature Generation

The ECDSA peripheral of ESP32-C61 also supports generation of deterministic signatures using deterministic derivation of the parameter K as specified in the RFC 6979 section 3.2.

## Non-Determinisitic Signature Generation

### Dependency on TRNG

ECDSA peripheral relies on the hardware True Random Number Generator (TRNG) for its internal entropy requirement for generating non-deterministic signatures. During ECDSA signature creation, the algorithm requires a random integer to be generated as specified in the RFC 6090 section 5.3.2.

Please ensure that hardware RNG is enabled before starting ECDSA computations (primarily signing) in the application.

## Application Outline

Please refer to the ECDSA Peripheral with ESP-TLS guide for details on how-to use ECDSA peripheral for establishing a mutually authenticated TLS connection.

The ECDSA peripheral in Mbed TLS stack is integrated by overriding the ECDSA signing and verifying APIs. Please note that, the ECDSA peripheral does not support all curves or hash algorithms, and hence for cases where the hardware requirements are not met, the implementation falls back to the software.

For a particular TLS context, additional APIs have been supplied to populate certain fields (e.g., private key ctx) to differentiate routing to hardware. ESP-TLS layer integrates these APIs internally and hence no additional work is required at the application layer. However, for custom use-cases please refer to API details below.

## API Reference

### Header File

- components/mbedtls/port/psa_driver/include/psa_crypto_driver_esp_ecdsa_contexts.h

- This header file can be included with:

  >     #include "psa_crypto_driver_esp_ecdsa_contexts.h"

- This header file is a part of the API provided by the `mbedtls` component. To declare that your component depends on `mbedtls`, add the following to your CMakeLists.txt:

  >     REQUIRES mbedtls

  > or

  >     PRIV_REQUIRES mbedtls

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.