# Peripherals

[中文]

## Common Changes

### Legacy Driver Dependencies Removal

The legacy driver component driver has been deprecated and no longer contains public dependencies on the following driver components:

- esp_driver_ana_cmpr

- esp_driver_dac

- esp_driver_gptimer

- esp_driver_i2s

- esp_driver_ledc

- esp_driver_mcpwm

- esp_driver_parlio

- esp_driver_pcnt

- esp_driver_rmt

- esp_driver_sdio

- esp_driver_sdm

- esp_driver_sdmmc

- esp_driver_sdspi

- esp_driver_spi

- esp_driver_tsens

- esp_driver_twai

- esp_driver_uart

- esp_driver_usb_serial_jtag

If your project uses legacy driver component, it is strongly recommended to remove driver component dependencies, and add new driver component (usually `esp_driver_xxx`) dependencies to your project.

If you still need to keep legacy driver component (e.g. your project depends on the legacy `i2c` driver), please keep the driver component remaining in the dependency list of your project (usually `<project_root>/main/CMakeLists.txt`), and manually add component dependencies that are no longer included in driver as needed.

### All drivers' `io_loop_back` configuration have been removed

Different driver objects can share the same GPIO number, enabling more complex functionalities. For example, you can bind the TX and RX channels of the RMT peripheral to the same GPIO to simulate 1-Wire bus read and write timing. In previous versions, you needed to configure the `io_loop_back` setting in the driver to achieve this "loopback" functionality. Now, this configuration has been removed. Simply configuring the same GPIO number in different drivers will achieve the same functionality.

### Peripheral Clock Gating

Peripheral clock gating is managed within the driver layer. Users do not need to manually handle peripheral module clock gating. Its corresponding APIs are included via a private header file `esp_private/periph_ctrl.h`. There used to be another header file `driver/periph_ctrl.h` for the same purpose, which is now removed.

### RTC Subsystem Control

Low power modules usually share some common resources like interrupt number. To avoid conflicts, some private APIs are created in the `esp_private/rtc_ctrl.h` header file to manage these shared resources with ease. There used to be another header file `driver/rtc_cntl.h` for the same purpose, which is now removed.

### Removal of FreeRTOS Dependencies from Driver Header Files

Starting from v6.0, to improve the portability of IDF drivers, all public driver header files no longer include operating-system–specific (FreeRTOS) headers. Therefore, application code that previously relied on this implicit inclusion must explicitly include the corresponding FreeRTOS headers when using v6.0 or later.

## ADC

The legacy ADC driver `driver/adc.h` is deprecated since version 5.0 (see ADC). Starting from version 6.0, the legacy driver is completely removed. The new driver is placed in the esp_adc, and the header file path is `esp_adc/adc_oneshot.h`, `esp_adc/adc_continuous.h`, `esp_adc/adc_cali.h` and `esp_adc/adc_cali_scheme.h`.

## RMT

The `io_od_mode` member in the `rmt_tx_channel_config_t` configuration structure has been removed. If you want to use open-drain mode, you need to manually call the `gpio_od_enable()` function.

## MCPWM

The `io_od_mode` member in the `mcpwm_generator_config_t` configuration structure has been removed. If you want to use open-drain mode, you need to manually call the `gpio_od_enable()` function.

The `pull_up` and `pull_down` members have been removed from the following configuration structures. You need to manually call the `gpio_set_pull_mode()` function to configure the pull-up and pull-down resistors for the IO:

- `mcpwm_generator_config_t`

- `mcpwm_gpio_fault_config_t`

- `mcpwm_gpio_sync_src_config_t`

- `mcpwm_capture_channel_config_t`

The default MCPWM group clock divider has been changed to 1. This allows you to obtain a higher default resolution.

### Legacy MCPWM Driver is Removed

The legacy MCPWM driver `driver/mcpwm.h` is deprecated since version 5.0 (see Legacy MCPWM Driver is Deprecated). Starting from version 6.0, the legacy driver is completely removed. The new driver is placed in the esp_driver_mcpwm, and the header file path is `driver/mcpwm_prelude`.

### Variadic Generator APIs are Removed

The legacy variadic ("varg") generator APIs have been removed in this release. Code that used vararg-style calls for generator action setup must be migrated to the explicit, typed APIs. These APIs use configuration structs and clearly-typed setter functions (for example, `mcpwm_generator_config_t`, `mcpwm_gen_timer_event_action_t` and `mcpwm_generator_set_action_on_timer_event`).

Migration steps (summary):

- Replace varg-style action configuration with helper structs/macros and dedicated setter functions:

      .. code-block:: c

          /* Old (varg) */
          mcpwm_generator_set_actions_on_compare_event(my_generator,
              MCPWM_GEN_COMPARE_EVENT_ACTION(MCPWM_TIMER_DIRECTION_UP, my_comparator, MCPWM_GEN_ACTION_LOW),
              MCPWM_GEN_COMPARE_EVENT_ACTION(MCPWM_TIMER_DIRECTION_DOWN, my_comparator, MCPWM_GEN_ACTION_HIGH),
              MCPWM_GEN_COMPARE_EVENT_ACTION_END());

          /* New */
          mcpwm_generator_set_action_on_compare_event(my_generator,
              MCPWM_GEN_COMPARE_EVENT_ACTION(MCPWM_TIMER_DIRECTION_UP, my_comparator, MCPWM_GEN_ACTION_LOW));
          mcpwm_generator_set_action_on_compare_event(my_generator,
              MCPWM_GEN_COMPARE_EVENT_ACTION(MCPWM_TIMER_DIRECTION_DOWN, my_comparator, MCPWM_GEN_ACTION_HIGH));

## GPIO

- `gpio_iomux_in()` and `gpio_iomux_out()` have been replaced by `gpio_iomux_input()` and `gpio_iomux_output()`, and have been moved to `esp_private/gpio.h` header file as private APIs for internal use only.

- `rom_` prefix has been added to all GPIO ROM APIs in `components/esp_rom/esp32xx/include/esp32xx/rom/gpio.h`. For example, `gpio_iomux_in()` is now `rom_gpio_iomux_in()`.

- `MAX_PAD_GPIO_NUM`, `MAX_GPIO_NUM`, and `DIG_IO_HOLD_BIT_SHIFT` macros have been removed.

- Added the `esp_err_t` return type to `gpio_uninstall_isr_service()`.

### GPIO Deep Sleep Wakeup APIs Removed

The following GPIO driver APIs have been removed:

- `gpio_deep_sleep_wakeup_enable()` - Use `gpio_wakeup_enable_on_hp_periph_powerdown_sleep()` instead

- `gpio_deep_sleep_wakeup_disable()` - Use `gpio_wakeup_disable_on_hp_periph_powerdown_sleep()` instead

The deprecated macro `GPIO_IS_DEEP_SLEEP_WAKEUP_VALID_GPIO()` has been removed. Use `GPIO_IS_HP_PERIPH_PD_WAKEUP_VALID_IO()` instead.

Migration Example:

Old code:

    #include "driver/gpio.h"

    // Enable GPIO wakeup
    gpio_deep_sleep_wakeup_enable(GPIO_NUM_0, GPIO_INTR_LOW_LEVEL);

    // Check validity
    if (GPIO_IS_DEEP_SLEEP_WAKEUP_VALID_GPIO(GPIO_NUM_0)) {
        // ...
    }

New code:

    #include "driver/gpio.h"

    // Enable GPIO wakeup (works for both deep sleep and light sleep with peripheral powerdown)
    gpio_wakeup_enable_on_hp_periph_powerdown_sleep(GPIO_NUM_0, GPIO_INTR_LOW_LEVEL);

    // Check validity
    if (GPIO_IS_HP_PERIPH_PD_WAKEUP_VALID_IO(GPIO_NUM_0)) {
        // ...
    }

For more details, see the GPIO Wakeup API Changes section in the System migration guide.

## LEDC

- `ledc_timer_set()` has been removed. Use `ledc_timer_config()` or `ledc_set_freq()` instead.

- `LEDC_APB_CLK_HZ` and `LEDC_REF_CLK_HZ` have been removed.

- `LEDC_SLOW_CLK_RTC8M` macro has been removed. Please use `LEDC_SLOW_CLK_RC_FAST` instead.

- Removed esp_driver_gpio as a public required component from esp_driver_ledc.

- `ledc_isr_register()` has been deprecated. LEDC interrupt handling is implemented by driver itself, please only register event callbacks if necessary.

- `ledc_channel_config_t::intr_type` has been deprecated. LEDC_INTR_FADE_END interrupt enable / disable control is handled by the driver internally. Users can still register a callback for this interrupt by `ledc_cb_register()`.

- `soc_periph_ledc_clk_src_legacy_t::LEDC_USE_RTC8M_CLK` has been removed. Please use `LEDC_USE_RC_FAST_CLK` instead.

## UART

- `UART_FIFO_LEN` macro has been removed. Please use `UART_HW_FIFO_LEN` instead.

- `soc/uart_channel.h` header file has been removed. All UART GPIO lookup macros can be found in `soc/uart_pins.h`. For example, `UART_NUM_0_TXD_DIRECT_GPIO_NUM` is equivalent to `U0TXD_GPIO_NUM`.

## I2C

### Legacy I2C Driver End-of-Life

Warning

The legacy I2C driver (`driver/i2c.h`) has been marked as End-of-Life (EOL) in ESP-IDF v6.0 and is scheduled for removal in v7.0.

- ESP-IDF will not provide updates, bug fixes, or security patches for the legacy driver timely.

- Users are strongly recommended to migrate to the new I2C drivers: `driver/i2c_master.h` and `driver/i2c_slave.h`.

- To temporarily suppress the compile-time warning, enable `Component config` > `Legacy Driver Configurations` > `Legacy I2C Driver Configurations` > `Suppress legacy driver deprecated warning` in menuconfig.

The new I2C drivers provide improved slave and master functionality. For details, please refer to the I2C Migration Guide and the I2C Driver Programming Guide.

### I2C Slave Driver Updates

The I2C slave driver has been redesigned in v5.4. In the current version, the old I2C slave driver has been removed.

#### Major Changes in Concepts

- Previously, the I2C slave driver performed active read and write operations. In the new version, these operations are handled passively via callbacks triggered by master events, aligning with standard I2C slave behavior.

#### Major Changes in Usage

- `i2c_slave_receive` has been removed. In the new driver, data reception is handled via callbacks.

- `i2c_slave_transmit` has been replaced by `i2c_slave_write`.

- `i2c_slave_write_ram` has been removed.

- `i2c_slave_read_ram` has been removed.

### I2C Master Driver Updates

The I2C master driver also has some changes in its API definitions.

#### Major Changes in Usage

Following functions now will return `ESP_ERR_INVALID_RESPONSE` instead of `ESP_ERR_INVALID_STATE` when NACK from the bus is detected:

- `i2c_master_transmit`

- `i2c_master_multi_buffer_transmit`

- `i2c_master_transmit_receive`

- `i2c_master_execute_defined_operations`

## Legacy Timer Group Driver is Removed

The legacy timer group driver `driver/timer.h` is deprecated since version 5.0 (see Legacy Timer Group Driver is Deprecated). Starting from version 6.0, the legacy driver is completely removed. The new driver is placed in the esp_driver_gptimer, and the header file path is `driver/gptimer.h`.

## Legacy I2S Driver is Removed

- The legacy i2s driver `driver/i2s.h` is deprecated since version 5.0 (see I2S Driver). Starting from version 6.0, the legacy driver is completely removed. The new driver is placed in the esp_driver_i2s, and the header file path is `driver/i2s_std.h`, `driver/i2s_pdm.h` and `driver/i2s_tdm.h`.

- API `i2s_set_adc_mode`, `i2s_adc_enable` and `i2s_adc_disable` are deprecated since version 5.0. Starting from version 6.0, these APIs are completely removed.

## Legacy PCNT Driver is Removed

The legacy PCNT driver `driver/pcnt.h` is deprecated since version 5.0 (see Legacy PCNT Driver is Deprecated). Starting from version 6.0, the legacy driver is completely removed. The new driver is placed in the esp_driver_pcnt, and the header file path is `driver/pulse_cnt.h`.

## Legacy RMT Driver is Removed

The legacy RMT driver `driver/rmt.h` is deprecated since version 5.0 (see Legacy RMT Driver is Deprecated). Starting from version 6.0, the legacy driver is completely removed. The new driver is placed in the esp_driver_rmt, and the header file path is `driver/rmt_tx.h`, `driver/rmt_rx.h` and `driver/rmt_encoder.h`.

## DMA Driver

- The DMA core driver has been moved out of the original `esp_hw_support` component and is now provided as a separate `esp_driver_dma` component. If you are using the `esp_async_memcpy.h` and `esp_dma_utils.h` drivers, please ensure that you add a dependency on the `esp_driver_dma` component in your project.

- The `GDMA_ISR_IRAM_SAFE` Kconfig option has been removed due to potential risks. Now, the interrupt behavior of different DMA channels during Cache disabled periods are independent of each other.

- `gdma_new_channel` is removed. When requesting a GDMA channel, use either `gdma_new_ahb_channel` or `gdma_new_axi_channel` according to the bus type.

- The `sram_trans_align` and `psram_trans_align` members have been removed from `async_memcpy_config_t`. Use `async_memcpy_config_t::dma_burst_size` to set the DMA burst transfer size.

- The `esp_dma_capable_malloc` and `esp_dma_capable_calloc` functions have been removed. Use `heap_caps_malloc()` and `heap_caps_calloc()` from heap/include/esp_heap_caps.h with `MALLOC_CAP_DMA|MALLOC_CAP_CACHE_ALIGNED` to allocate memory suitable for DMA and cache alignment.

## SDMMC

- The `get_dma_info` member in the `sdmmc_host_t` structure, as well as the `sdspi_host_get_dma_info` and `sdmmc_host_get_dma_info` functions, have been removed. DMA configuration is now handled internally by the driver.

## Legacy Temperature Sensor Driver is Removed

The legacy temperature sensor driver `driver/temp_sensor.h` is deprecated since version 5.0 (see Legacy Temperature Sensor Driver is Deprecated). Starting from version 6.0, the legacy driver is completely removed. The new driver is placed in the esp_driver_tsens, and the header file path is `driver/temperature_sensor.h`.

## Legacy Sigma-Delta Modulator Driver is Removed

The legacy Sigma-Delta Modulator driver `driver/sigmadelta.h` is deprecated since version 5.0 (see Legacy Sigma-Delta Modulator Driver is Deprecated). Starting from version 6.0, the legacy driver is completely removed. The new driver is placed in the esp_driver_sdm, and the header file path is `driver/sdm.h`.

- `sdm_channel_set_duty()` has been removed. Use `sdm_channel_set_pulse_density()` instead.

## LCD

- The GPIO number type in the LCD driver has been changed from `int` to the more type-safe `gpio_num_t`. For example, instead of using `5` as the GPIO number, you now need to use `GPIO_NUM_5`.

- The `psram_trans_align` and `sram_trans_align` members in the `esp_lcd_i80_bus_config_t` structure have been replaced by the `esp_lcd_i80_bus_config_t::dma_burst_size` member, which sets the DMA burst transfer size.

- The `psram_trans_align` and `sram_trans_align` members in the `esp_lcd_rgb_panel_config_t` structure have also been replaced by the `esp_lcd_rgb_panel_config_t::dma_burst_size` member for configuring the DMA burst transfer size.

- The `color_space` and `rgb_endian` configuration options in the `esp_lcd_panel_dev_config_t` structure have been replaced by the `esp_lcd_panel_dev_config_t::rgb_ele_order` member, which sets the RGB element order. The corresponding types `lcd_color_rgb_endian_t` and `esp_lcd_color_space_t` have also been removed; use `lcd_rgb_element_order_t` instead.

- The `esp_lcd_panel_disp_off` function has been removed. Please use the `esp_lcd_panel_disp_on_off()` function to control display on/off.

- The `on_bounce_frame_finish` member in `esp_lcd_rgb_panel_event_callbacks_t` has been replaced by `esp_lcd_rgb_panel_event_callbacks_t::on_frame_buf_complete`, which indicates that a complete frame buffer has been sent to the LCD controller.

- The LCD IO layer driver for the I2C interface previously had two implementations, based on the new and legacy I2C master bus drivers. As the legacy I2C driver is being deprecated, support for it in the LCD IO layer has been removed. Only the APIs provided in `driver/i2c_master.h` are now used.

- `pixel_format` member in the `esp_lcd_dpi_panel_config_t` structure has been removed. It is recommended to only use `esp_lcd_dpi_panel_config_t::in_color_format` to set the MIPI DSI driver's input pixel data format.

- `bits_per_pixel` member in the `esp_lcd_rgb_panel_config_t` structure has been removed. The color depth of the internal framebuffer is now determined by the `esp_lcd_rgb_panel_config_t::in_color_format` member.

- `esp_lcd_dpi_panel_set_color_conversion` function is replaced by `esp_lcd_dpi_panel_set_yuv_conversion()` to set YUV to RGB color conversion profile.

- `esp_lcd_rgb_panel_set_yuv_conversion()` function has a different signature. The `esp_lcd_yuv_conv_config_t` configuration type is now replaced by `esp_lcd_color_conv_yuv_config_t`.

- The NT35510 LCD device driver has been moved out of ESP-IDF and is now hosted in the ESP Component Registry. If your project uses the NT35510 driver, you can add it to your project by running `idf.py add-dependency "espressif/esp_lcd_nt35510"`.

- The `use_dma2d` member in the `esp_lcd_dpi_panel_config_t` has been removed. Please use the `esp_lcd_dpi_panel_enable_dma2d()` function to enable DMA2D for the DPI panel. When not using DMA2D, the binary file size can be reduced by around 10KB.

## Color Types

The following types in the `components/hal/include/hal/color_types.h` header file have been removed. Please use FourCC format (`esp_color_fourcc_t`) instead:

- `color_space_t` - The color space enumeration type has been removed. Please use FourCC format to specify color space and pixel format.

- `color_space_pixel_format_t` - The color space pixel format union has been removed. Please use `esp_color_fourcc_t` type and corresponding FourCC macro definitions to specify pixel format.

Migration example:

    /* Old */
    color_space_pixel_format_t format = {
        .color_space = COLOR_SPACE_RGB,
        .pixel_format = COLOR_PIXEL_RGB565
    };

    /* New */
    esp_color_fourcc_t format = ESP_COLOR_FOURCC_RGB565;

## SPI

- The CONFIG_SPI_MASTER_IN_IRAM option is now invisible by default in menuconfig and depends on CONFIG_FREERTOS_IN_IRAM. This change was made to prevent potential crashes when SPI functions in IRAM call FreeRTOS functions that are placed in flash.

- To enable SPI master IRAM optimization:

  > 1. Navigate to `Component config` → `FreeRTOS` → `Port` in menuconfig.

  > 2. Enable `Place FreeRTOS functions in IRAM` (CONFIG_FREERTOS_IN_IRAM).

  > 3. Navigate to `Component config` → `ESP-Driver:SPI Configurations` in menuconfig.

  > 4. Enable `Place transmitting functions of SPI master into IRAM` (CONFIG_SPI_MASTER_IN_IRAM).

  > Note

  > Note that enabling CONFIG_FREERTOS_IN_IRAM will increase IRAM usage. Consider this trade-off when optimizing for SPI performance.

- Deprecated HSPI and VSPI related IOMUX pin macros on ESP32 and ESP32S2 have been removed.

## PSRAM

Deprecated header file `esp_spiram.h` has been removed. Please use `esp_psram.h` instead.

## SPI Flash Driver

- Deprecated `enum` type `esp_flash_speed_t` has been removed. The main flash speed is controlled by CONFIG_ESPTOOLPY_FLASHFREQ option.

- Deprecated header file `esp_spi_flash.h` has been removed. Please use `spi_flash_mmap.h` instead.

- Deprecated API `spi_flash_dump_counters` has been removed. Please use `esp_flash_dump_counters()` instead.

- Deprecated API `spi_flash_get_counters` has been removed. Please use `esp_flash_get_counters()` instead.

- Deprecated API `spi_flash_reset_counters` has been removed. Please use `esp_flash_reset_counters()` instead.

- New argument `flags` is added to `esp_flash_os_functions_t::start`. Caller and implementer should handle this argument properly.

- Kconfig option `CONFIG_SPI_FLASH_ROM_DRIVER_PATCH` has been removed. Considering that this option is unlikely to be widely used by users and may cause serious issues if misused, it has been decided to remove it.

### Header File Reorganization

Several internal header files have been reorganized to better reflect their visibility and intended usage:

- Flash chip driver related headers have been moved to `esp_flash_chips/` directory: - `spi_flash_chip_driver.h` - `spi_flash_chip_*.h` - `spi_flash_defs.h` - `spi_flash_override.h` - `esp_flash_types.h` - The `esp_flash_t` structure definition has been moved from `esp_flash.h` to `esp_flash_chips/esp_flash_types.h`. Applications should not access structure members directly; use the public APIs instead (e.g., use `esp_flash_get_size()` instead of accessing `chip->size` directly). - The `esp_flash_os_functions_t` structure definition has been moved from `esp_flash.h` to `esp_flash_chips/esp_flash_types.h`. - The `spi_flash_chip_t` type forward declaration has been removed from `esp_flash.h` and all ROM headers (`components/esp_rom/esp32xx/include/esp32xx/rom/esp_flash.h`). The type is now only defined in `esp_flash_chips/esp_flash_types.h`. Applications should not use this type directly; it is only intended for custom chip driver implementations.

  Note

  The headers in `esp_flash_chips/` are semi-public - they are intended for expert users who need to implement custom chip drivers for unsupported flash chips, but they are not considered stable API and may change without notice. For most use cases, you should use the public APIs in `esp_flash.h` instead. See Override Driver for SPI Flash for more details.

- Internal headers have been moved to `esp_private/` directory and not included in the public (stable) header files: - `esp_flash_internal.h` - `memspi_host_driver.h`

## Touch Element

The `touch_element` component is moved to ESP Component Registry.

You can add this dependency to your project by running `idf.py add-dependency "espressif/touch_element"`.

## Touch Sensor

The `touch_sensor_sample_config_t::bypass_shield_output` member for version 3 touch sensor has been removed because it is not supported in the version 3 hardware.

The dependencies of legacy touch sensor driver are removed from ULP touch driver, now you need to use `int` instead of `touch_pad_t` to indicate the touch channel ID.

## I2S

- `i2s_port_t` type has been removed. Please use `int` type instead. Its enum items `I2S_NUM_0`, `I2S_NUM_1`, `I2S_NUM_2` and `I2S_NUM_AUTO` have been replaced by macro definitions to ensure compatibility.

## USB

The `usb` component has been moved to ESP Component Registry.

You can add this dependency to your project by running `idf.py add-dependency "espressif/usb"`.

## TWAI

TWAI has provided a new driver interface in version 5.5, which supports more flexible configurations and richer features. The legacy driver is not recommended to be used anymore. Please refer to the 5.5 migration guide TWAI migration guide and the new driver programming guide TWAI driver programming guide for migration.

If you still need to use the legacy driver, you can enable the configuration option CONFIG_TWAI_SUPPRESS_DEPRECATE_WARN to close the deprecation warnings.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.