# ULP LP Core Coprocessor Programming

[中文]

The ULP LP core (Low-power core) coprocessor is a variant of the ULP present in ESP32-P4. It features ultra-low power consumption while also being able to stay powered on while the main CPU stays in low-power modes. This enables the LP core coprocessor to handle tasks like GPIO or sensor readings while the main CPU is in sleep mode, resulting in significant overall power savings for the entire system.

The ULP LP core coprocessor has the following features:

- An RV32I (32-bit RISC-V ISA) processor, with the multiplication/division (M), atomic (A), and compressed (C) extensions.

- Interrupt controller.

- Includes a debug module that supports external debugging via JTAG.

- Can access all of the High-power (HP) SRAM and peripherals when the entire system is active.

- Can access the Low-power (LP) SRAM and peripherals when the HP system is in sleep mode.

## Compiling Code for the ULP LP Core

The ULP LP core code is compiled together with your ESP-IDF project as a separate binary and automatically embedded into the main project binary. There are two ways to achieve this:

### Using `ulp_embed_binary`

1. Place the ULP LP core code, written in C or assembly (with the `.S` extension), in a dedicated directory within the component directory, such as `ulp/`.

2. After registering the component in the `CMakeLists.txt` file, call the `ulp_embed_binary` function. Here is an example:

    idf_component_register()

    set(ulp_app_name ulp_${COMPONENT_NAME})
    set(ulp_sources "ulp/ulp_c_source_file.c" "ulp/ulp_assembly_source_file.S")
    set(ulp_exp_dep_srcs "ulp_c_source_file.c")

    ulp_embed_binary(${ulp_app_name} "${ulp_sources}" "${ulp_exp_dep_srcs}")

The first argument to `ulp_embed_binary` specifies the ULP binary name. The name specified here is also used by other generated artifacts such as the ELF file, map file, header file, and linker export file. The second argument specifies the ULP source files. Finally, the third argument specifies the list of component source files which include the header file to be generated. This list is needed to build the dependencies correctly and ensure that the generated header file is created before any of these files are compiled. See the section below for the concept of generated header files for ULP applications.

Variables in the ULP code will be prefixed with `ulp_` (default value) in this generated header file.

If you need to embed multiple ULP programs, you may add a custom prefix in order to avoid conflicting variable names like this:

    idf_component_register()

    set(ulp_app_name ulp_${COMPONENT_NAME})
    set(ulp_sources "ulp/ulp_c_source_file.c" "ulp/ulp_assembly_source_file.S")
    set(ulp_exp_dep_srcs "ulp_c_source_file.c")

    ulp_embed_binary(${ulp_app_name} "${ulp_sources}" "${ulp_exp_dep_srcs}" PREFIX "ULP::")

The additional PREFIX argument can be a C style prefix (like `ulp2_`) or a C++ style prefix (like `ULP::`).

### Using a Custom CMake Project

It is also possible to create a custom CMake project for the LP core. This gives more control over the build process and allows you to set compile options, link external libraries and all other things that are possible with a regular CMake project.

To do this, add the ULP project as an external project in your component `CMakeLists.txt` file:

    ulp_add_project("ULP_APP_NAME" "${CMAKE_SOURCE_DIR}/PATH_TO_DIR_WITH_ULP_PROJECT_FILE/")

Create a folder which contains your ULP project files and a `CMakeLists.txt` file, located at the path given to `ulp_add_project`. The `CMakeLists.txt` file should look like this:

    cmake_minimum_required(VERSION 3.22)

    # Project/target name is passed from the main project to allow IDF to have a dependency on this target
    # as well as embed the binary into the main app
    project(${ULP_APP_NAME})
    add_executable(${ULP_APP_NAME} main.c)

    # Import the ULP project helper functions
    include(IDFULPProject)

    # Apply default compile options
    ulp_apply_default_options(${ULP_APP_NAME})

    # Apply default sources provided by the IDF ULP component
    ulp_apply_default_sources(${ULP_APP_NAME})

    # Add targets for building the binary, as well as the linkerscript which exports ULP shared variables to the main app
    ulp_add_build_binary_targets(${ULP_APP_NAME})

    # Everything below this line is optional and can be used to customize the build process

    # Create a custom library
    set(lib_path "${CMAKE_CURRENT_LIST_DIR}/lib")
    add_library(custom_lib STATIC "${lib_path}/lib_src.c")
    target_include_directories(custom_lib PUBLIC "${lib_path}/")

    # Link the library
    target_link_libraries(${ULP_APP_NAME} PRIVATE custom_lib)

    # Set custom compile flags
    target_compile_options(${ULP_APP_NAME} PRIVATE -msave-restore)

### Building Your Project

To compile and build your project:

1. Enable both CONFIG_ULP_COPROC_ENABLED and CONFIG_ULP_COPROC_TYPE in menuconfig, and set CONFIG_ULP_COPROC_TYPE to `CONFIG_ULP_COPROC_TYPE_LP_CORE`. The CONFIG_ULP_COPROC_RESERVE_MEM option reserves RTC memory for the ULP, and must be set to a value big enough to store both the ULP LP core code and data. If the application components contain multiple ULP programs, then the size of the RTC memory must be sufficient to hold the largest one.

2. Build the application as usual (e.g., `idf.py app`).

During the build process, the following steps are taken to build ULP program:

> 1. Run each source file through the C compiler and assembler. This step generates the object files `.obj.c` or `.obj.S` in the component build directory depending on the source file processed.

> 2. Run the linker script template through the C preprocessor. The template is located in `components/ulp/ld` directory.

> 3. Link the object files into an output ELF file (`ulp_app_name.elf`). The Map file `ulp_app_name.map` generated at this stage may be useful for debugging purposes.

> 4. Dump the contents of the ELF file into a binary (`ulp_app_name.bin`) which can then be embedded into the application.

> 5. Generate a list of global symbols (`ulp_app_name.sym`) in the ELF file using `riscv32-esp-elf-nm`.

> 6. Create an LD export script and a header file `ulp_app_name.ld` and `ulp_app_name.h` containing the symbols from `ulp_app_name.sym`. This is done using the `esp32ulp_mapgen.py` utility.

> 7. Add the generated binary to the list of binary files to be embedded into the application.

## Accessing the ULP LP Core Program Variables

Global symbols defined in the ULP LP core program may be used inside the main program.

For example, the ULP LP core program may define a variable `measurement_count` which defines the number of GPIO measurements the program needs to make before waking up the chip from Deep-sleep.

    volatile int measurement_count;

    int some_function()
    {
        //read the measurement count for later use.
        int temp = measurement_count;

        ...do something.
    }

The main program can access the global ULP LP core program variables as the build system makes this possible by generating the `${ULP_APP_NAME}.h` and `${ULP_APP_NAME}.ld` files which define the global symbols present in the ULP LP core program. Each global symbol defined in the ULP LP core program is included in these files and are prefixed with `ulp_`.

The header file contains the declaration of the symbol:

    extern uint32_t ulp_measurement_count;

Note that all symbols (variables, functions) are declared as `uint32_t`. Arrays are declared as `uint32_t [SIZE]`. For functions, take the address of the symbol and cast it to the appropriate type.

To access the ULP LP core program variables from the main program, the generated header file should be included using an `include` statement. This allows the ULP LP core program variables to be accessed as regular variables.

    #include "ulp_app_name.h"

    void init_ulp_vars() {
        ulp_measurement_count = 64;
    }

Note

- Variables declared in the global scope of the LP core program reside in either the `.bss` or `.data` section of the binary. These sections are initialized when the LP core binary is loaded and executed. Accessing these variables from the main program on the HP-Core before the first LP core run may result in undefined behavior.

- The `ulp_` prefix is the default value. You can specify the prefix to use with `ulp_embed_binary` to avoid name collisions for multiple ULP programs.

## Starting the ULP LP Core Program

To run a ULP LP core program, the main application needs to load the ULP program into RTC memory using the `ulp_lp_core_load_binary()` function, and then start it using the `ulp_lp_core_run()` function.

Each ULP LP core program is embedded into the ESP-IDF application as a binary blob. The application can reference this blob and load it in the following way (supposed ULP_APP_NAME was defined to `ulp_app_name`):

    extern const uint8_t bin_start[] asm("_binary_ulp_app_name_bin_start");
    extern const uint8_t bin_end[]   asm("_binary_ulp_app_name_bin_end");

    void start_ulp_program() {
        ESP_ERROR_CHECK( ulp_lp_core_load_binary( bin_start,
            (bin_end - bin_start)) );
    }

Once the program is loaded into LP memory, the application can be configured and started by calling `ulp_lp_core_run()`:

    ulp_lp_core_cfg_t cfg = {
        .wakeup_source = ULP_LP_CORE_WAKEUP_SOURCE_LP_TIMER, // LP core will be woken up periodically by LP timer
        .lp_timer_sleep_duration_us = 10000,
    };

    ESP_ERROR_CHECK( ulp_lp_core_run(&cfg) );

## ULP LP Core Program Flow

How the ULP LP core coprocessor is started depends on the wake-up source selected in `ulp_lp_core_cfg_t`. The most common use-case is for the ULP to periodically wake up, do some measurements before either waking up the main CPU or going back to sleep again.

The ULP has the following wake-up sources:

  - `ULP_LP_CORE_WAKEUP_SOURCE_HP_CPU` - LP core can be woken up by the HP CPU.

  - `ULP_LP_CORE_WAKEUP_SOURCE_LP_TIMER` - LP core can be woken up by the LP timer.

  - `ULP_LP_CORE_WAKEUP_SOURCE_ETM` - LP core can be woken up by an ETM event.

  - `ULP_LP_CORE_WAKEUP_SOURCE_LP_IO` - LP core can be woken up when LP IO level changes.

  - `ULP_LP_CORE_WAKEUP_SOURCE_LP_UART` - LP core can be woken up when LP UART receives wakeup data based on different modes.

When the ULP is woken up, it will go through the following steps:

1. Unless `ulp_lp_core_cfg_t::skip_lp_rom_boot` is specified, run ROM start-up code and jump to the entry point in LP RAM. ROM start-up code will initialize LP UART as well as print boot messages.

2. Initialize system feature, e.g., interrupts

3. Call user code `main()`

4. Return from `main()`

5. If `lp_timer_sleep_duration_us` is specified, then configure the next wake-up alarm

6. Call `ulp_lp_core_halt()`

## ULP LP Core Peripheral Support

To enhance the capabilities of the ULP LP core coprocessor, it has access to peripherals that operate in the low-power domain. The ULP LP core coprocessor can interact with these peripherals when the main CPU is in sleep mode, and can wake up the main CPU once a wake-up condition is reached. The following peripherals are supported:

- LP IO

- LP I2C

- LP UART

- LP SPI

- LP Mailbox

## ULP LP Core ROM

The ULP LP core ROM is a small pre-built piece of code located in LP-ROM, which can't be modified. Similar to the bootloader ROM code ran by the main CPU, this code is executed when the ULP LP core coprocessor is started. The ROM code initializes the ULP LP core coprocessor and then jumps to the user program. The ROM code also prints boot messages if the LP UART has been initialized.

The ROM code is not executed if `ulp_lp_core_cfg_t::skip_lp_rom_boot` is set to true. This is useful when you need the ULP to wake-up as quickly as possible and the extra overhead of initializing and printing is unwanted.

In addition to the boot-up code mentioned above, the ROM code also provides the following functions and interfaces:

- ROM.ld Interface

- newlib.ld Interface

Since these functions are already present in LP-ROM no matter what, using these in your program allows you to reduce the RAM footprint of your ULP application.

## ULP LP Core Interrupts

The LP core coprocessor can be configured to handle interrupts from various sources. Examples of such interrupts could be LP IO low/high or LP timer interrupts. To register a handler for an interrupt, simply override any of the weak handlers provided by IDF. A complete list of handlers can be found in ulp_lp_core_interrupts.h . For details on which interrupts are available on a specific target, please consult ESP32-P4 Technical Reference Manual [PDF].

For example, to override the handler for the LP IO interrupt, you can define the following function in your ULP LP core code:

    void LP_CORE_ISR_ATTR ulp_lp_core_lp_io_intr_handler(void)
    {
        // Handle the interrupt and clear the interrupt source
    }

`LP_CORE_ISR_ATTR` is a macro that is used to define the interrupt handler function. This macro ensures that registers are saved and restored correctly when the interrupt handler is called.

In addition to configuring the interrupt related registers for the interrupt source you want to handle, you also need to enable the interrupts globally in the LP core interrupt controller. This can be done using the `ulp_lp_core_intr_enable()` function.

## ULP LP Core Clock Configuration

The ULP LP Core clock source is based on the system clock `LP_FAST_CLK`, see TRM > `Reset and Clock` for more details.

On ESP32-P4, `LP_FAST_CLK` supports using the external 40 MHz crystal (XTAL) as its clock source. This allows the ULP LP Core to run at a higher frequency than with the default `RTC_FAST_CLOCK`, which runs at around 20 MHz. However, there is a trade-off: this clock is normally powered down during sleep to reduce power consumption, but if XTAL is selected as the source, it will remain powered up during sleep, which increases power consumption. If you only plan to use the LP Core as a coprocessor while the HP Core is active, then selecting XTAL can enhance both the performance and frequency stability of the LP Core.

To enable this feature, set CONFIG_RTC_FAST_CLK_SRC to `CONFIG_RTC_FAST_CLK_SRC_XTAL`.

## Debugging ULP LP-Core Applications

When programming the LP core, it can sometimes be challenging to figure out why the program is not behaving as expected. Here are some strategies to help you debug your LP core program:

- Use the LP UART to print: the LP core has access to the LP UART peripheral, which can be used for printing information independently of the main CPU sleep state. See system/ulp/lp_core/lp_uart/lp_uart_print for an example of how to use this driver.

- Routing `lp_core_printf()` to the HP-Core console UART with CONFIG_ULP_HP_UART_CONSOLE_PRINT. This allows you to easily print LP core information to the already connected HP-Core console UART. The drawback of this approach is that it requires the main CPU to be awake and since there is no synchronization between the LP and HP cores, the output may be interleaved.

- Share program state through shared variables: as described in Accessing the ULP LP Core Program Variables, both the main CPU and the ULP core can easily access global variables in RTC memory. Writing state information to such a variable from the ULP and reading it from the main CPU can help you discern what is happening on the ULP core. The downside of this approach is that it requires the main CPU to be awake, which will not always be the case. Keeping the main CPU awake might even, in some cases, mask problems, as some issues may only occur when certain power domains are powered down.

- Panic handler: the LP core has a panic handler that can dump the state of the LP core registers by the LP UART when an exception is detected. To enable the panic handler, set the CONFIG_ULP_PANIC_OUTPUT_ENABLE option to `y`. This option can be kept disabled to reduce LP-RAM usage by the LP core application. To recover a backtrace from the panic dump, it is possible to use `idf.py monitor`.

Warning

If multiple ULP applications are used in a single project, backtrace decoding might not work correctly. In such cases, it is recommended to use the esp-idf-monitor tool directly with the correct ULP ELF file:

    python -m esp_idf_monitor --toolchain-prefix riscv32-esp-elf- --target esp32p4 --decode-panic backtrace PATH_TO_ULP_ELF_FILE

## Debugging ULP LP Core Applications with GDB and OpenOCD

It is also possible to debug code running on LP core using GDB and OpenOCD as you usually do for HP cores, but it has some specifics and limitations.

### Debugging Session

Run OpenOCD with special config file for LP core debugging support. And then run GDB with special `gdbinit` file.

    openocd -f board/esp32p4-lpcore-builtin.cfg
    riscv32-esp-elf-gdb -x gdbinit <path to main program ELF>

Below is the `gdbinit` file content with inline comments. For more details, see the next section.

    # connect to target
    target extended-remote :3333
    # reset chip
    mon reset halt
    maintenance flush register-cache
    # add symbols and debugging info for ULP program
    add-symbol <path to ULP program ELF>
    # temporary HW breakpoint to setup breakpoints
    # if you need more than HW supports
    thb main
    commands
    # set breakpoints here
    # At this moment ULP program is loaded into RAM and when there are
    # no free HW breakpoints slots available GDB will set SW ones
    b func1
    b func2
    b func3
    # resume execution
    c
    end
    # start main program after reset
    c

### LP Core Debugging Specifics

1. For convenient debugging, you may need to add `-O0` compile option for ULP app in its `CMakeLists.txt`. See system/ulp/lp_core/debugging/ on how to do this.

2. To be able to debug program running on LP core, debugging information and symbols need to be loaded to GDB. It can be done via GDB command line or in `gdbinit` file. See section above.

3. Upon startup, LP core application is loaded into RAM, so all SW breakpoints set before that moment will get overwritten. The best moment to set breakpoints for LP core application is to do this when LP core program reaches main function.

4. When using IDEs, it may lack support for configuring breakpoint actions or commands shown in `gdbinit` above. Consequently, you have to preset all breakpoints before debug session start and disable all of them except for `main`. When program stops at `main`, enable the remaining breakpoints and resume execution manually.

### Limitations

1. Currently, debugging is not supported when either HP or LP core enters any sleep mode. So it limits available debugging scenarios.

2. FreeRTOS support in OpenOCD is disabled when debugging LP core, so you won't be able to see tasks running in the system. Instead, there will be several threads representing HP and LP cores:

    (gdb) info thread
        Id   Target Id                                                          Frame
        1    Thread 1 "esp32p4.cpu0" (Name: esp32p4.cpu0, state: debug-request) 0x40803772 in esp_cpu_wait_for_intr ()
            at /home/user/projects/esp/esp-idf/components/esp_hw_support/cpu.c:64
      * 2    Thread 2 "esp32p4.cpu1" (Name: esp32p4.cpu1, state: breakpoint)    do_things (max=1000000000)
            at /home/user/projects/esp/esp-idf/examples/system/ulp/lp_core/debugging/main/lp_core/main.c:21

1. When setting HW breakpoint in GDB, it is set on both cores, so the number of available HW breakpoints is limited to the number of them supported by LP core (3 for ESP32-P4).

2. OpenOCD flash support is disabled. It does not matter for LP core application because it is run completely from RAM and GDB can use SW breakpoints for it. But if you want to set a breakpoint on function from flash used by the code running on HP core (e.g., app_main), you should request to set HW breakpoint explicitly via `hb` and `thb` GDB commands.

3. Since the main and ULP programs are linked as separate binaries, it is possible for them to have global symbols (such as functions or variables) with the same name. If you set a breakpoint using the function name, GDB will apply it to all instances of that function. This can cause issues if one of the functions is located in the flash, as OpenOCD currently doesn't support flash when debugging the LP core. In such cases, you can set breakpoints using the source line or the function's memory address instead.

## Application Examples

- system/ulp/lp_core/gpio polls GPIO while main CPU is in Deep-sleep.

- system/ulp/lp_core/lp_uart/lp_uart_echo reads data written to a serial console and echoes it back. This example demonstrates the usage of the LP UART driver running on the LP core.

- system/ulp/lp_core/lp_uart/lp_uart_print shows how to print various statements from a program running on the LP core.

- system/ulp/lp_core/lp_uart/lp_uart_char_seq_wakeup shows how to trigger a wakeup using the LP UART specific character sequence wakeup mode.

- system/ulp/lp_core/lp_mailbox shows how to use the mailbox for both synchronous and asynchronous communication between the HP and LP cores. Depending on the target, the implementation may use the hardware mailbox controller (if available) or a software-only implementation using interrupts.

- system/ulp/lp_core/interrupt shows how to register an interrupt handler on the LP core to receive an interrupt triggered by the main CPU.

- system/ulp/lp_core/gpio_intr_pulse_counter shows how to use GPIO interrupts to count pulses while the main CPU is in Deep-sleep mode.

- system/ulp/lp_core/build_system/ demonstrates how to include custom `CMakeLists.txt` file for the ULP app.

- system/ulp/lp_core/debugging shows how to debug code running on LP core using GDB and OpenOCD.

## API Reference

### Main CPU API Reference

#### Header File

- components/ulp/lp_core/include/ulp_lp_core.h

- This header file can be included with:

  >     #include "ulp_lp_core.h"

- This header file is a part of the API provided by the `ulp` component. To declare that your component depends on `ulp`, add the following to your CMakeLists.txt:

  >     REQUIRES ulp

  > or

  >     PRIV_REQUIRES ulp

#### Functions

esp_err_t ulp_lp_core_run(ulp_lp_core_cfg_t *cfg)

  Configure the ULP and run the program loaded into RTC memory.

  Returns:

    ESP_OK on success

esp_err_t ulp_lp_core_load_binary(const uint8_t *program_binary, size_t program_size_bytes)

  Load the program binary into RTC memory.

  Parameters:

    - program_binary -- pointer to program binary

    - program_size_bytes -- size of the program binary

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_SIZE if program_size_bytes is more than KiB

void ulp_lp_core_stop(void)

  Puts the ulp to sleep and disables all wakeup sources. To restart the ULP call ulp_lp_core_run() with the desired wake up trigger.

void ulp_lp_core_sw_intr_from_lp_enable(bool enable)

  Enable or disable the software interrupts requested by the LP CPU via the PMU.

void ulp_lp_core_sw_intr_from_lp_clear(void)

  Clear the software interrupt requested by the LP CPU via the PMU.

void ulp_lp_core_sw_intr_to_lp_trigger(void)

  Trigger a software interrupt to the LP CPU from the PMU.

  Note

  This is the same SW trigger that is used to wake up the LP CPU

static inline void ulp_lp_core_sw_intr_trigger(void)

  Trigger a software interrupt to the LP CPU from the PMU.

  Note

  This function is an alias for `ulp_lp_core_sw_intr_to_lp_trigger`

void ulp_lp_core_sw_intr_trigger_self(void)

  Trigger a software interrupt on the HP core from the PMU.

  Note

  This function generates the same software interrupt that the LP core would normally use to notify the HP core. It can be called directly by the HP core itself in order to simulate or re-issue such a notification. This is particularly useful if the HP core missed a previous interrupt from the LP core and needs to retrigger the notification sequence.

#### Structures

struct ulp_lp_core_cfg_t

  ULP LP core init parameters.

  Public Members

  uint32_t wakeup_source

    Wakeup source flags

  uint32_t lp_timer_sleep_duration_us

    Sleep duration when ULP_LP_CORE_WAKEUP_SOURCE_LP_TIMER is specified. Measurement unit: us

  bool skip_lp_rom_boot

    Skips the LP rom code and boots directly into the app code placed in LP RAM, this gives faster boot time for time sensitive use-cases at the cost of skipping setup e.g. of UART

#### Macros

ULP_LP_CORE_WAKEUP_SOURCE_HP_CPU

ULP_LP_CORE_WAKEUP_SOURCE_LP_UART

ULP_LP_CORE_WAKEUP_SOURCE_LP_IO

ULP_LP_CORE_WAKEUP_SOURCE_ETM

ULP_LP_CORE_WAKEUP_SOURCE_LP_TIMER

ULP_LP_CORE_WAKEUP_SOURCE_LP_VAD

#### Header File

- components/ulp/lp_core/include/lp_core_i2c.h

- This header file can be included with:

  >     #include "lp_core_i2c.h"

- This header file is a part of the API provided by the `ulp` component. To declare that your component depends on `ulp`, add the following to your CMakeLists.txt:

  >     REQUIRES ulp

  > or

  >     PRIV_REQUIRES ulp

#### Functions

esp_err_t lp_core_i2c_master_init(i2c_port_t lp_i2c_num, const lp_core_i2c_cfg_t *cfg)

  Initialize and configure the LP I2C for use by the LP core Currently LP I2C can only be used in master mode.

  Note

  The internal pull-up resistors for SDA and SCL pins, if enabled, will provide a weak pull-up value of about 30-50 kOhm. Users are advised to enable external pull-ups for better performance at higher SCL frequencies.

  Parameters:

    - lp_i2c_num -- LP I2C port number

    - cfg -- Configuration parameters

  Returns:

    esp_err_t ESP_OK when successful

#### Structures

struct lp_core_i2c_pin_cfg_t

  LP Core I2C pin config parameters.

  Public Members

  gpio_num_t sda_io_num

    GPIO pin for SDA signal. Only GPIO#6 can be used as the SDA pin.

  gpio_num_t scl_io_num

    GPIO pin for SCL signal. Only GPIO#7 can be used as the SCL pin.

  bool sda_pullup_en

    SDA line enable internal pullup. Can be configured if external pullup is not used.

  bool scl_pullup_en

    SCL line enable internal pullup. Can be configured if external pullup is not used.

struct lp_core_i2c_timing_cfg_t

  LP Core I2C timing config parameters.

  Public Members

  uint32_t clk_speed_hz

    LP I2C clock speed for master mode

struct lp_core_i2c_cfg_t

  LP Core I2C config parameters.

  Public Members

  lp_core_i2c_pin_cfg_t i2c_pin_cfg

    LP I2C pin configuration

  lp_core_i2c_timing_cfg_t i2c_timing_cfg

    LP I2C timing configuration

  soc_periph_lp_i2c_clk_src_t i2c_src_clk

    LP I2C source clock type

#### Macros

LP_I2C_SCL_IO

LP_I2C_SDA_IO

LP_I2C_DEFAULT_GPIO_CONFIG()

LP_I2C_FAST_MODE_CONFIG()

LP_I2C_STANDARD_MODE_CONFIG()

LP_I2C_DEFAULT_SRC_CLK()

LP_CORE_I2C_DEFAULT_CONFIG()

#### Header File

- components/ulp/lp_core/include/lp_core_uart.h

- This header file can be included with:

  >     #include "lp_core_uart.h"

- This header file is a part of the API provided by the `ulp` component. To declare that your component depends on `ulp`, add the following to your CMakeLists.txt:

  >     REQUIRES ulp

  > or

  >     PRIV_REQUIRES ulp

#### Functions

esp_err_t lp_core_uart_init(const lp_core_uart_cfg_t *cfg)

  Initialize and configure the LP UART to be used from the LP core.

  Note

  The LP UART initialization must be called from the main core (HP CPU)

  Parameters:

    cfg -- Configuration parameters

  Returns:

    esp_err_t ESP_OK when successful

#### Structures

struct lp_core_uart_pin_cfg_t

  LP UART IO pins configuration.

  Public Members

  gpio_num_t tx_io_num

    GPIO pin for UART Tx signal. Only GPIO#5 can be used as the UART Tx pin

  gpio_num_t rx_io_num

    GPIO pin for UART Rx signal. Only GPIO#4 can be used as the UART Rx pin

  gpio_num_t rts_io_num

    GPIO pin for UART RTS signal. Only GPIO#2 can be used as the UART RTS pin

  gpio_num_t cts_io_num

    GPIO pin for UART CTS signal. Only GPIO#3 can be used as the UART CTS pin

struct lp_core_uart_proto_cfg_t

  LP UART protocol configuration.

  Public Members

  int baud_rate

    LP UART baud rate

  uart_word_length_t data_bits

    LP UART byte size

  uart_parity_t parity

    LP UART parity mode

  uart_stop_bits_t stop_bits

    LP UART stop bits

  uart_hw_flowcontrol_t flow_ctrl

    LP UART HW flow control mode (cts/rts)

  uint8_t rx_flow_ctrl_thresh

    LP UART HW RTS threshold

struct lp_core_uart_cfg_t

  LP UART configuration parameters.

  Public Members

  lp_core_uart_pin_cfg_t uart_pin_cfg

    LP UART pin configuration

  lp_core_uart_proto_cfg_t uart_proto_cfg

    LP UART protocol configuration

  lp_uart_sclk_t lp_uart_source_clk

    LP UART source clock selection

#### Macros

LP_UART_DEFAULT_TX_GPIO_NUM

  Default LP_IO Mux pins for LP UART

LP_UART_DEFAULT_RX_GPIO_NUM

LP_UART_DEFAULT_RTS_GPIO_NUM

LP_UART_DEFAULT_CTS_GPIO_NUM

LP_UART_DEFAULT_GPIO_CONFIG()

LP_UART_DEFAULT_PROTO_CONFIG()

LP_UART_DEFAULT_CLOCK_CONFIG()

LP_CORE_UART_DEFAULT_CONFIG()

#### Header File

- components/ulp/lp_core/include/lp_core_spi.h

- This header file can be included with:

  >     #include "lp_core_spi.h"

- This header file is a part of the API provided by the `ulp` component. To declare that your component depends on `ulp`, add the following to your CMakeLists.txt:

  >     REQUIRES ulp

  > or

  >     PRIV_REQUIRES ulp

#### Functions

esp_err_t lp_core_lp_spi_bus_initialize(lp_spi_host_t host_id, const lp_spi_bus_config_t *bus_config)

  Initialize the LP SPI bus for use by the LP core.

  Parameters:

    - host_id -- LP SPI host number

    - bus_config -- LP SPI bus configuration parameters

  Returns:

    esp_err_t ESP_OK when successful ESP_ERR_INVALID_ARG if the configuration is invalid

esp_err_t lp_core_lp_spi_bus_add_device(lp_spi_host_t host_id, const lp_spi_device_config_t *dev_config)

  Initialize the LP SPI controller in master mode and add an SPI device to the LP SPI bus.

  Parameters:

    - host_id -- LP SPI host number

    - dev_config -- LP SPI device configuration parameters

  Returns:

    esp_err_t ESP_OK when successful ESP_ERR_INVALID_ARG if the configuration is invalid ESP_FAIL if the device could not be added

esp_err_t lp_core_lp_spi_slave_initialize(lp_spi_host_t host_id, const lp_spi_slave_config_t *slave_config)

  Initialize the LP SPI controller in slave mode.

  Parameters:

    - host_id -- LP SPI host number

    - slave_config -- LP SPI slave configuration parameters

  Returns:

    esp_err_t ESP_OK when successful ESP_FAIL if the SPI controller could not be initialized in slave mode

#### Structures

struct lp_spi_bus_config_t

  LP SPI bus configuration parameters.

  Public Members

  int mosi_io_num

    GPIO pin for Master out, Slave In signal, a.k.a, SPI_D.

  int miso_io_num

    GPIO pin for Master in, Slave Out signal, a.k.a, SPI_Q.

  int sclk_io_num

    GPIO pin for LP SPI Clock signal.

struct lp_spi_device_config_t

  LP SPI device configuration parameters.

  Public Members

  int cs_io_num

    GPIO pin for the device Chip Select (CS) signal.

  int clock_speed_hz

    SPI clock speed in Hz.

  int spi_mode

    SPI mode, representing a pair of Clock Polarity (CPOL) and Clock Phase (CPHA) configuration:

    - SPI Mode 0: (0, 0)

    - SPI Mode 1: (0, 1)

    - SPI Mode 2: (1, 0)

    - SPI Mode 3: (1, 1)

  int duty_cycle

    Duty cycle of positive SPI clock, in 1/256th increments (128 = 50% duty cycle). Setting this to 0 (=not setting it) is equivalent to setting this to 128.

  int flags

    Bitwise OR of LP_SPI_DEVICE_* flags

  int cs_ena_pretrans

    Amount of SPI bit-cycles the CS should be active for, before the transmission (0-16). This only works on half-duplex transactions.

  int cs_ena_posttrans

    Amount of SPI bit-cycles the CS should stay active for, after the transmission (0-16). This only works on half-duplex transactions.

struct lp_spi_slave_config_t

  LP SPI slave configuration parameters.

  Public Members

  int cs_io_num

    GPIO pin for the device Chip Select (CS) signal.

  int spi_mode

    SPI mode, representing a pair of Clock Polarity (CPOL) and Clock Phase (CPHA) configuration:

    - SPI Mode 0: (0, 0)

    - SPI Mode 1: (0, 1)

    - SPI Mode 2: (1, 0)

    - SPI Mode 3: (1, 1)

  int flags

    Bitwise OR of LP_SPI_DEVICE_* flags

#### Macros

LP_SPI_DEVICE_TXBIT_LSBFIRST

  LP SPI device configuration flags.

  Transmit command/address/data LSB first instead of the default MSB first

LP_SPI_DEVICE_RXBIT_LSBFIRST

  Receive data LSB first instead of the default MSB first

LP_SPI_DEVICE_BIT_LSBFIRST

  Transmit and receive LSB first

LP_SPI_DEVICE_3WIRE

  Use MOSI (=spid) for both sending and receiving data

LP_SPI_DEVICE_CS_ACTIVE_HIGH

  Make CS line active-high during a transanction instead of the default active-low state. Only available in SPI master mode.

LP_SPI_DEVICE_HALF_DUPLEX

  Transmit data before receiving it, instead of simultaneously. Only available in SPI master mode.

#### Type Definitions

typedef uint32_t lp_spi_host_t

  LP SPI peripheral Since we have just one LP SPI peripheral, we can define it as a uint32_t type for now, instead of an enum.

#### Header File

- components/ulp/lp_core/include/lp_core_etm.h

- This header file can be included with:

  >     #include "lp_core_etm.h"

- This header file is a part of the API provided by the `ulp` component. To declare that your component depends on `ulp`, add the following to your CMakeLists.txt:

  >     REQUIRES ulp

  > or

  >     PRIV_REQUIRES ulp

#### Functions

esp_err_t lp_core_new_etm_event(const lp_core_etm_event_config_t *config, esp_etm_event_handle_t *out_event)

  Create a ETM event for LP-Core.

  Note

  The created ETM event object can be deleted later by calling `esp_etm_del_event`

  Parameters:

    - config -- [in] LP-Core ETM event configuration

    - out_event -- [out] Returned ETM event handle

  Returns:

    - ESP_OK: Get ETM event successfully

    - ESP_ERR_INVALID_ARG: Get ETM event failed because of invalid argument

    - ESP_FAIL: Get ETM event failed because of other error

esp_err_t lp_core_new_etm_task(const lp_core_etm_task_config_t *config, esp_etm_task_handle_t *out_task)

  Create a ETM task for LP-Core.

  Note

  The created ETM task object can be deleted later by calling `esp_etm_del_task`

  Parameters:

    - config -- [in] LP-Core ETM task configuration

    - out_task -- [out] Returned ETM task handle

  Returns:

    - ESP_OK: Get ETM task successfully

    - ESP_ERR_INVALID_ARG: Get ETM task failed because of invalid argument

    - ESP_FAIL: Get ETM task failed because of other error

#### Structures

struct lp_core_etm_event_config_t

  LP-Core ETM event configuration.

  Public Members

  lp_core_etm_event_type_t event_type

    LP-Core ETM event type

struct lp_core_etm_task_config_t

  LP-Core ETM task configuration.

  Public Members

  lp_core_etm_task_type_t task_type

    LP-Core ETM task type

#### Header File

- components/hal/include/hal/lp_core_types.h

- This header file can be included with:

  >     #include "hal/lp_core_types.h"

#### Enumerations

enum lp_core_etm_event_type_t

  LP-Core event types enum.

  Values:

  enumerator LP_CORE_EVENT_ERR_INTR

    Exception triggered on LP-Core

  enumerator LP_CORE_EVENT_START_INTR

    LP-Core clock has been turned on

  enumerator LP_CORE_EVENT_MAX

    Maximum number of LP-Core events

enum lp_core_etm_task_type_t

  LP-Core task types enum.

  Values:

  enumerator LP_CORE_TASK_WAKEUP_CPU

    LP-Core wake-up task

  enumerator LP_CORE_TASK_MAX

    Maximum number of LP-Core tasks

### LP Core API Reference

#### Header File

- components/ulp/lp_core/lp_core/include/ulp_lp_core_utils.h

#### Functions

void ulp_lp_core_update_wakeup_cause(void)

  Traverse all possible wake-up sources and update the wake-up cause so that ulp_lp_core_get_wakeup_cause can obtain the bitmap of the wake-up reasons.

  Note

  Do not call it from user ULP programs because it will clear the wake-up cause bits which were set at ULP startup in lp_core_startup().

uint32_t ulp_lp_core_get_wakeup_cause(void)

  Get the wakeup source which caused LP_CPU to wakeup from sleep.

  Returns:

    Wakeup cause in bit map, for the meaning of each bit, refer to the definition of wakeup source in lp_core_ll.h

void ulp_lp_core_wakeup_main_processor(void)

  Wakeup main CPU from sleep or deep sleep.

  This raises a software interrupt signal, if the main CPU has configured the ULP as a wakeup source calling this function will make the main CPU to exit from sleep or deep sleep.

static inline uint32_t ulp_lp_core_get_cpu_cycles(void)

  Retrieves the current number of CPU cycles.

  Returns:

    The current CPU cycle count.

void ulp_lp_core_delay_us(uint32_t us)

  Makes the co-processor busy wait for a certain number of microseconds.

  Parameters:

    us -- Number of microseconds to busy-wait for

void ulp_lp_core_delay_cycles(uint32_t cycles)

  Makes the co-processor busy wait for a certain number of cycles.

  Parameters:

    cycles -- Number of cycles to busy-wait for

void ulp_lp_core_lp_uart_reset_wakeup_en(void)

  Reset LP CORE uart wakeup enable.

void ulp_lp_core_halt(void)

  Finishes the ULP program and powers down the ULP until next wakeup.

  Note

  This function does not return. After called it will fully reset the ULP.

  Note

  The program will automatically call this function when returning from main().

  Note

  To stop the ULP from waking up, call ulp_lp_core_lp_timer_disable() before halting.

void ulp_lp_core_stop_lp_core(void)

  The LP core puts itself to sleep and disables all wakeup sources.

void ulp_lp_core_abort(void)

  Abort LP core operation.

void ulp_lp_core_sw_intr_to_hp_trigger(void)

  Trigger a software interrupt on the HP core.

void ulp_lp_core_sw_intr_from_hp_enable(bool enable)

  Enable the SW triggered interrupt from the PMU.

  Note

  This is the same SW trigger interrupt that is used to wake up the LP CPU

  Parameters:

    enable -- true to enable, false to disable

static inline void ulp_lp_core_sw_intr_enable(bool enable)

  Enable the SW triggered interrupt from the PMU.

  Note

  Alias for the `ulp_lp_core_sw_intr_from_hp_enable` function, for backward compatibility.

  Parameters:

    enable -- true to enable, false to disable

void ulp_lp_core_sw_intr_from_hp_clear(void)

  Clear the interrupt status for the SW triggered interrupt from the PMU.

static inline void ulp_lp_core_sw_intr_clear(void)

  Clear the interrupt status for the SW triggered interrupt from the PMU.

  Note

  Alias for the `ulp_lp_core_sw_intr_from_hp_clear` function, for backward compatibility.

void ulp_lp_core_lp_timer_intr_enable(bool enable)

  Enable the LP Timer interrupt.

void ulp_lp_core_lp_timer_intr_clear(void)

  Clear the interrupt status for the LP Timer interrupt.

void ulp_lp_core_wait_for_intr(void)

  Puts the CPU into a wait state until an interrupt is triggered.

  Note

  The CPU will draw less power when in this state compared to actively running

#### Header File

- components/ulp/lp_core/lp_core/include/ulp_lp_core_gpio.h

#### Functions

static inline void ulp_lp_core_gpio_init(lp_io_num_t lp_io_num)

  Initialize a rtcio pin.

  Note

  If IO is used in LP application, `rtc_gpio_init` must be called at least once for the using IO before loading LP core firmware in HP Code.

  Parameters:

    lp_io_num -- The rtc io pin to initialize

static inline void ulp_lp_core_gpio_output_enable(lp_io_num_t lp_io_num)

  Enable output.

  Parameters:

    lp_io_num -- The rtc io pin to enable output for

static inline void ulp_lp_core_gpio_output_disable(lp_io_num_t lp_io_num)

  Disable output.

  Parameters:

    lp_io_num -- The rtc io pin to disable output for

static inline void ulp_lp_core_gpio_input_enable(lp_io_num_t lp_io_num)

  Enable input.

  Parameters:

    lp_io_num -- The rtc io pin to enable input for

static inline void ulp_lp_core_gpio_input_disable(lp_io_num_t lp_io_num)

  Disable input.

  Parameters:

    lp_io_num -- The rtc io pin to disable input for

static inline void ulp_lp_core_gpio_set_level(lp_io_num_t lp_io_num, uint8_t level)

  Set rtcio output level.

  Parameters:

    - lp_io_num -- The rtc io pin to set the output level for

    - level -- 0: output low; 1: output high.

static inline uint32_t ulp_lp_core_gpio_get_level(lp_io_num_t lp_io_num)

  Get rtcio output level.

  Parameters:

    lp_io_num -- The rtc io pin to get the output level for

static inline void ulp_lp_core_gpio_set_output_mode(lp_io_num_t lp_io_num, rtcio_ll_out_mode_t mode)

  Set rtcio output mode.

  Parameters:

    - lp_io_num -- The rtc io pin to set the output mode for

    - mode -- RTCIO_LL_OUTPUT_NORMAL: normal, RTCIO_LL_OUTPUT_OD: open drain

static inline void ulp_lp_core_gpio_pullup_enable(lp_io_num_t lp_io_num)

  Enable internal pull-up resistor.

  Parameters:

    lp_io_num -- The rtc io pin to enable pull-up for

static inline void ulp_lp_core_gpio_pullup_disable(lp_io_num_t lp_io_num)

  Disable internal pull-up resistor.

  Parameters:

    lp_io_num -- The rtc io pin to disable pull-up for

static inline void ulp_lp_core_gpio_pulldown_enable(lp_io_num_t lp_io_num)

  Enable internal pull-down resistor.

  Parameters:

    lp_io_num -- The rtc io pin to enable pull-down for

static inline void ulp_lp_core_gpio_pulldown_disable(lp_io_num_t lp_io_num)

  Disable internal pull-down resistor.

  Parameters:

    lp_io_num -- The rtc io pin to disable pull-down for

static inline void ulp_lp_core_gpio_intr_enable(lp_io_num_t lp_io_num, gpio_int_type_t intr_type)

  Enable interrupt for lp io pin.

  Parameters:

    - lp_io_num -- The lp io pin to enable interrupt for

    - intr_type -- The interrupt type to enable

static inline void ulp_lp_core_gpio_clear_intr_status(void)

  Clear interrupt status for all lp io.

static inline void ulp_lp_core_gpio_wakeup_enable(lp_io_num_t lp_io_num, gpio_int_type_t intr_type)

  Enable wake up for lp io pin.

  Parameters:

    - lp_io_num -- The lp io pin to enable the wake up for

    - intr_type -- The interrupt type to enable wake up for

static inline void ulp_lp_core_gpio_wakeup_disable(lp_io_num_t lp_io_num)

  Disable wake up for lp io pin.

  Parameters:

    lp_io_num -- The lp io pin to disable the wake up for

#### Macros

RTCIO_OUTPUT_NORMAL

RTCIO_OUTPUT_OD

#### Enumerations

enum lp_io_num_t

  Values:

  enumerator LP_IO_NUM_0

    GPIO0, input and output

  enumerator LP_IO_NUM_1

    GPIO1, input and output

  enumerator LP_IO_NUM_2

    GPIO2, input and output

  enumerator LP_IO_NUM_3

    GPIO3, input and output

  enumerator LP_IO_NUM_4

    GPIO4, input and output

  enumerator LP_IO_NUM_5

    GPIO5, input and output

  enumerator LP_IO_NUM_6

    GPIO6, input and output

  enumerator LP_IO_NUM_7

    GPIO7, input and output

  enumerator LP_IO_NUM_8

    GPIO8, input and output

  enumerator LP_IO_NUM_9

    GPIO9, input and output

  enumerator LP_IO_NUM_10

    GPIO10, input and output

  enumerator LP_IO_NUM_11

    GPIO11, input and output

  enumerator LP_IO_NUM_12

    GPIO12, input and output

  enumerator LP_IO_NUM_13

    GPIO13, input and output

  enumerator LP_IO_NUM_14

    GPIO14, input and output

  enumerator LP_IO_NUM_15

    GPIO15, input and output

#### Header File

- components/ulp/lp_core/lp_core/include/ulp_lp_core_i2c.h

#### Functions

esp_err_t lp_core_i2c_master_read_from_device(i2c_port_t lp_i2c_num, uint16_t device_addr, uint8_t *data_rd, size_t size, int32_t ticks_to_wait)

  Read from I2C device.

  Note

  The LP I2C must have been initialized from the HP core using the lp_core_i2c_master_init() API before invoking this API.

  Note

  the LP I2C does not support 10-bit I2C device addresses.

  Note

  the LP I2C port number is ignored at the moment.

  Parameters:

    - lp_i2c_num -- LP I2C port number

    - device_addr -- I2C device address (7-bit)

    - data_rd -- Buffer to hold data to be read

    - size -- Size of data to be read in bytes

    - ticks_to_wait -- Operation timeout in CPU cycles. Set to -1 to wait forever.

  Returns:

    esp_err_t ESP_OK when successful

esp_err_t lp_core_i2c_master_write_to_device(i2c_port_t lp_i2c_num, uint16_t device_addr, const uint8_t *data_wr, size_t size, int32_t ticks_to_wait)

  Write to I2C device.

  Note

  The LP I2C must have been initialized from the HP core using the lp_core_i2c_master_init() API before invoking this API.

  Note

  the LP I2C does not support 10-bit I2C device addresses.

  Note

  the LP I2C port number is ignored at the moment.

  Parameters:

    - lp_i2c_num -- LP I2C port number

    - device_addr -- I2C device address (7-bit)

    - data_wr -- Buffer which holds the data to be written

    - size -- Size of data to be written in bytes

    - ticks_to_wait -- Operation timeout in CPU cycles. Set to -1 to wait forever.

  Returns:

    esp_err_t ESP_OK when successful

esp_err_t lp_core_i2c_master_write_read_device(i2c_port_t lp_i2c_num, uint16_t device_addr, const uint8_t *data_wr, size_t write_size, uint8_t *data_rd, size_t read_size, int32_t ticks_to_wait)

  Write to and then read from an I2C device in a single transaction.

  Note

  The LP I2C must have been initialized from the HP core using the lp_core_i2c_master_init() API before invoking this API.

  Note

  the LP I2C does not support 10-bit I2C device addresses.

  Note

  the LP I2C port number is ignored at the moment.

  Parameters:

    - lp_i2c_num -- LP I2C port number

    - device_addr -- I2C device address (7-bit)

    - data_wr -- Buffer which holds the data to be written

    - write_size -- Size of data to be written in bytes

    - data_rd -- Buffer to hold data to be read

    - read_size -- Size of data to be read in bytes

    - ticks_to_wait -- Operation timeout in CPU cycles. Set to -1 to wait forever.

  Returns:

    esp_err_t ESP_OK when successful

void lp_core_i2c_master_set_ack_check_en(i2c_port_t lp_i2c_num, bool ack_check_en)

  Enable or disable ACK checking by the LP_I2C controller during write operations.

  When ACK checking is enabled, the hardware will check the ACK/NACK level received during write operations against the expected ACK/NACK level. If the received ACK/NACK level does not match the expected ACK/NACK level then the hardware will generate the I2C_NACK_INT and a STOP condition will be generated to stop the data transfer.

  Note

  ACK checking is enabled by default

  Note

  the LP I2C port number is ignored at the moment.

  Parameters:

    - lp_i2c_num -- LP I2C port number

    - ack_check_en -- true: enable ACK check false: disable ACK check

#### Header File

- components/ulp/lp_core/lp_core/include/ulp_lp_core_uart.h

#### Functions

int lp_core_uart_tx_chars(uart_port_t lp_uart_num, const void *src, size_t size)

  Send data to the LP UART port if there is space available in the Tx FIFO.

  This function will not wait for enough space in the Tx FIFO to be available. It will just fill the available Tx FIFO slots and return when the FIFO is full. If there are no empty slots in the Tx FIFO, this function will not write any data.

  Parameters:

    - lp_uart_num -- LP UART port number

    - src -- data buffer address

    - size -- data length to send

  Returns:

    - (-1) Error

    - OTHERS (>=0) The number of bytes pushed to the Tx FIFO

esp_err_t lp_core_uart_write_bytes(uart_port_t lp_uart_num, const void *src, size_t size, int32_t timeout)

  Write data to the LP UART port.

  This function will write data to the Tx FIFO. If a timeout value is configured, this function will timeout once the number of CPU cycles expire.

  Parameters:

    - lp_uart_num -- LP UART port number

    - src -- data buffer address

    - size -- data length to send

    - timeout -- Operation timeout in CPU cycles. Set to -1 to wait forever.

  Returns:

    esp_err_t ESP_OK when successful

int lp_core_uart_read_bytes(uart_port_t lp_uart_num, void *buf, size_t size, int32_t timeout)

  Read data from the LP UART port.

  This function will read data from the Rx FIFO. If a timeout value is configured, then this function will timeout once the number of CPU cycles expire.

  Parameters:

    - lp_uart_num -- LP UART port number

    - buf -- data buffer address

    - size -- data length to send

    - timeout -- Operation timeout in CPU cycles. Set to -1 to wait forever.

  Returns:

    - (-1) Error

    - OTHERS (>=0) The number of bytes read from the Rx FIFO

void lp_core_uart_tx_flush(uart_port_t lp_uart_num)

  Flush LP UART Tx FIFO.

  This function is automatically called before the LP core powers down once the main() function returns. It can also be called manually in the application to flush the Tx FIFO.

  Parameters:

    lp_uart_num -- LP UART port number

#### Header File

- components/ulp/lp_core/lp_core/include/ulp_lp_core_mailbox.h

#### Functions

esp_err_t lp_core_mailbox_init(lp_mailbox_t *mailbox, lp_mailbox_config_t *config)

  Initialize a mailbox.

  Parameters:

    - mailbox -- Pointer to the mailbox instance to initialize.

    - config -- Pointer to the configuration structure, can be NULL to use default values.

  Returns:

    ESP_OK on success

void lp_core_mailbox_deinit(lp_mailbox_t mailbox)

  Deinitialize a mailbox.

  Parameters:

    mailbox -- Pointer to the mailbox instance to deinitialize.

esp_err_t lp_core_mailbox_send(lp_mailbox_t mailbox, lp_message_t msg, int32_t timeout)

  Send a message through the mailbox.

  Note

  This function will put a message in the mailbox and wait for a receiver to get it.

  Parameters:

    - mailbox -- Pointer to the mailbox instance.

    - msg -- Message to be sent.

    - timeout -- Operation timeout in CPU cycles. Set to -1 to wait forever.

  Returns:

    ESP_OK on success. ESP_INVALID_ARGUMENT if `mailbox` is NULL. ESP_TIMEOUT if timeout was reached and no receiver took the message.

esp_err_t lp_core_mailbox_send_async(lp_mailbox_t mailbox, lp_message_t msg)

  Send a message through the mailbox asynchronously.

  Note

  Unlike the synchronous send function, this function does not wait for a receiver to acknowledge the message.

  Parameters:

    - mailbox -- Pointer to the mailbox instance.

    - msg -- Message to be sent.

  Returns:

    ESP_OK on success. ESP_INVALID_ARGUMENT if `mailbox` is NULL.

esp_err_t lp_core_mailbox_receive(lp_mailbox_t mailbox, lp_message_t *msg, int32_t timeout)

  Receive a message from the mailbox.

  Note

  This function waits for a message to be sent by a sender.

  Parameters:

    - mailbox -- Pointer to the mailbox instance.

    - msg -- Pointer to store the received message.

    - timeout -- Timeout for the operation in CPU cycles. Use -1 to wait indefinitely.

  Returns:

    ESP_OK on success. ESP_INVALID_ARGUMENT if `mailbox` is NULL. ESP_TIMEOUT if the timeout expires without receiving a message.

esp_err_t lp_core_mailbox_receive_async(lp_mailbox_t mailbox, uint32_t count, lp_core_mailbox_callback_t cb)

  Receive a message from the mailbox.

  Parameters:

    - mailbox -- Pointer to the mailbox instance.

    - count -- Number of messages to receive asynchronously. To terminate it at anytime, use lp_core_mailbox_receive_async_cancel() to terminate it.

    - cb -- Callback invoked as soon as a message is received. Please note that this function will be invoked from an ISR context.

  Returns:

    ESP_OK on success. ESP_INVALID_ARGUMENT if `mailbox` or `cb` is NULL.

esp_err_t lp_core_mailbox_receive_async_cancel(lp_mailbox_t mailbox, uint32_t *remaining)

  Cancel an ongoing asynchronous mailbox receive.

  This stops any pending lp_core_mailbox_receive_async().

  Parameters:

    - mailbox -- Pointer to the mailbox instance.

    - remaining -- Optional pointer to store the number of messages left to receive.

  Returns:

    ESP_OK on success, ESP_ERR_INVALID_STATE if no async receive was active.

#### Structures

struct lp_mailbox_config_t

  Configuration structure for the mailbox.

  Public Members

  uint32_t dummy

    Placeholder for future field, ignored for now

#### Type Definitions

typedef intptr_t lp_message_t

typedef void (*lp_core_mailbox_callback_t)(lp_message_t msg)

  Represents a callback function type triggered when a message is received in asynchronous mode.

  Note: There is no guarantee regarding the order in which messages are processed between synchronous and asynchronous modes.

  Param msg:

    The received message, represented as an `lp_message_t` object.

typedef struct lp_mailbox_t *lp_mailbox_t

  Mailbox structure.

#### Header File

- components/ulp/lp_core/lp_core/include/ulp_lp_core_print.h

#### Functions

void lp_core_printf(const char *format, ...)

  Print from the LP core.

  Note

  This function uses the LP UART peripheral to enable prints.The LP UART must be initialized with lp_core_uart_init() before using this function.

  Note

  This function is not a standard printf function and may not support all format specifiers or special characters.

  Parameters:

    - format -- string to be printed

    - ... -- variable argument list

void lp_core_print_char(char c)

  Print a single character from the LP core.

  Parameters:

    c -- character to be printed

void lp_core_print_str(const char *str)

  Print a null-terminated string from the LP core.

  Parameters:

    str -- null-terminated string to be printed

void lp_core_print_hex(int h)

  Print a hex value from the LP core.

  Note

  Does not print '0x', only the digits (will always print 8 digits)

  Parameters:

    h -- hex value to be printed

void lp_core_print_dec_two_digits(int d)

  Print a two digit integer from the LP-Core.

  Parameters:

    d -- integer to be printed

#### Header File

- components/ulp/lp_core/lp_core/include/ulp_lp_core_interrupts.h

#### Functions

void ulp_lp_core_intr_enable(void)

  Enables interrupts globally for the low power core.

  Available interrupt handlers for the low power core are as follows:

  ulp_lp_core_lp_io_intr_handler(void); ulp_lp_core_lp_i2c_intr_handler(void); ulp_lp_core_lp_uart_intr_handler(void); ulp_lp_core_lp_timer_intr_handler(void); ulp_lp_core_lp_pmu_intr_handler(void); ulp_lp_core_lp_spi_intr_handler(void); ulp_lp_core_trng_intr_handler(void); ulp_lp_core_lp_adc_intr_handler(void); ulp_lp_core_lp_touch_intr_handler(void); ulp_lp_core_tsens_intr_handler(void); ulp_lp_core_efuse_intr_handler(void); ulp_lp_core_lp_sysreg_intr_handler(void); ulp_lp_core_lp_ana_peri_intr_handler(void); ulp_lp_core_mailbox_intr_handler(void); ulp_lp_core_lp_wdt_intr_handler(void); ulp_lp_core_lp_rtc_intr_handler(void); ulp_lp_core_sw_intr_handler(void);

  Not all handlers are available on all chips. Please refer to the Technical Reference Manual for your chip for more information.

void ulp_lp_core_intr_disable(void)

  Disables interrupts globally for the low power core.

#### Macros

LP_CORE_ISR_ATTR

#### Header File

- components/ulp/lp_core/lp_core/include/ulp_lp_core_spi.h

#### Functions

esp_err_t lp_core_lp_spi_master_transfer(lp_spi_transaction_t *trans_desc, int32_t ticks_to_wait)

  Initiate an LP SPI transaction in master mode to transmit device to an SPI device and optionally receive data from the device.

  Parameters:

    - trans_desc -- LP SPI transaction configuration descriptor

    - ticks_to_wait -- Operation timeout in CPU cycles. Set to -1 to wait forever.

  Returns:

    esp_err_t ESP_OK when successful ESP_ERR_INVALID_ARG if the configuration is invalid ESP_ERR_TIMEOUT when the operation times out

esp_err_t lp_core_lp_spi_slave_transfer(lp_spi_transaction_t *trans_desc, int32_t ticks_to_wait)

  Initiate an LP SPI transaction in slave mode to receive data from an SPI master and optionally transmit data back to the master.

  Parameters:

    - trans_desc -- LP SPI transaction configuration descriptor

    - ticks_to_wait -- Operation timeout in CPU cycles. Set to -1 to wait forever.

  Returns:

    esp_err_t ESP_OK when successful ESP_ERR_INVALID_ARG if the configuration is invalid ESP_ERR_TIMEOUT when the operation times out

#### Structures

struct lp_spi_transaction_t

  This structure describes one SPI transaction. The descriptor should not be modified until the transaction finishes.

  Public Members

  uint32_t tx_length

    Total data length to transmit in bytes

  uint32_t rx_length

    Total data length to receive in bytes

  const void *tx_buffer

    Pointer to the transmit buffer. Must be set for master mode transactions. Can be NULL for slave mode transactions.

  void *rx_buffer

    Pointer to the receive buffer. Must be set for slave mode transactions. Can be NULL for master mode transactions.

  lp_spi_bus_t bus

    The LP SPI bus to transmit the data on

  int command

    Command data, of which the length is set in the `command_bits` field of this structure.

  uint32_t address

    Address data, of which the length is set in the `address_bits` field of this structure.

  uint8_t command_bits

    Default amount of bits in command phase

  uint8_t address_bits

    Default amount of bits in address phase

  uint8_t dummy_bits

    Amount of dummy bits to insert between address and data phase.

#### Type Definitions

typedef uint32_t lp_spi_bus_t

  The LP SPI bus identifier to initiate a transaction on.

#### Header File

- components/ulp/lp_core/shared/include/ulp_lp_core_lp_uart_shared.h

- This header file can be included with:

  >     #include "ulp_lp_core_lp_uart_shared.h"

- This header file is a part of the API provided by the `ulp` component. To declare that your component depends on `ulp`, add the following to your CMakeLists.txt:

  >     REQUIRES ulp

  > or

  >     PRIV_REQUIRES ulp

#### Functions

esp_err_t lp_core_uart_wakeup_setup(const uart_wakeup_cfg_t *cfg)

  Initialize and configure the LP UART wakeup mode.

  Note

  This function configures the LP UART wakeup mode. Ensure that the UART has already been initialized with the lp_core_uart_init() call. Once the LP Core wakes up due to the LP UART, the wakeup feature is disabled. To re-enable the wakeup from the LP UART, you must call ulp_lp_core_lp_uart_reset_wakeup_en() again before the LP core goes to sleep. Also be aware of limitations in different modes mentioned in the uart_wakeup_cfg_t struct.

  Parameters:

    cfg -- Configuration for LP UART wakeup mode.

  Returns:

    esp_err_t ESP_OK when successful

void lp_core_uart_clear_buf(void)

  Clear LP UART rx tx buffer.

  Note

  Clear LP UART rx tx buffer.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.