Warning

This document is not updated for ESP32C5 yet, so some of the content may not be correct.

This warning was automatically inserted due to the source file being in the add_warnings_pages list.

# Peripherals API

[中文]

- GPIO & RTC GPIO
- General Purpose Timer (GPTimer)
- LCD
- LED Control (LEDC)
- SPI Flash API
- Universal Asynchronous Receiver/Transmitter (UART)

Code examples for this API section are provided in the peripherals directory of ESP-IDF examples.

Provide feedback about this document