# Peripherals API

[中文]

- Analog to Digital Converter (ADC) Oneshot Mode Driver
- Analog to Digital Converter (ADC) Calibration Driver
- Clock Tree
- GPIO & RTC GPIO
- General Purpose Timer (GPTimer)
- Dedicated GPIO
- Inter-Integrated Circuit (I2C)
- LCD
- LED Control (LEDC)
- SD SPI Host Driver
- SPI Flash API
- SPI Master Driver
- SPI Slave Driver
- SPI Slave Half Duplex
- Temperature Sensor
- Universal Asynchronous Receiver/Transmitter (UART)

Code examples for this API section are provided in the peripherals directory of ESP-IDF examples.

Provide feedback about this document