Mbed TLS
========

:link_to_translation:`zh_CN:[中文]`

`Mbed TLS <https://github.com/Mbed-TLS/mbedtls>`_ is a C library that implements cryptographic primitives, X.509 certificate manipulation and the SSL/TLS and DTLS protocols. Its small code footprint makes it suitable for embedded systems.

.. note::

    ESP-IDF uses a `fork <https://github.com/espressif/mbedtls>`_ of Mbed TLS which includes a few patches (related to hardware routines of certain modules like ``bignum (MPI)`` and ``ECC``) over vanilla Mbed TLS.

Mbed TLS supports TLS 1.2, TLS 1.3 and DTLS 1.2 communication by providing the following:

- TCP/IP communication functions: listen, connect, accept, read/write.
- SSL/TLS communication functions: init, handshake, read/write.
- X.509 functions: CRT, CRL and key handling
- Random number generation
- Hashing
- Encryption/decryption

.. note::

    Mbed TLS v3.x.x series supports only TLS 1.2 and TLS 1.3 protocols. Support for SSL 3.0, TLS 1.0/1.1 and DTLS 1.0 has been removed (deprecated). TLS 1.3 is fully supported starting Mbed TLS v3.6.0 release, before this release some features were still in experimental state. Please refer to :component_file:`Mbed TLS ChangeLog <mbedtls/mbedtls/ChangeLog>` for more details.

Mbed TLS Documentation
----------------------

For Mbed TLS documentation please refer to the following (upstream) pointers:

- `API Reference`_
- `Knowledge Base`_

Mbed TLS Support in ESP-IDF
---------------------------

Please find the information about the Mbed TLS versions presented in different branches of ESP-IDF `here <https://github.com/espressif/mbedtls/wiki#mbed-tls-support-in-esp-idf>`__.

.. note::

    Please refer the :ref:`migration_guide_mbedtls` to migrate from Mbed TLS version 2.x to version 3.0 or greater.

Application Examples
--------------------

Examples in ESP-IDF use :doc:`/api-reference/protocols/esp_tls` which provides a simplified API interface for accessing the commonly used TLS functionality.

Refer to the examples :example:`protocols/https_server/simple` (Simple HTTPS server) and :example:`protocols/https_request` (Make HTTPS requests) for more information.

If the Mbed TLS API is to be used directly, refer to the example :example:`protocols/https_mbedtls`.


Alternatives
------------

:doc:`/api-reference/protocols/esp_tls` acts as an abstraction layer over the underlying SSL/TLS library and thus has an option to use Mbed TLS or wolfSSL as the underlying library. By default, only Mbed TLS is available and used in ESP-IDF whereas wolfSSL is available publicly at `<https://github.com/espressif/esp-wolfSSL>` with the upstream submodule pointer.

Please refer to :ref:`ESP-TLS: Underlying SSL/TLS Library Options <esp_tls_wolfssl>` docs for more information on this and comparison of Mbed TLS and wolfSSL.


Important Config Options
------------------------

Following is a brief list of important config options accessible at ``Component Config -> mbedTLS``. The full list of config options can be found :ref:`here <CONFIG_MBEDTLS_MEM_ALLOC_MODE>`.

.. list::

    - :ref:`CONFIG_MBEDTLS_SSL_PROTO_TLS1_2`: Support for TLS 1.2
    - :ref:`CONFIG_MBEDTLS_SSL_PROTO_TLS1_3`: Support for TLS 1.3
    - :ref:`CONFIG_MBEDTLS_CERTIFICATE_BUNDLE`: Support for trusted root certificate bundle (more about this: :doc:`/api-reference/protocols/esp_crt_bundle`)
    - :ref:`CONFIG_MBEDTLS_CLIENT_SSL_SESSION_TICKETS`: Support for TLS Session Resumption: Client session tickets
    - :ref:`CONFIG_MBEDTLS_SERVER_SSL_SESSION_TICKETS`: Support for TLS Session Resumption: Server session tickets
    :SOC_SHA_SUPPORTED: - :ref:`CONFIG_MBEDTLS_HARDWARE_SHA`: Support for hardware SHA acceleration
    :SOC_AES_SUPPORTED: - :ref:`CONFIG_MBEDTLS_HARDWARE_AES`: Support for hardware AES acceleration
    :SOC_MPI_SUPPORTED: - :ref:`CONFIG_MBEDTLS_HARDWARE_MPI`: Support for hardware MPI (bignum) acceleration
    :SOC_ECC_SUPPORTED: - :ref:`CONFIG_MBEDTLS_HARDWARE_ECC`: Support for hardware ECC acceleration

Performance and Memory Tweaks
-----------------------------

.. _reducing_ram_usage_mbedtls:

Reducing Heap Usage
^^^^^^^^^^^^^^^^^^^

The following table shows typical memory usage with different configs when the :example:`protocols/https_request` example (with Server Validation enabled) was run with Mbed TLS as the SSL/TLS library.

.. list-table::
    :header-rows: 1
    :widths: 25 60 30
    :align: center

    * - Mbed TLS Test
      - Related Configs
      - Heap Usage (approx.)
    * - Default
      - NA
      - 42196 B
    * - Enable SSL Variable Length
      - :ref:`CONFIG_MBEDTLS_SSL_VARIABLE_BUFFER_LENGTH`
      -  42120 B
    * - Disable Keep Peer Certificate
      - :ref:`CONFIG_MBEDTLS_SSL_KEEP_PEER_CERTIFICATE`
      - 38533 B
    * - Enable Dynamic TX/RX Buffer
      - :ref:`CONFIG_MBEDTLS_DYNAMIC_BUFFER`
        :ref:`CONFIG_MBEDTLS_DYNAMIC_FREE_CONFIG_DATA`
        :ref:`CONFIG_MBEDTLS_DYNAMIC_FREE_CA_CERT`
      - 22013 B

.. note::

    These values are subject to change with change in configuration options and versions of Mbed TLS.


Reducing Binary Size
^^^^^^^^^^^^^^^^^^^^

Under ``Component Config -> mbedTLS``, there are multiple Mbed TLS features which are enabled by default but can be disabled if not needed to save code size. More information can be about this can be found in :ref:`Minimizing Binary Size <minimizing_binary_mbedtls>` docs.


.. _`API Reference`: https://mbed-tls.readthedocs.io/projects/api/en/v3.6.5/
.. _`Knowledge Base`: https://mbed-tls.readthedocs.io/en/latest/kb/
