Warning

This document is not updated for ESP32C61 yet, so some of the content may not be correct.

This warning was automatically inserted due to the source file being in the add_warnings_pages list.

# Standard Setup of Toolchain for Windows

[中文]

## Introduction

ESP-IDF requires some prerequisite tools to be installed so you can build firmware for supported chips. The prerequisite tools include Python, Git, cross-compilers, CMake and Ninja build tools.

For this Getting Started we are going to use the Command Prompt, but after ESP-IDF is installed you can use Eclipse Plugin or another graphical IDE with CMake support instead.

Note

Limitations:

- The installation path of ESP-IDF and ESP-IDF Tools must not be longer than 90 characters. Too long installation paths might result in a failed build.

- The installation path of Python or ESP-IDF must not contain white spaces or parentheses.

- The installation path of Python or ESP-IDF should not contain special characters (non-ASCII) unless the operating system is configured with "Unicode UTF-8" support.

System Administrator can enable the support via `Control Panel` > Change `date`, `time`, or `number` formats > `Administrative tab` > Change `system locale` > check the option `Beta: Use Unicode UTF-8 for worldwide language support` > `Ok` > reboot the computer.

## ESP-IDF Tools Installer

The easiest way to install ESP-IDF's prerequisites is to download one of ESP-IDF Tools Installers.

| Windows Installer Download

### What Is the Usecase for Online and Offline Installer

Online Installer is very small and allows the installation of all available releases of ESP-IDF. The installer downloads only necessary dependencies including Git For Windows during the installation process. The installer stores downloaded files in the cache directory `%userprofile%\.espressif`

Offline Installer does not require any network connection. The installer contains all required dependencies including Git For Windows.

### Components of the Installation

The installer deploys the following components:

- Embedded Python

- Cross-compilers

- OpenOCD

- CMake and Ninja build tools

- ESP-IDF

The installer also allows reusing the existing directory with ESP-IDF. The recommended directory is `%userprofile%\Desktop\esp-idf` where `%userprofile%` is your home directory.

### Launching ESP-IDF Environment

At the end of the installation process you can check out option `Run ESP-IDF PowerShell Environment` or `Run ESP-IDF Command Prompt (cmd.exe)`. The installer launches ESP-IDF environment in selected prompt.

`Run ESP-IDF PowerShell Environment`:

Completing the ESP-IDF Tools Setup Wizard with Run ESP-IDF PowerShell Environment

ESP-IDF PowerShell

`Run ESP-IDF Command Prompt (cmd.exe)`:

Completing the ESP-IDF Tools Setup Wizard with Run ESP-IDF Command Prompt (cmd.exe)

ESP-IDF Command Prompt

## Using the Command Prompt

For the remaining Getting Started steps, we are going to use the Windows Command Prompt.

ESP-IDF Tools Installer also creates a shortcut in the Start menu to launch the ESP-IDF Command Prompt. This shortcut launches the Command Prompt (cmd.exe) and runs `export.bat` script to set up the environment variables (`PATH`, `IDF_PATH` and others). Inside this command prompt, all the installed tools are available.

Note that this shortcut is specific to the ESP-IDF directory selected in the ESP-IDF Tools Installer. If you have multiple ESP-IDF directories on the computer (for example, to work with different versions of ESP-IDF), you have two options to use them:

1. Create a copy of the shortcut created by the ESP-IDF Tools Installer, and change the working directory of the new shortcut to the ESP-IDF directory you wish to use.

2. Alternatively, run `cmd.exe`, then change to the ESP-IDF directory you wish to use, and run `export.bat`. Note that unlike the previous option, this way requires Python and Git to be present in `PATH`. If you get errors related to Python or Git not being found, use the first option.

## First Steps on ESP-IDF

Now since all requirements are met, the next topic guides you on how to start your first project.

This guide helps you on the first steps using ESP-IDF. Follow this guide to start a new project on the ESP32-C61 and build, flash, and monitor the device output.

Note

If you have not yet installed ESP-IDF, please go to Installation and follow the instruction in order to get all the software needed to use this guide.

## Start a Project

Now you are ready to prepare your application for ESP32-C61. You can start with get-started/hello_world project from examples directory in ESP-IDF.

Important

The ESP-IDF build system does not support spaces in the paths to either ESP-IDF or to projects.

Copy the project get-started/hello_world to `~/esp` directory:

    cd %userprofile%\esp
    xcopy /e /i %IDF_PATH%\examples\get-started\hello_world hello_world

Note

There is a range of example projects in the examples directory in ESP-IDF. You can copy any project in the same way as presented above and run it. It is also possible to build examples in-place without copying them first.

## Connect Your Device

Now connect your ESP32-C61 board to the computer and check under which serial port the board is visible.

Serial port names start with `COM` in Windows.

If you are not sure how to check the serial port name, please refer to Establish Serial Connection with ESP32-C61 for full details.

Note

Keep the port name handy as it is needed in the next steps.

## Configure Your Project

Navigate to your `hello_world` directory, set ESP32-C61 as the target, and run the project configuration utility `menuconfig`.

### Windows

    cd %userprofile%\esp\hello_world
    idf.py set-target esp32c61
    idf.py menuconfig

After opening a new project, you should first set the target with `idf.py set-target esp32c61`. Note that existing builds and configurations in the project, if any, are cleared and initialized in this process. The target may be saved in the environment variable to skip this step at all. See Select the Target Chip: set-target for additional information.

If the previous steps have been done correctly, the following menu appears:

Project configuration - Home window

You are using this menu to set up project specific variables, e.g., Wi-Fi network name and password, the processor speed, etc. Setting up the project with menuconfig may be skipped for "hello_word", since this example runs with default configuration.

Note

The colors of the menu could be different in your terminal. You can change the appearance with the option `--style`. Please run `idf.py menuconfig --help` for further information.

## Build the Project

Build the project by running:

    idf.py build

This command compiles the application and all ESP-IDF components, then it generates the bootloader, partition table, and application binaries.

    $ idf.py build
    Running cmake in directory /path/to/hello_world/build
    Executing "cmake -G Ninja --warn-uninitialized /path/to/hello_world"...
    Warn about uninitialized values.
    -- Found Git: /usr/bin/git (found version "2.17.0")
    -- Building empty aws_iot component due to configuration
    -- Component names: ...
    -- Component paths: ...

    ... (more lines of build system output)

    [527/527] Generating hello_world.bin
    esptool.py v2.3.1

    Project build complete. To flash, run this command:
    ../../../components/esptool_py/esptool/esptool.py -p (PORT) -b 921600 write_flash --flash_mode dio --flash_size detect --flash_freq 40m 0x10000 build/hello_world.bin  build 0x1000 build/bootloader/bootloader.bin 0x8000 build/partition_table/partition-table.bin
    or run 'idf.py -p PORT flash'

If there are no errors, the build finishes by generating the firmware binary .bin files.

## Flash onto the Device

To flash the binaries that you just built for the ESP32-C61 in the previous step, you need to run the following command:

    idf.py -p PORT flash

Replace `PORT` with your ESP32-C61 board's USB port name. If the `PORT` is not defined, the idf.py will try to connect automatically using the available USB ports.

For more information on `idf.py` arguments, see idf.py.

Note

The option `flash` automatically builds and flashes the project, so running `idf.py build` is not necessary.

Encountered Issues While Flashing? See the "Additional Tips" below. You can also refer to Flashing Troubleshooting page or Establish Serial Connection with ESP32-C61 for more detailed information.

### Normal Operation

When flashing, you will see the output log similar to the following:

    ...

If there are no issues by the end of the flash process, the board will reboot and start up the "hello_world" application.

If you would like to use the Eclipse or VS Code IDE instead of running `idf.py`, check out Eclipse Plugin, VSCode Extension.

## Monitor the Output

To check if "hello_world" is indeed running, type `idf.py -p PORT monitor` (Do not forget to replace PORT with your serial port name).

This command launches the IDF Monitor application.

    $ idf.py -p <PORT> monitor
    Running idf_monitor in directory [...]/esp/hello_world/build
    Executing "python [...]/esp-idf/tools/idf_monitor.py -b 115200 [...]/esp/hello_world/build/hello_world.elf"...
    --- idf_monitor on <PORT> 115200 ---
    --- Quit: Ctrl+] | Menu: Ctrl+T | Help: Ctrl+T followed by Ctrl+H ---
    ets Jun  8 2016 00:22:57

    rst:0x1 (POWERON_RESET),boot:0x13 (SPI_FAST_FLASH_BOOT)
    ets Jun  8 2016 00:22:57
    ...

After startup and diagnostic logs scroll up, you should see "Hello world!" printed out by the application.

        ...
        Hello world!
        Restarting in 10 seconds...
        This is esp32c61 chip with 1 CPU core(s), [NEEDS TO BE UPDATED]
    Minimum free heap size: [NEEDS TO BE UPDATED] bytes
        Restarting in 9 seconds...
        Restarting in 8 seconds...
        Restarting in 7 seconds...

To exit IDF monitor use the shortcut `Ctrl+]`.

Note

You can combine building, flashing and monitoring into one step by running:

    idf.py -p PORT flash monitor

See also:

- IDF Monitor for handy shortcuts and more details on using IDF monitor.

- idf.py for a full reference of `idf.py` commands and options.

That is all that you need to get started with ESP32-C61!

Now you are ready to try some other examples, or go straight to developing your own applications.

Important

Some of examples do not support ESP32-C61 because required hardware is not included in ESP32-C61 so it cannot be supported.

If building an example, please check the README file for the `Supported Targets` table. If this is present including ESP32-C61 target, or the table does not exist at all, the example will work on ESP32-C61.

## Additional Tips

### Permission Denied Issue

With some Linux distributions, you may get the error message similar to `Could not open port <PORT>: Permission denied: '<PORT>'` when flashing the ESP32-C61. This can be solved by adding the current user to the specific group, such as `dialout` or `uucp` group.

### Python Compatibility

ESP-IDF supports Python 3.8 or newer. It is recommended to upgrade your operating system to a recent version satisfying this requirement. Other options include the installation of Python from sources or the use of a Python version management system such as pyenv.

### Flash Erase

Erasing the flash is also possible. To erase the entire flash memory you can run the following command:

    idf.py -p PORT erase-flash

For erasing the OTA data, if present, you can run this command:

    idf.py -p PORT erase-otadata

The flash erase command can take a while to be done. Do not disconnect your device while the flash erasing is in progress.

## Related Documents

For advanced users who want to customize the install process:

- Updating ESP-IDF Tools on Windows

- Establish Serial Connection with ESP32-C61

- Eclipse Plugin

- VSCode Extension

- IDF Monitor

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.