# Touch Sensor

[中文]

## Introduction

A touch sensor system is built on a substrate which carries electrodes and relevant connections under a protective flat surface. When the surface is touched, the capacitance variation is used to evaluate if the touch was valid.

The sensing pads can be arranged in different combinations (e.g., matrix, slider), so that a larger area or more points can be detected. The touch pad sensing process is under the control of a hardware-implemented finite-state machine (FSM) which is initiated by software or a dedicated hardware timer.

For design, operation, and control registers of a touch sensor, see ESP32-S2 Technical Reference Manual > On-Chip Sensors and Analog Signal Processing [PDF].

In-depth design details of touch sensors and firmware development guidelines for ESP32-S2 are available in Touch Sensor Application Note.

## Functionality Overview

Description of API is broken down into groups of functions to provide a quick overview of the following features:

- Initialization of touch pad driver

- Configuration of touch pad GPIO pins

- Taking measurements

- Adjusting parameters of measurements

- Filtering measurements

- Touch detection methods

- Setting up interrupts to report touch detection

- Waking up from Sleep mode on interrupt

For detailed description of a particular function, please go to Section API Reference. Practical implementation of this API is covered in Section Application Examples.

### Initialization

Before using a touch pad, you need to initialize the touch pad driver by calling the function `touch_pad_init()`. This function sets several `.._DEFAULT` driver parameters listed in API Reference under Macros. It also removes the information about which pads have been touched before, if any, and disables interrupts.

If the driver is not required anymore, deinitialize it by calling `touch_pad_deinit()`.

### Configuration

Enabling the touch sensor functionality for a particular GPIO is done with `touch_pad_config()`. The following 14 capacitive touch pads are supported for ESP32-S2.

Touch Pad | GPIO Pin
--- | ---
T0 | Internal channel, not connect to a GPIO
T1 | GPIO1
T2 | GPIO2
T3 | GPIO3
T4 | GPIO4
T5 | GPIO5
T6 | GPIO6
T7 | GPIO7
T8 | GPIO8
T9 | GPIO9
T10 | GPIO10
T11 | GPIO11
T12 | GPIO12
T13 | GPIO13
T14 | GPIO14

Use the function `touch_pad_set_fsm_mode()` to select if touch pad measurement (operated by FSM) should be started automatically by a hardware timer, or by software. If software mode is selected, use `touch_pad_sw_start()` to start the FSM.

### Touch State Measurements

The following function come in handy to read raw measurements from the sensor:

- `touch_pad_read_raw_data()`

It can also be used, for example, to evaluate a particular touch pad design by checking the range of sensor readings when a pad is touched or released. This information can be then used to establish a touch threshold.

For the demonstration of how to read the touch pad data, check the application example peripherals/touch_sensor/touch_sensor_v2/touch_pad_read.

### Method of Measurements

The touch sensor records the period of time (i.e., the number of clock cycles) over a fixed charge/discharge cycles (specified by `touch_pad_set_charge_discharge_times()`). The count result is the raw data that read from `touch_pad_read_raw_data()`. After finishing one measurement, the touch sensor sleeps until the next measurement start, this interval between two measurements can be set by `touch_pad_set_measurement_interval()`.

Note

If the specified charge and discharge cycles for measurement is too small, the result may be inaccurate, but increasing charge and discharge cycles will increase the power consumption as well. Additionally, the response of the touch sensor will slow down if the total time of the interval and measurement is too long.

### Optimization of Measurements

A touch sensor has several configurable parameters to match the characteristics of a particular touch pad design. For instance, to sense smaller capacity changes, it is possible to narrow down the reference voltage range within which the touch pads are charged/discharged. The high and low reference voltages are set using the function `touch_pad_set_voltage()`.

Besides the ability to discern smaller capacity changes, a positive side effect is reduction of power consumption for low power applications. A likely negative effect is an increase in measurement noise. If the dynamic range of obtained readings is still satisfactory, then further reduction of power consumption might be done by reducing the measurement time with `touch_pad_set_charge_discharge_times()`.

The following list summarizes available measurement parameters and corresponding 'set' functions:

- Touch pad charge / discharge parameters:

  > - voltage range: `touch_pad_set_voltage()`

  > - speed (slope): `touch_pad_set_cnt_mode()`

- Charge and discharge times of one measurement: `touch_pad_set_charge_discharge_times()`

Relationship between the voltage range (high/low reference voltages), speed (slope), and measurement time is shown in the figure below.

Touch pad - relationship between measurement parameters

The last chart Output represents the touch sensor reading, i.e., the time taken to accumulate the fixed number of cycles.

All functions are provided in pairs to set a specific parameter and to get the current parameter's value, e.g., `touch_pad_set_voltage()` and `touch_pad_get_voltage()`.

### Filtering of Measurements

If measurements are noisy, you can filter them with provided API functions. The ESP32-S2's touch functionality provide two sets of APIs for doing this.

There is an internal touch channel that is not connected to any external GPIO. The measurements from this denoise pad can be used to filters out interference introduced on all channels, such as noise introduced by the power supply and external EMI.

The denoise parameters are set with the function `touch_pad_denoise_set_config()` and started by with `touch_pad_denoise_enable()`

There is also a configurable hardware implemented IIR-filter (infinite impulse response). This IIR-filter is configured with the function `touch_pad_filter_set_config()` and enabled by calling `touch_pad_filter_enable()`

### Touch Detection

Touch detection is implemented in ESP32's hardware based on the user-configured threshold and raw measurements executed by FSM. Use the functions `touch_pad_get_status()` to check which pads have been touched and `touch_pad_clear_status()` to clear the touch status information.

Hardware touch detection can also be wired to interrupts. This is described in the next section.

If measurements are noisy and capacity changes are small, hardware touch detection might be unreliable. To resolve this issue, instead of using hardware detection/provided interrupts, implement measurement filtering and perform touch detection in your own application. For sample implementation of both methods of touch detection, see peripherals/touch_sensor/touch_sensor_v2/touch_pad_interrupt.

### Touch Triggered Interrupts

Before enabling an interrupt on a touch detection, you should establish a touch detection threshold. Use the functions described in Touch State Measurements to read and display sensor measurements when a pad is touched and released. Apply a filter if measurements are noisy and relative capacity changes are small. Depending on your application and environment conditions, test the influence of temperature and power supply voltage changes on measured values.

Once a detection threshold is established, it can be set during initialization with `touch_pad_config()` or at the runtime with `touch_pad_set_thresh()`.

Finally, configure and manage interrupt calls using the following functions:

- `touch_pad_isr_register()` / `touch_pad_isr_deregister()`

- `touch_pad_intr_enable()` / `touch_pad_intr_disable()`

When interrupts are operational, you can obtain the information from which particular pad an interrupt came by invoking `touch_pad_get_status()` and clear the pad status with `touch_pad_clear_status()`.

## Application Examples

- peripherals/touch_sensor/touch_sensor_v2/touch_pad_read demonstrates how to read and display raw values from capacitive touch pad sensors on ESP32-S2, including how to calibrate the sensors and detect touch actions.

- peripherals/touch_sensor/touch_sensor_v2/touch_pad_interrupt demonstrates how to set up ESP32-S2's capacitive touch pad peripheral to trigger an interrupt when a pad is touched, and how to detect the touch event by the software for sensor designs when greater touch detection sensitivity is required.

## API Reference

### Header File

- components/driver/touch_sensor/esp32s2/include/driver/touch_sensor.h

- This header file can be included with:

  >     #include "driver/touch_sensor.h"

- This header file is a part of the API provided by the `driver` component. To declare that your component depends on `driver`, add the following to your CMakeLists.txt:

  >     REQUIRES driver

  > or

  >     PRIV_REQUIRES driver

### Functions

esp_err_t touch_pad_fsm_start(void)

  Set touch sensor FSM start.

  Note

  Start FSM after the touch sensor FSM mode is set.

  Note

  Call this function will reset benchmark of all touch channels.

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_fsm_stop(void)

  Stop touch sensor FSM.

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_sw_start(void)

  Trigger a touch sensor measurement, only support in SW mode of FSM.

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_set_charge_discharge_times(uint16_t charge_discharge_times)

  Set charge and discharge times of each measurement.

  Note

  This function will specify the charge and discharge times in each measurement period The clock is sourced from SOC_MOD_CLK_RTC_FAST, and its default frequency is SOC_CLK_RC_FAST_FREQ_APPROX The touch sensor will record the total clock cycles of all the charge and discharge cycles as the final result (raw value)

  Note

  If the charge and discharge times is too small, it may lead to inaccurate results.

  Parameters:

    charge_discharge_times -- Charge and discharge times, range: 0 ~ 0xffff. No exact typical value can be recommended because the capacity is influenced by the hardware design and how finger touches, but suggest adjusting this value to make the measurement time around 1 ms.

  Returns:

    - ESP_OK Set charge and discharge times success

esp_err_t touch_pad_get_charge_discharge_times(uint16_t *charge_discharge_times)

  Get charge and discharge times of each measurement.

  Parameters:

    charge_discharge_times -- Charge and discharge times

  Returns:

    - ESP_OK Get charge_discharge_times success

    - ESP_ERR_INVALID_ARG The input parameter is NULL

esp_err_t touch_pad_set_measurement_interval(uint16_t interval_cycle)

  Set the interval between two measurements.

  Note

  The touch sensor will sleep between two measurements This function is to set the interval cycle And the interval is clocked from SOC_MOD_CLK_RTC_SLOW, its default frequency is SOC_CLK_RC_SLOW_FREQ_APPROX

  Parameters:

    interval_cycle -- The interval between two measurements sleep_time = interval_cycle / SOC_CLK_RC_SLOW_FREQ_APPROX. The approximate frequency value of RTC_SLOW_CLK can be obtained using rtc_clk_slow_freq_get_hz function.

  Returns:

    - ESP_OK Set interval cycle success

esp_err_t touch_pad_get_measurement_interval(uint16_t *interval_cycle)

  Get the interval between two measurements.

  Parameters:

    interval_cycle -- The interval between two measurements

  Returns:

    - ESP_OK Get interval cycle success

    - ESP_ERR_INVALID_ARG The input parameter is NULL

esp_err_t touch_pad_set_meas_time(uint16_t sleep_cycle, uint16_t meas_times)

  Set touch sensor times of charge and discharge and sleep time. Excessive total time will slow down the touch response. Too small measurement time will not be sampled enough, resulting in inaccurate measurements.

  Note

  The touch sensor will measure time of a fixed number of charge/discharge cycles (specified as the second parameter). That means the time (raw value) will increase as the capacity of the touch pad is increasing. The time (raw value) here is the number of clock cycles which is sourced from SOC_MOD_CLK_RTC_FAST and at (SOC_CLK_RC_FAST_FREQ_APPROX) Hz as default

  Note

  The greater the duty cycle of the measurement time, the more system power is consumed.

  Parameters:

    - sleep_cycle -- The touch sensor will sleep after each measurement. sleep_cycle decide the interval between each measurement. t_sleep = sleep_cycle / SOC_CLK_RC_SLOW_FREQ_APPROX. The approximate frequency value of RTC_SLOW_CLK can be obtained using rtc_clk_slow_freq_get_hz function.

    - meas_times -- The times of charge and discharge in each measurement of touch channels. Range: 0 ~ 0xffff. Recommended typical value: Modify this value to make the measurement time around 1 ms.

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_get_meas_time(uint16_t *sleep_cycle, uint16_t *meas_times)

  Get touch sensor times of charge and discharge and sleep time.

  Parameters:

    - sleep_cycle -- Pointer to accept sleep cycle number

    - meas_times -- Pointer to accept measurement times count.

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_set_idle_channel_connect(touch_pad_conn_type_t type)

  Set the connection type of touch channels in idle status. When a channel is in measurement mode, other initialized channels are in idle mode. The touch channel is generally adjacent to the trace, so the connection state of the idle channel affects the stability and sensitivity of the test channel. The `CONN_HIGHZ`(high resistance) setting increases the sensitivity of touch channels. The `CONN_GND`(grounding) setting increases the stability of touch channels.

  Parameters:

    type -- Select idle channel connect to high resistance state or ground.

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_get_idle_channel_connect(touch_pad_conn_type_t *type)

  Get the connection type of touch channels in idle status. When a channel is in measurement mode, other initialized channels are in idle mode. The touch channel is generally adjacent to the trace, so the connection state of the idle channel affects the stability and sensitivity of the test channel. The `CONN_HIGHZ`(high resistance) setting increases the sensitivity of touch channels. The `CONN_GND`(grounding) setting increases the stability of touch channels.

  Parameters:

    type -- Pointer to connection type.

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_set_thresh(touch_pad_t touch_num, uint32_t threshold)

  Set the trigger threshold of touch sensor. The threshold determines the sensitivity of the touch sensor. The threshold is the original value of the trigger state minus the benchmark value.

  Note

  If set "TOUCH_PAD_THRESHOLD_MAX", the touch is never be triggered.

  Parameters:

    - touch_num -- touch pad index

    - threshold -- threshold of touch sensor. Should be less than the max change value of touch.

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_get_thresh(touch_pad_t touch_num, uint32_t *threshold)

  Get touch sensor trigger threshold.

  Parameters:

    - touch_num -- touch pad index

    - threshold -- pointer to accept threshold

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if argument is wrong

esp_err_t touch_pad_set_channel_mask(uint16_t enable_mask)

  Register touch channel into touch sensor scan group. The working mode of the touch sensor is cyclically scanned. This function will set the scan bits according to the given bitmask.

  Note

  If set this mask, the FSM timer should be stop firsty.

  Note

  The touch sensor that in scan map, should be deinit GPIO function firstly by `touch_pad_io_init`.

  Parameters:

    enable_mask -- bitmask of touch sensor scan group. e.g. TOUCH_PAD_NUM14 -> BIT(14)

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_get_channel_mask(uint16_t *enable_mask)

  Get the touch sensor scan group bit mask.

  Parameters:

    enable_mask -- Pointer to bitmask of touch sensor scan group. e.g. TOUCH_PAD_NUM14 -> BIT(14)

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_clear_channel_mask(uint16_t enable_mask)

  Clear touch channel from touch sensor scan group. The working mode of the touch sensor is cyclically scanned. This function will clear the scan bits according to the given bitmask.

  Note

  If clear all mask, the FSM timer should be stop firsty.

  Parameters:

    enable_mask -- bitmask of touch sensor scan group. e.g. TOUCH_PAD_NUM14 -> BIT(14)

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_config(touch_pad_t touch_num)

  Configure parameter for each touch channel.

  Note

  Touch num 0 is denoise channel, please use `touch_pad_denoise_enable` to set denoise function

  Parameters:

    touch_num -- touch pad index

  Returns:

    - ESP_OK Success

    - ESP_ERR_INVALID_ARG if argument wrong

    - ESP_FAIL if touch pad not initialized

esp_err_t touch_pad_reset(void)

  Reset the FSM of touch module.

  Note

  Call this function after `touch_pad_fsm_stop`.

  Returns:

    - ESP_OK Success

touch_pad_t touch_pad_get_current_meas_channel(void)

  Get the current measure channel.

  Note

  Should be called when touch sensor measurement is in cyclic scan mode.

  Returns:

    - touch channel number

uint32_t touch_pad_read_intr_status_mask(void)

  Get the touch sensor interrupt status mask.

  Returns:

    - touch interrupt bit

esp_err_t touch_pad_intr_enable(touch_pad_intr_mask_t int_mask)

  Enable touch sensor interrupt by bitmask.

  Note

  This API can be called in ISR handler.

  Parameters:

    int_mask -- Pad mask to enable interrupts

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_intr_disable(touch_pad_intr_mask_t int_mask)

  Disable touch sensor interrupt by bitmask.

  Note

  This API can be called in ISR handler.

  Parameters:

    int_mask -- Pad mask to disable interrupts

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_intr_clear(touch_pad_intr_mask_t int_mask)

  Clear touch sensor interrupt by bitmask.

  Parameters:

    int_mask -- Pad mask to clear interrupts

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_isr_register(intr_handler_t fn, void *arg, touch_pad_intr_mask_t intr_mask)

  Register touch-pad ISR. The handler will be attached to the same CPU core that this function is running on.

  Parameters:

    - fn -- Pointer to ISR handler

    - arg -- Parameter for ISR

    - intr_mask -- Enable touch sensor interrupt handler by bitmask.

  Returns:

    - ESP_OK Success

    - ESP_ERR_INVALID_ARG Arguments error

    - ESP_ERR_NO_MEM No memory

esp_err_t touch_pad_timeout_set(bool enable, uint32_t threshold)

  Enable/disable the timeout check and set timeout threshold for all touch sensor channels measurements. If enable: When the touch reading of a touch channel exceeds the measurement threshold, a timeout interrupt will be generated. If disable: the FSM does not check if the channel under measurement times out.

  Note

  The threshold compared with touch readings.

  Note

  In order to avoid abnormal short circuit of some touch channels. This function should be turned on. Ensure the normal operation of other touch channels.

  Parameters:

    - enable -- true(default): Enable the timeout check; false: Disable the timeout check.

    - threshold -- For all channels, the maximum value that will not be exceeded during normal operation.

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_timeout_resume(void)

  Call this interface after timeout to make the touch channel resume normal work. Point on the next channel to measure. If this API is not called, the touch FSM will stop the measurement after timeout interrupt.

  Note

  Call this API after finishes the exception handling by user.

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_read_raw_data(touch_pad_t touch_num, uint32_t *raw_data)

  get raw data of touch sensor.

  Note

  After the initialization is complete, the "raw_data" is max value. You need to wait for a measurement cycle before you can read the correct touch value.

  Parameters:

    - touch_num -- touch pad index

    - raw_data -- pointer to accept touch sensor value

  Returns:

    - ESP_OK Success

    - ESP_FAIL Touch channel 0 haven't this parameter.

esp_err_t touch_pad_read_benchmark(touch_pad_t touch_num, uint32_t *benchmark)

  get benchmark of touch sensor.

  Note

  After initialization, the benchmark value is the maximum during the first measurement period.

  Parameters:

    - touch_num -- touch pad index

    - benchmark -- pointer to accept touch sensor benchmark value

  Returns:

    - ESP_OK Success

    - ESP_ERR_INVALID_ARG Touch channel 0 haven't this parameter.

esp_err_t touch_pad_filter_read_smooth(touch_pad_t touch_num, uint32_t *smooth)

  Get smoothed data that obtained by filtering the raw data.

  Parameters:

    - touch_num -- touch pad index

    - smooth -- pointer to smoothed data

esp_err_t touch_pad_reset_benchmark(touch_pad_t touch_num)

  Force reset benchmark to raw data of touch sensor.

  Parameters:

    touch_num -- touch pad index

    - TOUCH_PAD_MAX Reset basaline of all channels

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_filter_set_config(const touch_filter_config_t *filter_info)

  set parameter of touch sensor filter and detection algorithm. For more details on the detection algorithm, please refer to the application documentation.

  Parameters:

    filter_info -- select filter type and threshold of detection algorithm

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_filter_get_config(touch_filter_config_t *filter_info)

  get parameter of touch sensor filter and detection algorithm. For more details on the detection algorithm, please refer to the application documentation.

  Parameters:

    filter_info -- select filter type and threshold of detection algorithm

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_filter_enable(void)

  enable touch sensor filter for detection algorithm. For more details on the detection algorithm, please refer to the application documentation.

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_filter_disable(void)

  disable touch sensor filter for detection algorithm. For more details on the detection algorithm, please refer to the application documentation.

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_denoise_set_config(const touch_pad_denoise_t *denoise)

  set parameter of denoise pad (TOUCH_PAD_NUM0). T0 is an internal channel that does not have a corresponding external GPIO. T0 will work simultaneously with the measured channel Tn. Finally, the actual measured value of Tn is the value after subtracting lower bits of T0. The noise reduction function filters out interference introduced simultaneously on all channels, such as noise introduced by power supplies and external EMI.

  Parameters:

    denoise -- parameter of denoise

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_denoise_get_config(touch_pad_denoise_t *denoise)

  get parameter of denoise pad (TOUCH_PAD_NUM0).

  Parameters:

    denoise -- Pointer to parameter of denoise

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_denoise_enable(void)

  enable denoise function. T0 is an internal channel that does not have a corresponding external GPIO. T0 will work simultaneously with the measured channel Tn. Finally, the actual measured value of Tn is the value after subtracting lower bits of T0. The noise reduction function filters out interference introduced simultaneously on all channels, such as noise introduced by power supplies and external EMI.

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_denoise_disable(void)

  disable denoise function.

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_denoise_read_data(uint32_t *data)

  Get denoise measure value (TOUCH_PAD_NUM0).

  Parameters:

    data -- Pointer to receive denoise value

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_waterproof_set_config(const touch_pad_waterproof_t *waterproof)

  set parameter of waterproof function.

         The waterproof function includes a shielded channel (TOUCH_PAD_NUM14) and a guard channel.
         Guard pad is used to detect the large area of water covering the touch panel.
         Shield pad is used to shield the influence of water droplets covering the touch panel.
         It is generally designed as a grid and is placed around the touch buttons.

  Parameters:

    waterproof -- parameter of waterproof

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_waterproof_get_config(touch_pad_waterproof_t *waterproof)

  get parameter of waterproof function.

  Parameters:

    waterproof -- parameter of waterproof

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_waterproof_enable(void)

  Enable parameter of waterproof function. Should be called after function `touch_pad_waterproof_set_config`.

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_waterproof_disable(void)

  Disable parameter of waterproof function.

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_proximity_enable(touch_pad_t touch_num, bool enabled)

  Enable/disable proximity function of touch channels. The proximity sensor measurement is the accumulation of touch channel measurements.

  Note

  Supports up to three touch channels configured as proximity sensors.

  Parameters:

    - touch_num -- touch pad index

    - enabled -- true: enable the proximity function; false: disable the proximity function

  Returns:

    - ESP_OK: Configured correctly.

    - ESP_ERR_INVALID_ARG: Touch channel number error.

    - ESP_ERR_NOT_SUPPORTED: Don't support configured.

esp_err_t touch_pad_proximity_set_count(touch_pad_t touch_num, uint32_t count)

  Set measure count of proximity channel. The proximity sensor measurement is the accumulation of touch channel measurements.

  Note

  All proximity channels use the same `count` value. So please pass the parameter `TOUCH_PAD_MAX`.

  Parameters:

    - touch_num -- Touch pad index. In this version, pass the parameter `TOUCH_PAD_MAX`.

    - count -- The cumulative times of measurements for proximity pad. Range: 0 ~ 255.

  Returns:

    - ESP_OK: Configured correctly.

    - ESP_ERR_INVALID_ARG: Touch channel number error.

esp_err_t touch_pad_proximity_get_count(touch_pad_t touch_num, uint32_t *count)

  Get measure count of proximity channel. The proximity sensor measurement is the accumulation of touch channel measurements.

  Note

  All proximity channels use the same `count` value. So please pass the parameter `TOUCH_PAD_MAX`.

  Parameters:

    - touch_num -- Touch pad index. In this version, pass the parameter `TOUCH_PAD_MAX`.

    - count -- The cumulative times of measurements for proximity pad. Range: 0 ~ 255.

  Returns:

    - ESP_OK: Configured correctly.

    - ESP_ERR_INVALID_ARG: Touch channel number error.

esp_err_t touch_pad_proximity_get_data(touch_pad_t touch_num, uint32_t *measure_out)

  Get the accumulated measurement of the proximity sensor. The proximity sensor measurement is the accumulation of touch channel measurements.

  Parameters:

    - touch_num -- touch pad index

    - measure_out -- If the accumulation process does not end, the `measure_out` is the process value.

  Returns:

    - ESP_OK Success

    - ESP_ERR_INVALID_ARG Touch num is not proximity

esp_err_t touch_pad_sleep_channel_get_info(touch_pad_sleep_channel_t *slp_config)

  Get parameter of touch sensor sleep channel. The touch sensor can works in sleep mode to wake up sleep.

  Note

  After the sleep channel is configured, Please use special functions for sleep channel. e.g. The user should uses `touch_pad_sleep_channel_read_data` instead of `touch_pad_read_raw_data` to obtain the sleep channel reading.

  Parameters:

    slp_config -- touch sleep pad config.

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_sleep_channel_enable(touch_pad_t pad_num, bool enable)

  Enable/Disable sleep channel function for touch sensor. The touch sensor can works in sleep mode to wake up sleep.

  Note

  ESP32S2 only support one sleep channel.

  Note

  After the sleep channel is configured, Please use special functions for sleep channel. e.g. The user should uses `touch_pad_sleep_channel_read_data` instead of `touch_pad_read_raw_data` to obtain the sleep channel reading.

  Parameters:

    - pad_num -- Set touch channel number for sleep pad. Only one touch sensor channel is supported in deep sleep mode.

    - enable -- true: enable sleep pad for touch sensor; false: disable sleep pad for touch sensor;

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_sleep_channel_enable_proximity(touch_pad_t pad_num, bool enable)

  Enable/Disable proximity function for sleep channel. The touch sensor can works in sleep mode to wake up sleep.

  Note

  ESP32S2 only support one sleep channel.

  Parameters:

    - pad_num -- Set touch channel number for sleep pad. Only one touch sensor channel is supported in deep sleep mode.

    - enable -- true: enable proximity for sleep channel; false: disable proximity for sleep channel;

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_sleep_set_threshold(touch_pad_t pad_num, uint32_t touch_thres)

  Set the trigger threshold of touch sensor in deep sleep. The threshold determines the sensitivity of the touch sensor.

  Note

  In general, the touch threshold during sleep can use the threshold parameter parameters before sleep.

  Parameters:

    - pad_num -- Set touch channel number for sleep pad. Only one touch sensor channel is supported in deep sleep mode.

    - touch_thres -- touch sleep pad threshold

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_sleep_get_threshold(touch_pad_t pad_num, uint32_t *touch_thres)

  Get the trigger threshold of touch sensor in deep sleep. The threshold determines the sensitivity of the touch sensor.

  Note

  In general, the touch threshold during sleep can use the threshold parameter parameters before sleep.

  Parameters:

    - pad_num -- Set touch channel number for sleep pad. Only one touch sensor channel is supported in deep sleep mode.

    - touch_thres -- touch sleep pad threshold

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_sleep_channel_read_benchmark(touch_pad_t pad_num, uint32_t *benchmark)

  Read benchmark of touch sensor sleep channel.

  Parameters:

    - pad_num -- Set touch channel number for sleep pad. Only one touch sensor channel is supported in deep sleep mode.

    - benchmark -- pointer to accept touch sensor benchmark value

  Returns:

    - ESP_OK Success

    - ESP_ERR_INVALID_ARG parameter is NULL

esp_err_t touch_pad_sleep_channel_read_smooth(touch_pad_t pad_num, uint32_t *smooth_data)

  Read smoothed data of touch sensor sleep channel. Smoothed data is filtered from the raw data.

  Parameters:

    - pad_num -- Set touch channel number for sleep pad. Only one touch sensor channel is supported in deep sleep mode.

    - smooth_data -- pointer to accept touch sensor smoothed data

  Returns:

    - ESP_OK Success

    - ESP_ERR_INVALID_ARG parameter is NULL

esp_err_t touch_pad_sleep_channel_read_data(touch_pad_t pad_num, uint32_t *raw_data)

  Read raw data of touch sensor sleep channel.

  Parameters:

    - pad_num -- Set touch channel number for sleep pad. Only one touch sensor channel is supported in deep sleep mode.

    - raw_data -- pointer to accept touch sensor raw data

  Returns:

    - ESP_OK Success

    - ESP_ERR_INVALID_ARG parameter is NULL

esp_err_t touch_pad_sleep_channel_reset_benchmark(void)

  Reset benchmark of touch sensor sleep channel.

  Returns:

    - ESP_OK Success

esp_err_t touch_pad_sleep_channel_read_proximity_cnt(touch_pad_t pad_num, uint32_t *proximity_cnt)

  Read proximity count of touch sensor sleep channel.

  Parameters:

    - pad_num -- Set touch channel number for sleep pad. Only one touch sensor channel is supported in deep sleep mode.

    - proximity_cnt -- pointer to accept touch sensor proximity count value

  Returns:

    - ESP_OK Success

    - ESP_ERR_INVALID_ARG parameter is NULL

esp_err_t touch_pad_sleep_channel_set_work_time(uint16_t sleep_cycle, uint16_t meas_times)

  Change the operating frequency of touch pad in deep sleep state. Reducing the operating frequency can effectively reduce power consumption. If this function is not called, the working frequency of touch in the deep sleep state is the same as that in the wake-up state.

  Parameters:

    - sleep_cycle -- The touch sensor will sleep after each measurement. sleep_cycle decide the interval between each measurement. t_sleep = sleep_cycle / (RTC_SLOW_CLK frequency). The approximate frequency value of RTC_SLOW_CLK can be obtained using rtc_clk_slow_freq_get_hz function.

    - meas_times -- The times of charge and discharge in each measure process of touch channels. The timer frequency is 8Mhz. Range: 0 ~ 0xffff. Recommended typical value: Modify this value to make the measurement time around 1ms.

  Returns:

    - ESP_OK Success

### Header File

- components/driver/touch_sensor/include/driver/touch_sensor_common.h

- This header file can be included with:

  >     #include "driver/touch_sensor_common.h"

- This header file is a part of the API provided by the `driver` component. To declare that your component depends on `driver`, add the following to your CMakeLists.txt:

  >     REQUIRES driver

  > or

  >     PRIV_REQUIRES driver

### Functions

esp_err_t touch_pad_init(void)

  Initialize touch module.

  Note

  If default parameter don't match the usage scenario, it can be changed after this function.

  Returns:

    - ESP_OK Success

    - ESP_ERR_NO_MEM Touch pad init error

    - ESP_ERR_NOT_SUPPORTED Touch pad is providing current to external XTAL

esp_err_t touch_pad_deinit(void)

  Un-install touch pad driver.

  Note

  After this function is called, other touch functions are prohibited from being called.

  Returns:

    - ESP_OK Success

    - ESP_FAIL Touch pad driver not initialized

esp_err_t touch_pad_io_init(touch_pad_t touch_num)

  Initialize touch pad GPIO.

  Parameters:

    touch_num -- touch pad index

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if argument is wrong

esp_err_t touch_pad_set_voltage(touch_high_volt_t refh, touch_low_volt_t refl, touch_volt_atten_t atten)

  Set touch sensor high voltage threshold of chanrge. The touch sensor measures the channel capacitance value by charging and discharging the channel. So the high threshold should be less than the supply voltage.

  Parameters:

    - refh -- the value of DREFH

    - refl -- the value of DREFL

    - atten -- the attenuation on DREFH

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if argument is wrong

esp_err_t touch_pad_get_voltage(touch_high_volt_t *refh, touch_low_volt_t *refl, touch_volt_atten_t *atten)

  Get touch sensor reference voltage,.

  Parameters:

    - refh -- pointer to accept DREFH value

    - refl -- pointer to accept DREFL value

    - atten -- pointer to accept the attenuation on DREFH

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_set_cnt_mode(touch_pad_t touch_num, touch_cnt_slope_t slope, touch_tie_opt_t opt)

  Set touch sensor charge/discharge speed for each pad. If the slope is 0, the counter would always be zero. If the slope is 1, the charging and discharging would be slow, accordingly. If the slope is set 7, which is the maximum value, the charging and discharging would be fast.

  Note

  The higher the charge and discharge current, the greater the immunity of the touch channel, but it will increase the system power consumption.

  Parameters:

    - touch_num -- touch pad index

    - slope -- touch pad charge/discharge speed

    - opt -- the initial voltage

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if argument is wrong

esp_err_t touch_pad_get_cnt_mode(touch_pad_t touch_num, touch_cnt_slope_t *slope, touch_tie_opt_t *opt)

  Get touch sensor charge/discharge speed for each pad.

  Parameters:

    - touch_num -- touch pad index

    - slope -- pointer to accept touch pad charge/discharge slope

    - opt -- pointer to accept the initial voltage

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if argument is wrong

esp_err_t touch_pad_isr_deregister(void (*fn)(void*), void *arg)

  Deregister the handler previously registered using touch_pad_isr_handler_register.

  Parameters:

    - fn -- handler function to call (as passed to touch_pad_isr_handler_register)

    - arg -- argument of the handler (as passed to touch_pad_isr_handler_register)

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_STATE if a handler matching both fn and arg isn't registered

esp_err_t touch_pad_get_wakeup_status(touch_pad_t *pad_num)

  Get the touch pad which caused wakeup from deep sleep.

  Parameters:

    pad_num -- pointer to touch pad which caused wakeup

  Returns:

    - ESP_OK Success

    - ESP_ERR_INVALID_ARG parameter is NULL

esp_err_t touch_pad_set_fsm_mode(touch_fsm_mode_t mode)

  Set touch sensor FSM mode, the test action can be triggered by the timer, as well as by the software.

  Parameters:

    mode -- FSM mode

  Returns:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if argument is wrong

esp_err_t touch_pad_get_fsm_mode(touch_fsm_mode_t *mode)

  Get touch sensor FSM mode.

  Parameters:

    mode -- pointer to accept FSM mode

  Returns:

    - ESP_OK on success

esp_err_t touch_pad_clear_status(void)

  To clear the touch sensor channel active status.

  Note

  The FSM automatically updates the touch sensor status. It is generally not necessary to call this API to clear the status.

  Returns:

    - ESP_OK on success

uint32_t touch_pad_get_status(void)

  Get the touch sensor channel active status mask. The bit position represents the channel number. The 0/1 status of the bit represents the trigger status.

  Returns:

    - The touch sensor status. e.g. Touch1 trigger status is `status_mask & (BIT1)`.

bool touch_pad_meas_is_done(void)

  Check touch sensor measurement status.

  Returns:

    - True measurement is under way

    - False measurement done

### GPIO Lookup Macros

Some useful macros can be used to specified the GPIO number of a touch pad channel, or vice versa. e.g.,

1. `TOUCH_PAD_NUM5_GPIO_NUM` is the GPIO number of channel 5 (12);

2. `TOUCH_PAD_GPIO4_CHANNEL` is the channel number of GPIO 4 (channel 0).

### Header File

- components/soc/esp32s2/include/soc/touch_sensor_channel.h

- This header file can be included with:

  >     #include "soc/touch_sensor_channel.h"

### Macros

TOUCH_PAD_GPIO1_CHANNEL

TOUCH_PAD_NUM1_GPIO_NUM

TOUCH_PAD_GPIO2_CHANNEL

TOUCH_PAD_NUM2_GPIO_NUM

TOUCH_PAD_GPIO3_CHANNEL

TOUCH_PAD_NUM3_GPIO_NUM

TOUCH_PAD_GPIO4_CHANNEL

TOUCH_PAD_NUM4_GPIO_NUM

TOUCH_PAD_GPIO5_CHANNEL

TOUCH_PAD_NUM5_GPIO_NUM

TOUCH_PAD_GPIO6_CHANNEL

TOUCH_PAD_NUM6_GPIO_NUM

TOUCH_PAD_GPIO7_CHANNEL

TOUCH_PAD_NUM7_GPIO_NUM

TOUCH_PAD_GPIO8_CHANNEL

TOUCH_PAD_NUM8_GPIO_NUM

TOUCH_PAD_GPIO9_CHANNEL

TOUCH_PAD_NUM9_GPIO_NUM

TOUCH_PAD_GPIO10_CHANNEL

TOUCH_PAD_NUM10_GPIO_NUM

TOUCH_PAD_GPIO11_CHANNEL

TOUCH_PAD_NUM11_GPIO_NUM

TOUCH_PAD_GPIO12_CHANNEL

TOUCH_PAD_NUM12_GPIO_NUM

TOUCH_PAD_GPIO13_CHANNEL

TOUCH_PAD_NUM13_GPIO_NUM

TOUCH_PAD_GPIO14_CHANNEL

TOUCH_PAD_NUM14_GPIO_NUM

### Header File

- components/hal/include/hal/touch_sensor_types.h

- This header file can be included with:

  >     #include "hal/touch_sensor_types.h"

### Structures

struct touch_pad_denoise

  Touch sensor denoise configuration

  Public Members

  touch_pad_denoise_grade_t grade

    Select denoise range of denoise channel. Determined by measuring the noise amplitude of the denoise channel.

  touch_pad_denoise_cap_t cap_level

    Select internal reference capacitance of denoise channel. Ensure that the denoise readings are closest to the readings of the channel being measured. Use `touch_pad_denoise_read_data` to get the reading of denoise channel. The equivalent capacitance of the shielded channel can be calculated from the reading of denoise channel.

struct touch_pad_waterproof

  Touch sensor waterproof configuration

  Public Members

  touch_pad_t guard_ring_pad

    Waterproof. Select touch channel use for guard pad. Guard pad is used to detect the large area of water covering the touch panel.

  touch_pad_shield_driver_t shield_driver

    Waterproof. Shield channel drive capability configuration. Shield pad is used to shield the influence of water droplets covering the touch panel. When the waterproof function is enabled, Touch14 is set as shield channel by default. The larger the parasitic capacitance on the shielding channel, the higher the drive capability needs to be set. The equivalent capacitance of the shield channel can be estimated through the reading value of the denoise channel(Touch0).

struct touch_filter_config

  Touch sensor filter configuration

  Public Members

  touch_filter_mode_t mode

    Set filter mode. The input of the filter is the raw value of touch reading, and the output of the filter is involved in the judgment of the touch state.

  uint32_t debounce_cnt

    Set debounce count, such as `n`. If the measured values continue to exceed the threshold for `n+1` times, the touch sensor state changes. Range: 0 ~ 7

  uint32_t noise_thr

    Noise threshold coefficient. Higher = More noise resistance. The actual noise should be less than (noise coefficient * touch threshold). Range: 0 ~ 3. The coefficient is 0: 4/8; 1: 3/8; 2: 2/8; 3: 1;

  uint32_t jitter_step

    Set jitter filter step size. Range: 0 ~ 15

  touch_smooth_mode_t smh_lvl

    Level of filter applied on the original data against large noise interference.

struct touch_pad_sleep_channel_t

  Touch sensor channel sleep configuration

  Public Members

  touch_pad_t touch_num

    Set touch channel number for sleep pad. Only one touch sensor channel is supported in deep sleep mode. If clear the sleep channel, point this pad to `TOUCH_PAD_NUM0`

  bool en_proximity

    enable proximity function for sleep pad

### Macros

TOUCH_PAD_BIT_MASK_ALL

TOUCH_PAD_SLOPE_DEFAULT

TOUCH_PAD_TIE_OPT_DEFAULT

TOUCH_PAD_BIT_MASK_MAX

TOUCH_PAD_HIGH_VOLTAGE_THRESHOLD

TOUCH_PAD_LOW_VOLTAGE_THRESHOLD

TOUCH_PAD_ATTEN_VOLTAGE_THRESHOLD

TOUCH_PAD_IDLE_CH_CONNECT_DEFAULT

TOUCH_PAD_THRESHOLD_MAX

  If set touch threshold max value, The touch sensor can't be in touched status

TOUCH_PAD_SLEEP_CYCLE_DEFAULT

  Excessive total time will slow down the touch response. Too small measurement time will not be sampled enough, resulting in inaccurate measurements.

  Note

  The greater the duty cycle of the measurement time, the more system power is consumed. The number of sleep cycle in each measure process of touch channels. The timer frequency is RTC_SLOW_CLK (can be 150k or 32k depending on the options). Range: 0 ~ 0xffff

TOUCH_PAD_MEASURE_CYCLE_DEFAULT

  The times of charge and discharge in each measure process of touch channels. The timer frequency is 8Mhz. Recommended typical value: Modify this value to make the measurement time around 1ms. Range: 0 ~ 0xffff

TOUCH_PAD_INTR_MASK_ALL

  All touch interrupt type enable.

TOUCH_PROXIMITY_MEAS_NUM_MAX

  Touch sensor proximity detection configuration

TOUCH_DEBOUNCE_CNT_MAX

TOUCH_NOISE_THR_MAX

TOUCH_JITTER_STEP_MAX

### Type Definitions

typedef struct touch_pad_denoise touch_pad_denoise_t

  Touch sensor denoise configuration

typedef struct touch_pad_waterproof touch_pad_waterproof_t

  Touch sensor waterproof configuration

typedef struct touch_filter_config touch_filter_config_t

  Touch sensor filter configuration

### Enumerations

enum touch_pad_t

  Touch pad channel

  Values:

  enumerator TOUCH_PAD_NUM0

    Touch pad channel 0 is GPIO4(ESP32)

  enumerator TOUCH_PAD_NUM1

    Touch pad channel 1 is GPIO0(ESP32) / GPIO1(ESP32-S2)

  enumerator TOUCH_PAD_NUM2

    Touch pad channel 2 is GPIO2(ESP32) / GPIO2(ESP32-S2)

  enumerator TOUCH_PAD_NUM3

    Touch pad channel 3 is GPIO15(ESP32) / GPIO3(ESP32-S2)

  enumerator TOUCH_PAD_NUM4

    Touch pad channel 4 is GPIO13(ESP32) / GPIO4(ESP32-S2)

  enumerator TOUCH_PAD_NUM5

    Touch pad channel 5 is GPIO12(ESP32) / GPIO5(ESP32-S2)

  enumerator TOUCH_PAD_NUM6

    Touch pad channel 6 is GPIO14(ESP32) / GPIO6(ESP32-S2)

  enumerator TOUCH_PAD_NUM7

    Touch pad channel 7 is GPIO27(ESP32) / GPIO7(ESP32-S2)

  enumerator TOUCH_PAD_NUM8

    Touch pad channel 8 is GPIO33(ESP32) / GPIO8(ESP32-S2)

  enumerator TOUCH_PAD_NUM9

    Touch pad channel 9 is GPIO32(ESP32) / GPIO9(ESP32-S2)

  enumerator TOUCH_PAD_NUM10

    Touch channel 10 is GPIO10(ESP32-S2)

  enumerator TOUCH_PAD_NUM11

    Touch channel 11 is GPIO11(ESP32-S2)

  enumerator TOUCH_PAD_NUM12

    Touch channel 12 is GPIO12(ESP32-S2)

  enumerator TOUCH_PAD_NUM13

    Touch channel 13 is GPIO13(ESP32-S2)

  enumerator TOUCH_PAD_NUM14

    Touch channel 14 is GPIO14(ESP32-S2)

  enumerator TOUCH_PAD_MAX

enum touch_high_volt_t

  Touch sensor high reference voltage

  Values:

  enumerator TOUCH_HVOLT_KEEP

    Touch sensor high reference voltage, no change

  enumerator TOUCH_HVOLT_2V4

    Touch sensor high reference voltage, 2.4V

  enumerator TOUCH_HVOLT_2V5

    Touch sensor high reference voltage, 2.5V

  enumerator TOUCH_HVOLT_2V6

    Touch sensor high reference voltage, 2.6V

  enumerator TOUCH_HVOLT_2V7

    Touch sensor high reference voltage, 2.7V

  enumerator TOUCH_HVOLT_MAX

enum touch_low_volt_t

  Touch sensor low reference voltage

  Values:

  enumerator TOUCH_LVOLT_KEEP

    Touch sensor low reference voltage, no change

  enumerator TOUCH_LVOLT_0V5

    Touch sensor low reference voltage, 0.5V

  enumerator TOUCH_LVOLT_0V6

    Touch sensor low reference voltage, 0.6V

  enumerator TOUCH_LVOLT_0V7

    Touch sensor low reference voltage, 0.7V

  enumerator TOUCH_LVOLT_0V8

    Touch sensor low reference voltage, 0.8V

  enumerator TOUCH_LVOLT_MAX

enum touch_volt_atten_t

  Touch sensor high reference voltage attenuation

  Values:

  enumerator TOUCH_HVOLT_ATTEN_KEEP

    Touch sensor high reference voltage attenuation, no change

  enumerator TOUCH_HVOLT_ATTEN_1V5

    Touch sensor high reference voltage attenuation, 1.5V attenuation

  enumerator TOUCH_HVOLT_ATTEN_1V

    Touch sensor high reference voltage attenuation, 1.0V attenuation

  enumerator TOUCH_HVOLT_ATTEN_0V5

    Touch sensor high reference voltage attenuation, 0.5V attenuation

  enumerator TOUCH_HVOLT_ATTEN_0V

    Touch sensor high reference voltage attenuation, 0V attenuation

  enumerator TOUCH_HVOLT_ATTEN_MAX

enum touch_cnt_slope_t

  Touch sensor charge/discharge speed

  Values:

  enumerator TOUCH_PAD_SLOPE_0

    Touch sensor charge / discharge speed, always zero

  enumerator TOUCH_PAD_SLOPE_1

    Touch sensor charge / discharge speed, slowest

  enumerator TOUCH_PAD_SLOPE_2

    Touch sensor charge / discharge speed

  enumerator TOUCH_PAD_SLOPE_3

    Touch sensor charge / discharge speed

  enumerator TOUCH_PAD_SLOPE_4

    Touch sensor charge / discharge speed

  enumerator TOUCH_PAD_SLOPE_5

    Touch sensor charge / discharge speed

  enumerator TOUCH_PAD_SLOPE_6

    Touch sensor charge / discharge speed

  enumerator TOUCH_PAD_SLOPE_7

    Touch sensor charge / discharge speed, fast

  enumerator TOUCH_PAD_SLOPE_MAX

enum touch_tie_opt_t

  Touch sensor initial charge level

  Values:

  enumerator TOUCH_PAD_TIE_OPT_LOW

    Initial level of charging voltage, low level

  enumerator TOUCH_PAD_TIE_OPT_HIGH

    Initial level of charging voltage, high level

  enumerator TOUCH_PAD_TIE_OPT_FLOAT

    Initial level of charging voltage, float

  enumerator TOUCH_PAD_TIE_OPT_MAX

    The max tie options

enum touch_fsm_mode_t

  Touch sensor FSM mode

  Values:

  enumerator TOUCH_FSM_MODE_TIMER

    To start touch FSM by timer

  enumerator TOUCH_FSM_MODE_SW

    To start touch FSM by software trigger

  enumerator TOUCH_FSM_MODE_MAX

enum touch_trigger_mode_t

  Values:

  enumerator TOUCH_TRIGGER_BELOW

    Touch interrupt will happen if counter value is less than threshold.

  enumerator TOUCH_TRIGGER_ABOVE

    Touch interrupt will happen if counter value is larger than threshold.

  enumerator TOUCH_TRIGGER_MAX

enum touch_trigger_src_t

  Values:

  enumerator TOUCH_TRIGGER_SOURCE_BOTH

    wakeup interrupt is generated if both SET1 and SET2 are "touched"

  enumerator TOUCH_TRIGGER_SOURCE_SET1

    wakeup interrupt is generated if SET1 is "touched"

  enumerator TOUCH_TRIGGER_SOURCE_MAX

enum touch_pad_intr_mask_t

  Values:

  enumerator TOUCH_PAD_INTR_MASK_DONE

    Measurement done for one of the enabled channels.

  enumerator TOUCH_PAD_INTR_MASK_ACTIVE

    Active for one of the enabled channels.

  enumerator TOUCH_PAD_INTR_MASK_INACTIVE

    Inactive for one of the enabled channels.

  enumerator TOUCH_PAD_INTR_MASK_SCAN_DONE

    Measurement done for all the enabled channels.

  enumerator TOUCH_PAD_INTR_MASK_TIMEOUT

    Timeout for one of the enabled channels.

enum touch_pad_denoise_grade_t

  Values:

  enumerator TOUCH_PAD_DENOISE_BIT12

    Denoise range is 12bit

  enumerator TOUCH_PAD_DENOISE_BIT10

    Denoise range is 10bit

  enumerator TOUCH_PAD_DENOISE_BIT8

    Denoise range is 8bit

  enumerator TOUCH_PAD_DENOISE_BIT4

    Denoise range is 4bit

  enumerator TOUCH_PAD_DENOISE_MAX

enum touch_pad_denoise_cap_t

  Values:

  enumerator TOUCH_PAD_DENOISE_CAP_L0

    Denoise channel internal reference capacitance is 5pf

  enumerator TOUCH_PAD_DENOISE_CAP_L1

    Denoise channel internal reference capacitance is 6.4pf

  enumerator TOUCH_PAD_DENOISE_CAP_L2

    Denoise channel internal reference capacitance is 7.8pf

  enumerator TOUCH_PAD_DENOISE_CAP_L3

    Denoise channel internal reference capacitance is 9.2pf

  enumerator TOUCH_PAD_DENOISE_CAP_L4

    Denoise channel internal reference capacitance is 10.6pf

  enumerator TOUCH_PAD_DENOISE_CAP_L5

    Denoise channel internal reference capacitance is 12.0pf

  enumerator TOUCH_PAD_DENOISE_CAP_L6

    Denoise channel internal reference capacitance is 13.4pf

  enumerator TOUCH_PAD_DENOISE_CAP_L7

    Denoise channel internal reference capacitance is 14.8pf

  enumerator TOUCH_PAD_DENOISE_CAP_MAX

enum touch_pad_shield_driver_t

  Touch sensor shield channel drive capability level

  Values:

  enumerator TOUCH_PAD_SHIELD_DRV_L0

    The max equivalent capacitance in shield channel is 40pf

  enumerator TOUCH_PAD_SHIELD_DRV_L1

    The max equivalent capacitance in shield channel is 80pf

  enumerator TOUCH_PAD_SHIELD_DRV_L2

    The max equivalent capacitance in shield channel is 120pf

  enumerator TOUCH_PAD_SHIELD_DRV_L3

    The max equivalent capacitance in shield channel is 160pf

  enumerator TOUCH_PAD_SHIELD_DRV_L4

    The max equivalent capacitance in shield channel is 200pf

  enumerator TOUCH_PAD_SHIELD_DRV_L5

    The max equivalent capacitance in shield channel is 240pf

  enumerator TOUCH_PAD_SHIELD_DRV_L6

    The max equivalent capacitance in shield channel is 280pf

  enumerator TOUCH_PAD_SHIELD_DRV_L7

    The max equivalent capacitance in shield channel is 320pf

  enumerator TOUCH_PAD_SHIELD_DRV_MAX

enum touch_pad_conn_type_t

  Touch channel idle state configuration

  Values:

  enumerator TOUCH_PAD_CONN_HIGHZ

    Idle status of touch channel is high resistance state

  enumerator TOUCH_PAD_CONN_GND

    Idle status of touch channel is ground connection

  enumerator TOUCH_PAD_CONN_MAX

enum touch_filter_mode_t

  Touch channel IIR filter coefficient configuration.

  Note

  On ESP32S2. There is an error in the IIR calculation. The magnitude of the error is twice the filter coefficient. So please select a smaller filter coefficient on the basis of meeting the filtering requirements. Recommended filter coefficient selection `IIR_16`.

  Values:

  enumerator TOUCH_PAD_FILTER_IIR_4

    The filter mode is first-order IIR filter. The coefficient is 4.

  enumerator TOUCH_PAD_FILTER_IIR_8

    The filter mode is first-order IIR filter. The coefficient is 8.

  enumerator TOUCH_PAD_FILTER_IIR_16

    The filter mode is first-order IIR filter. The coefficient is 16 (Typical value).

  enumerator TOUCH_PAD_FILTER_IIR_32

    The filter mode is first-order IIR filter. The coefficient is 32.

  enumerator TOUCH_PAD_FILTER_IIR_64

    The filter mode is first-order IIR filter. The coefficient is 64.

  enumerator TOUCH_PAD_FILTER_IIR_128

    The filter mode is first-order IIR filter. The coefficient is 128.

  enumerator TOUCH_PAD_FILTER_IIR_256

    The filter mode is first-order IIR filter. The coefficient is 256.

  enumerator TOUCH_PAD_FILTER_JITTER

    The filter mode is jitter filter

  enumerator TOUCH_PAD_FILTER_MAX

enum touch_smooth_mode_t

  Level of filter applied on the original data against large noise interference.

  Note

  On ESP32S2. There is an error in the IIR calculation. The magnitude of the error is twice the filter coefficient. So please select a smaller filter coefficient on the basis of meeting the filtering requirements. Recommended filter coefficient selection `IIR_2`.

  Values:

  enumerator TOUCH_PAD_SMOOTH_OFF

    No filtering of raw data.

  enumerator TOUCH_PAD_SMOOTH_IIR_2

    Filter the raw data. The coefficient is 2 (Typical value).

  enumerator TOUCH_PAD_SMOOTH_IIR_4

    Filter the raw data. The coefficient is 4.

  enumerator TOUCH_PAD_SMOOTH_IIR_8

    Filter the raw data. The coefficient is 8.

  enumerator TOUCH_PAD_SMOOTH_MAX

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.