# Support for External RAM

[中文]

## Introduction

ESP32-S3 has a few hundred kilobytes of internal RAM, residing on the same die as the rest of the chip components. It can be insufficient for some purposes, so ESP32-S3 has the ability to use up to 32 MB of virtual addresses for external PSRAM (Psuedostatic RAM) memory. The external memory is incorporated in the memory map and, with certain restrictions, is usable in the same way as internal data RAM.

The 32 MB virtual addresses are shared with flash instructions and rodata.

## Hardware

ESP32-S3 supports PSRAM connected in parallel with the SPI flash chip. While ESP32-S3 is capable of supporting several types of RAM chips, ESP-IDF currently only supports Espressif branded PSRAM chips (e.g., ESP-PSRAM32, ESP-PSRAM64, etc).

Note

Some PSRAM chips are 1.8 V devices and some are 3.3 V. The working voltage of the PSRAM chip must match the working voltage of the flash component. Consult the datasheet for your PSRAM chip and ESP32-S3 device to find out the working voltages. For a 1.8 V PSRAM chip, make sure to either set the MTDI pin to a high signal level on boot-up, or program ESP32-S3 eFuses to always use the VDD_SIO level of 1.8 V. Not doing this can damage the PSRAM and/or flash chip.

Note

Espressif produces both modules and system-in-package chips that integrate compatible PSRAM and flash and are ready to mount on a product PCB. Consult the Espressif website for more information. If you are using a custom PSRAM chip, ESP-IDF SDK might not be compatible with it.

For specific details about connecting the SoC or module pins to an external PSRAM chip, consult the SoC or module datasheet.

## Configuring External RAM

Note

The `SPI RAM` configuration options are available only if the `esp_psram` component is included in the build. To include `SPI RAM` into your project, add the `esp_psram` component as a dependency in either `REQUIRES` or `PRIV_REQUIRES` when registering your component with `idf_component_register`.

ESP-IDF fully supports the use of external RAM in applications. Once the external RAM is initialized at startup, ESP-IDF can be configured to integrate the external RAM in several ways:

- Integrate RAM into the ESP32-S3 Memory Map

- Add External RAM to the Capability Allocator

- Provide External RAM via malloc() (default)

- Allow .bss Segment to Be Placed in External Memory

- Allow .noinit Segment to Be Placed in External Memory

- Execute In Place (XiP) from PSRAM

### Integrate RAM into the ESP32-S3 Memory Map

Select this option by choosing `Integrate RAM into memory map` from CONFIG_SPIRAM_USE.

This is the most basic option for external RAM integration. Most likely, you will need another, more advanced option.

During the ESP-IDF startup, external RAM is mapped into the data virtual address space. The address space is dynamically allocated. The length will be the minimum length between the PSRAM size and the available data virtual address space size.

Applications can manually place data in external memory by creating pointers to this region. So if an application uses external memory, it is responsible for all management of the external RAM: coordinating buffer usage, preventing corruption, etc.

It is recommended to access the PSRAM by ESP-IDF heap memory allocator (see next chapter).

### Add External RAM to the Capability Allocator

Select this option by choosing `Make RAM allocatable using heap_caps_malloc(..., MALLOC_CAP_SPIRAM)` from CONFIG_SPIRAM_USE.

When enabled, memory is mapped to data virtual address space and also added to the capabilities-based heap memory allocator using `MALLOC_CAP_SPIRAM`.

To allocate memory from external RAM, a program should call `heap_caps_malloc(size, MALLOC_CAP_SPIRAM)`. After use, this memory can be freed by calling the normal `free()` function.

### Provide External RAM via malloc()

Select this option by choosing `Make RAM allocatable using malloc() as well` from CONFIG_SPIRAM_USE. This is the default option.

In this case, memory is added to the capability allocator as described for the previous option. However, it is also added to the pool of RAM that can be returned by the standard `malloc()` function.

This allows any application to use the external RAM without having to rewrite the code to use `heap_caps_malloc(..., MALLOC_CAP_SPIRAM)`.

An additional configuration item, CONFIG_SPIRAM_MALLOC_ALWAYSINTERNAL, can be used to set the size threshold when a single allocation should prefer external memory:

- When allocating a size less than or equal to the threshold, the allocator will try internal memory first.

- When allocating a size larger than the threshold, the allocator will try external memory first.

If a suitable block of preferred internal/external memory is not available, the allocator will try the other type of memory.

Because some buffers can only be allocated in internal memory, a second configuration item CONFIG_SPIRAM_MALLOC_RESERVE_INTERNAL defines a pool of internal memory which is reserved for only explicitly internal allocations (such as memory for DMA use). Regular `malloc()` will not allocate from this pool. The MALLOC_CAP_DMA and `MALLOC_CAP_INTERNAL` flags can be used to allocate memory from this pool.

### Allow .bss Segment to Be Placed in External Memory

Enable this option by checking CONFIG_SPIRAM_ALLOW_BSS_SEG_EXTERNAL_MEMORY.

If enabled, the region of the data virtual address space where the PSRAM is mapped to will be used to store zero-initialized data (BSS segment) from the lwIP, net80211, libpp, wpa_supplicant and bluedroid ESP-IDF libraries.

Additional data can be moved from the internal BSS segment to external RAM by applying the macro `EXT_RAM_BSS_ATTR` to any static declaration (which is not initialized to a non-zero value).

It is also possible to place the BSS section of a component or a library to external RAM using linker fragment scheme `extram_bss`.

This option reduces the internal static memory used by the BSS segment.

Remaining external RAM can also be added to the capability heap allocator using the method shown above.

### Allow .noinit Segment to Be Placed in External Memory

Enable this option by checking CONFIG_SPIRAM_ALLOW_NOINIT_SEG_EXTERNAL_MEMORY. If enabled, the region of the data virtual address space where the PSRAM is mapped to will be used to store non-initialized data. The values placed in this segment will not be initialized or modified even during startup or restart.

By applying the macro `EXT_RAM_NOINIT_ATTR`, data could be moved from the internal NOINIT segment to external RAM. Remaining external RAM can still be added to the capability heap allocator using the method shown above, Add External RAM to the Capability Allocator.

#### Move Instructions in Flash to PSRAM

The CONFIG_SPIRAM_FETCH_INSTRUCTIONS option allows the flash `.text` sections (for instructions) to be placed in PSRAM.

By enabling the CONFIG_SPIRAM_FETCH_INSTRUCTIONS option,

- Instructions from the `.text` sections of flash are moved into PSRAM on system startup.

- The corresponding virtual memory range of those instructions will also be re-mapped to PSRAM.

#### Move Read-Only Data in Flash to PSRAM

The CONFIG_SPIRAM_RODATA option allows the flash `.rodata` sections (for read only data) to be placed in PSRAM.

By enabling the CONFIG_SPIRAM_RODATA option,

- Instructions from the `.rodata` sections of flash are moved into PSRAM on system startup.

- The corresponding virtual memory range of those rodata will also be re-mapped to PSRAM.

#### Execute In Place (XiP) from PSRAM

The CONFIG_SPIRAM_XIP_FROM_PSRAM is a helper option for you to select both the CONFIG_SPIRAM_FETCH_INSTRUCTIONS and CONFIG_SPIRAM_RODATA.

The benefits of XiP from PSRAM is:

- PSRAM access speed may be faster than flash access, so the overall application performance may be better. For example, if the PSRAM is an Octal mode (8-line PSRAM) and is configured to 80 MHz, then it is faster than a Quad flash (4-line flash) which is configured to 80 MHz.

- The cache will not be disabled during an SPI1 flash operation, thus optimizing the code execution performance during SPI1 flash operations. For ISRs, ISR callbacks and data which might be accessed during this period, you do not need to place them in internal RAM, thus internal RAM usage can be optimized. This feature is useful for high throughput peripheral involved applications to improve the performance during SPI1 flash operations.

system/xip_from_psram demonstrates the usage of XiP from PSRAM, optimizing internal RAM usage and avoiding cache disabling during flash operations from user call (e.g., flash erase/read/write operations).

## Restrictions

External RAM use has the following restrictions:

- When flash cache is disabled (for example, if the flash is being written to), the external RAM also becomes inaccessible. Any read operations from or write operations to it will lead to an illegal cache access exception. This is also the reason why ESP-IDF does not by default allocate any task stacks in external RAM (see below).

- Although ESP32-S3 has hardware support for DMA to or from external RAM, there are still limitations:

- DMA transaction descriptors cannot be placed in PSRAM.

- The bandwidth that DMA accesses external RAM is very limited, especially when the core is trying to access the external RAM at the same time.

- You can configure CONFIG_SPIRAM_SPEED as 120 MHz for an octal PSRAM. The bandwidth will be improved. However there are still restrictions for this option. See All Supported PSRAM Modes and Speeds for more details.

- External RAM uses the same cache region as the external flash. This means that frequently accessed variables in external RAM can be read and modified almost as quickly as in internal RAM. However, when accessing large chunks of data (> 32 KB), the cache can be insufficient, and speeds will fall back to the access speed of the external RAM. Moreover, accessing large chunks of data can "push out" cached flash, possibly making the execution of code slower afterwards.

- In general, external RAM will not be used as task stack memory. `xTaskCreate()` and similar functions will always allocate internal memory for stack and task TCBs.

The option CONFIG_FREERTOS_TASK_CREATE_ALLOW_EXT_MEM can be used to allow placing task stacks into external memory. In these cases `xTaskCreateStatic()` must be used to specify a task stack buffer allocated from external memory, otherwise task stacks will still be allocated from internal memory.

## Failure to Initialize

By default, failure to initialize external RAM will cause the ESP-IDF startup to abort. This can be disabled by enabling the config item CONFIG_SPIRAM_IGNORE_NOTFOUND.

## Encryption

It is possible to enable automatic encryption for data stored in external RAM. When this is enabled any data read and written through the cache will automatically be encrypted or decrypted by the external memory encryption hardware.

This feature is enabled whenever flash encryption is enabled. For more information on how to enable and how it works see Flash Encryption.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.