# RF Calibration

[中文]

ESP32-S2 supports three RF calibration methods during RF initialization:

1. Partial calibration

2. Full calibration

3. No calibration

## Partial Calibration

During RF initialization, the partial calibration method is used by default for RF calibration. It is done based on the full calibration data which is stored in the NVS. To use this method, please go to `menuconfig` and enable CONFIG_ESP_PHY_CALIBRATION_AND_DATA_STORAGE.

## Full Calibration

Full calibration is triggered in the following conditions:

1. NVS does not exist.

2. The NVS partition to store calibration data has been erased.

3. Hardware MAC address has changed.

4. PHY library version has changed.

5. The RF calibration data loaded from the NVS partition is broken.

Full calibration takes 100 ms longer than the partial calibration method. If boot duration is not of critical importance to the application, the full calibration method is recommended. To switch to the full calibration method, go to `menuconfig` and disable CONFIG_ESP_PHY_CALIBRATION_AND_DATA_STORAGE. If you use the default method of RF calibration, there are two ways to add the function of triggering full calibration as a last-resort remedy.

1. Erase the NVS partition if you do not mind all of the data stored in the NVS partition is erased. That is indeed the easiest way.

2. Call API `esp_phy_erase_cal_data_in_nvs()` before initializing Wi-Fi and Bluetooth®/Bluetooth Low Energy based on some conditions (e.g., an option provided in some diagnostic mode). In this case, only the PHY namespace of the NVS partition is erased.

## No Calibration

The no calibration method is only used when the device wakes up from Deep-sleep mode.

## PHY Initialization Data

The PHY initialization data is used for RF calibration. There are two ways to get the PHY initialization data.

One is to use the default initialization data which is located in the header file components/esp_phy/esp32s2/include/phy_init_data.h. It is embedded into the application binary after compiling and then stored into read-only memory (DROM). To use the default initialization data, please go to `menuconfig` and disable CONFIG_ESP_PHY_INIT_DATA_IN_PARTITION.

An alternative is to store the initialization data in a PHY data partition. A PHY data partition is included in the default partition table. However, when using a custom partition table, please ensure that a PHY data partition (type: `data`, subtype: `phy`) is included in the custom partition table. Whether you are using a custom partition table or the default partition table, if initialization data is stored in a partition, it has to be flashed there, otherwise a runtime error occurs. If you want to use initialization data stored in a partition, go to `menuconfig` and enable the option CONFIG_ESP_PHY_INIT_DATA_IN_PARTITION.

## API Reference

### Header File

- components/esp_phy/include/esp_phy_init.h

- This header file can be included with:

  >     #include "esp_phy_init.h"

- This header file is a part of the API provided by the `esp_phy` component. To declare that your component depends on `esp_phy`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_phy

  > or

  >     PRIV_REQUIRES esp_phy

### Functions

const esp_phy_init_data_t *esp_phy_get_init_data(void)

  Get PHY init data.

  If "Use a partition to store PHY init data" option is set in menuconfig, This function will load PHY init data from a partition. Otherwise, PHY init data will be compiled into the application itself, and this function will return a pointer to PHY init data located in read-only memory (DROM).

  If "Use a partition to store PHY init data" option is enabled, this function may return NULL if the data loaded from flash is not valid.

  Note

  Call esp_phy_release_init_data to release the pointer obtained using this function after the call to esp_wifi_init.

  Returns:

    pointer to PHY init data structure

void esp_phy_release_init_data(const esp_phy_init_data_t *data)

  Release PHY init data.

  Parameters:

    data -- pointer to PHY init data structure obtained from esp_phy_get_init_data function

esp_err_t esp_phy_load_cal_data_from_nvs(esp_phy_calibration_data_t *out_cal_data)

  Function called by esp_phy_load_cal_and_init to load PHY calibration data.

  This is a convenience function which can be used to load PHY calibration data from NVS. Data can be stored to NVS using esp_phy_store_cal_data_to_nvs function.

  If calibration data is not present in the NVS, or data is not valid (was obtained for a chip with a different MAC address, or obtained for a different version of software), this function will return an error.

  Parameters:

    out_cal_data -- pointer to calibration data structure to be filled with loaded data.

  Returns:

    ESP_OK on success

esp_err_t esp_phy_store_cal_data_to_nvs(const esp_phy_calibration_data_t *cal_data)

  Function called by esp_phy_load_cal_and_init to store PHY calibration data.

  This is a convenience function which can be used to store PHY calibration data to the NVS. Calibration data is returned by esp_phy_load_cal_and_init function. Data saved using this function to the NVS can later be loaded using esp_phy_store_cal_data_to_nvs function.

  Parameters:

    cal_data -- pointer to calibration data which has to be saved.

  Returns:

    ESP_OK on success

esp_err_t esp_phy_erase_cal_data_in_nvs(void)

  Erase PHY calibration data which is stored in the NVS.

  This is a function which can be used to trigger full calibration as a last-resort remedy if partial calibration is used. It can be called in the application based on some conditions (e.g. an option provided in some diagnostic mode).

  Returns:

    ESP_OK on success

  Returns:

    others on fail. Please refer to NVS API return value error number.

void esp_phy_enable(esp_phy_modem_t modem)

  Enable PHY and RF module.

  PHY and RF module should be enabled in order to use WiFi or BT. Now PHY and RF enabling job is done automatically when start WiFi or BT. Users should not call this API in their application.

  Parameters:

    modem -- the modem to call the phy enable.

void esp_phy_disable(esp_phy_modem_t modem)

  Disable PHY and RF module.

  PHY module should be disabled in order to shutdown WiFi or BT. Now PHY and RF disabling job is done automatically when stop WiFi or BT. Users should not call this API in their application.

  Parameters:

    modem -- the modem to call the phy disable.

void esp_btbb_enable(void)

  Enable BTBB module.

  BTBB module should be enabled in order to use IEEE802154 or BT. Now BTBB enabling job is done automatically when start IEEE802154 or BT. Users should not call this API in their application.

void esp_btbb_disable(void)

  Disable BTBB module.

  Disable BTBB module, used by IEEE802154 or Bluetooth. Users should not call this API in their application.

void esp_phy_load_cal_and_init(void)

  Load calibration data from NVS and initialize PHY and RF module.

void esp_phy_modem_init(void)

  Initialize backup memory for Phy power up/down.

void esp_phy_modem_deinit(void)

  Deinitialize backup memory for Phy power up/down Set phy_init_flag if all modems deinit on ESP32C3.

void esp_phy_common_clock_enable(void)

  Enable WiFi/BT common clock.

void esp_phy_common_clock_disable(void)

  Disable WiFi/BT common clock.

int64_t esp_phy_rf_get_on_ts(void)

  Get the time stamp when PHY/RF was switched on.

  Returns:

    return 0 if PHY/RF is never switched on. Otherwise return time in microsecond since boot when phy/rf was last switched on

esp_err_t esp_phy_update_country_info(const char *country)

  Update the corresponding PHY init type according to the country code of Wi-Fi.

  Parameters:

    country -- country code

  Returns:

    ESP_OK on success.

  Returns:

    esp_err_t code describing the error on fail

char *get_phy_version_str(void)

  Get PHY lib version.

  Returns:

    PHY lib version.

void phy_init_param_set(uint8_t param)

  Set PHY init parameters.

  Parameters:

    param -- is 1 means combo module

void phy_wifi_enable_set(uint8_t enable)

  Wi-Fi RX enable.

  Parameters:

    enable -- True for enable wifi receiving mode as default, false for closing wifi receiving mode as default.

void esp_wifi_bt_power_domain_on(void)

  Power on Bluetooth Wi-Fi power domain.

void esp_wifi_bt_power_domain_off(void)

  Power off Bluetooth Wi-Fi power domain.

### Structures

struct esp_phy_init_data_t

  Structure holding PHY init parameters.

  Public Members

  uint8_t params[128]

    opaque PHY initialization parameters

struct esp_phy_calibration_data_t

  Opaque PHY calibration data.

  Public Members

  uint8_t version[4]

    PHY version

  uint8_t mac[6]

    The MAC address of the station

  uint8_t opaque[1894]

    calibration data

### Enumerations

enum esp_phy_modem_t

  PHY enable or disable modem.

  Values:

  enumerator PHY_MODEM_WIFI

    PHY modem WIFI

  enumerator PHY_MODEM_BT

    PHY modem BT

  enumerator PHY_MODEM_IEEE802154

    PHY modem IEEE802154

  enumerator PHY_MODEM_MAX

    Don't use it. Used by ESP_PHY_MODEM_COUNT_MAX

enum esp_phy_calibration_mode_t

  PHY calibration mode.

  Values:

  enumerator PHY_RF_CAL_PARTIAL

    Do part of RF calibration. This should be used after power-on reset.

  enumerator PHY_RF_CAL_NONE

    Don't do any RF calibration. This mode is only suggested to be used after deep sleep reset.

  enumerator PHY_RF_CAL_FULL

    Do full RF calibration. Produces best results, but also consumes a lot of time and current. Suggested to be used once.

### Header File

- components/esp_phy/include/esp_phy_cert_test.h

- This header file can be included with:

  >     #include "esp_phy_cert_test.h"

- This header file is a part of the API provided by the `esp_phy` component. To declare that your component depends on `esp_phy`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_phy

  > or

  >     PRIV_REQUIRES esp_phy

### Functions

void esp_wifi_power_domain_on(void)

  Wifi power domain power on.

void esp_wifi_power_domain_off(void)

  Wifi power domain power off.

void esp_phy_rftest_config(uint8_t conf)

  Environment variable configuration.

  Parameters:

    conf -- Set to 1 to enter RF test mode.

void esp_phy_rftest_init(void)

  RF initialization configuration.

void esp_phy_tx_contin_en(bool contin_en)

  TX Continuous mode.

  Parameters:

    contin_en -- Set to true for continuous packet sending, which can be used for certification testing; Set to false to cancel continuous mode, which is the default mode and can be used for WLAN tester.

void esp_phy_cbw40m_en(bool en)

  HT40/HT20 mode selection.

  Parameters:

    en -- Set to false to enter 11n HT20 mode; Set to true to enter 11n HT40 mode;

void esp_phy_wifi_tx(uint32_t chan, esp_phy_wifi_rate_t rate, int8_t backoff, uint32_t length_byte, uint32_t packet_delay, uint32_t packet_num)

  Wi-Fi TX command.

  Parameters:

    - chan -- channel setting, 1~14;

    - rate -- rate setting;

    - backoff -- Transmit power attenuation, unit is 0.25dB. For example, 4 means that the power is attenuated by 1dB;

    - length_byte -- TX packet length configuration, indicating PSDU Length, unit is byte;

    - packet_delay -- TX packet interval configuration, unit is us;

    - packet_num -- The number of packets sent, 0 means sending packets continuously, other values represent the number of packets to send.

void esp_phy_test_start_stop(uint8_t value)

  Test start/stop command, used to stop transmitting or receiving state.

  Parameters:

    value -- Value should be set to 3 before TX/RX. Set value to 0 to end TX/RX state.

void esp_phy_wifi_rx(uint32_t chan, esp_phy_wifi_rate_t rate)

  Wi-Fi RX command.

  Parameters:

    - chan -- channel setting, 1~14;

    - rate -- rate setting;

void esp_phy_wifi_tx_tone(uint32_t start, uint32_t chan, uint32_t backoff)

  Wi-Fi Carrier Wave(CW) TX command.

  Parameters:

    - start -- enable CW, 1 means transmit, 0 means stop transmitting;

    - chan -- CW channel setting, 1~14;

    - backoff -- CW power attenuation parameter, unit is 0.25dB. 4 indicates the power is attenuated by 1dB.

void esp_phy_ble_tx(uint32_t txpwr, uint32_t chan, uint32_t len, esp_phy_ble_type_t data_type, uint32_t syncw, esp_phy_ble_rate_t rate, uint32_t tx_num_in)

  BLE TX command.

  Parameters:

    - txpwr -- Transmit power level. Tx power is about (level-8)*3 dBm, step is 3dB. Level 8 is around 0 dBm;

    - chan -- channel setting, range is 0~39, corresponding frequency = 2402+chan*2;

    - len -- Payload length setting, range is 0-255, unit is byte, 37 bytes is employed generally;

    - data_type -- Data type setting;

    - syncw -- Packet identification (need to be provided by the packet generator or instrument manufacturer), 0x71764129 is employed generally;

    - rate -- rate setting;

    - tx_num_in -- The number of packets sent, 0 means sending packets continuously, other values represent the number of packets to send.

void esp_phy_ble_rx(uint32_t chan, uint32_t syncw, esp_phy_ble_rate_t rate)

  BLE RX command.

  Parameters:

    - chan -- channel selection, range is 0-39; Channels 0, 1, 2~10 correspond to 2404MHz, 2406MHz, 2408MHz~2424MHz respectively; Channels 11, 12, 13~36 correspond to 2428MHz, 2430MHz, 2432MHz~2478MHz respectively; Channel 37: 2402MHz, Channel 38: 2426MHz, Channel 39: 2480MHz;

    - syncw -- Packet identification (need to be provided by the packet generator or instrument manufacturer), 0x71764129 is employed generally;

    - rate -- rate setting;

void esp_phy_bt_tx_tone(uint32_t start, uint32_t chan, uint32_t power)

  BLE Carrier Wave(CW) TX command.

  Parameters:

    - start -- enable CW, 1 means transmit, 0 means stop transmitting;

    - chan -- Single carrier transmission channel selection, range is 0~39, corresponding frequency freq = 2402+chan*2;

    - power -- CW power attenuation parameter, unit is 0.25dB. 4 indicates the power is attenuated by 1dB.

void esp_phy_get_rx_result(esp_phy_rx_result_t *rx_result)

  Get some RX information.

  Parameters:

    rx_result -- This struct for storing RX information;

### Structures

struct esp_phy_rx_result_t

  Structure holding PHY RX result.

  Public Members

  uint32_t phy_rx_correct_count

    The number of desired packets received

  int phy_rx_rssi

    Average RSSI of desired packets

  uint32_t phy_rx_total_count

    The number of total packets received

  uint32_t phy_rx_result_flag

    0 means no RX info; 1 means the latest Wi-Fi RX info; 2 means the latest BLE RX info.

### Enumerations

enum esp_phy_wifi_rate_t

  Values:

  enumerator PHY_RATE_1M
  enumerator PHY_RATE_2M
  enumerator PHY_RATE_5M5
  enumerator PHY_RATE_11M
  enumerator PHY_RATE_6M
  enumerator PHY_RATE_9M
  enumerator PHY_RATE_12M
  enumerator PHY_RATE_18M
  enumerator PHY_RATE_24M
  enumerator PHY_RATE_36M
  enumerator PHY_RATE_48M
  enumerator PHY_RATE_54M
  enumerator PHY_RATE_MCS0
  enumerator PHY_RATE_MCS1
  enumerator PHY_RATE_MCS2
  enumerator PHY_RATE_MCS3
  enumerator PHY_RATE_MCS4
  enumerator PHY_RATE_MCS5
  enumerator PHY_RATE_MCS6
  enumerator PHY_RATE_MCS7
  enumerator PHY_WIFI_RATE_MAX

enum esp_phy_ble_rate_t

  Values:

  enumerator PHY_BLE_RATE_1M
  enumerator PHY_BLE_RATE_2M
  enumerator PHY_BLE_RATE_125K
  enumerator PHY_BLE_RATE_500k
  enumerator PHY_BLE_RATE_MAX

enum esp_phy_ble_type_t

  Values:

  enumerator PHY_BLE_TYPE_1010
  enumerator PHY_BLE_TYPE_00001111
  enumerator PHY_BLE_TYPE_prbs9
  enumerator PHY_BLE_TYPE_00111100
  enumerator PHY_BLE_TYPE_MAX

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.