# Security Overview

[中文]

This guide provides an overview of the overall security features available in various Espressif solutions. It is highly recommended to consider this guide while designing the products with the Espressif platform and the ESP-IDF software stack from the security perspective.

Note

In this guide, most used commands are in the form of `idf.py secure-<command>`, which is a wrapper around corresponding `espsecure.py <command>`. The `idf.py` based commands provides more user-friendly experience, although may lack some of the advanced functionality of their `espsecure.py` based counterparts.

## Goals

High level security goals are as follows:

1. Preventing untrustworthy code from being executed

2. Protecting the identity and integrity of the code stored in the off-chip flash memory

3. Securing device identity

4. Secure storage for confidential data

5. Authenticated and encrypted communication from the device

## Platform Security

### Secure Boot

The Secure Boot feature ensures that only authenticated software can execute on the device. The Secure Boot process forms a chain of trust by verifying all mutable software entities involved in the Application Startup Flow. Signature verification happens during both boot-up as well as in OTA updates.

Please refer to Secure Boot v2 for detailed documentation about this feature.

Important

It is highly recommended that Secure Boot be enabled on all production devices.

#### Secure Boot Best Practices

- Generate the signing key on a system with a quality source of entropy.

- Always keep the signing key private. A leak of this key will compromise the Secure Boot system.

- Do not allow any third party to observe any aspects of the key generation or signing process using `idf.py secure-` or `espsecure.py` commands. Both processes are vulnerable to timing or other side-channel attacks.

- Ensure that all security eFuses have been correctly programmed, including disabling of the debug interfaces, non-required boot mediums (e.g., UART DL mode), etc.

### Flash Encryption

The Flash Encryption feature helps to encrypt the contents on the off-chip flash memory and thus provides the confidentiality aspect to the software or data stored in the flash memory.

Please refer to Flash Encryption for detailed information about this feature.

If ESP32-C5 is connected to an external SPI RAM, the contents written to or read from the SPI RAM will also be encrypted and decrypted respectively (via the MMU's flash cache, provided that FLash Encryption is enabled). This provides an additional safety layer for the data stored in SPI RAM, hence configurations like `CONFIG_MBEDTLS_EXTERNAL_MEM_ALLOC` can be safely enabled in this case.

#### Flash Encryption Best Practices

- It is recommended to use flash Encryption release mode for the production use-cases.

- It is recommended to have a unique flash encryption key per device.

- Enable Secure Boot as an extra layer of protection, and to prevent an attacker from selectively corrupting any part of the flash before boot.

### Device Identity

The Digital Signature peripheral in ESP32-C5 produces hardware-accelerated RSA digital signatures with the assistance of HMAC, without the RSA private key being accessible by software. This allows the private key to be kept secured on the device without anyone other than the device hardware being able to access it.

ESP32-C5 also supports ECDSA peripheral for generating hardware-accelerated ECDSA digital signatures. ECDSA private key can be directly programmed in an eFuse block and marked as read protected from the software.

DS or ECDSA peripheral can help to establish the Secure Device Identity to the remote endpoint, e.g., in the case of TLS mutual authentication based on the RSA or ECDSA cipher scheme.

Please refer to the Elliptic Curve Digital Signature Algorithm (ECDSA) and Digital Signature (DS) guides for detailed documentation.

### Memory Protection

ESP32-C5 supports the Memory Protection scheme, either through architecture or special peripheral like PMS, which provides an ability to enforce and monitor permission attributes to memory and, in some cases, peripherals. ESP-IDF application startup code configures the permissions attributes like Read/Write access on data memories and Read/Execute access on instruction memories using the relevant peripheral. If there is any attempt made that breaks these permission attributes, e.g., a write operation to instruction memory region, then a violation interrupt is raised, and it results in system panic.

This feature depends on the config option CONFIG_ESP_SYSTEM_MEMPROT_FEATURE and it is kept enabled by default. Please note that the API for this feature is private and used exclusively by ESP-IDF code only.

Note

This feature can help to prevent the possibility of remote code injection due to the existing vulnerabilities in the software.

### Protection Against Side-Channel Attacks

#### DPA (Differential Power Analysis) Protection

ESP32-C5 has support for protection mechanisms against the Differential Power Analysis related security attacks. DPA protection dynamically adjusts the clock frequency of the crypto peripherals, thereby blurring the power consumption trajectory during its operation. Based on the configured DPA security level, the clock variation range changes. Please refer to the ESP32-C5 Technical Reference Manual [PDF]. for more details on this topic.

CONFIG_ESP_CRYPTO_DPA_PROTECTION_LEVEL can help to select the DPA level. Higher level means better security, but it can also have an associated performance impact. By default, the lowest DPA level is kept enabled but it can be modified based on the security requirement.

Note

Please note that hardware RNG must be enabled for DPA protection to work correctly.

#### AES Peripheral's Pseudo-Round Function

ESP32-C5 incorporates a pseudo-round function in the AES peripheral, thus enabling the peripheral to randomly insert pseudo-rounds before and after the original operation rounds and also generate a pseudo key to perform these dummy operations. These operations do not alter the original result, but they increase the complexity to perform side channel analysis attacks by randomizing the power profile.

CONFIG_MBEDTLS_AES_USE_PSEUDO_ROUND_FUNC_STRENGTH can be used to select the strength of the pseudo-round function. Increasing the strength improves the security provided, but would slow down the encrryption/decryption operations.

Performance impact on AES operations per strength level
Strength | Performance Impact [1]
--- | ---
Low | 20.9 %
Medium | 47.6 %
High | 72.4 %

[1]

The above performance numbers have been calculated using the AES performance test of the mbedtls test application test_aes_perf.c .

Considering the above performance impact, ESP-IDF by-default does not enable the pseudo-round function to avoid any performance-related degrade. But it is recommended to enable the pseudo-round function for better security.

### Debug Interfaces

#### JTAG

- JTAG interface stays disabled if any of the security features are enabled. Please refer to JTAG with Flash Encryption or Secure Boot for more information.

- JTAG interface can also be disabled in the absence of any other security features using eFuse API.

- ESP32-C5 supports soft disabling the JTAG interface and it can be re-enabled by programming a secret key through HMAC. (HMAC for Enabling JTAG)

#### UART Download Mode

In ESP32-C5, Secure UART Download mode gets activated if any of the security features are enabled.

- Secure UART Download mode can also be enabled by calling `esp_efuse_enable_rom_secure_download_mode()`.

- This mode does not allow any arbitrary code to execute if downloaded through the UART download mode.

- It also limits the available commands in Download mode to update SPI config, e.g., changing baud rate, basic flash write, and the command to return a summary of currently enabled security features (`get_security_info`).

- To disable Download Mode entirely, select the CONFIG_SECURE_UART_ROM_DL_MODE to the recommended option `Permanently disable ROM Download Mode` or call `esp_efuse_disable_rom_download_mode()` at runtime.

Important

In Secure UART Download mode, `esptool.py` can only work with the argument `--no-stub`.

## Network Security

### Wi-Fi

In addition to the traditional security methods (WEP/WPA-TKIP/WPA2-CCMP), Wi-Fi driver in ESP-IDF also supports additional state-of-the-art security protocols. Please refer to the Wi-Fi Security for detailed documentation.

### TLS (Transport Layer Security)

It is recommended to use TLS (Transport Layer Security) in all external communications (e.g., cloud communication, OTA updates) from the ESP device. ESP-IDF supports Mbed TLS as the official TLS stack.

TLS is default integrated in ESP HTTP Client, HTTPS Server and several other components that ship with ESP-IDF.

Note

It is recommended to use the ESP-IDF protocol components in their default configuration, which has been ensured to be secure. Disabling of HTTPS and similar security-critical configurations should be avoided.

#### ESP-TLS Abstraction

ESP-IDF provides an abstraction layer for the most-used TLS functionalities. Hence, it is recommended that an application uses the API exposed by ESP-TLS.

TLS Server Verification section highlights diverse ways in which the identity of server could be established on the device side.

#### ESP Certificate Bundle

The ESP x509 Certificate Bundle API provides an easy way to include a bundle of custom x509 root certificates for TLS server verification. The certificate bundle is the easiest way to verify the identity of almost all standard TLS servers.

Important

It is highly recommended to verify the identity of the server based on X.509 certificates to avoid establishing communication with the fake server.

#### Managing Root Certificates

Root Certificates embedded inside the application must be managed carefully. Any update to the root certificate list or the ESP x509 Certificate Bundle can have an impact on the TLS connection with the remote endpoint. This includes a connection to the OTA update server. In some cases, the problem shall be visible on the next OTA update and it may leave device unable to perform OTA updates forever.

Root certificates list update could have following reasons:

- New firmware has different set of remote endpoint(s).

- The existing certificate has expired.

- The certificate has been added or retracted from the upstream certificate bundle.

- The certificate list changed due to market share statistics (`CONFIG_MBEDTLS_CERTIFICATE_BUNDLE_DEFAULT_CMN` case).

Some guidelines to consider on this topic:

- Please consider enabling OTA rollback and then keep the successful connection to the OTA update server as the checkpoint to cancel the rollback process. This ensures that the newly updated firmware can successfully reach till the OTA update server, otherwise rollback process will go back to the previous firmware on the device.

- If you plan to enable the CONFIG_MBEDTLS_HAVE_TIME_DATE option, then please consider to have the time sync mechanism (SNTP) and sufficient number of trusted certificates in place.

## Product Security

### Secure Provisioning

Secure Provisioning refers to a process of secure on-boarding of the ESP device on to the Wi-Fi network. This mechanism also allows provision of additional custom configuration data during the initial provisioning phase from the provisioning entity, e.g., Smartphone.

ESP-IDF provides various security schemes to establish a secure session between ESP and the provisioning entity, they are highlighted at Security Schemes.

Please refer to the Wi-Fi Provisioning documentation for details and the example code for this feature.

Note

Espressif provides Android and iOS Phone Apps along with their sources, so that it could be easy to further customize them as per the product requirement.

### Secure OTA (Over-the-air) Updates

- OTA Updates must happen over secure transport, e.g., HTTPS.

- ESP-IDF provides a simplified abstraction layer ESP HTTPS OTA for this.

- If Secure Boot is enabled, then the server should host the signed application image.

- If Flash Encryption is enabled, then no additional steps are required on the server side, encryption shall be taken care on the device itself during flash write.

- OTA update Rollback Process can help to switch the application as `active` only after its functionality has been verified.

#### Anti-Rollback Protection

Anti-rollback protection feature ensures that device only executes the application that meets the security version criteria as stored in its eFuse. So even though the application is trusted and signed by legitimate key, it may contain some revoked security feature or credential. Hence, device must reject any such application.

ESP-IDF allows this feature for the application only and it is managed through 2nd stage bootloader. The security version is stored in the device eFuse and it is compared against the application image header during both boot-up and over-the-air updates.

Please see more information to enable this feature in the Anti-rollback guide.

#### Encrypted Firmware Distribution

Encrypted firmware distribution during over-the-air updates ensures that the application stays encrypted in transit from the server to the the device. This can act as an additional layer of protection on top of the TLS communication during OTA updates and protect the identity of the application.

Please see working example for this documented in OTA Upgrades with Pre-Encrypted Firmware section.

### Secure Storage

Secure storage refers to the application-specific data that can be stored in a secure manner on the device, i.e., off-chip flash memory. This is typically a read-write flash partition and holds device specific configuration data, e.g., Wi-Fi credentials.

ESP-IDF provides the NVS (Non-volatile Storage) management component which allows encrypted data partitions. This feature is tied with the platform Flash Encryption feature described earlier.

Please refer to the NVS Encryption for detailed documentation on the working and instructions to enable this feature.

Important

By default, ESP-IDF components writes the device specific data into the default NVS partition, including Wi-Fi credentials too, and it is recommended to protect this data using NVS Encryption feature.

### Secure Device Control

ESP-IDF provides capability to control an ESP device over `Wi-Fi/Ethernet + HTTP` or `BLE` in a secure manner using ESP Local Control component.

Please refer to the ESP Local Control for detailed documentation about this feature.

## Security Policy

The ESP-IDF GitHub repository has attached Security Policy Brief.

### Advisories

- Espressif publishes critical Security Advisories, which includes security advisories regarding both hardware and software.

- The specific advisories of the ESP-IDF software components are published through the GitHub repository.

### Software Updates

Critical security issues in the ESP-IDF components, and third-party libraries are fixed as and when we find them or when they are reported to us. Gradually, we make the fixes available in all applicable release branches in ESP-IDF.

Applicable security issues and CVEs for the ESP-IDF components, third-party libraries are mentioned in the ESP-IDF release notes.

Important

We recommend periodically updating to the latest bugfix version of the ESP-IDF release to have all critical security fixes available.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.