# Configure ESP-WROVER-KIT JTAG Interface

[中文]

All versions of ESP-WROVER-KIT boards have built-in JTAG functionality. Putting it to work requires setting jumpers or DIP switches to enable JTAG functionality, and configuring USB drivers. Please refer to step by step instructions below.

## Configure Hardware

- Enable on-board JTAG functionality by setting JP8 according to ESP-WROVER-KIT.

- Verify if ESP32 pins used for JTAG communication are not connected to some other h/w that may disturb JTAG operation:

  > ESP32 JTAG pins
  > ESP32 Pin | JTAG Signal
  > --- | ---
  > MTDO / GPIO15 | TDO
  > MTDI / GPIO12 | TDI
  > MTCK / GPIO13 | TCK
  > MTMS / GPIO14 | TMS

## Configure USB Drivers

Install and configure USB drivers, so OpenOCD is able to communicate with JTAG interface on ESP-WROVER-KIT board as well as with UART interface used to upload application for flash. Follow steps below specific to your operating system.

Note

ESP-WROVER-KIT uses an FT2232 adapter. The following instructions can also be used for other FT2232 based JTAG adapters.

### Windows

1. Using standard USB A/micro USB B cable connect ESP-WROVER-KIT to the computer. Switch the ESP-WROVER-KIT on.

2. Wait until USB ports of ESP-WROVER-KIT are recognized by Windows and drives are installed. If they do not install automatically, then download them from https://ftdichip.com/drivers/d2xx-drivers/ and install manually.

3. Download ESP-WROVER-KIT driver from https://github.com/espressif/esp-win-usb-drivers/releases. Extract the driver files and install the driver. This should change the driver for Dual RS232-HS (Interface 0).

4. Now ESP-WROVER-KIT's JTAG interface should be available to the OpenOCD. To carry on with the debugging environment setup, proceed to section Run OpenOCD.

Note

If the driver installation fails or OpenOCD is not working try the following manual driver change. Otherwise, this can be skipped.

### Windows - manual driver change

1. Download Zadig tool (Zadig_X.X.exe) from https://zadig.akeo.ie/ and run it.

2. In Zadig tool go to Options and check List All Devices.

3. Check the list of devices that should contain two ESP-WROVER-KIT specific USB entries: Dual RS232-HS (Interface 0) and Dual RS232-HS (Interface 1). The driver name would be FTDIBUS (vxxxx) and USB ID: 0403 6010.

   Configuration of JTAG USB driver in Zadig tool

4. The first device (Dual RS232-HS (Interface 0)) is connected to the JTAG port of the ESP32. Original FTDIBUS (vxxxx) driver of this device should be replaced with WinUSB (v6xxxxx). To do so, select "Dual RS232-HS (Interface 0) and reinstall attached driver to the "WinUSB (v6xxxxx)", see picture above.

Note

Do not change the second device Dual RS232-HS (Interface 1). It is routed to ESP32's serial port (UART) used for upload of application to ESP32's flash.

### Linux

1. Using standard USB A/micro USB B cable connect ESP-WROVER-KIT board to the computer. Power on the board.

2. Open a terminal, enter `ls -l /dev/ttyUSB*` command and check, if board's USB ports are recognized by the OS. You are looking for similar result:

       user-name@computer-name:~/esp$ ls -l /dev/ttyUSB*
       crw-rw---- 1 root dialout 188, 0 Jul 10 19:04 /dev/ttyUSB0
       crw-rw---- 1 root dialout 188, 1 Jul 10 19:04 /dev/ttyUSB1

3. To set up access permissions to USB devices supported by OpenOCD, copy the udev rules file into the `/etc/udev/rules.d` directory.

4. Log off and login, then cycle the power to the board to make the changes effective. In terminal enter again `ls -l /dev/ttyUSB*` command to verify, if group-owner has changed from `dialout` to `plugdev`:

       user-name@computer-name:~/esp$ ls -l /dev/ttyUSB*
       crw-rw-r-- 1 root plugdev 188, 0 Jul 10 19:07 /dev/ttyUSB0
       crw-rw-r-- 1 root plugdev 188, 1 Jul 10 19:07 /dev/ttyUSB1

   If you see similar result and you are a member of `plugdev` group, then the set up is complete.

   The `/dev/ttyUSBn` interface with lower number is used for JTAG communication. The other interface is routed to ESP32's serial port (UART) used for upload of application to ESP32's flash.

Now ESP-WROVER-KIT's JTAG interface should be available to the OpenOCD. To carry on with debugging environment setup, proceed to section Run OpenOCD.

### MacOS

On macOS, using FT2232 for JTAG and serial port at the same time needs some additional steps. When the OS loads FTDI serial port driver, it does so for both channels of FT2232 chip. However only one of these channels is used as a serial port, while the other is used as JTAG. If the OS has loaded FTDI serial port driver for the channel used for JTAG, OpenOCD will not be able to connect to the chip. There are two ways around this:

1. Manually unload the FTDI serial port driver before starting OpenOCD, start OpenOCD, then load the serial port driver.

2. Modify FTDI driver configuration so that it does not load itself for channel A of FT2232 chip, which is the channel used for JTAG on ESP-WROVER-KIT.

#### Manually unloading the driver

1. Install FTDI driver from FTDI official website.

2. Connect USB cable to the ESP-WROVER-KIT.

3. Unload the serial port driver:

       sudo kextunload -b com.FTDI.driver.FTDIUSBSerialDriver

   In some cases you may need to unload Apple's FTDI driver as well:

   - macOS < 10.15:

         sudo kextunload -b com.apple.driver.AppleUSBFTDI

   - macOS 10.15:

         sudo kextunload -b com.apple.DriverKit-AppleUSBFTDI

   Warning

   Attempting to use serial over the wrong channel with the FTDI driver will cause a kernel panic. The ESP-WROVER-KIT uses channel A for JTAG and channel B for serial.

4. Run OpenOCD:

       openocd -f board/esp32-wrover-kit-3.3v.cfg

5. In another terminal window, load FTDI serial port driver again:

       sudo kextload -b com.FTDI.driver.FTDIUSBSerialDriver

Note

If you need to restart OpenOCD, there is no need to unload FTDI driver again — just stop OpenOCD and start it again. The driver only needs to be unloaded if ESP-WROVER-KIT was reconnected or power was toggled.

This procedure can be wrapped into a shell script, if desired.

#### Modifying FTDI driver

In a nutshell, this approach requires modification to FTDI driver configuration file, which prevents the driver from being loaded for channel B of FT2232H.

Note

Other boards may use channel A for JTAG, so use this option with caution.

Warning

This approach also needs signature verification of drivers to be disabled, so may not be acceptable for all users.

1. Open FTDI driver configuration file using a text editor (note `sudo`):

       sudo nano /Library/Extensions/FTDIUSBSerialDriver.kext/Contents/Info.plist

2. Find and delete the following lines:

       <key>FT2232H_B</key>
       <dict>
           <key>CFBundleIdentifier</key>
           <string>com.FTDI.driver.FTDIUSBSerialDriver</string>
           <key>IOClass</key>
           <string>FTDIUSBSerialDriver</string>
           <key>IOProviderClass</key>
           <string>IOUSBInterface</string>
           <key>bConfigurationValue</key>
           <integer>1</integer>
           <key>bInterfaceNumber</key>
           <integer>1</integer>
           <key>bcdDevice</key>
           <integer>1792</integer>
           <key>idProduct</key>
           <integer>24592</integer>
           <key>idVendor</key>
           <integer>1027</integer>
       </dict>

3. Save and close the file

4. Disable driver signature verification:

   1. Open Apple logo menu, choose "Restart..."

   2. When you hear the chime after reboot, press CMD+R immediately

   3. Once Recovery mode starts up, open Terminal

   4. Run the command:

          csrutil enable --without kext

   5. Restart again

After these steps, serial port and JTAG can be used at the same time.

To carry on with debugging environment setup, proceed to section Run OpenOCD.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.