# SPI Flash API

[中文]

## Overview

The spi_flash component contains API functions related to reading, writing, erasing, and memory mapping for data in the external flash.

For higher-level API functions which work with partitions defined in the partition table, see Partitions API

Note

`esp_partition_*` APIs are recommended to be used instead of the lower level `esp_flash_*` API functions when accessing the main SPI flash chip, since they conduct bounds checking and are guaranteed to calculate correct offsets in flash based on the information in the partition table. `esp_flash_*` functions can still be used directly when accessing an external (secondary) SPI flash chip.

Different from the API before ESP-IDF v4.0, the functionality of `esp_flash_*` APIs is not limited to the "main" SPI flash chip (the same SPI flash chip from which program runs). With different chip pointers, you can access external flash chips connected to not only SPI0/1 but also other SPI buses like SPI2.

Note

Instead of going through the cache connected to the SPI0 peripheral, most `esp_flash_*` APIs go through other SPI peripherals like SPI1, SPI2, etc. This makes them able to access not only the main flash, but also external (secondary) flash.

However, due to the limitations of the cache, operations through the cache are limited to the main flash. The address range limitation for these operations is also on the cache side. The cache is not able to access external flash chips or address range above its capabilities. These cache operations include: mmap, encrypted read/write, executing code or access to variables in the flash.

Note

Flash APIs after ESP-IDF v4.0 are no longer atomic. If a write operation occurs during another on-going read operation, and the flash addresses of both operations overlap, the data returned from the read operation may contain both old data and new data (that was updated written by the write operation).

Note

Encrypted flash operations are only supported with the main flash chip (and not with other flash chips, that is on SPI1 with different CS, or on other SPI buses). Reading through cache is only supported on the main flash, which is determined by the HW.

## Support for Features of Flash Chips

### Quad/Dual Mode Chips

Features of different flashes are implemented in different ways and thus need special support. The fast/slow read and Dual mode (DOUT/DIO) of almost all flashes with 24-bit address are supported, because they do not need any vendor-specific commands.

Quad mode (QIO/QOUT) is supported on the following chip types:

1. ISSI

2. GD

3. MXIC

4. FM

5. Winbond

6. XMC

7. BOYA

Note

Only when one flash series listed above is supported by ESP32-P4, this flash series is supported by the chip driver by default. You can use `Component config` > `SPI Flash driver` > `Auto-detect flash chips` in menuconfig to enable/disable a flash series.

### Optional Features

There are some features that are not supported by all flash chips, or not supported by all Espressif chips. These features include:

- 32-bit address flash - usually means that the flash has higher capacity (equal to or larger than 16 MB) that needs longer addresses.

- Flash unique ID - means that flash supports its unique 64-bit ID.

- Suspend & Resume - means that flash can accept suspend/resume command during its writing/erasing. The ESP32-P4 may keep the cache on when the flash is being written/erased and suspend it to read its contents randomly.

If you want to use these features, please ensure both ESP32-P4 and ALL flash chips in your product support these features. For more details, refer to Optional Features for Flash.

You may also customise your own flash chip driver. See Overriding Default Chip Drivers for more details.

## Initializing a Flash Device

To use the `esp_flash_*` APIs, you need to initialise a flash chip on a certain SPI bus, as shown below:

1. Call `spi_bus_initialize()` to properly initialize an SPI bus. This function initializes the resources (I/O, DMA, interrupts) shared among devices attached to this bus.

2. Call `spi_bus_add_flash_device()` to attach the flash device to the bus. This function allocates memory and fills the members for the `esp_flash_t` structure. The CS I/O is also initialized here.

3. Call `esp_flash_init()` to actually communicate with the chip. This also detects the chip type, and influence the following operations.

Note

Multiple flash chips can be attached to the same bus now.

## SPI Flash Access API

This is the set of API functions for working with data in flash:

- `esp_flash_read()` reads data from flash to RAM

- `esp_flash_write()` writes data from RAM to flash

- `esp_flash_erase_region()` erases specific region of flash

- `esp_flash_erase_chip()` erases the whole flash

- `esp_flash_get_chip_size()` returns flash chip size, in bytes, as configured in menuconfig

Generally, try to avoid using the raw SPI flash functions to the "main" SPI flash chip in favour of partition-specific functions.

## SPI Flash Size

The SPI flash size is configured by writing a field in the ESP-IDF second stage bootloader image header, flashed at offset 0x1000.

By default, the SPI flash size is detected by `esptool.py` when this bootloader is written to flash, and the header is updated with the correct size. Alternatively, it is possible to generate a fixed flash size by setting CONFIG_ESPTOOLPY_FLASHSIZE in the project configuration.

If it is necessary to override the configured flash size at runtime, it is possible to set the `chip_size` member of the `g_rom_flashchip` structure. This size is used by `esp_flash_*` functions (in both software & ROM) to check the bounds.

## Concurrency Constraints for Flash on SPI1

Attention

The SPI0/1 bus is shared between the instruction & data cache (for firmware execution) and the SPI1 peripheral (controlled by the drivers including this SPI flash driver). Hence, calling SPI Flash API on SPI1 bus (including the main flash) causes significant influence to the whole system. See Concurrency Constraints for Flash on SPI1 for more details.

## SPI Flash Encryption

It is possible to encrypt the contents of SPI flash and have it transparently decrypted by hardware.

Refer to the Flash Encryption documentation for more details.

## Memory Mapping API

ESP32-P4 features memory hardware which allows regions of flash memory to be mapped into instruction and data address spaces. This mapping works only for read operations. It is not possible to modify contents of flash memory by writing to a mapped memory region.

Mapping happens in 64 KB pages. Memory mapping hardware can map flash into the data address space and the instruction address space. See the technical reference manual for more details and limitations about memory mapping hardware.

Note that some pages are used to map the application itself into memory, so the actual number of available pages may be less than the capability of the hardware.

Reading data from flash using a memory mapped region is the only way to decrypt contents of flash when flash encryption is enabled. Decryption is performed at the hardware level.

Memory mapping API are declared in `spi_flash_mmap.h` and `esp_partition.h`:

- `spi_flash_mmap()` maps a region of physical flash addresses into instruction space or data space of the CPU.

- `spi_flash_munmap()` unmaps previously mapped region.

- `esp_partition_mmap()` maps part of a partition into the instruction space or data space of the CPU.

Differences between `spi_flash_mmap()` and `esp_partition_mmap()` are as follows:

- `spi_flash_mmap()` must be given a 64 KB aligned physical address.

- `esp_partition_mmap()` may be given any arbitrary offset within the partition. It adjusts the returned pointer to mapped memory as necessary.

Note that since memory mapping happens in pages, it may be possible to read data outside of the partition provided to `esp_partition_mmap`, regardless of the partition boundary.

Note

mmap is supported by cache, so it can only be used on main flash.

## SPI Flash Implementation

The `esp_flash_t` structure holds chip data as well as three important parts of this API:

1. The host driver, which provides the hardware support to access the chip;

2. The chip driver, which provides compatibility service to different chips;

3. The OS functions, provide support of some OS functions (e.g., lock, delay) in different stages (1st/2nd boot, or the app).

### Host Driver

The host driver relies on an interface (`spi_flash_host_driver_t`) defined in the `spi_flash_types.h` (in the `hal/include/hal` folder). This interface provides some common functions to communicate with the chip.

In other files of the SPI HAL, some of these functions are implemented with existing ESP32-P4 memory-spi functionalities. However, due to the speed limitations of ESP32-P4, the HAL layer cannot provide high-speed implementations to some reading commands (so the support for it was dropped). The files (`memspi_host_driver.h` and `.c`) implement the high-speed version of these commands with the `common_command` function provided in the HAL, and wrap these functions as `spi_flash_host_driver_t` for upper layer to use.

You can also implement your own host driver, even with the GPIO. As long as all the functions in the `spi_flash_host_driver_t` are implemented, the esp_flash API can access the flash regardless of the low-level hardware.

### Chip Driver

The chip driver, defined in `spi_flash_chip_driver.h`, wraps basic functions provided by the host driver for the API layer to use.

Some operations need some commands to be sent first, or read some status afterwards. Some chips need different commands or values, or need special communication ways.

There is a type of chip called `generic chip` which stands for common chips. Other special chip drivers can be developed on the base of the generic chip.

The chip driver relies on the host driver.

### OS Functions

Currently the OS function layer provides entries of a lock and delay.

The lock (see SPI Bus Lock) is used to resolve the conflicts among the access of devices on the same SPI bus, and the SPI Flash chip access. E.g.

1. On SPI1 bus, the cache (used to fetch the data (code) in the Flash and PSRAM) should be disabled when the flash chip on the SPI0/1 is being accessed.

2. On the other buses, the flash driver needs to disable the ISR registered by SPI Master driver, to avoid conflicts.

3. Some devices of SPI Master driver may require to use the bus monopolized during a period (especially when the device does not have a CS wire, or the wire is controlled by software like SDSPI driver).

The delay is used by some long operations which requires the master to wait or polling periodically.

The top API wraps these the chip driver and OS functions into an entire component, and also provides some argument checking.

OS functions can also help to avoid a watchdog timeout when erasing large flash areas. During this time, the CPU is occupied with the flash erasing task. This stops other tasks from being executed. Among these tasks is the idle task to feed the watchdog timer (WDT). If the configuration option CONFIG_ESP_TASK_WDT_PANIC is selected and the flash operation time is longer than the watchdog timeout period, the system will reboot.

It is pretty hard to totally eliminate this risk, because the erasing time varies with different flash chips, making it hard to be compatible in flash drivers. Therefore, users need to pay attention to it. Please use the following guidelines:

1. It is recommended to enable the CONFIG_SPI_FLASH_YIELD_DURING_ERASE option to allow the scheduler to re-schedule during erasing flash memory. Besides, following parameters can also be used.

- Increase CONFIG_SPI_FLASH_ERASE_YIELD_TICKS or decrease CONFIG_SPI_FLASH_ERASE_YIELD_DURATION_MS in menuconfig.

- You can also increase CONFIG_ESP_TASK_WDT_TIMEOUT_S in menuconfig for a larger watchdog timeout period. However, with larger watchdog timeout period, previously detected timeouts may no longer be detected.

2. Please be aware of the consequences of enabling the CONFIG_ESP_TASK_WDT_PANIC option when doing long-running SPI flash operations which triggers the panic handler when it times out. However, this option can also help dealing with unexpected exceptions in your application. Please decide whether this is needed to be enabled according to actual condition.

3. During your development, please carefully review the actual flash operation according to the specific requirements and time limits on erasing flash memory of your projects. Always allow reasonable redundancy based on your specific product requirements when configuring the flash erasing timeout threshold, thus improving the reliability of your product.

## Implementation Details

In order to perform some flash operations, it is necessary to make sure that both CPUs are not running any code from flash for the duration of the flash operation:

- In a single-core setup, the SDK needs to disable interrupts or scheduler before performing the flash operation.

- In a dual-core setup, the SDK needs to make sure that both CPUs are not running any code from flash.

When SPI flash API is called on CPU A (can be PRO or APP), start the `spi_flash_op_block_func` function on CPU B using the `esp_ipc_call` API. This API wakes up a high priority task on CPU B and tells it to execute a given function, in this case, `spi_flash_op_block_func`. This function disables cache on CPU B and signals that the cache is disabled by setting the `s_flash_op_can_start` flag. Then the task on CPU A disables cache as well and proceeds to execute flash operation.

While a flash operation is running, interrupts can still run on CPUs A and B. It is assumed that all interrupt code is placed into RAM. Once the interrupt allocation API is added, a flag should be added to request the interrupt to be disabled for the duration of a flash operations.

Once the flash operation is complete, the function on CPU A sets another flag, `s_flash_op_complete`, to let the task on CPU B know that it can re-enable cache and release the CPU. Then the function on CPU A re-enables the cache on CPU A as well and returns control to the calling code.

Additionally, all API functions are protected with a mutex (`s_flash_op_mutex`).

In a single core environment (CONFIG_FREERTOS_UNICORE enabled), you need to disable both caches, so that no inter-CPU communication can take place.

## Internal Memory Saving For Flash Driver

The ESP-IDF provides options to optimize the usage of IRAM by selectively placing certain functions into flash memory via turning off CONFIG_SPI_FLASH_PLACE_FUNCTIONS_IN_IRAM. It allows SPI flash operation functions to be executed from flash memory instead of IRAM. Thus it saves IRAM memory for other significant time-critical functions or tasks.

However, this has some implications for flash itself. Functions placed into flash memory may have slightly increased execution times compared to those placed in IRAM. Applications with strict timing requirements or those heavily reliant on SPI flash operations may need to evaluate the trade-offs before enabling this option.

Note

CONFIG_SPI_FLASH_PLACE_FUNCTIONS_IN_IRAM should not be turned off when CONFIG_SPI_FLASH_AUTO_SUSPEND is not enabled, otherwise it will cause critical crash. As for flash suspend feature, please refer to Flash Auto Suspend Feature for more information.

### Resource Consumption

Use the IDF Size tool to check the code and data consumption of the SPI flash driver. The following are the test results under 2 different conditions (using ESP32-C2 as an example):

Note that the following data are not exact values and are for reference only; they may differ on different chip models.

Resource consumption when CONFIG_SPI_FLASH_PLACE_FUNCTIONS_IN_IRAM is enabled:

Resource Consumption
Component Layer | Total Size | DIRAM | .bss | .data | .text | Flash Code | .text | Flash Data | .rodata
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
hal | 4624 | 4038 | 0 | 0 | 4038 | 586 | 586 | 0 | 0
spi_flash | 14074 | 11597 | 82 | 1589 | 9926 | 2230 | 2230 | 247 | 247

Resource consumption when CONFIG_SPI_FLASH_PLACE_FUNCTIONS_IN_IRAM is disabled:

Resource Consumption
Component Layer | Total Size | DIRAM | .bss | .data | .text | Flash Code | .text | Flash Data | .rodata
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
hal | 4632 | 0 | 0 | 0 | 0 | 4632 | 4632 | 0 | 0
spi_flash | 14569 | 1399 | 22 | 429 | 948 | 11648 | 11648 | 1522 | 1522

## Related Documents

- Optional Features for Flash

- Concurrency Constraints for Flash on SPI1

## API Reference - SPI Flash

### Header File

- components/spi_flash/include/esp_flash_spi_init.h

- This header file can be included with:

  >     #include "esp_flash_spi_init.h"

- This header file is a part of the API provided by the `spi_flash` component. To declare that your component depends on `spi_flash`, add the following to your CMakeLists.txt:

  >     REQUIRES spi_flash

  > or

  >     PRIV_REQUIRES spi_flash

### Functions

esp_err_t spi_bus_add_flash_device(esp_flash_t **out_chip, const esp_flash_spi_device_config_t *config)

  Add a SPI Flash device onto the SPI bus.

  The bus should be already initialized by `spi_bus_initialization`.

  Parameters:

    - out_chip -- Pointer to hold the initialized chip.

    - config -- Configuration of the chips to initialize.

  Returns:

    - ESP_ERR_INVALID_ARG: out_chip is NULL, or some field in the config is invalid.

    - ESP_ERR_NO_MEM: failed to allocate memory for the chip structures.

    - ESP_OK: success.

esp_err_t spi_bus_remove_flash_device(esp_flash_t *chip)

  Remove a SPI Flash device from the SPI bus.

  Parameters:

    chip -- The flash device to remove.

  Returns:

    - ESP_ERR_INVALID_ARG: The chip is invalid.

    - ESP_OK: success.

### Structures

struct esp_flash_spi_device_config_t

  Configurations for the SPI Flash to init.

  Public Members

  spi_host_device_t host_id

    Bus to use.

  int cs_io_num

    GPIO pin to output the CS signal.

  esp_flash_io_mode_t io_mode

    IO mode to read from the Flash.

  enum esp_flash_speed_s speed

    Speed of the Flash clock. Replaced by freq_mhz.

  int input_delay_ns

    Input delay of the data pins, in ns. Set to 0 if unknown.

  int cs_id

    CS line ID, ignored when not `host_id` is not SPI1_HOST, or `CONFIG_SPI_FLASH_SHARE_SPI1_BUS` is enabled. In this case, the CS line used is automatically assigned by the SPI bus lock.

  int freq_mhz

    The frequency of flash chip(MHZ)

  spi_clock_source_t clock_source

    Select SPI clock source, `SPI_CLK_SRC_DEFAULT` by default.

### Header File

- components/spi_flash/include/esp_flash.h

- This header file can be included with:

  >     #include "esp_flash.h"

- This header file is a part of the API provided by the `spi_flash` component. To declare that your component depends on `spi_flash`, add the following to your CMakeLists.txt:

  >     REQUIRES spi_flash

  > or

  >     PRIV_REQUIRES spi_flash

### Functions

esp_err_t esp_flash_init(esp_flash_t *chip)

  Initialise SPI flash chip interface.

  This function must be called before any other API functions are called for this chip.

  Note

  Only the `host` and `read_mode` fields of the chip structure must be initialised before this function is called. Other fields may be auto-detected if left set to zero or NULL.

  Note

  If the chip->drv pointer is NULL, chip chip_drv will be auto-detected based on its manufacturer & product IDs. See `esp_flash_registered_flash_drivers` pointer for details of this process.

  Parameters:

    chip -- Pointer to SPI flash chip to use. If NULL, esp_flash_default_chip is substituted.

  Returns:

    ESP_OK on success, or a flash error code if initialisation fails.

bool esp_flash_chip_driver_initialized(const esp_flash_t *chip)

  Check if appropriate chip driver is set.

  Parameters:

    chip -- Pointer to SPI flash chip to use. If NULL, esp_flash_default_chip is substituted.

  Returns:

    true if set, otherwise false.

esp_err_t esp_flash_read_id(esp_flash_t *chip, uint32_t *out_id)

  Read flash ID via the common "RDID" SPI flash command.

  ID is a 24-bit value. Lower 16 bits of 'id' are the chip ID, upper 8 bits are the manufacturer ID.

  Parameters:

    - chip -- Pointer to identify flash chip. Must have been successfully initialised via esp_flash_init()

    - out_id -- [out] Pointer to receive ID value.

  Returns:

    ESP_OK on success, or a flash error code if operation failed.

esp_err_t esp_flash_get_size(esp_flash_t *chip, uint32_t *out_size)

  Detect flash size based on flash ID.

  Note

  1. Most flash chips use a common format for flash ID, where the lower 4 bits specify the size as a power of 2. If the manufacturer doesn't follow this convention, the size may be incorrectly detected.

  1. The out_size returned only stands for The out_size stands for the size in the binary image header. If you want to get the real size of the chip, please call `esp_flash_get_physical_size` instead.

  Parameters:

    - chip -- Pointer to identify flash chip. Must have been successfully initialised via esp_flash_init()

    - out_size -- [out] Detected size in bytes, standing for the size in the binary image header.

  Returns:

    ESP_OK on success, or a flash error code if operation failed.

esp_err_t esp_flash_get_physical_size(esp_flash_t *chip, uint32_t *flash_size)

  Detect flash size based on flash ID.

  Note

  Most flash chips use a common format for flash ID, where the lower 4 bits specify the size as a power of 2. If the manufacturer doesn't follow this convention, the size may be incorrectly detected.

  Parameters:

    - chip -- Pointer to identify flash chip. Must have been successfully initialised via esp_flash_init()

    - flash_size -- [out] Detected size in bytes.

  Returns:

    ESP_OK on success, or a flash error code if operation failed.

esp_err_t esp_flash_read_unique_chip_id(esp_flash_t *chip, uint64_t *out_id)

  Read flash unique ID via the common "RDUID" SPI flash command.

  ID is a 64-bit value.

  Note

  This is an optional feature, which is not supported on all flash chips. READ PROGRAMMING GUIDE FIRST!

  Parameters:

    - chip -- Pointer to identify flash chip. Must have been successfully initialised via esp_flash_init().

    - out_id -- [out] Pointer to receive unique ID value.

  Returns:

    - ESP_OK on success, or a flash error code if operation failed.

    - ESP_ERR_NOT_SUPPORTED if the chip doesn't support read id.

esp_err_t esp_flash_erase_chip(esp_flash_t *chip)

  Erase flash chip contents.

  Parameters:

    chip -- Pointer to identify flash chip. Must have been successfully initialised via esp_flash_init()

  Returns:

    - ESP_OK on success,

    - ESP_ERR_NOT_SUPPORTED if the chip is not able to perform the operation. This is indicated by WREN = 1 after the command is sent.

    - ESP_ERR_NOT_ALLOWED if a read-only partition is present.

    - Other flash error code if operation failed.

esp_err_t esp_flash_erase_region(esp_flash_t *chip, uint32_t start, uint32_t len)

  Erase a region of the flash chip.

  Sector size is specified in chip->drv->sector_size field (typically 4096 bytes.) ESP_ERR_INVALID_ARG will be returned if the start & length are not a multiple of this size.

  Erase is performed using block (multi-sector) erases where possible (block size is specified in chip->drv->block_erase_size field, typically 65536 bytes). Remaining sectors are erased using individual sector erase commands.

  Parameters:

    - chip -- Pointer to identify flash chip. If NULL, esp_flash_default_chip is substituted. Must have been successfully initialised via esp_flash_init()

    - start -- Address to start erasing flash. Must be sector aligned.

    - len -- Length of region to erase. Must also be sector aligned.

  Returns:

    - ESP_OK on success,

    - ESP_ERR_NOT_SUPPORTED if the chip is not able to perform the operation. This is indicated by WREN = 1 after the command is sent.

    - ESP_ERR_NOT_ALLOWED if the address range (start – start + len) overlaps with a read-only partition address space

    - Other flash error code if operation failed.

esp_err_t esp_flash_get_chip_write_protect(esp_flash_t *chip, bool *write_protected)

  Read if the entire chip is write protected.

  Note

  A correct result for this flag depends on the SPI flash chip model and chip_drv in use (via the 'chip->drv' field).

  Parameters:

    - chip -- Pointer to identify flash chip. If NULL, esp_flash_default_chip is substituted. Must have been successfully initialised via esp_flash_init()

    - write_protected -- [out] Pointer to boolean, set to the value of the write protect flag.

  Returns:

    ESP_OK on success, or a flash error code if operation failed.

esp_err_t esp_flash_set_chip_write_protect(esp_flash_t *chip, bool write_protect)

  Set write protection for the SPI flash chip.

  Some SPI flash chips may require a power cycle before write protect status can be cleared. Otherwise, write protection can be removed via a follow-up call to this function.

  Note

  Correct behaviour of this function depends on the SPI flash chip model and chip_drv in use (via the 'chip->drv' field).

  Parameters:

    - chip -- Pointer to identify flash chip. If NULL, esp_flash_default_chip is substituted. Must have been successfully initialised via esp_flash_init()

    - write_protect -- Boolean value for the write protect flag

  Returns:

    ESP_OK on success, or a flash error code if operation failed.

esp_err_t esp_flash_get_protectable_regions(const esp_flash_t *chip, const esp_flash_region_t **out_regions, uint32_t *out_num_regions)

  Read the list of individually protectable regions of this SPI flash chip.

  Note

  Correct behaviour of this function depends on the SPI flash chip model and chip_drv in use (via the 'chip->drv' field).

  Parameters:

    - chip -- Pointer to identify flash chip. Must have been successfully initialised via esp_flash_init()

    - out_regions -- [out] Pointer to receive a pointer to the array of protectable regions of the chip.

    - out_num_regions -- [out] Pointer to an integer receiving the count of protectable regions in the array returned in 'regions'.

  Returns:

    ESP_OK on success, or a flash error code if operation failed.

esp_err_t esp_flash_get_protected_region(esp_flash_t *chip, const esp_flash_region_t *region, bool *out_protected)

  Detect if a region of the SPI flash chip is protected.

  Note

  It is possible for this result to be false and write operations to still fail, if protection is enabled for the entire chip.

  Note

  Correct behaviour of this function depends on the SPI flash chip model and chip_drv in use (via the 'chip->drv' field).

  Parameters:

    - chip -- Pointer to identify flash chip. Must have been successfully initialised via esp_flash_init()

    - region -- Pointer to a struct describing a protected region. This must match one of the regions returned from esp_flash_get_protectable_regions(...).

    - out_protected -- [out] Pointer to a flag which is set based on the protected status for this region.

  Returns:

    ESP_OK on success, or a flash error code if operation failed.

esp_err_t esp_flash_set_protected_region(esp_flash_t *chip, const esp_flash_region_t *region, bool protect)

  Update the protected status for a region of the SPI flash chip.

  Note

  It is possible for the region protection flag to be cleared and write operations to still fail, if protection is enabled for the entire chip.

  Note

  Correct behaviour of this function depends on the SPI flash chip model and chip_drv in use (via the 'chip->drv' field).

  Parameters:

    - chip -- Pointer to identify flash chip. Must have been successfully initialised via esp_flash_init()

    - region -- Pointer to a struct describing a protected region. This must match one of the regions returned from esp_flash_get_protectable_regions(...).

    - protect -- Write protection flag to set.

  Returns:

    ESP_OK on success, or a flash error code if operation failed.

esp_err_t esp_flash_read(esp_flash_t *chip, void *buffer, uint32_t address, uint32_t length)

  Read data from the SPI flash chip.

  There are no alignment constraints on buffer, address or length.

  Note

  If on-chip flash encryption is used, this function returns raw (ie encrypted) data. Use the flash cache to transparently decrypt data.

  Parameters:

    - chip -- Pointer to identify flash chip. If NULL, esp_flash_default_chip is substituted. Must have been successfully initialised via esp_flash_init()

    - buffer -- Pointer to a buffer where the data will be read. To get better performance, this should be in the DRAM and word aligned.

    - address -- Address on flash to read from. Must be less than chip->size field.

    - length -- Length (in bytes) of data to read.

  Returns:

    - ESP_OK: success

    - ESP_ERR_NO_MEM: Buffer is in external PSRAM which cannot be concurrently accessed, and a temporary internal buffer could not be allocated.

    - or a flash error code if operation failed.

esp_err_t esp_flash_write(esp_flash_t *chip, const void *buffer, uint32_t address, uint32_t length)

  Write data to the SPI flash chip.

  There are no alignment constraints on buffer, address or length.

  Parameters:

    - chip -- Pointer to identify flash chip. If NULL, esp_flash_default_chip is substituted. Must have been successfully initialised via esp_flash_init()

    - address -- Address on flash to write to. Must be previously erased (SPI NOR flash can only write bits 1->0).

    - buffer -- Pointer to a buffer with the data to write. To get better performance, this should be in the DRAM and word aligned.

    - length -- Length (in bytes) of data to write.

  Returns:

    - ESP_OK on success

    - ESP_FAIL, bad write, this will be detected only when CONFIG_SPI_FLASH_VERIFY_WRITE is enabled

    - ESP_ERR_NOT_SUPPORTED if the chip is not able to perform the operation. This is indicated by WREN = 1 after the command is sent.

    - ESP_ERR_NOT_ALLOWED if the address range (address – address + length) overlaps with a read-only partition address space

    - Other flash error code if operation failed.

esp_err_t esp_flash_write_encrypted(esp_flash_t *chip, uint32_t address, const void *buffer, uint32_t length)

  Encrypted and write data to the SPI flash chip using on-chip hardware flash encryption.

  Note

  Both address & length must be 16 byte aligned, as this is the encryption block size

  Parameters:

    - chip -- Pointer to identify flash chip. Must be NULL (the main flash chip). For other chips, encrypted write is not supported.

    - address -- Address on flash to write to. 16 byte aligned. Must be previously erased (SPI NOR flash can only write bits 1->0).

    - buffer -- Pointer to a buffer with the data to write.

    - length -- Length (in bytes) of data to write. 16 byte aligned.

  Returns:

    - ESP_OK: on success

    - ESP_FAIL: bad write, this will be detected only when CONFIG_SPI_FLASH_VERIFY_WRITE is enabled

    - ESP_ERR_NOT_SUPPORTED: encrypted write not supported for this chip.

    - ESP_ERR_INVALID_ARG: Either the address, buffer or length is invalid.

    - ESP_ERR_NOT_ALLOWED if the address range (address – address + length) overlaps with a read-only partition address space

esp_err_t esp_flash_read_encrypted(esp_flash_t *chip, uint32_t address, void *out_buffer, uint32_t length)

  Read and decrypt data from the SPI flash chip using on-chip hardware flash encryption.

  Parameters:

    - chip -- Pointer to identify flash chip. Must be NULL (the main flash chip). For other chips, encrypted read is not supported.

    - address -- Address on flash to read from.

    - out_buffer -- Pointer to a buffer for the data to read to.

    - length -- Length (in bytes) of data to read.

  Returns:

    - ESP_OK: on success

    - ESP_ERR_NOT_SUPPORTED: encrypted read not supported for this chip.

static inline bool esp_flash_is_quad_mode(const esp_flash_t *chip)

  Returns true if chip is configured for Quad I/O or Quad Fast Read.

  Parameters:

    chip -- Pointer to SPI flash chip to use. If NULL, esp_flash_default_chip is substituted.

  Returns:

    true if flash works in quad mode, otherwise false

### Structures

struct esp_flash_region_t

  Structure for describing a region of flash.

  Public Members

  uint32_t offset

    Start address of this region.

  uint32_t size

    Size of the region.

struct esp_flash_os_functions_t

  OS-level integration hooks for accessing flash chips inside a running OS.

  It's in the public header because some instances should be allocated statically in the startup code. May be updated according to hardware version and new flash chip feature requirements, shouldn't be treated as public API.

  For advanced developers, you may replace some of them with your implementations at your own risk.

  Public Members

  esp_err_t (*start)(void *arg, uint32_t flags)

    Called before commencing any flash operation. Does not need to be recursive (ie is called at most once for each call to 'end').

  esp_err_t (*end)(void *arg)

    Called after completing any flash operation.

  esp_err_t (*region_protected)(void *arg, size_t start_addr, size_t size)

    Called before any erase/write operations to check whether the region is limited by the OS

  esp_err_t (*delay_us)(void *arg, uint32_t us)

    Delay for at least 'us' microseconds. Called in between 'start' and 'end'.

  void *(*get_temp_buffer)(void *arg, size_t reqest_size, size_t *out_size)

    Called for get temp buffer when buffer from application cannot be directly read into/write from.

  void (*release_temp_buffer)(void *arg, void *temp_buf)

    Called for release temp buffer.

  esp_err_t (*check_yield)(void *arg, uint32_t chip_status, uint32_t *out_request)

    Yield to other tasks. Called during erase operations.

    Return:

      ESP_OK means yield needs to be called (got an event to handle), while ESP_ERR_TIMEOUT means skip yield.

  esp_err_t (*yield)(void *arg, uint32_t *out_status)

    Yield to other tasks. Called during erase operations.

  int64_t (*get_system_time)(void *arg)

    Called for get system time.

  void (*set_flash_op_status)(uint32_t op_status)

    Call to set flash operation status

struct esp_flash_t

  Structure to describe a SPI flash chip connected to the system.

  Structure must be initialized before use (passed to esp_flash_init()). It's in the public header because some instances should be allocated statically in the startup code. May be updated according to hardware version and new flash chip feature requirements, shouldn't be treated as public API.

  For advanced developers, you may replace some of them with your implementations at your own risk.

  Public Members

  spi_flash_host_inst_t *host

    Pointer to hardware-specific "host_driver" structure. Must be initialized before used.

  const spi_flash_chip_t *chip_drv

    Pointer to chip-model-specific "adapter" structure. If NULL, will be detected during initialisation.

  const esp_flash_os_functions_t *os_func

    Pointer to os-specific hook structure. Call `esp_flash_init_os_functions()` to setup this field, after the host is properly initialized.

  void *os_func_data

    Pointer to argument for os-specific hooks. Left NULL and will be initialized with `os_func`.

  esp_flash_io_mode_t read_mode

    Configured SPI flash read mode. Set before `esp_flash_init` is called.

  uint32_t size

    Size of SPI flash in bytes. If 0, size will be detected during initialisation. Note: this stands for the size in the binary image header. If you want to get the flash physical size, please call `esp_flash_get_physical_size`.

  uint32_t chip_id

    Detected chip id.

  uint32_t busy

    This flag is used to verify chip's status.

  uint32_t hpm_dummy_ena

    This flag is used to verify whether flash works under HPM status.

  uint32_t reserved_flags

    reserved.

  int clock_source

    Clock source for GPSPI.

### Macros

ESP_FLASH_START_FLAG_LIMIT_CPU_FREQ

  Flags for start function Limit CPU frequency during flash operations (ESP32-C5 only, 240MHz).

SPI_FLASH_YIELD_REQ_YIELD

SPI_FLASH_YIELD_REQ_SUSPEND

SPI_FLASH_YIELD_STA_RESUME

SPI_FLASH_OS_IS_ERASING_STATUS_FLAG

### Type Definitions

typedef struct spi_flash_chip_t spi_flash_chip_t

### Header File

- components/spi_flash/include/spi_flash_mmap.h

- This header file can be included with:

  >     #include "spi_flash_mmap.h"

- This header file is a part of the API provided by the `spi_flash` component. To declare that your component depends on `spi_flash`, add the following to your CMakeLists.txt:

  >     REQUIRES spi_flash

  > or

  >     PRIV_REQUIRES spi_flash

### Functions

esp_err_t spi_flash_mmap(size_t src_addr, size_t size, spi_flash_mmap_memory_t memory, const void **out_ptr, spi_flash_mmap_handle_t *out_handle)

  Map region of flash memory into data or instruction address space.

  This function allocates sufficient number of 64kB MMU pages and configures them to map the requested region of flash memory into the address space. It may reuse MMU pages which already provide the required mapping.

  As with any allocator, if mmap/munmap are heavily used then the address space may become fragmented. To troubleshoot issues with page allocation, use spi_flash_mmap_dump() function.

  Parameters:

    - src_addr -- Physical address in flash where requested region starts. This address must be aligned to 64kB boundary (SPI_FLASH_MMU_PAGE_SIZE)

    - size -- Size of region to be mapped. This size will be rounded up to a 64kB boundary

    - memory -- Address space where the region should be mapped (data or instruction)

    - out_ptr -- [out] Output, pointer to the mapped memory region

    - out_handle -- [out] Output, handle which should be used for spi_flash_munmap call

  Returns:

    ESP_OK on success, ESP_ERR_NO_MEM if pages can not be allocated

esp_err_t spi_flash_mmap_pages(const int *pages, size_t page_count, spi_flash_mmap_memory_t memory, const void **out_ptr, spi_flash_mmap_handle_t *out_handle)

  Map sequences of pages of flash memory into data or instruction address space.

  This function allocates sufficient number of 64kB MMU pages and configures them to map the indicated pages of flash memory contiguously into address space. In this respect, it works in a similar way as spi_flash_mmap() but it allows mapping a (maybe non-contiguous) set of pages into a contiguous region of memory.

  Parameters:

    - pages -- An array of numbers indicating the 64kB pages in flash to be mapped contiguously into memory. These indicate the indexes of the 64kB pages, not the byte-size addresses as used in other functions. Array must be located in internal memory.

    - page_count -- Number of entries in the pages array

    - memory -- Address space where the region should be mapped (instruction or data)

    - out_ptr -- [out] Output, pointer to the mapped memory region

    - out_handle -- [out] Output, handle which should be used for spi_flash_munmap call

  Returns:

    - ESP_OK on success

    - ESP_ERR_NO_MEM if pages can not be allocated

    - ESP_ERR_INVALID_ARG if pagecount is zero or pages array is not in internal memory

void spi_flash_munmap(spi_flash_mmap_handle_t handle)

  Release region previously obtained using spi_flash_mmap.

  Note

  Calling this function will not necessarily unmap memory region. Region will only be unmapped when there are no other handles which reference this region. In case of partially overlapping regions it is possible that memory will be unmapped partially.

  Parameters:

    handle -- Handle obtained from spi_flash_mmap

void spi_flash_mmap_dump(void)

  Display information about mapped regions.

  This function lists handles obtained using spi_flash_mmap, along with range of pages allocated to each handle. It also lists all non-zero entries of MMU table and corresponding reference counts.

uint32_t spi_flash_mmap_get_free_pages(spi_flash_mmap_memory_t memory)

  get free pages number which can be mmap

  This function will return number of free pages available in mmu table. This could be useful before calling actual spi_flash_mmap (maps flash range to DCache or ICache memory) to check if there is sufficient space available for mapping.

  Parameters:

    memory -- memory type of MMU table free page

  Returns:

    number of free pages which can be mmaped

size_t spi_flash_cache2phys(const void *cached)

  Given a memory address where flash is mapped, return the corresponding physical flash offset.

  Cache address does not have have been assigned via spi_flash_mmap(), any address in memory mapped flash space can be looked up.

  Parameters:

    cached -- Pointer to flashed cached memory.

  Returns:

    - SPI_FLASH_CACHE2PHYS_FAIL If cache address is outside flash cache region, or the address is not mapped.

    - Otherwise, returns physical offset in flash

const void *spi_flash_phys2cache(size_t phys_offs, spi_flash_mmap_memory_t memory)

  Given a physical offset in flash, return the address where it is mapped in the memory space.

  Physical address does not have to have been assigned via spi_flash_mmap(), any address in flash can be looked up.

  Note

  Only the first matching cache address is returned. If MMU flash cache table is configured so multiple entries point to the same physical address, there may be more than one cache address corresponding to that physical address. It is also possible for a single physical address to be mapped to both the IROM and DROM regions.

  Note

  This function doesn't impose any alignment constraints, but if memory argument is SPI_FLASH_MMAP_INST and phys_offs is not 4-byte aligned, then reading from the returned pointer will result in a crash.

  Parameters:

    - phys_offs -- Physical offset in flash memory to look up.

    - memory -- Address space type to look up a flash cache address mapping for (instruction or data)

  Returns:

    - NULL if the physical address is invalid or not mapped to flash cache of the specified memory type.

    - Cached memory address (in IROM or DROM space) corresponding to phys_offs.

### Macros

ESP_ERR_FLASH_OP_FAIL

  This file contains `spi_flash_mmap_xx` APIs, mainly for doing memory mapping to an SPI0-connected external Flash, as well as some helper functions to convert between virtual and physical address

ESP_ERR_FLASH_OP_TIMEOUT

SPI_FLASH_SEC_SIZE

  SPI Flash sector size

SPI_FLASH_MMU_PAGE_SIZE

  Flash cache MMU mapping page size

SPI_FLASH_CACHE2PHYS_FAIL

### Type Definitions

typedef uint32_t spi_flash_mmap_handle_t

  Opaque handle for memory region obtained from spi_flash_mmap.

### Enumerations

enum spi_flash_mmap_memory_t

  Enumeration which specifies memory space requested in an mmap call.

  Values:

  enumerator SPI_FLASH_MMAP_DATA

    map to data memory, allows byte-aligned access

  enumerator SPI_FLASH_MMAP_INST

    map to instruction memory, allows only 4-byte-aligned access

### Header File

- components/hal/include/hal/spi_flash_types.h

- This header file can be included with:

  >     #include "hal/spi_flash_types.h"

### Structures

struct spi_flash_trans_t

  Definition of a common transaction. Also holds the return value.

  Public Members

  uint8_t reserved

    Reserved, must be 0.

  uint8_t mosi_len

    Output data length, in bytes.

  uint8_t miso_len

    Input data length, in bytes.

  uint8_t address_bitlen

    Length of address in bits, set to 0 if command does not need an address.

  uint32_t address

    Address to perform operation on.

  const uint8_t *mosi_data

    Output data to salve.

  uint8_t *miso_data

    [out] Input data from slave, little endian

  uint32_t flags

    Flags for this transaction. Set to 0 for now.

  uint16_t command

    Command to send.

  uint8_t dummy_bitlen

    Basic dummy bits to use.

  uint32_t io_mode

    Flash working mode when `SPI_FLASH_IGNORE_BASEIO` is specified.

struct spi_flash_sus_cmd_conf

  Configuration structure for the flash chip suspend feature.

  Public Members

  uint32_t sus_mask

    SUS/SUS1/SUS2 bit in flash register.

  uint32_t cmd_rdsr

    Read flash status register(2) command.

  uint32_t sus_cmd

    Flash suspend command.

  uint32_t res_cmd

    Flash resume command.

  uint32_t reserved

    Reserved, set to 0.

struct spi_flash_encryption_t

  Structure for flash encryption operations.

  Public Members

  void (*flash_encryption_enable)(void)

    Enable the flash encryption.

  void (*flash_encryption_disable)(void)

    Disable the flash encryption.

  void (*flash_encryption_data_prepare)(uint32_t address, const uint32_t *buffer, uint32_t size)

    Prepare flash encryption before operation.

    Note

    address and buffer must be 8-word aligned.

    Param address:

      The destination address in flash for the write operation.

    Param buffer:

      Data for programming

    Param size:

      Size to program.

  void (*flash_encryption_done)(void)

    flash data encryption operation is done.

  void (*flash_encryption_destroy)(void)

    Destroy encrypted result

  bool (*flash_encryption_check)(uint32_t address, uint32_t length)

    Check if is qualified to encrypt the buffer

    Param address:

      the address of written flash partition.

    Param length:

      Buffer size.

struct spi_flash_host_inst_t

  SPI Flash Host driver instance

  Public Members

  const struct spi_flash_host_driver_s *driver

    Pointer to the implementation function table.

struct spi_flash_host_driver_s

  Host driver configuration and context structure.

  Public Members

  esp_err_t (*dev_config)(spi_flash_host_inst_t *host)

    Configure the device-related register before transactions. This saves some time to re-configure those registers when we send continuously

  esp_err_t (*common_command)(spi_flash_host_inst_t *host, spi_flash_trans_t *t)

    Send an user-defined spi transaction to the device.

  esp_err_t (*read_id)(spi_flash_host_inst_t *host, uint32_t *id)

    Read flash ID.

  void (*erase_chip)(spi_flash_host_inst_t *host)

    Erase whole flash chip.

  void (*erase_sector)(spi_flash_host_inst_t *host, uint32_t start_address)

    Erase a specific sector by its start address.

  void (*erase_block)(spi_flash_host_inst_t *host, uint32_t start_address)

    Erase a specific block by its start address.

  esp_err_t (*read_status)(spi_flash_host_inst_t *host, uint8_t *out_sr)

    Read the status of the flash chip.

  esp_err_t (*set_write_protect)(spi_flash_host_inst_t *host, bool wp)

    Disable write protection.

  void (*program_page)(spi_flash_host_inst_t *host, const void *buffer, uint32_t address, uint32_t length)

    Program a page of the flash. Check `max_write_bytes` for the maximum allowed writing length.

  bool (*supports_direct_write)(spi_flash_host_inst_t *host, const void *p)

    Check whether the SPI host supports direct write.

    When cache is disabled, SPI1 doesn't support directly write when buffer isn't internal.

  int (*write_data_slicer)(spi_flash_host_inst_t *host, uint32_t address, uint32_t len, uint32_t *align_addr, uint32_t page_size)

    Slicer for write data. The `program_page` should be called iteratively with the return value of this function.

    Param address:

      Beginning flash address to write

    Param len:

      Length request to write

    Param align_addr:

      Output of the aligned address to write to

    Param page_size:

      Physical page size of the flash chip

    Return:

      Length that can be actually written in one `program_page` call

  esp_err_t (*read)(spi_flash_host_inst_t *host, void *buffer, uint32_t address, uint32_t read_len)

    Read data from the flash. Check `max_read_bytes` for the maximum allowed reading length.

  bool (*supports_direct_read)(spi_flash_host_inst_t *host, const void *p)

    Check whether the SPI host supports direct read.

    When cache is disabled, SPI1 doesn't support directly read when the given buffer isn't internal.

  int (*read_data_slicer)(spi_flash_host_inst_t *host, uint32_t address, uint32_t len, uint32_t *align_addr, uint32_t page_size)

    Slicer for read data. The `read` should be called iteratively with the return value of this function.

    Param address:

      Beginning flash address to read

    Param len:

      Length request to read

    Param align_addr:

      Output of the aligned address to read

    Param page_size:

      Physical page size of the flash chip

    Return:

      Length that can be actually read in one `read` call

  uint32_t (*host_status)(spi_flash_host_inst_t *host)

    Check the host status, 0:busy, 1:idle, 2:suspended.

  esp_err_t (*configure_host_io_mode)(spi_flash_host_inst_t *host, uint32_t command, uint32_t addr_bitlen, int dummy_bitlen_base, esp_flash_io_mode_t io_mode)

    Configure the host to work at different read mode. Responsible to compensate the timing and set IO mode.

  void (*poll_cmd_done)(spi_flash_host_inst_t *host)

    Internal use, poll the HW until the last operation is done.

  esp_err_t (*flush_cache)(spi_flash_host_inst_t *host, uint32_t addr, uint32_t size)

    For some host (SPI1), they are shared with a cache. When the data is modified, the cache needs to be flushed. Left NULL if not supported.

  void (*check_suspend)(spi_flash_host_inst_t *host)

    Suspend check erase/program operation, reserved for ESP32-C3 and ESP32-S3 spi flash ROM IMPL.

  void (*resume)(spi_flash_host_inst_t *host)

    Resume flash from suspend manually

  void (*suspend)(spi_flash_host_inst_t *host)

    Set flash in suspend status manually

  esp_err_t (*sus_setup)(spi_flash_host_inst_t *host, const spi_flash_sus_cmd_conf *sus_conf)

    Suspend feature setup for setting cmd and status register mask.

### Macros

SPI_FLASH_TRANS_FLAG_CMD16

  Send command of 16 bits.

SPI_FLASH_TRANS_FLAG_IGNORE_BASEIO

  Not applying the basic io mode configuration for this transaction.

SPI_FLASH_TRANS_FLAG_BYTE_SWAP

  Used for DTR mode, to swap the bytes of a pair of rising/falling edge.

SPI_FLASH_TRANS_FLAG_PE_CMD

  Indicates that this transaction is to erase/program flash chip.

SPI_FLASH_CONFIG_CONF_BITS

  OR the io_mode with this mask, to enable the dummy output feature or replace the first several dummy bits into address to meet the requirements of conf bits. (Used in DIO/QIO/OIO mode)

SPI_FLASH_OPI_FLAG

  A flag for flash work in opi mode, the io mode below are opi, above are SPI/QSPI mode. DO NOT use this value in any API.

SPI_FLASH_READ_MODE_MIN

  Slowest io mode supported by ESP32, currently SlowRd.

### Type Definitions

typedef enum esp_flash_speed_s esp_flash_speed_t

  SPI flash clock speed values, always refer to them by the enum rather than the actual value (more speed may be appended into the list).

  A strategy to select the maximum allowed speed is to enumerate from the `ESP_FLSH_SPEED_MAX-1` or highest frequency supported by your flash, and decrease the speed until the probing success.

typedef struct spi_flash_host_driver_s spi_flash_host_driver_t

### Enumerations

enum esp_flash_speed_s

  SPI flash clock speed values, always refer to them by the enum rather than the actual value (more speed may be appended into the list).

  A strategy to select the maximum allowed speed is to enumerate from the `ESP_FLSH_SPEED_MAX-1` or highest frequency supported by your flash, and decrease the speed until the probing success.

  Values:

  enumerator ESP_FLASH_5MHZ

    The flash runs under 5MHz.

  enumerator ESP_FLASH_10MHZ

    The flash runs under 10MHz.

  enumerator ESP_FLASH_20MHZ

    The flash runs under 20MHz.

  enumerator ESP_FLASH_26MHZ

    The flash runs under 26MHz.

  enumerator ESP_FLASH_40MHZ

    The flash runs under 40MHz.

  enumerator ESP_FLASH_80MHZ

    The flash runs under 80MHz.

  enumerator ESP_FLASH_120MHZ

    The flash runs under 120MHz, 120MHZ can only be used by main flash after timing tuning in system. Do not use this directly in any API.

  enumerator ESP_FLASH_SPEED_MAX

    The maximum frequency supported by the host is `ESP_FLASH_SPEED_MAX-1`.

enum esp_flash_io_mode_t

  Mode used for reading from SPI flash.

  Values:

  enumerator SPI_FLASH_SLOWRD

    Data read using single I/O, some limits on speed.

  enumerator SPI_FLASH_FASTRD

    Data read using single I/O, no limit on speed.

  enumerator SPI_FLASH_DOUT

    Data read using dual I/O.

  enumerator SPI_FLASH_DIO

    Both address & data transferred using dual I/O.

  enumerator SPI_FLASH_QOUT

    Data read using quad I/O.

  enumerator SPI_FLASH_QIO

    Both address & data transferred using quad I/O.

  enumerator SPI_FLASH_OPI_STR

    Only support on OPI flash, flash read and write under STR mode.

  enumerator SPI_FLASH_OPI_DTR

    Only support on OPI flash, flash read and write under DTR mode.

  enumerator SPI_FLASH_READ_MODE_MAX

    The fastest io mode supported by the host is `ESP_FLASH_READ_MODE_MAX-1`.

### Header File

- components/hal/include/hal/esp_flash_err.h

- This header file can be included with:

  >     #include "hal/esp_flash_err.h"

### Macros

ESP_ERR_FLASH_NOT_INITIALISED

  esp_flash_chip_t structure not correctly initialised by esp_flash_init().

ESP_ERR_FLASH_UNSUPPORTED_HOST

  Requested operation isn't supported via this host SPI bus (chip->spi field).

ESP_ERR_FLASH_UNSUPPORTED_CHIP

  Requested operation isn't supported by this model of SPI flash chip.

ESP_ERR_FLASH_PROTECTED

  Write operation failed due to chip's write protection being enabled.

### Header File

- components/spi_flash/include/esp_spi_flash_counters.h

- This header file can be included with:

  >     #include "esp_spi_flash_counters.h"

- This header file is a part of the API provided by the `spi_flash` component. To declare that your component depends on `spi_flash`, add the following to your CMakeLists.txt:

  >     REQUIRES spi_flash

  > or

  >     PRIV_REQUIRES spi_flash

### Functions

void esp_flash_reset_counters(void)

  Reset SPI flash operation counters.

void spi_flash_reset_counters(void)

void esp_flash_dump_counters(FILE *stream)

  Print SPI flash operation counters.

void spi_flash_dump_counters(void)

const esp_flash_counters_t *esp_flash_get_counters(void)

  Return current SPI flash operation counters.

  Returns:

    pointer to the esp_flash_counters_t structure holding values of the operation counters

const spi_flash_counters_t *spi_flash_get_counters(void)

### Structures

struct esp_flash_counter_t

  Structure holding statistics for one type of operation

  Public Members

  uint32_t count

    number of times operation was executed

  uint32_t time

    total time taken, in microseconds

  uint32_t bytes

    total number of bytes

struct esp_flash_counters_t

  Structure for counters of flash actions

  Public Members

  esp_flash_counter_t read

    counters for read action, like `esp_flash_read`

  esp_flash_counter_t write

    counters for write action, like `esp_flash_write`

  esp_flash_counter_t erase

    counters for erase action, like `esp_flash_erase`

### Type Definitions

typedef esp_flash_counter_t spi_flash_counter_t

typedef esp_flash_counters_t spi_flash_counters_t

## API Reference - Flash Encrypt

### Header File

- components/bootloader_support/include/esp_flash_encrypt.h

- This header file can be included with:

  >     #include "esp_flash_encrypt.h"

- This header file is a part of the API provided by the `bootloader_support` component. To declare that your component depends on `bootloader_support`, add the following to your CMakeLists.txt:

  >     REQUIRES bootloader_support

  > or

  >     PRIV_REQUIRES bootloader_support

### Functions

bool esp_flash_encryption_enabled(void)

  Is flash encryption currently enabled in hardware?

  Flash encryption is enabled if the FLASH_CRYPT_CNT efuse has an odd number of bits set.

  Returns:

    true if flash encryption is enabled.

esp_err_t esp_flash_encrypt_check_and_update(void)

bool esp_flash_encrypt_state(void)

  Returns the Flash Encryption state and prints it.

  Returns:

    True - Flash Encryption is enabled False - Flash Encryption is not enabled

bool esp_flash_encrypt_initialized_once(void)

  Checks if the first initialization was done.

  If the first initialization was done then FLASH_CRYPT_CNT != 0

  Returns:

    true - the first initialization was done false - the first initialization was NOT done

esp_err_t esp_flash_encrypt_init(void)

  The first initialization of Flash Encryption key and related eFuses.

  Returns:

    ESP_OK if all operations succeeded

esp_err_t esp_flash_encrypt_contents(void)

  Encrypts flash content.

  Returns:

    ESP_OK if all operations succeeded

esp_err_t esp_flash_encrypt_enable(void)

  Activates Flash encryption on the chip.

  It burns FLASH_CRYPT_CNT eFuse based on the CONFIG_SECURE_FLASH_ENCRYPTION_MODE_RELEASE option.

  Returns:

    ESP_OK if all operations succeeded

bool esp_flash_encrypt_is_write_protected(bool print_error)

  Returns True if the write protection of FLASH_CRYPT_CNT is set.

  Parameters:

    print_error -- Print error if it is write protected

  Returns:

    true - if FLASH_CRYPT_CNT is write protected

esp_err_t esp_flash_encrypt_region(uint32_t src_addr, size_t data_length)

  Encrypt-in-place a block of flash sectors.

  Note

  This function resets RTC_WDT between operations with sectors.

  Parameters:

    - src_addr -- Source offset in flash. Should be multiple of 4096 bytes.

    - data_length -- Length of data to encrypt in bytes. Will be rounded up to next multiple of 4096 bytes.

  Returns:

    ESP_OK if all operations succeeded, ESP_ERR_FLASH_OP_FAIL if SPI flash fails, ESP_ERR_FLASH_OP_TIMEOUT if flash times out.

void esp_flash_write_protect_crypt_cnt(void)

  Write protect FLASH_CRYPT_CNT.

  Intended to be called as a part of boot process if flash encryption is enabled but secure boot is not used. This should protect against serial re-flashing of an unauthorised code in absence of secure boot.

  Note

  On ESP32 V3 only, write protecting FLASH_CRYPT_CNT will also prevent disabling UART Download Mode. If both are wanted, call esp_efuse_disable_rom_download_mode() before calling this function.

esp_flash_enc_mode_t esp_get_flash_encryption_mode(void)

  Return the flash encryption mode.

  The API is called during boot process but can also be called by application to check the current flash encryption mode of ESP32

  Returns:

void esp_flash_encryption_init_checks(void)

  Check the flash encryption mode during startup.

  Verifies the flash encryption config during startup:

  - Correct any insecure flash encryption settings if hardware Secure Boot is enabled.

  - Log warnings if the efuse config doesn't match the project config in any way

  Note

  This function is called automatically during app startup, it doesn't need to be called from the app.

bool esp_flash_encryption_cfg_verify_release_mode(void)

  Returns the verification status for all physical security features of flash encryption in release mode.

  If the device has flash encryption feature configured in the release mode, then it is highly recommended to call this API in the application startup code. This API verifies the sanity of the eFuse configuration against the release (production) mode of the flash encryption feature.

  Returns:

    - True - all eFuses are configured correctly

    - False - not all eFuses are configured correctly.

void esp_flash_encryption_set_release_mode(void)

  Switches Flash Encryption from "Development" to "Release".

  If already in "Release" mode, the function will do nothing. If flash encryption efuse is not enabled yet then abort. It burns:

  - "disable encrypt in dl mode"

  - set FLASH_CRYPT_CNT efuse to max

  In case of the targets that support the XTS-AES peripheral's pseudo rounds function, this API would configure the pseudo rounds level efuse bit to level low if the efuse bit is not set already.

### Enumerations

enum esp_flash_enc_mode_t

  Values:

  enumerator ESP_FLASH_ENC_MODE_DISABLED
  enumerator ESP_FLASH_ENC_MODE_DEVELOPMENT
  enumerator ESP_FLASH_ENC_MODE_RELEASE

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.