# Wi-Fi

[中文]

## Breaking Changes

The parameters for the ESP-NOW sending data callback function has changed from `uint8_t *mac_addr` to `esp_now_send_info_t *tx_info`.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.