# RF Coexistence

[中文]

## Overview

ESP boards now support three modules: Bluetooth (BT & BLE), IEEE 802.15.4 (Thread / Zigbee), and Wi-Fi. Each type of board has only one 2.4 GHz ISM band RF module, shared by two or three modules. Consequently, a module cannot receive or transmit data while another module is engaged in data transmission or reception. In such scenarios, ESP32-C2 employs the time-division multiplexing method to manage the reception and transmission of packets.

## Supported Coexistence Scenario for ESP32-C2

Supported Features of Wi-Fi and BLE Coexistence
| BLE
Scan | Advertising | Connected
Wi-Fi | STA | Scan | Y | Y | Y
Connecting | Y | Y | Y
Connected | Y | Y | Y
SOFTAP | TX Beacon | Y | Y | Y
Connecting | C1 | C1 | C1
Connected | C1 | C1 | C1
Sniffer | RX | C1 | C1 | C1
ESP-NOW | RX | S | S | S
TX | Y | Y | Y

Note

- Y: supported and the performance is stable

- C1: supported but the performance is unstable

- X: not supported

- S: supported and the performance is stable in STA mode, otherwise not supported

## Coexistence Mechanism and Policy

### Coexistence Mechanism

The RF resource allocation mechanism is based on priority. As shown below, Wi-Fi, Bluetooth and 802.15.4 modules request RF resources from the coexistence module, and the coexistence module decides who will use the RF resource based on their priority.

Coexistence Mechanism

### Coexistence Policy

#### Coexistence Period and Time Slice

Wi-Fi and BLE have their fixed time slice to use the RF. In the Wi-Fi time slice, Wi-Fi will send a higher priority request to the coexistence arbitration module. Similarly, BLE can enjoy higher priority at their own time slice. The duration of the coexistence period and the proportion of each time slice are divided into four categories according to the Wi-Fi status:

1. IDLE status: RF module is controlled by Bluetooth module.

2. CONNECTED status: the coexistence period starts at the Target Beacon Transmission Time (TBTT) and is more than 100 ms.

3. SCAN status: Wi-Fi slice and coexistence period are longer than in the CONNECTED status. To ensure Bluetooth performance, the Bluetooth time slice will also be adjusted accordingly.

4. CONNECTING status: Wi-Fi slice is longer than in the CONNECTED status. To ensure Bluetooth performance, the Bluetooth time slice will also be adjusted accordingly.

According to the coexistence logic, different coexistence periods and time slice strategies will be selected based on the Wi-Fi and Bluetooth usage scenarios. A Coexistence policy corresponding to a certain usage scenarios is called a "coexistence scheme". For example, the scenario of Wi-Fi CONNECTED and BLE CONNECTED has a corresponding coexistence scheme. In this scheme, the time slices of Wi-Fi and BLE in a coexistence period each account for 50%. The time allocation is shown in the following figure:

Time Slice Under the Status of Wi-Fi CONNECTED and BLE CONNECTED

#### Dynamic Priority

The coexistence module assigns varying priorities to different statuses of each module, and these priorities are dynamic. For example, in every N BLE Advertising events, there is always one event with high priority. If a high-priority BLE Advertising event occurs within the Wi-Fi time slice, the right to use the RF may be preempted by BLE.

#### Wi-Fi Connectionless Modules Coexistence

To some extent, some combinations of connectionless power-saving parameters Window and Interval would lead to extra Wi-Fi priority request out of Wi-Fi time slice. It`s for obtaining RF resources at coexistence for customized parameters, while leading to impact on Bluetooth performance.

If connectionless power-saving parameters are configured with default values, the coexistence module would perform in stable mode and the behaviour above would not happen. So please configure Wi-Fi connectionless power-saving parameters to default values unless you have plenty of coexistence performance tests for customized parameters.

Please refer to connectionless module power save to get more detail.

## How to Use the Coexistence Feature

### Coexistence API

For most coexistence cases, ESP32-C2 will switch the coexistence status automatically without calling API. However, ESP32-C2 provides two APIs for the coexistence of BLE MESH and Wi-Fi. When the status of BLE MESH changes, call `esp_coex_status_bit_clear` to clear the previous status first and then call `esp_coex_status_bit_set` to set the current status.

#### BLE MESH Coexistence Status

As the firmware of Wi-Fi and Bluetooth are not aware of the current scenario of the upper layer application, some coexistence schemes require application code to call the coexistence API to take effect. The application layer needs to pass the working status of BLE MESH to the coexistence module for selecting the coexistence scheme.

> - ESP_COEX_BLE_ST_MESH_CONFIG: network is provisioning

> - ESP_COEX_BLE_ST_MESH_TRAFFIC: data is transmitting

> - ESP_COEX_BLE_ST_MESH_STANDBY: in idle status with no significant data interaction

### Coexistence API Error Codes

All coexistence APIs have custom return values, i.e., error codes. These error codes can be categorized as:

> - No error. For example, the return value ESP_OK signifies the API returned successfully.

> - Recoverable errors. For example, the return value ESP_ERR_INVALID_ARG signifies API parameter errors.

### Setting Coexistence Compile-time Options

- After writing the coexistence program, you must check CONFIG_ESP_COEX_SW_COEXIST_ENABLE option through menuconfig to open coexistence configuration on software, otherwise the coexistence function mentioned above cannot be used.

- When using LE Coded PHY during a BLE connection, to avoid affecting Wi-Fi performance due to the long duration of Bluetooth packets, you can select BT_LE_COEX_PHY_CODED_TX_RX_TLIM_EN in the sub-options of CONFIG_BT_LE_COEX_PHY_CODED_TX_RX_TLIM to limit the maximum time of TX/RX.

- You can reduce the memory consumption by configuring the following options on menuconfig.

  - CONFIG_BT_BLE_DYNAMIC_ENV_MEMORY: enable the configuration of dynamic memory for Bluetooth protocol stack.

  - CONFIG_ESP_WIFI_STATIC_RX_BUFFER_NUM: reduce the number of Wi-Fi static RX buffers.

  - CONFIG_ESP_WIFI_DYNAMIC_RX_BUFFER_NUM: reduce the number of Wi-Fi dynamic RX buffers.

  - CONFIG_ESP_WIFI_TX_BUFFER: enable the configuration of dynamic allocation TX buffers.

  - CONFIG_ESP_WIFI_DYNAMIC_TX_BUFFER_NUM: reduce the number of Wi-Fi dynamic TX buffers.

  - CONFIG_ESP_WIFI_TX_BA_WIN: reduce the number of Wi-Fi Block Ack TX windows.

  - CONFIG_ESP_WIFI_RX_BA_WIN: reduce the number of Wi-Fi Block Ack RX windows.

  - CONFIG_ESP_WIFI_MGMT_SBUF_NUM: reduce the number of Wi-Fi Management Short Buffer.

  - CONFIG_ESP_WIFI_RX_IRAM_OPT: turning off this configuration option will reduce the IRAM memory by approximately 17 KB.

  - CONFIG_LWIP_TCP_SND_BUF_DEFAULT: reduce the default TX buffer size for TCP sockets.

  - CONFIG_LWIP_TCP_WND_DEFAULT: reduce the default size of the RX window for TCP sockets.

  - CONFIG_LWIP_TCP_RECVMBOX_SIZE: reduce the size of the TCP receive mailbox. Receive mailbox buffers data within active connections and handles data flow during connections。

  - CONFIG_LWIP_TCP_ACCEPTMBOX_SIZE: reduce the size of the TCP accept mailbox. Accept mailbox queues incoming connection requests and manages the initiation of new connections.

  - CONFIG_LWIP_UDP_RECVMBOX_SIZE: reduce the size of the UDP receive mailbox.

  - CONFIG_LWIP_TCPIP_RECVMBOX_SIZE: reduce the size of TCPIP task receive mailbox.

Note

As the coexistence configuration option relies on the presence of any two enabled modules, please ensure that both modules are activated before configuring any coexistence features.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.