Protocols
=========

:link_to_translation:`zh_CN:[中文]`

ESP HTTPS OTA
-------------

Breaking Changes (Summary)
~~~~~~~~~~~~~~~~~~~~~~~~~~

- If the image length is found in the HTTP header and :cpp:member:`esp_https_ota_config_t::bulk_flash_erase` is set to true, then instead of erasing the entire flash, the erase operation will be performed to accommodate the size of the image length.
