# ESP-NETIF Developer's manual

[中文]

As shown in the ESP-NETIF Architecture diagram, ESP-NETIF is in fact an intermediary between the I/O driver and the TCP/IP stack. This manual describes customization of these two sides, that is if you need to implement ESP-NETIF Custom I/O Driver or if you need to employ ESP-NETIF Custom TCP/IP Stack.

## ESP-NETIF Custom I/O Driver

This section outlines implementing a new I/O driver with ESP-NETIF connection capabilities.

By convention, the I/O driver has to register itself as an ESP-NETIF driver, and thus holds a dependency on ESP-NETIF component and is responsible for providing data path functions, post-attach callback and in most cases, also default event handlers to define network interface actions based on driver's lifecycle transitions.

### Packet Input/Output

According to the diagram shown in the ESP-NETIF Architecture part, the following three API functions for the packet data path must be defined for connecting with ESP-NETIF:

- `esp_netif_transmit()`

- `esp_netif_free_rx_buffer()`

- `esp_netif_receive()`

The first two functions for transmitting and freeing the rx buffer are provided as callbacks, i.e., they get called from ESP-NETIF (and its underlying TCP/IP stack) and I/O driver provides their implementation.

The receiving function on the other hand gets called from the I/O driver, so that the driver's code simply calls `esp_netif_receive()` on a new data received event.

### Post Attach Callback

A final part of the network interface initialization consists of attaching the ESP-NETIF instance to the I/O driver, by means of calling the following API:

    esp_err_t esp_netif_attach(esp_netif_t *esp_netif, esp_netif_iodriver_handle driver_handle);

It is assumed that the `esp_netif_iodriver_handle` is a pointer to driver's object, a struct derived from `struct esp_netif_driver_base_s`, so that the first member of I/O driver structure must be this base structure with pointers to:

- post-attach function callback

- related ESP-NETIF instance

As a result, the I/O driver has to create an instance of the struct per below:

    typedef struct my_netif_driver_s {
            esp_netif_driver_base_t base;           /*!< base structure reserved as esp-netif driver */
            driver_impl             *h;             /*!< handle of driver implementation */
        } my_netif_driver_t;

with actual values of `my_netif_driver_t::base.post_attach` and the actual drivers handle `my_netif_driver_t::h`.

So when the `esp_netif_attach()` gets called from the initialization code, the post-attach callback from I/O driver's code gets executed to mutually register callbacks between ESP-NETIF and I/O driver instances. Typically the driver is started as well in the post-attach callback. An example of a simple post-attach callback is outlined below:

    static esp_err_t my_post_attach_start(esp_netif_t * esp_netif, void * args)
    {
        my_netif_driver_t *driver = args;
        const esp_netif_driver_ifconfig_t driver_ifconfig = {
                .driver_free_rx_buffer = my_free_rx_buf,
                .transmit = my_transmit,
                .handle = driver->driver_impl
        };
        driver->base.netif = esp_netif;
        ESP_ERROR_CHECK(esp_netif_set_driver_config(esp_netif, &driver_ifconfig));
        my_driver_start(driver->driver_impl);
        return ESP_OK;
    }

### Default Handlers

I/O drivers also typically provide default definitions of lifecycle behavior of related network interfaces based on state transitions of I/O drivers. For example driver start `->` network start, etc.

An example of such a default handler is provided below:

    esp_err_t my_driver_netif_set_default_handlers(my_netif_driver_t *driver, esp_netif_t * esp_netif)
    {
        driver_set_event_handler(driver->driver_impl, esp_netif_action_start, MY_DRV_EVENT_START, esp_netif);
        driver_set_event_handler(driver->driver_impl, esp_netif_action_stop, MY_DRV_EVENT_STOP, esp_netif);
        return ESP_OK;
    }

## Network Stack Connection

The packet data path functions for transmitting and freeing the rx buffer (defined in the I/O driver) are called from the ESP-NETIF, specifically from its TCP/IP stack connecting layer.

Note that ESP-IDF provides several network stack configurations for the most common network interfaces, such as for the Wi-Fi station or Ethernet. These configurations are defined in esp_netif/include/esp_netif_defaults.h and should be sufficient for most network drivers.

In some cases, you might want to define a custom lwIP based interface, for example if you need to update esp_netif/lwip/netif/wlanif.c with a specific packet pool. In that case, you would have to define an explicit dependency to lwIP and include esp_netif/include/lwip/esp_netif_net_stack.h for the relevant lwIP configuration structures.

## ESP-NETIF Custom TCP/IP Stack

It is possible to use a custom TCP/IP stack with ESP-IDF, provided it implements BSD API. You can add support for your own TCP/IP stack, while using the generic ESP-NETIF functionality, so the application code can stay the same as with the lwIP.

In this case, please choose `ESP_NETIF_PROVIDE_CUSTOM_IMPLEMENTATION` in the ESP-NETIF component configuration menu. This option will disable lwIP implementation of the ESP-NETIF functions and provide only header files with declarations of types and API. You will have to supply the necessary implementation in your custom component. You can refer to the esp_netif/loopback/esp_netif_loopback.c for example of dummy implementations of these functions.

It is also possible to build ESP-IDF without lwIP, please refer to components/esp_netif_stack/README.md.

## API Reference

The following API reference outlines these network stack interaction with the ESP-NETIF:

### Header File

- components/esp_netif/include/esp_netif_net_stack.h

- This header file can be included with:

  >     #include "esp_netif_net_stack.h"

- This header file is a part of the API provided by the `esp_netif` component. To declare that your component depends on `esp_netif`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_netif

  > or

  >     PRIV_REQUIRES esp_netif

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.