# Wi-Fi

This document outlines the Wi-Fi related breaking changes in release v6.0.

## Removed Functions and Types

The following functions and types have been removed.

- DPP:

    - The DPP event callback `esp_supp_dpp_event_cb_t` and event enum `esp_supp_dpp_event_t` have been removed. Please use Wi-Fi events directly (e.g. `WIFI_EVENT_DPP_URI_READY`, `WIFI_EVENT_DPP_CFG_RECVD`, `WIFI_EVENT_DPP_FAILED`).

- RRM: The function `esp_rrm_send_neighbor_rep_request` has been removed. Use `esp_rrm_send_neighbor_report_request` instead.

- Antenna Configuration:

    - The functions `esp_wifi_set_ant_gpio`, `esp_wifi_get_ant_gpio`, `esp_wifi_set_ant`, and `esp_wifi_get_ant` have been removed. Please use the equivalent functions from `esp_phy` component: `esp_phy_set_ant_gpio`, `esp_phy_get_ant_gpio`, `esp_phy_set_ant`, and `esp_phy_get_ant`.

- ESP-NOW: The function `esp_wifi_config_espnow_rate` has been removed. Use `esp_now_set_peer_rate_config` instead.

## Removed Variables, Macros and Enum Values

- Authentication Modes: The authentication modes `WIFI_AUTH_WPA3_EXT_PSK` and `WIFI_AUTH_WPA3_EXT_PSK_MIXED_MODE` have been removed. Use `WIFI_AUTH_WPA3_PSK` instead.

- Neighbor Report Event: In the `wifi_event_neighbor_report_t` structure, the `report` field has been removed. Please use the `n_report` field instead, which is a flexible array member.

- Wi-Fi Interface: The header file `components/esp_wifi/include/esp_interface.h` has been removed. The `wifi_interface_t` enum is now defined in components/esp_wifi/include/esp_wifi_types_generic.h. The enum values (e.g. `WIFI_IF_STA`, `WIFI_IF_AP`) are no longer defined based on `ESP_IF_WIFI_STA`, `ESP_IF_WIFI_AP`, etc.

- Wi-Fi Interface Macros: The macros `ESP_IF_WIFI_STA` and `ESP_IF_WIFI_AP` have been removed. Please use the enum values `WIFI_IF_STA` and `WIFI_IF_AP` directly.

- Wi-Fi Disconnection Reasons: The disconnection reason codes `WIFI_REASON_ASSOC_EXPIRE`, `WIFI_REASON_NOT_AUTHED`, and `WIFI_REASON_NOT_ASSOCED` have been removed. Please use `WIFI_REASON_AUTH_EXPIRE`, `WIFI_REASON_CLASS2_FRAME_FROM_NONAUTH_STA`, and `WIFI_REASON_CLASS3_FRAME_FROM_NONASSOC_STA` respectively.

- NAN:

    - Field `svc_info` from structures `wifi_nan_publish_cfg_t`, `wifi_nan_subscribe_cfg_t`, `wifi_nan_followup_params_t`, `wifi_event_ndp_indication_t`, `wifi_event_ndp_confirm_t` has been removed. Please use the equivalent fields `ssi` and `ssi_len` instead.

    - Field `peer_svc_info` from structure `wifi_event_nan_receive_t` has been removed. Please use the equivalent fields `ssi` and `ssi_len` instead.

- FTM: Field `use_get_report_api` from structure `wifi_ftm_initiator_cfg_t` and field `ftm_report_data` from structure `wifi_event_ftm_report_t` has been removed. Please use `esp_wifi_ftm_get_report` to fetch raw FTM report data instead.

## Modified Functions and Types

The following Wi-Fi functions have been modified.

- DPP: The function `esp_supp_dpp_init` no longer accepts a callback and should be called as `esp_supp_dpp_init(void)`.

- WPS: The function `esp_wifi_wps_start` no longer accepts a `timeout_ms` argument. It should now be called as `esp_wifi_wps_start(void)`.

- NAN:
    - NAN API's are modified so that they can be shared between two separate NAN modes of operation called NAN Synchronization (NAN-Sync) and NAN Unsynchronized Discovery (NAN-USD) roles:

        - `esp_wifi_nan_sync_start` and `esp_wifi_nan_sync_stop` replace the previous `esp_wifi_nan_start` / `esp_wifi_nan_stop` pair.

        - Functions starting with prefix `esp_wifi_nan_*` are shared by both NAN-Sync and NAN-USD modes (for example `esp_wifi_nan_publish_service` and `esp_wifi_nan_subscribe_service`).

        - Use `WIFI_NAN_SYNC_CONFIG_DEFAULT()` instead of the former `WIFI_NAN_CONFIG_DEFAULT()` macro when initialising synchronized NAN configuration.

        - The structure `wifi_nan_config_t` has been renamed to `wifi_nan_sync_config_t`; update declarations such as `wifi_config_t.nan` to use the new type.

        - NAN datapath APIs and associated structures are valid for NAN Synchronization (NAN-Sync) clusters only.

    - Wi-Fi events `WIFI_EVENT_NAN_STARTED` / `WIFI_EVENT_NAN_STOPPED` have been renamed to `WIFI_EVENT_NAN_SYNC_STARTED` / `WIFI_EVENT_NAN_SYNC_STOPPED`.

    - The function argument `ndp_resp_needed` of `esp_wifi_nan_publish_service` has been moved to structure `wifi_nan_publish_cfg_t`.

    - The structure `wifi_nan_wfa_ssi_t` now declares its `proto` field as `uint8_t` (previously `wifi_nan_svc_proto_t`). Update code that stores pointers to this field or relies on its size to treat it as a single octet.

    - The structures `wifi_nan_publish_cfg_t` and `wifi_nan_subscribe_cfg_t` now include a `usd_discovery_flag` bitfield together with corresponding `wifi_nan_usd_config_t` members. Add designated initialisers for these fields when constructing the structures to avoid accidental field shifts.

- Off-Channel Operations:

    - The structure `wifi_action_tx_req_t` now includes a `bssid` field that is placed in Address3 of the transmitted action frame. Initialise this field explicitly; leaving it all zeros retains the previous behaviour where the Wi-Fi driver inserts the broadcast address, so frames do not carry unintended BSSID values.

    - The structure `wifi_roc_req_t` now includes an `allow_broadcast` flag that controls whether broadcast and multicast action frames are passed to the `rx_cb` callback during remain-on-channel operations. Existing applications should review the default `false` value and enable it when discovery of broadcast peers is required. Frames whose Address3/BSSID is already broadcast continue to reach the callback even when `allow_broadcast` remains `false`.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.