# SPI Master Driver

[中文]

SPI Master driver is a program that controls ESP32-C2's General Purpose SPI (GP-SPI) peripheral(s) when it functions as a master.

For more hardware information about the GP-SPI peripheral(s), see ESP32-C2 Technical Reference Manual > SPI Controller [PDF].

## Terminology

The terms used in relation to the SPI Master driver are given in the table below.

Term | Definition
--- | ---
Host | The SPI controller peripheral inside ESP32-C2 initiates SPI transmissions over the bus and acts as an SPI Master.
Device | SPI slave Device. An SPI bus may be connected to one or more Devices. Each Device shares the MOSI, MISO, and SCLK signals but is only active on the bus when the Host asserts the Device's individual CS line.
Bus | A signal bus, common to all Devices connected to one Host. In general, a bus includes the following lines: MISO, MOSI, SCLK, one or more CS lines, and, optionally, QUADWP and QUADHD. So Devices are connected to the same lines, with the exception that each Device has its own CS line. Several Devices can also share one CS line if connected in a daisy-chain manner.
MOSI | Master Out, Slave In, a.k.a. D. Data transmission from a Host to Device. Also data0 signal in Octal/OPI mode.
MISO | Master In, Slave Out, a.k.a. Q. Data transmission from a Device to Host. Also data1 signal in Octal/OPI mode.
SCLK | Serial Clock. The oscillating signal generated by a Host keeps the transmission of data bits in sync.
CS | Chip Select. Allows a Host to select individual Device(s) connected to the bus in order to send or receive data.
QUADWP | Write Protect signal. Used for 4-bit (qio/qout) transactions. Also for the data2 signal in Octal/OPI mode.
QUADHD | Hold signal. Used for 4-bit (qio/qout) transactions. Also for the data3 signal in Octal/OPI mode.
DATA4 | Data4 signal in Octal/OPI mode.
DATA5 | Data5 signal in Octal/OPI mode.
DATA6 | Data6 signal in Octal/OPI mode.
DATA7 | Data7 signal in Octal/OPI mode.
Assertion | The action of activating a line.
De-assertion | The action of returning the line back to inactive (back to idle) status.
Transaction | One instance of a Host asserting a CS line, transferring data to and from a Device, and de-asserting the CS line. Transactions are atomic, which means they can never be interrupted by another transaction.
Launch Edge | Edge of the clock at which the source register launches the signal onto the line.
Latch Edge | Edge of the clock at which the destination register latches in the signal.

## Driver Features

The SPI Master driver governs the communications between Hosts and Devices. The driver supports the following features:

- Multi-threaded environments

- Transparent handling of DMA transfers while reading and writing data

- Automatic time-division multiplexing of data coming from different Devices on the same signal bus, see SPI Bus Lock.

Warning

The SPI Master driver allows multiple Devices to be connected on a same SPI bus (sharing a single ESP32-C2 SPI peripheral). As long as each Device is accessed by only one task, the driver is thread-safe. However, if multiple tasks try to access the same SPI Device, the driver is not thread-safe. In this case, it is recommended to either:

- Refactor your application so that each SPI peripheral is only accessed by a single task at a time. You can use `spi_bus_config_t::isr_cpu_id` to register the SPI ISR to the same core as SPI peripheral-related tasks to ensure thread safety.

- Add a mutex lock around the shared Device using `xSemaphoreCreateMutex`.

## SPI Transactions

An SPI bus transaction consists of five phases which can be found in the table below. Any of these phases can be skipped.

Phase | Description
--- | ---
Command | In this phase, a command (0-16 bit) is written to the bus by the Host.
Address | In this phase, an address (0-32 bit) is transmitted over the bus by the Host.
Dummy | This phase is configurable and is used to meet the timing requirements.
Write | Host sends data to a Device. This data follows the optional command and address phases and is indistinguishable from them at the electrical level.
Read | Device sends data to its Host.

The attributes of a transaction are determined by the bus configuration structure `spi_bus_config_t`, Device configuration structure `spi_device_interface_config_t`, and transaction configuration structure `spi_transaction_t`.

An SPI Host can send full-duplex transactions, during which the Read and Write phases occur simultaneously. The total transaction length is determined by the sum of the following members:

- `spi_device_interface_config_t::command_bits`

- `spi_device_interface_config_t::address_bits`

- `spi_transaction_t::length`

While the member `spi_transaction_t::rxlength` only determines the length of data received into the buffer.

In half-duplex transactions, the Read and Write phases are not simultaneous (one direction at a time). The lengths of the Write and Read phases are determined by `spi_transaction_t::length` and `spi_transaction_t::rxlength` respectively.

The Command and Address phases are optional, as not every SPI Device requires a command and/or address. This is reflected in the Device's configuration: if `spi_device_interface_config_t::command_bits` and/or `spi_device_interface_config_t::address_bits` are set to zero, no Command or Address phase will occur.

The Read and Write phases can also be optional, as not every transaction requires both writing and reading data. If `spi_transaction_t::rx_buffer` is `NULL` and `SPI_TRANS_USE_RXDATA` is not set, the Read phase is skipped. If `spi_transaction_t::tx_buffer` is `NULL` and `SPI_TRANS_USE_TXDATA` is not set, the Write phase is skipped.

The driver supports two types of transactions: interrupt transactions and polling transactions. The programmer can choose to use a different transaction type per Device. If your Device requires both transaction types, see Notes on Sending Mixed Transactions to the Same Device.

### Interrupt Transactions

Interrupt transactions blocks the transaction routine until the transaction completes, thus allowing the CPU to run other tasks.

An application task can queue multiple transactions, and the driver automatically handles them one by one in the interrupt service routine (ISR). It allows the task to switch to other procedures until all the transactions are complete.

### Polling Transactions

Polling transactions do not use interrupts. The routine keeps polling the SPI Host's status bit until the transaction is finished.

All the tasks that use interrupt transactions can be blocked by the queue. At this point, they need to wait for the ISR to run twice before the transaction is finished. Polling transactions save time otherwise spent on queue handling and context switching, which results in smaller transaction duration. The disadvantage is that the CPU is busy while these transactions are in progress.

The `spi_device_polling_end()` routine needs an overhead of at least 1 µs to unblock other tasks when the transaction is finished. It is strongly recommended to wrap a series of polling transactions using the functions `spi_device_acquire_bus()` and `spi_device_release_bus()` to avoid the overhead. For more information, see Bus Acquiring.

### Transaction Line Mode

Supported line modes for ESP32-C2 are listed as follows, to make use of these modes, set the member `flags` in the struct `spi_transaction_t` as shown in the `Transaction Flag` column. If you want to check if corresponding IO pins are set or not, set the member `flags` in the `spi_bus_config_t` as shown in the `Bus IO setting Flag` column.

Mode name | Command Line Width | Address Line Width | Data Line Width | Transaction Flag | Bus IO Setting Flag
--- | --- | --- | --- | --- | ---
Normal SPI | 1 | 1 | 1 | 0 | 0
Dual Output | 1 | 1 | 2 | SPI_TRANS_MODE_DIO | SPICOMMON_BUSFLAG_DUAL
Dual I/O | 1 | 2 | 2 | SPI_TRANS_MODE_DIO SPI_TRANS_MULTILINE_ADDR | SPICOMMON_BUSFLAG_DUAL
Quad Output | 1 | 1 | 4 | SPI_TRANS_MODE_QIO | SPICOMMON_BUSFLAG_QUAD
Quad I/O | 1 | 4 | 4 | SPI_TRANS_MODE_QIO SPI_TRANS_MULTILINE_ADDR | SPICOMMON_BUSFLAG_QUAD

### Command and Address Phases

During the Command and Address phases, the members `spi_transaction_t::cmd` and `spi_transaction_t::addr` are sent to the bus, nothing is read at this time. The default lengths of the Command and Address phases are set in `spi_device_interface_config_t` by calling `spi_bus_add_device()`. If the flags `SPI_TRANS_VARIABLE_CMD` and `SPI_TRANS_VARIABLE_ADDR` in the member `spi_transaction_t::flags` are not set, the driver automatically sets the length of these phases to default values during Device initialization.

If the lengths of the Command and Address phases need to be variable, declare the struct `spi_transaction_ext_t`, set the flags `SPI_TRANS_VARIABLE_CMD` and/or `SPI_TRANS_VARIABLE_ADDR` in the member `spi_transaction_ext_t::base` and configure the rest of base as usual. Then the length of each phase will be equal to `spi_transaction_ext_t::command_bits` and `spi_transaction_ext_t::address_bits` set in the struct `spi_transaction_ext_t`.

If the Command and Address phase need to have the same number of lines as the data phase, you need to set `SPI_TRANS_MULTILINE_CMD` and/or `SPI_TRANS_MULTILINE_ADDR` to the `flags` member in the struct `spi_transaction_t`. Also see Transaction Line Mode.

### Write and Read Phases

Normally, the data that needs to be transferred to or from a Device is read from or written to a chunk of memory indicated by the members `spi_transaction_t::rx_buffer` and `spi_transaction_t::tx_buffer`. If DMA is enabled for transfers, the buffers are required to be:

> 1. Allocated in DMA-capable internal memory (MALLOC_CAP_DMA), see DMA-Capable Memory.

> 2. 32-bit aligned (starting from a 32-bit boundary and having a length of multiples of 4 bytes).

If these requirements are not satisfied, the transaction efficiency will be affected due to the allocation and copying of temporary buffers.

If using more than one data line to transmit, please set `SPI_DEVICE_HALFDUPLEX` flag for the member `flags` in the struct `spi_device_interface_config_t`. And the member `flags` in the struct `spi_transaction_t` should be set as described in Transaction Line Mode.

Note

Half-duplex transactions with both Read and Write phases are not supported. Please use full duplex mode.

### Bus Acquiring

Sometimes you might want to send SPI transactions exclusively and continuously so that it takes as little time as possible. For this, you can use bus acquiring, which helps to suspend transactions (both polling or interrupt) to other Devices until the bus is released. To acquire and release a bus, use the functions `spi_device_acquire_bus()` and `spi_device_release_bus()`.

## Driver Usage

- Initialize an SPI bus by calling the function `spi_bus_initialize()`. Make sure to set the correct I/O pins in the struct `spi_bus_config_t`. Set the signals that are not needed to `-1`.

- Register a Device connected to the bus with the driver by calling the function `spi_bus_add_device()`. Make sure to configure any timing requirements the Device might need with the parameter `dev_config`. You should now have obtained the Device's handle which will be used when sending a transaction to it.

- To interact with the Device, fill one or more `spi_transaction_t` structs with any transaction parameters required. Then send the structs either using a polling transaction or an interrupt transaction:

  > - Interrupt

  >     Either queue all transactions by calling the function `spi_device_queue_trans()` and, at a later time, query the result using the function `spi_device_get_trans_result()`, or handle all requests synchronously by feeding them into `spi_device_transmit()`.

  > - Polling

  >     Call the function `spi_device_polling_transmit()` to send polling transactions. Alternatively, if you want to insert something in between, send the transactions by using `spi_device_polling_start()` and `spi_device_polling_end()`.

- (Optional) To perform back-to-back transactions with a Device, call the function `spi_device_acquire_bus()` before sending transactions and `spi_device_release_bus()` after the transactions have been sent.

- (Optional) To remove a certain Device from the bus, call `spi_bus_remove_device()` with the Device handle as an argument.

- (Optional) To remove the driver from the bus, make sure no more devices are attached and call `spi_bus_free()`.

The example code for the SPI Master driver can be found in the peripherals/spi_master directory of ESP-IDF examples.

### Transactions with Data Not Exceeding 32 Bits

When the transaction data size is equal to or less than 32 bits, it will be sub-optimal to allocate a buffer for the data. The data can be directly stored in the transaction struct instead. For transmitted data, it can be achieved by using the `spi_transaction_t::tx_data` member and setting the `SPI_TRANS_USE_TXDATA` flag on the transmission. For received data, use `spi_transaction_t::rx_data` and set `SPI_TRANS_USE_RXDATA`. In both cases, do not touch the `spi_transaction_t::tx_buffer` or `spi_transaction_t::rx_buffer` members, because they use the same memory locations as `spi_transaction_t::tx_data` and `spi_transaction_t::rx_data`.

### Transactions with Integers Other than `uint8_t`

An SPI Host reads and writes data into memory byte by byte. By default, data is sent with the most significant bit (MSB) first, as LSB is first used in rare cases. If a value of fewer than 8 bits needs to be sent, the bits should be written into memory in the MSB first manner.

For example, if `0b00010` needs to be sent, it should be written into a `uint8_t` variable, and the length for reading should be set to 5 bits. The Device will still receive 8 bits with 3 additional "random" bits, so the reading must be performed correctly.

Not all chips support data transmission with any bit lengths. Sending or receiving unsupported bit lengths will return `ESP_ERR_NOT_SUPPORTED` error. The supported lengths are shown in the table below (YES means support any bits length, NO means bytes (8 bits) only):

| ESP32 | ESP32-S2 | ESP32-S3/C2/C3/C6 | ESP32-H2/P4/C5/C61
--- | --- | --- | --- | ---
TX | DMA | YES | YES | (bit_len % 8) != 1 | YES
NO DMA | YES | YES | (bit_len % 8) != 1 | YES
RX | DMA | NO | NO | YES | YES
NO DMA | YES | NO | YES | YES

If you still need to use unsupported bit lengths, you can use the following alternatives:

1. Use `spi_transaction_t::cmd` and `spi_transaction_t::addr` and data phase combination. The drawback is that the command and address phases do not receive data from the slave device.

2. Use two supported length transmissions combination, like `2+7` to implement `9 bit` transmission, while keeping the CS line valid. The drawback is that there is a minimum time interval between two transmissions (see Transaction Duration), and the overall transfer rate is lower.

On top of that, ESP32-C2 is a little-endian chip, which means that the least significant byte of `uint16_t` and `uint32_t` variables is stored at the smallest address. Hence, if `uint16_t` is stored in memory, bits [7:0] are sent first, followed by bits [15:8].

For cases when the data to be transmitted has a size differing from `uint8_t` arrays, the following macros can be used to transform data to the format that can be sent by the SPI driver directly:

- `SPI_SWAP_DATA_TX` for data to be transmitted

- `SPI_SWAP_DATA_RX` for data received

### Notes on Sending Mixed Transactions to the Same Device

To reduce coding complexity, send only one type of transaction (interrupt or polling) to one Device. However, you still can send both interrupt and polling transactions alternately. The notes below explain how to do this.

The polling transactions should be initiated only after all the polling and interrupt transactions are finished.

Since an unfinished polling transaction blocks other transactions, please do not forget to call the function `spi_device_polling_end()` after `spi_device_polling_start()` to allow other transactions or to allow other Devices to use the bus. Remember that if there is no need to switch to other tasks during your polling transaction, you can initiate a transaction with `spi_device_polling_transmit()` so that it will be ended automatically.

In-flight polling transactions are disturbed by the ISR operation to accommodate interrupt transactions. Always make sure that all the interrupt transactions sent to the ISR are finished before you call `spi_device_polling_start()`. To do that, you can keep calling `spi_device_get_trans_result()` until all the transactions are returned.

To have better control of the calling sequence of functions, send mixed transactions to the same Device only within a single task.

### GPIO Matrix and IO_MUX

Most of the chip's peripheral signals have a direct connection to their dedicated IO_MUX pins. However, the signals can also be routed to any other available pins using the less direct GPIO matrix. If at least one signal is routed through the GPIO matrix, then all signals will be routed through it.

When an SPI Host is set to 40 MHz or lower frequencies, routing SPI pins via the GPIO matrix will behave the same compared to routing them via IOMUX.

The IO_MUX pins for SPI buses are given below.

Pin Name | GPIO Number (SPI2)
--- | ---
CS0 [1] | 10
SCLK | 6
MISO | 2
MOSI | 7
QUADWP | 5
QUADHD | 4

[1]

Only the first Device attached to the bus can use the CS0 pin.

## Transfer Speed Considerations

There are three factors limiting the transfer speed:

- Transaction interval

- SPI clock frequency

- Cache miss of SPI functions, including callbacks

The main parameter that determines the transfer speed for large transactions is clock frequency. For multiple small transactions, the transfer speed is mostly determined by the length of transaction intervals.

### Transaction Duration

Transaction duration includes setting up SPI peripheral registers, copying data to FIFOs or setting up DMA links, and the time for SPI transactions.

Interrupt transactions allow appending extra overhead to accommodate the cost of FreeRTOS queues and the time needed for switching between tasks and the ISR.

For interrupt transactions, the CPU can switch to other tasks when a transaction is in progress. This saves CPU time but increases the transaction duration. See Interrupt Transactions. For polling transactions, it does not block the task but allows to do polling when the transaction is in progress. For more information, see Polling Transactions.

If DMA is enabled, setting up the linked list requires about 2 µs per transaction. When a master is transferring data, it automatically reads the data from the linked list. If DMA is not enabled, the CPU has to write and read each byte from the FIFO by itself. Usually, this is faster than 2 µs, but the transaction length is limited to 64 bytes for both write and read.

The typical transaction duration for one byte of data is given below.

- Interrupt Transaction via DMA: 42 µs.

- Interrupt Transaction via CPU: 40 µs.

- Polling Transaction via DMA: 17 µs.

- Polling Transaction via CPU: 15 µs.

Note that these data are tested with CONFIG_SPI_MASTER_ISR_IN_IRAM enabled. SPI transaction related code are placed in the internal memory. If this option is turned off (for example, for internal memory optimization), the transaction duration may be affected.

### SPI Clock Frequency

The clock source of the GPSPI peripherals can be selected by setting `spi_device_interface_config_t::clock_source`. You can refer to `spi_clock_source_t` to know the supported clock sources.

By default driver sets clock source to `SPI_CLK_SRC_DEFAULT`. This usually stands for the highest frequency among GPSPI supported clock sources. Its value is different among chips.

The actual clock frequency of a device may not be exactly equal to the number you set, it is re-calculated by the driver to the nearest hardware-compatible number, and no more than the frequency of selected clock source. You can call `spi_device_get_actual_freq()` to know the actual frequency computed by the driver.

The clock frequency of the device can be changed during transmission by setting `spi_transaction_t::override_freq_hz`. This operation will use new clock frequency for the device's current and later transmissions. If the expected clock frequency cannot be achieved, the driver will print an warning and continue to use the previous clock frequency for transmission.

The theoretical maximum transfer speed of the Write or Read phase can be calculated according to the table below:

Line Width of Write/Read phase | Speed (Bps)
--- | ---
1-Line | SPI Frequency / 8
2-Line | SPI Frequency / 4
4-Line | SPI Frequency / 2

The transfer speed calculation of other phases (Command, Address, Dummy) is similar.

### Cache Missing

The default config puts only the ISR into the IRAM. Other SPI-related functions, including the driver itself and the callback, might suffer from cache misses and need to wait until the code is read from flash. Select CONFIG_SPI_MASTER_IN_IRAM to put the whole SPI driver into IRAM and put the entire callback(s) and its callee functions into IRAM to prevent cache missing.

Note

SPI driver implementation is based on FreeRTOS APIs, to use CONFIG_SPI_MASTER_IN_IRAM, you should enable CONFIG_FREERTOS_IN_IRAM.

For an interrupt transaction, the overall cost is 20+8n/Fspi[MHz] [µs] for n bytes transferred in one transaction. Hence, the transferring speed is: n/(20+8n/Fspi). An example of transferring speed at 8 MHz clock speed is given in the following table.

Frequency (MHz) | Transaction Interval (µs) | Transaction Length (bytes) | Total Time (µs) | Total Speed (KBps)
--- | --- | --- | --- | ---
8 | 25 | 1 | 26 | 38.5
8 | 25 | 8 | 33 | 242.4
8 | 25 | 16 | 41 | 490.2
8 | 25 | 64 | 89 | 719.1
8 | 25 | 128 | 153 | 836.6

When a transaction length is short, the cost of the transaction interval is high. If possible, try to squash several short transactions into one transaction to achieve a higher transfer speed.

Please note that the ISR is disabled during flash operation by default. To keep sending transactions during flash operations, enable CONFIG_SPI_MASTER_ISR_IN_IRAM and set `ESP_INTR_FLAG_IRAM` in the member `spi_bus_config_t::intr_flags`. In this case, all the transactions queued before starting flash operations are handled by the ISR in parallel. Also note that the callback of each Device and their `callee` functions should be in IRAM, or your callback will crash due to cache missing. For more details, see IRAM-Safe Interrupt Handlers.

## Application Examples

- peripherals/spi_master/hd_eeprom demonstrates how to use the SPI master half duplex mode to read/write an AT93C46D EEPROM (8-bit mode) on ESP32-C2.

- peripherals/spi_master/lcd demonstrates how to use the SPI master driver to display an animation on the LCD. With the help of the DMA, we can do render and flush in parallel. This example also illustrates using the SPI transaction hook function to drive the D/C signal level.

## API Reference - SPI Common

### Header File

- components/esp_hal_gpspi/include/hal/spi_types.h

- This header file can be included with:

  >     #include "hal/spi_types.h"

- This header file is a part of the API provided by the `esp_hal_gpspi` component. To declare that your component depends on `esp_hal_gpspi`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_hal_gpspi

  > or

  >     PRIV_REQUIRES esp_hal_gpspi

### Structures

struct spi_line_mode_t

  Line mode of SPI transaction phases: CMD, ADDR, DOUT/DIN.

  Public Members

  uint8_t cmd_lines

    The line width of command phase, e.g. 2-line-cmd-phase.

  uint8_t addr_lines

    The line width of address phase, e.g. 1-line-addr-phase.

  uint8_t data_lines

    The line width of data phase, e.g. 4-line-data-phase.

### Type Definitions

typedef soc_periph_spi_clk_src_t spi_clock_source_t

  Type of SPI clock source.

### Enumerations

enum spi_host_device_t

  General purpose SPI Host Controller ID.

  Values:

  enumerator SPI1_HOST

    SPI1.

  enumerator SPI2_HOST

    SPI2.

  enumerator SPI_HOST_MAX

    invalid host value

enum spi_event_t

  SPI Events.

  Values:

  enumerator SPI_EV_BUF_TX

    The buffer has sent data to master.

  enumerator SPI_EV_BUF_RX

    The buffer has received data from master.

  enumerator SPI_EV_SEND_DMA_READY

    Slave has loaded its TX data buffer to the hardware (DMA).

  enumerator SPI_EV_SEND

    Master has received certain number of the data, the number is determined by Master.

  enumerator SPI_EV_RECV_DMA_READY

    Slave has loaded its RX data buffer to the hardware (DMA).

  enumerator SPI_EV_RECV

    Slave has received certain number of data from master, the number is determined by Master.

  enumerator SPI_EV_CMD9

    Received CMD9 from master.

  enumerator SPI_EV_CMDA

    Received CMDA from master.

  enumerator SPI_EV_TRANS

    A transaction has done.

enum spi_command_t

  SPI command.

  Values:

  enumerator SPI_CMD_HD_WRBUF
  enumerator SPI_CMD_HD_RDBUF
  enumerator SPI_CMD_HD_WRDMA
  enumerator SPI_CMD_HD_RDDMA
  enumerator SPI_CMD_HD_SEG_END
  enumerator SPI_CMD_HD_EN_QPI
  enumerator SPI_CMD_HD_WR_END
  enumerator SPI_CMD_HD_INT0
  enumerator SPI_CMD_HD_INT1
  enumerator SPI_CMD_HD_INT2

enum spi_sampling_point_t

  SPI master RX sample point mode configuration.

  Values:

  enumerator SPI_SAMPLING_POINT_PHASE_0

    Data sampling point at 50% cycle delayed then standard timing, (default).

  enumerator SPI_SAMPLING_POINT_PHASE_1

    Data sampling point follows standard SPI timing in master mode.

### Header File

- components/esp_driver_spi/include/driver/spi_common.h

- This header file can be included with:

  >     #include "driver/spi_common.h"

- This header file is a part of the API provided by the `esp_driver_spi` component. To declare that your component depends on `esp_driver_spi`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_driver_spi

  > or

  >     PRIV_REQUIRES esp_driver_spi

### Functions

esp_err_t spi_bus_initialize(spi_host_device_t host_id, const spi_bus_config_t *bus_config, spi_dma_chan_t dma_chan)

  Initialize a SPI bus.

  Warning

  SPI0/1 is not supported

  Warning

  If a DMA channel is selected, any transmit and receive buffer used should be allocated in DMA-capable memory.

  Warning

  The ISR of SPI is always executed on the core which calls this function. Never starve the ISR on this core or the SPI transactions will not be handled.

  Parameters:

    - host_id -- SPI peripheral that controls this bus

    - bus_config -- Pointer to a spi_bus_config_t struct specifying how the host should be initialized

    - dma_chan -- - Selecting a DMA channel for an SPI bus allows transactions on the bus with size only limited by the amount of internal memory.

      - Selecting SPI_DMA_DISABLED limits the size of transactions.

      - Set to SPI_DMA_DISABLED if only the SPI flash uses this bus.

      - Set to SPI_DMA_CH_AUTO to let the driver to allocate the DMA channel.

  Returns:

    - ESP_ERR_INVALID_ARG if configuration is invalid

    - ESP_ERR_INVALID_STATE if host already is in use

    - ESP_ERR_NOT_FOUND if there is no available DMA channel

    - ESP_ERR_NO_MEM if out of memory

    - ESP_OK on success

esp_err_t spi_bus_free(spi_host_device_t host_id)

  Free a SPI bus.

  Warning

  In order for this to succeed, all devices have to be removed first.

  Parameters:

    host_id -- SPI peripheral to free

  Returns:

    - ESP_ERR_INVALID_ARG if parameter is invalid

    - ESP_ERR_INVALID_STATE if bus hasn't been initialized before, or not all devices on the bus are freed

    - ESP_OK on success

void *spi_bus_dma_memory_alloc(spi_host_device_t host_id, size_t size, uint32_t extra_heap_caps)

  Helper function for malloc DMA capable memory for SPI driver.

  Note

  Using this API AFTER spi_bus_initialize() is called, this API will take care of the cache and hardware alignment internally. To free/release memory allocated by this helper function, simply calling `free()`.

  Parameters:

    - host_id -- [in] SPI peripheral who will using the memory

    - size -- [in] Size in bytes, the amount of memory to allocate

    - extra_heap_caps -- [in] Extra heap caps based on MALLOC_CAP_DMA

  Returns:

    Pointer to the memory if allocated successfully

    - NULL If allocation failed or bus not initialized

### Structures

struct spi_bus_config_t

  This is a configuration structure for a SPI bus.

  You can use this structure to specify the GPIO pins of the bus. Normally, the driver will use the GPIO matrix to route the signals. An exception is made when all signals either can be routed through the IO_MUX or are -1. In that case, the IO_MUX is used. On ESP32, using GPIO matrix will bring about 25ns of input delay, which may cause incorrect read for >40MHz speeds.

  Note

  Be advised that the slave driver does not use the quadwp/quadhd lines and fields in spi_bus_config_t referring to these lines will be ignored and can thus safely be left uninitialized.

  Public Members

  int mosi_io_num

    [0] GPIO pin for Master Out Slave In (=spi_d) signal, or -1 if not used.

  int data0_io_num

    [0] GPIO pin for spi data0 signal in dual/quad/octal mode, or -1 if not used.

  int miso_io_num

    [1] GPIO pin for Master In Slave Out (=spi_q) signal, or -1 if not used.

  int data1_io_num

    [1] GPIO pin for spi data1 signal in dual/quad/octal mode, or -1 if not used.

  int sclk_io_num

    [2] GPIO pin for SPI Clock signal, or -1 if not used.

  int quadwp_io_num

    [3] GPIO pin for WP (Write Protect) signal, or -1 if not used.

  int data2_io_num

    [3] GPIO pin for spi data2 signal in quad/octal mode, or -1 if not used.

  int quadhd_io_num

    [4] GPIO pin for HD (Hold) signal, or -1 if not used.

  int data3_io_num

    [4] GPIO pin for spi data3 signal in quad/octal mode, or -1 if not used.

  int data4_io_num

    [5] GPIO pin for spi data4 signal in octal mode, or -1 if not used.

  int data5_io_num

    [6] GPIO pin for spi data5 signal in octal mode, or -1 if not used.

  int data6_io_num

    [7] GPIO pin for spi data6 signal in octal mode, or -1 if not used.

  int data7_io_num

    [8] GPIO pin for spi data7 signal in octal mode, or -1 if not used.

  int iocfg[9]

    GPIO config in array format follow the above order.

  bool data_io_default_level

    Output data IO default level when no transaction.

  int max_transfer_sz

    Maximum transfer size, in bytes. Defaults to 4092 if 0 when DMA enabled, or to `SOC_SPI_MAXIMUM_BUFFER_SIZE` if DMA is disabled.

  uint32_t flags

    Abilities of bus to be checked by the driver. Or-ed value of `SPICOMMON_BUSFLAG_*` flags.

  esp_intr_cpu_affinity_t isr_cpu_id

    Select cpu core to register SPI ISR.

  int intr_flags

    Interrupt flag for the bus to set the priority, and IRAM attribute, see `esp_intr_alloc.h`. Note that the EDGE, INTRDISABLED attribute are ignored by the driver. Note that if ESP_INTR_FLAG_IRAM is set, ALL the callbacks of the driver, and their callee functions, should be put in the IRAM.

### Macros

SPI_MAX_DMA_LEN

SPI_SWAP_DATA_TX(DATA, LEN)

  Transform unsigned integer of length <= 32 bits to the format which can be sent by the SPI driver directly.

  E.g. to send 9 bits of data, you can:

       uint16_t data = SPI_SWAP_DATA_TX(0x145, 9);

  Then points tx_buffer to `&data`.
  Parameters:

    - DATA -- Data to be sent, can be uint8_t, uint16_t or uint32_t.

    - LEN -- Length of data to be sent, since the SPI peripheral sends from the MSB, this helps to shift the data to the MSB.

SPI_SWAP_DATA_RX(DATA, LEN)

  Transform received data of length <= 32 bits to the format of an unsigned integer.

  E.g. to transform the data of 15 bits placed in a 4-byte array to integer:

       uint16_t data = SPI_SWAP_DATA_RX(*(uint32_t*)t->rx_data, 15);

  Parameters:

    - DATA -- Data to be rearranged, can be uint8_t, uint16_t or uint32_t.

    - LEN -- Length of data received, since the SPI peripheral writes from the MSB, this helps to shift the data to the LSB.

SPICOMMON_BUSFLAG_SLAVE

  Initialize I/O in slave mode.

SPICOMMON_BUSFLAG_MASTER

  Initialize I/O in master mode.

SPICOMMON_BUSFLAG_IOMUX_PINS

  Check using iomux pins. Or indicates the pins are configured through the IO mux rather than GPIO matrix.

SPICOMMON_BUSFLAG_GPIO_PINS

  Force the signals to be routed through GPIO matrix. Or indicates the pins are routed through the GPIO matrix.

SPICOMMON_BUSFLAG_SCLK

  Check existing of SCLK pin. Or indicates CLK line initialized.

SPICOMMON_BUSFLAG_MISO

  Check existing of MISO pin. Or indicates MISO line initialized.

SPICOMMON_BUSFLAG_MOSI

  Check existing of MOSI pin. Or indicates MOSI line initialized.

SPICOMMON_BUSFLAG_DUAL

  Check MOSI and MISO pins can output. Or indicates bus able to work under DIO mode.

SPICOMMON_BUSFLAG_WPHD

  Check existing of WP and HD pins. Or indicates WP & HD pins initialized.

SPICOMMON_BUSFLAG_QUAD

  Check existing of MOSI/MISO/WP/HD pins as output. Or indicates bus able to work under QIO mode.

SPICOMMON_BUSFLAG_IO4_IO7

  Check existing of IO4~IO7 pins. Or indicates IO4~IO7 pins initialized.

SPICOMMON_BUSFLAG_OCTAL

  Check existing of MOSI/MISO/WP/HD/SPIIO4/SPIIO5/SPIIO6/SPIIO7 pins as output. Or indicates bus able to work under octal mode.

SPICOMMON_BUSFLAG_NATIVE_PINS

SPICOMMON_BUSFLAG_SLP_ALLOW_PD

  Allow to power down the peripheral during light sleep, and auto recover then.

### Type Definitions

typedef spi_common_dma_t spi_dma_chan_t

### Enumerations

enum spi_common_dma_t

  SPI DMA channels.

  Values:

  enumerator SPI_DMA_DISABLED

    Do not enable DMA for SPI.

  enumerator SPI_DMA_CH_AUTO

    Enable DMA, channel is automatically selected by driver.

## API Reference - SPI Master

### Header File

- components/esp_driver_spi/include/driver/spi_master.h

- This header file can be included with:

  >     #include "driver/spi_master.h"

- This header file is a part of the API provided by the `esp_driver_spi` component. To declare that your component depends on `esp_driver_spi`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_driver_spi

  > or

  >     PRIV_REQUIRES esp_driver_spi

### Functions

esp_err_t spi_bus_add_device(spi_host_device_t host_id, const spi_device_interface_config_t *dev_config, spi_device_handle_t *handle)

  Allocate a device on a SPI bus.

  This initializes the internal structures for a device, plus allocates a CS pin on the indicated SPI master peripheral and routes it to the indicated GPIO. All SPI master devices have three CS pins and can thus control up to three devices.

  There's no notable delay on chips other than ESP32.

  Note

  On ESP32, due to the delay of GPIO matrix, the maximum frequency SPI Master can correctly samples the slave's output is lower than the case using IOMUX. Typical maximum frequency communicating with an ideal slave without data output delay: 80MHz (IOMUX pins) and 26MHz (GPIO matrix pins). With the help of extra dummy cycles in half-duplex mode, the delay can be compensated by setting `input_delay_ns` in `dev_config` structure correctly.

  Parameters:

    - host_id -- SPI peripheral to allocate device on

    - dev_config -- SPI interface protocol config for the device

    - handle -- Pointer to variable to hold the device handle

  Returns:

    - ESP_ERR_INVALID_ARG if parameter is invalid or configuration combination is not supported (e.g. `dev_config->post_cb` isn't set while flag `SPI_DEVICE_NO_RETURN_RESULT` is enabled)

    - ESP_ERR_INVALID_STATE if selected clock source is unavailable or spi bus not initialized

    - ESP_ERR_NOT_FOUND if host doesn't have any free CS slots

    - ESP_ERR_NO_MEM if out of memory

    - ESP_OK on success

esp_err_t spi_bus_remove_device(spi_device_handle_t handle)

  Remove a device from the SPI bus.

  Parameters:

    handle -- Device handle to free

  Returns:

    - ESP_ERR_INVALID_ARG if parameter is invalid

    - ESP_ERR_INVALID_STATE if device already is freed

    - ESP_OK on success

esp_err_t spi_device_queue_trans(spi_device_handle_t handle, spi_transaction_t *trans_desc, uint32_t ticks_to_wait)

  Queue a SPI transaction for interrupt transaction execution. Get the result by `spi_device_get_trans_result`.

  Note

  Normally a device cannot start (queue) polling and interrupt transactions simultaneously.

  Parameters:

    - handle -- Device handle obtained using spi_bus_add_device()

    - trans_desc -- Description of transaction to execute

    - ticks_to_wait -- Ticks to wait until there's room in the queue; use portMAX_DELAY to never time out.

  Returns:

    - ESP_ERR_INVALID_ARG if parameter is invalid. This can happen if SPI_TRANS_CS_KEEP_ACTIVE flag is specified while the bus was not acquired (`spi_device_acquire_bus()` should be called first) or set flag SPI_TRANS_DMA_BUFFER_ALIGN_MANUAL but tx or rx buffer not DMA-capable, or addr&len not align to cache line size

    - ESP_ERR_TIMEOUT if there was no room in the queue before ticks_to_wait expired

    - ESP_ERR_NO_MEM if allocating DMA-capable temporary buffer failed

    - ESP_ERR_INVALID_STATE if previous transactions are not finished

    - ESP_OK on success

esp_err_t spi_device_get_trans_result(spi_device_handle_t handle, spi_transaction_t **trans_desc, uint32_t ticks_to_wait)

  Get the result of a SPI transaction queued earlier by `spi_device_queue_trans`.

  This routine will wait until a transaction to the given device successfully completed. It will then return the description of the completed transaction so software can inspect the result and e.g. free the memory or reuse the buffers.

  Parameters:

    - handle -- Device handle obtained using spi_bus_add_device()

    - trans_desc -- Pointer to variable able to contain a pointer to the description of the transaction that is executed. The descriptor should not be modified until the descriptor is returned by spi_device_get_trans_result.

    - ticks_to_wait -- Ticks to wait until there's a returned item; use portMAX_DELAY to never time out.

  Returns:

    - ESP_ERR_INVALID_ARG if parameter is invalid

    - ESP_ERR_NOT_SUPPORTED if flag `SPI_DEVICE_NO_RETURN_RESULT` is set

    - ESP_ERR_TIMEOUT if there was no completed transaction before ticks_to_wait expired

    - ESP_OK on success

esp_err_t spi_device_transmit(spi_device_handle_t handle, spi_transaction_t *trans_desc)

  Send a SPI transaction, wait for it to complete, and return the result.

  This function is the equivalent of calling spi_device_queue_trans() followed by spi_device_get_trans_result(). Do not use this when there is still a transaction separately queued (started) from spi_device_queue_trans() or polling_start/transmit that hasn't been finalized.

  Note

  This function is not thread safe when multiple tasks access the same SPI device. Normally a device cannot start (queue) polling and interrupt transactions simutanuously.

  Parameters:

    - handle -- Device handle obtained using spi_bus_add_device()

    - trans_desc -- Description of transaction to execute

  Returns:

    - ESP_ERR_INVALID_ARG if parameter is invalid

    - ESP_OK on success

esp_err_t spi_device_polling_start(spi_device_handle_t handle, spi_transaction_t *trans_desc, uint32_t ticks_to_wait)

  Immediately start a polling transaction.

  Note

  Normally a device cannot start (queue) polling and interrupt transactions simutanuously. Moreover, a device cannot start a new polling transaction if another polling transaction is not finished.

  Parameters:

    - handle -- Device handle obtained using spi_bus_add_device()

    - trans_desc -- Description of transaction to execute

    - ticks_to_wait -- Ticks to wait until there's room in the queue; currently only portMAX_DELAY is supported.

  Returns:

    - ESP_ERR_INVALID_ARG if parameter is invalid. This can happen if SPI_TRANS_CS_KEEP_ACTIVE flag is specified while the bus was not acquired (`spi_device_acquire_bus()` should be called first) or set flag SPI_TRANS_DMA_BUFFER_ALIGN_MANUAL but tx or rx buffer not DMA-capable, or addr&len not align to cache line size

    - ESP_ERR_TIMEOUT if the device cannot get control of the bus before `ticks_to_wait` expired

    - ESP_ERR_NO_MEM if allocating DMA-capable temporary buffer failed

    - ESP_ERR_INVALID_STATE if previous transactions are not finished

    - ESP_OK on success

esp_err_t spi_device_polling_end(spi_device_handle_t handle, uint32_t ticks_to_wait)

  Poll until the polling transaction ends.

  This routine will not return until the transaction to the given device has successfully completed. The task is not blocked, but actively busy-spins for the transaction to be completed.

  Parameters:

    - handle -- Device handle obtained using spi_bus_add_device()

    - ticks_to_wait -- Ticks to wait until there's a returned item; use portMAX_DELAY to never time out.

  Returns:

    - ESP_ERR_INVALID_ARG if parameter is invalid

    - ESP_ERR_TIMEOUT if the transaction cannot finish before ticks_to_wait expired

    - ESP_OK on success

esp_err_t spi_device_polling_transmit(spi_device_handle_t handle, spi_transaction_t *trans_desc)

  Send a polling transaction, wait for it to complete, and return the result.

  This function is the equivalent of calling spi_device_polling_start() followed by spi_device_polling_end(). Do not use this when there is still a transaction that hasn't been finalized.

  Note

  This function is not thread safe when multiple tasks access the same SPI device. Normally a device cannot start (queue) polling and interrupt transactions simutanuously.

  Parameters:

    - handle -- Device handle obtained using spi_bus_add_device()

    - trans_desc -- Description of transaction to execute

  Returns:

    - ESP_ERR_INVALID_ARG if parameter is invalid

    - ESP_ERR_TIMEOUT if the device cannot get control of the bus

    - ESP_ERR_NO_MEM if allocating DMA-capable temporary buffer failed

    - ESP_ERR_INVALID_STATE if previous transactions of same device are not finished

    - ESP_OK on success

esp_err_t spi_device_acquire_bus(spi_device_handle_t device, uint32_t wait)

  Occupy the SPI bus for a device to do continuous transactions.

  Transactions to all other devices will be put off until `spi_device_release_bus` is called.

  Note

  The function will wait until all the existing transactions have been sent.

  Parameters:

    - device -- The device to occupy the bus.

    - wait -- Time to wait before the the bus is occupied by the device. Currently MUST set to portMAX_DELAY.

  Returns:

    - ESP_ERR_INVALID_ARG : `wait` is not set to portMAX_DELAY.

    - ESP_OK : Success.

void spi_device_release_bus(spi_device_handle_t dev)

  Release the SPI bus occupied by the device. All other devices can start sending transactions.

  Parameters:

    dev -- The device to release the bus.

esp_err_t spi_device_get_actual_freq(spi_device_handle_t handle, int *freq_khz)

  Calculate working frequency for specific device.

  Parameters:

    - handle -- SPI device handle

    - freq_khz -- [out] output parameter to hold calculated frequency in kHz

  Returns:

    - ESP_ERR_INVALID_ARG : `handle` or `freq_khz` parameter is NULL

    - ESP_OK : Success

int spi_get_actual_clock(int fapb, int hz, int duty_cycle)

  Calculate the working frequency that is most close to desired frequency.

  Parameters:

    - fapb -- The frequency of apb clock, should be `APB_CLK_FREQ`.

    - hz -- Desired working frequency

    - duty_cycle -- Duty cycle of the spi clock

  Returns:

    Actual working frequency that most fit.

void spi_get_timing(bool gpio_is_used, int input_delay_ns, int eff_clk, int *dummy_o, int *cycles_remain_o)

  Calculate the timing settings of specified frequency and settings.

  Note

  If **dummy_o* is not zero, it means dummy bits should be applied in half duplex mode, and full duplex mode may not work.

  Parameters:

    - gpio_is_used -- True if using GPIO matrix, or False if iomux pins are used.

    - input_delay_ns -- Input delay from SCLK launch edge to MISO data valid.

    - eff_clk -- Effective clock frequency (in Hz) from `spi_get_actual_clock()`.

    - dummy_o -- Address of dummy bits used output. Set to NULL if not needed.

    - cycles_remain_o -- Address of cycles remaining (after dummy bits are used) output.

      - -1 If too many cycles remaining, suggest to compensate half a clock.

      - 0 If no remaining cycles or dummy bits are not used.

      - positive value: cycles suggest to compensate.

int spi_get_freq_limit(bool gpio_is_used, int input_delay_ns)

  Get the frequency limit of current configurations. SPI master working at this limit is OK, while above the limit, full duplex mode and DMA will not work, and dummy bits will be applied in the half duplex mode.

  Parameters:

    - gpio_is_used -- True if using GPIO matrix, or False if native pins are used.

    - input_delay_ns -- Input delay from SCLK launch edge to MISO data valid.

  Returns:

    Frequency limit of current configurations.

esp_err_t spi_bus_get_max_transaction_len(spi_host_device_t host_id, size_t *max_bytes)

  Get max length (in bytes) of one transaction.

  Parameters:

    - host_id -- SPI peripheral

    - max_bytes -- [out] Max length of one transaction, in bytes

  Returns:

    - ESP_OK: On success

    - ESP_ERR_INVALID_ARG: Invalid argument

### Structures

struct spi_device_interface_config_t

  This is a configuration for a SPI slave device that is connected to one of the SPI buses.

  Public Members

  uint8_t command_bits

    Default amount of bits in command phase (0-16), used when `SPI_TRANS_VARIABLE_CMD` is not used, otherwise ignored.

  uint8_t address_bits

    Default amount of bits in address phase (0-64), used when `SPI_TRANS_VARIABLE_ADDR` is not used, otherwise ignored.

  uint8_t dummy_bits

    Amount of dummy bits to insert between address and data phase.

  uint8_t mode

    SPI mode, representing a pair of (CPOL, CPHA) configuration:

    - 0: (0, 0)

    - 1: (0, 1)

    - 2: (1, 0)

    - 3: (1, 1)

  spi_clock_source_t clock_source

    Select SPI clock source, `SPI_CLK_SRC_DEFAULT` by default.

  uint16_t duty_cycle_pos

    Duty cycle of positive clock, in 1/256th increments (128 = 50%/50% duty). Setting this to 0 (=not setting it) is equivalent to setting this to 128.

  uint16_t cs_ena_pretrans

    Amount of SPI bit-cycles the cs should be activated before the transmission (0-16). This only works on half-duplex transactions.

  uint8_t cs_ena_posttrans

    Amount of SPI bit-cycles the cs should stay active after the transmission (0-16)

  int clock_speed_hz

    SPI clock speed in Hz. Derived from `clock_source`.

  int input_delay_ns

    Maximum data valid time of slave. The time required between SCLK and MISO valid, including the possible clock delay from slave to master. The driver uses this value to give an extra delay before the MISO is ready on the line. Leave at 0 unless you know you need a delay. For better timing performance at high frequency (over 8MHz), it's suggest to have the right value.

  spi_sampling_point_t sample_point

    Sample point tuning of spi master receiving bit.

  int spics_io_num

    CS GPIO pin for this device, or -1 if not used.

  uint32_t flags

    Bitwise OR of SPI_DEVICE_* flags.

  int queue_size

    Transaction queue size. This sets how many transactions can be 'in the air' (queued using spi_device_queue_trans but not yet finished using spi_device_get_trans_result) at the same time.

  transaction_cb_t pre_cb

    Callback to be called before a transmission is started.

    This callback is called within interrupt context should be in IRAM for best performance, see "Transferring Speed" section in the SPI Master documentation for full details. If not, the callback may crash during flash operation when the driver is initialized with ESP_INTR_FLAG_IRAM.

  transaction_cb_t post_cb

    Callback to be called after a transmission has completed.

    This callback is called within interrupt context should be in IRAM for best performance, see "Transferring Speed" section in the SPI Master documentation for full details. If not, the callback may crash during flash operation when the driver is initialized with ESP_INTR_FLAG_IRAM.

struct spi_transaction_t

  This structure describes one SPI transaction. The descriptor should not be modified until the transaction finishes.

  Public Members

  uint32_t flags

    Bitwise OR of SPI_TRANS_* flags.

  uint16_t cmd

    Command data, of which the length is set in the `command_bits` of spi_device_interface_config_t.

    NOTE: this field, used to be "command" in ESP-IDF 2.1 and before, is re-written to be used in a new way in ESP-IDF 3.0.

    Example: write 0x0123 and command_bits=12 to send command 0x12, 0x3_ (in previous version, you may have to write 0x3_12).

  uint64_t addr

    Address data, of which the length is set in the `address_bits` of spi_device_interface_config_t.

    NOTE: this field, used to be "address" in ESP-IDF 2.1 and before, is re-written to be used in a new way in ESP-IDF3.0.

    Example: write 0x123400 and address_bits=24 to send address of 0x12, 0x34, 0x00 (in previous version, you may have to write 0x12340000).

  size_t length

    Total data length, in bits.

  size_t rxlength

    Total data length received, should be not greater than `length` in full-duplex mode (0 defaults this to the value of `length`).

  uint32_t override_freq_hz

    New freq speed value will override for current device, remain `0` to skip update. Need about 30us each time.

  void *user

    User-defined variable. Can be used to store eg transaction ID.

  const void *tx_buffer

    Pointer to transmit buffer, or NULL for no MOSI phase.

  uint8_t tx_data[4]

    If SPI_TRANS_USE_TXDATA is set, data set here is sent directly from this variable.

  void *rx_buffer

    Pointer to receive buffer, or NULL for no MISO phase. Written by 4 bytes-unit if DMA is used.

  uint8_t rx_data[4]

    If SPI_TRANS_USE_RXDATA is set, data is received directly to this variable.

struct spi_transaction_ext_t

  This struct is for SPI transactions which may change their address and command length. Please do set the flags in base to `SPI_TRANS_VARIABLE_CMD_ADR` to use the bit length here.

  Public Members

  struct spi_transaction_t base

    Transaction data, so that pointer to spi_transaction_t can be converted into spi_transaction_ext_t.

  uint8_t command_bits

    The command length in this transaction, in bits.

  uint8_t address_bits

    The address length in this transaction, in bits.

  uint8_t dummy_bits

    The dummy length in this transaction, in bits.

### Macros

SPI_MASTER_FREQ_8M

  SPI common used frequency (in Hz)

  Note

  SPI peripheral only has an integer divider, and the default clock source can be different on other targets, so the actual frequency may be slightly different from the desired frequency. 8MHz

SPI_MASTER_FREQ_9M

  8.89MHz

SPI_MASTER_FREQ_10M

  10MHz

SPI_MASTER_FREQ_11M

  11.43MHz

SPI_MASTER_FREQ_13M

  13.33MHz

SPI_MASTER_FREQ_16M

  16MHz

SPI_MASTER_FREQ_20M

  20MHz

SPI_MASTER_FREQ_26M

  26.67MHz

SPI_MASTER_FREQ_40M

  40MHz

SPI_MASTER_FREQ_80M

  80MHz

SPI_DEVICE_TXBIT_LSBFIRST

  Transmit command/address/data LSB first instead of the default MSB first.

SPI_DEVICE_RXBIT_LSBFIRST

  Receive data LSB first instead of the default MSB first.

SPI_DEVICE_BIT_LSBFIRST

  Transmit and receive LSB first.

SPI_DEVICE_3WIRE

  Use MOSI (=spid) for both sending and receiving data.

SPI_DEVICE_POSITIVE_CS

  Make CS positive during a transaction instead of negative.

SPI_DEVICE_HALFDUPLEX

  Transmit data before receiving it, instead of simultaneously.

SPI_DEVICE_CLK_AS_CS

  Output clock on CS line if CS is active.

SPI_DEVICE_NO_DUMMY

  There are timing issue when reading at high frequency (the frequency is related to whether iomux pins are used, valid time after slave sees the clock).

  - In half-duplex mode, the driver automatically inserts dummy bits before reading phase to fix the timing issue. Set this flag to disable this feature.

  - In full-duplex mode, however, the hardware cannot use dummy bits, so there is no way to prevent data being read from getting corrupted. Set this flag to confirm that you're going to work with output only, or read without dummy bits at your own risk.

SPI_DEVICE_DDRCLK

SPI_DEVICE_NO_RETURN_RESULT

  Don't return the descriptor to the host on completion (use post_cb to notify instead)

SPI_TRANS_MODE_DIO

  Transmit/receive data in 2-bit mode.

SPI_TRANS_MODE_QIO

  Transmit/receive data in 4-bit mode.

SPI_TRANS_USE_RXDATA

  Receive into rx_data member of spi_transaction_t instead into memory at rx_buffer.

SPI_TRANS_USE_TXDATA

  Transmit tx_data member of spi_transaction_t instead of data at tx_buffer. Do not set tx_buffer when using this.

SPI_TRANS_MODE_DIOQIO_ADDR

  Also transmit address in mode selected by SPI_MODE_DIO/SPI_MODE_QIO.

SPI_TRANS_VARIABLE_CMD

  Use the `command_bits` in `spi_transaction_ext_t` rather than default value in `spi_device_interface_config_t`.

SPI_TRANS_VARIABLE_ADDR

  Use the `address_bits` in `spi_transaction_ext_t` rather than default value in `spi_device_interface_config_t`.

SPI_TRANS_VARIABLE_DUMMY

  Use the `dummy_bits` in `spi_transaction_ext_t` rather than default value in `spi_device_interface_config_t`.

SPI_TRANS_CS_KEEP_ACTIVE

  Keep CS active after data transfer.

SPI_TRANS_MULTILINE_CMD

  The data lines used at command phase is the same as data phase (otherwise, only one data line is used at command phase)

SPI_TRANS_MODE_OCT

  Transmit/receive data in 8-bit mode.

SPI_TRANS_MULTILINE_ADDR

  The data lines used at address phase is the same as data phase (otherwise, only one data line is used at address phase)

SPI_TRANS_DMA_BUFFER_ALIGN_MANUAL

  By default driver will automatically re-alloc dma buffer if it doesn't meet hardware alignment or dma_capable requirements, this flag is for you to disable this feature, you will need to take care of the alignment otherwise driver will return you error ESP_ERR_INVALID_ARG.

SPI_TRANS_DMA_USE_PSRAM

  Use PSRAM for DMA buffer directly, has speed limit, but no temp buffer and save memory.

SPI_TRANS_DMA_RX_FAIL

  RX transaction data lose flag, indicate DMA RX overflow.

SPI_TRANS_DMA_TX_FAIL

  TX transaction data lose flag, indicate DMA TX underflow.

### Type Definitions

typedef void (*transaction_cb_t)(spi_transaction_t *trans)

typedef struct spi_device_t *spi_device_handle_t

  Handle for a device on a SPI bus.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.