# Event Task Matrix (ETM)

[中文]

## Introduction

Normally, if a peripheral X needs to notify peripheral Y of a particular event, this could only be done via a CPU interrupt from peripheral X, where the CPU notifies peripheral Y on behalf of peripheral X. However, in time-critical applications, the latency introduced by CPU interrupts is non-negligible.

With the help of the Event Task Matrix (ETM) module, some peripherals can directly notify other peripherals of events through pre-set connections without the intervention of CPU interrupts. This allows precise and low latency synchronization between peripherals, and lessens the CPU's workload as the CPU no longer needs to handle these events.

ETM channels Overview

The ETM module has multiple programmable channels, they are used to connect a particular Event to a particular Task. When an event is activated, the ETM channel will trigger the corresponding task automatically.

Peripherals that support ETM functionality provide their or unique set of events and tasks to be connected by the ETM. An ETM channel can connect any event to any task, even looping back an event to a task on the same peripheral. However, an ETM channel can only connect one event to one task at a time (i.e., 1 to 1 relation). If you want to use different events to trigger the same task, you can set up more ETM channels.

Typically, with the help of the ETM module, you can implement features like:

- Toggle the GPIO when a timer alarm event happens

- Start an ADC conversion when a pulse edge is detected on a GPIO

## Functional Overview

The following sections of this document cover the typical steps to configure and use the ETM module.

- ETM Channel Allocation - describes how to install and uninstall the ETM channel.

- ETM Event - describes how to allocate a new ETM event handle or fetch an existing handle from various peripherals.

- ETM Task - describes how to allocate a new ETM task handle or fetch an existing handle from various peripherals.

- ETM Channel Control - describes common ETM channel control functions.

- Power Management - describes the options and strategies provided by the driver in order to save power.

- Thread Safety - lists which APIs are guaranteed to be thread-safe by the driver.

- Kconfig Options - lists the supported Kconfig options that can be used to make a different effect on driver behavior.

### ETM Channel Allocation

There are many identical ETM channels in ESP32-C5 [1], and each channel is represented by `esp_etm_channel_handle_t` in the software. The ETM core driver manages all available hardware resources in a pool so that you do not need to care about which channel is in use and which is not. The ETM core driver will allocate a channel for you when you call `esp_etm_new_channel()` and delete it when you call `esp_etm_del_channel()`. All requirements needed for allocating a channel are provided in `esp_etm_channel_config_t`.

Before deleting an ETM channel, please disable it by `esp_etm_channel_disable()` in advance or make sure it has not been enabled yet by `esp_etm_channel_enable()`.

### ETM Event

ETM Event abstracts the event source, masking the details of specific event sources, and is represented by `esp_etm_event_handle_t` in the software, allowing applications to handle different types of events more easily. ETM events can be generated from a variety of peripherals, thus the way to get the event handle differs from peripherals. When an ETM event is no longer used, you should call `esp_etm_channel_connect()` with a `NULL` event handle to disconnect it and then call `esp_etm_del_event()` to free the event resource.

#### GPIO Events

GPIO edge event is the most common event type, it can be generated by any GPIO pin. You can call `gpio_new_etm_event()` to create a GPIO event handle, with the configurations provided in `gpio_etm_event_config_t`:

- `gpio_etm_event_config_t::edge` or `gpio_etm_event_config_t::edges` decides which edge(s) to trigger the event(s), supported edge types are listed in the `gpio_etm_event_edge_t`.

You need to build a connection between the GPIO ETM event handle and the GPIO number. So you should call `gpio_etm_event_bind_gpio()` afterwards. Please note, only the ETM event handle that created by `gpio_new_etm_event()` can set a GPIO number. Calling this function with other kinds of ETM events returns `ESP_ERR_INVALID_ARG` error. Needless to say, this function does not help with the GPIO initialization, you still need to call `gpio_config()` to set the property like direction, pull up/down mode separately.

#### Other Peripheral Events

- You can call `esp_systick_new_etm_alarm_event()` to get the ETM event from RTOS Systick, one per CPU core.

- Refer to ESP Timer (High Resolution Timer) for how to get the ETM event handle from esp_timer.

- Refer to GPTimer's ETM Events and Tasks for how to get the ETM event handle from GPTimer.

- Refer to Asynchronous Memory Copy for how to get the ETM event handle from async memcpy.

- Refer to Motor Control Pulse Width Modulator (MCPWM) for how to get the ETM event handle from MCPWM.

- Refer to Analog Comparator for how to get the ETM event handle from analog comparator.

- Refer to Inter-IC Sound (I2S) for how to get the ETM event handle from I2S.

- Refer to LED Control (LEDC) for how to get the ETM event handle from LEDC.

### ETM Task

ETM Task abstracts the task action and is represented by `esp_etm_task_handle_t` in the software, allowing tasks to be managed and represented in the same way. ETM tasks can be assigned to a variety of peripherals, thus the way to get the task handle differs from peripherals. When an ETM task is no longer used, you should call `esp_etm_channel_connect()` with a `NULL` task handle to disconnect it and then call `esp_etm_del_task()` to free the task resource.

#### GPIO Tasks

GPIO task is the most common task type. One GPIO can take one or more GPIO ETM task actions, and one GPIO ETM task action can even manage multiple GPIOs. When the task gets activated by the ETM channel, all managed GPIOs can set/clear/toggle at the same time. You can call `gpio_new_etm_task()` to create a GPIO task handle, with the configurations provided in `gpio_etm_task_config_t`:

- `gpio_etm_task_config_t::action` or `gpio_etm_task_config_t::actions` decides what GPIO action(s) would be taken by the ETM task. Supported actions are listed in the `gpio_etm_task_action_t`. If one GPIO needs to take more than one actions, the action tasks have to be created in one `gpio_new_etm_task()` call with filling the actions into the array of `gpio_etm_task_config_t::actions`.

To build a connection between the GPIO ETM task and the GPIO number, you should call `gpio_etm_task_add_gpio()`. You can call this function by several times if you want the task handle to manage more GPIOs. Please note, only the ETM task handle that created by `gpio_new_etm_task()` can manage a GPIO. Calling this function with other kinds of ETM tasks returns `ESP_ERR_INVALID_ARG` error. Needless to say, this function does not help with the GPIO initialization, you still need to call `gpio_config()` to set the property like direction, pull up/down mode separately.

Before you call `esp_etm_del_task()` to delete the GPIO ETM task, make sure that all previously added GPIOs are removed by `gpio_etm_task_rm_gpio()` in advance.

#### Other Peripheral Tasks

- Refer to GPTimer's ETM Events and Tasks for how to get the ETM task handle from GPTimer.

- Refer to Inter-IC Sound (I2S) for how to get the ETM task handle from I2S.

- Refer to LED Control (LEDC) for how to get the ETM task handle from LEDC.

### ETM Channel Control

#### Connect Event and Task

An ETM event has no association with an ETM task, until they are connected to the same ETM channel by calling `esp_etm_channel_connect()`. Especially, calling the function with a `NULL` task/event handle means disconnecting the channel from any task or event. Note that, this function can be called either before or after the channel is enabled. But calling this function at runtime to change the connection can be dangerous, because the channel may be in the middle of a cycle, and the new connection may not take effect immediately.

#### Enable and Disable Channel

You can call `esp_etm_channel_enable()` and `esp_etm_channel_disable()` to enable and disable the ETM channel from working.

#### ETM Channel Profiling

To check if the ETM channels are set with proper events and tasks, you can call `esp_etm_dump()` to dump all working ETM channels with their associated events and tasks. The dumping format is like:

    ===========ETM Dump Start==========
    channel 0: event 48 ==> task 17
    channel 1: event 48 ==> task 90
    channel 2: event 48 ==> task 94
    ===========ETM Dump End============

The digital ID printed in the dump information is defined in the `soc/soc_etm_source.h` file.

### Power Management

When power management is enabled, i.e., CONFIG_PM_ENABLE is on, the system may adjust or disable the clock source, and power off the ETM peripheral before going to sleep. As a result, the existing connection between events and tasks will be lost, and the ETM channels can't work correctly after wake up. So by default, the driver will acquire a power management lock internally to forbid the system from powering off the ETM peripheral.

If you want to save more power, you can set `esp_etm_channel_config_t::etm_chan_flags::allow_pd` to `true`. Then ETM registers will be backed up before sleep and restored after wake up. Please note, enabling this option will increase the memory consumption for saving the register context.

### Thread Safety

The ETM core driver is thread-safe.

- Factory functions (for example, `esp_etm_new_channel()`, `gpio_new_etm_task()`, and other `*_new_etm_*` creators) are thread-safe and can be called from different RTOS tasks concurrently.

- Channel control APIs (for example, `esp_etm_channel_connect()`, `esp_etm_channel_enable()`, `esp_etm_channel_disable()`, `esp_etm_del_channel()`) are also thread-safe. Concurrent operations on different channels are safe. Concurrent operations on the same channel are serialized internally; if an operation is incompatible with the current channel state, it will return `ESP_ERR_INVALID_STATE`.

- No functions are allowed to run within the ISR environment.

### Kconfig Options

- CONFIG_ETM_ENABLE_DEBUG_LOG is used to enable the debug log output. Enabling this option increases the firmware binary size as well.

## API Reference

### Header File

- components/esp_hw_support/etm/include/esp_etm.h

- This header file can be included with:

  >     #include "esp_etm.h"

### Functions

esp_err_t esp_etm_new_channel(const esp_etm_channel_config_t *config, esp_etm_channel_handle_t *ret_chan)

  Allocate an ETM channel.

  Note

  The channel can later be freed by `esp_etm_del_channel`

  Parameters:

    - config -- [in] ETM channel configuration

    - ret_chan -- [out] Returned ETM channel handle

  Returns:

    - ESP_OK: Allocate ETM channel successfully

    - ESP_ERR_INVALID_ARG: Allocate ETM channel failed because of invalid argument

    - ESP_ERR_NO_MEM: Allocate ETM channel failed because of out of memory

    - ESP_ERR_NOT_FOUND: Allocate ETM channel failed because all channels are used up and no more free one

    - ESP_FAIL: Allocate ETM channel failed because of other reasons

esp_err_t esp_etm_del_channel(esp_etm_channel_handle_t chan)

  Delete an ETM channel.

  Parameters:

    chan -- [in] ETM channel handle that created by `esp_etm_new_channel`

  Returns:

    - ESP_OK: Delete ETM channel successfully

    - ESP_ERR_INVALID_ARG: Delete ETM channel failed because of invalid argument

    - ESP_FAIL: Delete ETM channel failed because of other reasons

esp_err_t esp_etm_channel_enable(esp_etm_channel_handle_t chan)

  Enable ETM channel.

  Note

  This function will transit the channel state from init to enable.

  Parameters:

    chan -- [in] ETM channel handle that created by `esp_etm_new_channel`

  Returns:

    - ESP_OK: Enable ETM channel successfully

    - ESP_ERR_INVALID_ARG: Enable ETM channel failed because of invalid argument

    - ESP_ERR_INVALID_STATE: Enable ETM channel failed because the channel has been enabled already

    - ESP_FAIL: Enable ETM channel failed because of other reasons

esp_err_t esp_etm_channel_disable(esp_etm_channel_handle_t chan)

  Disable ETM channel.

  Note

  This function will transit the channel state from enable to init.

  Parameters:

    chan -- [in] ETM channel handle that created by `esp_etm_new_channel`

  Returns:

    - ESP_OK: Disable ETM channel successfully

    - ESP_ERR_INVALID_ARG: Disable ETM channel failed because of invalid argument

    - ESP_ERR_INVALID_STATE: Disable ETM channel failed because the channel is not enabled yet

    - ESP_FAIL: Disable ETM channel failed because of other reasons

esp_err_t esp_etm_channel_connect(esp_etm_channel_handle_t chan, esp_etm_event_handle_t event, esp_etm_task_handle_t task)

  Connect an ETM event to an ETM task via a previously allocated ETM channel.

  Note

  Setting the ETM event/task handle to NULL means to disconnect the channel from any event/task

  Parameters:

    - chan -- [in] ETM channel handle that created by `esp_etm_new_channel`

    - event -- [in] ETM event handle obtained from a driver/peripheral, e.g. `xxx_new_etm_event`

    - task -- [in] ETM task handle obtained from a driver/peripheral, e.g. `xxx_new_etm_task`

  Returns:

    - ESP_OK: Connect ETM event and task to the channel successfully

    - ESP_ERR_INVALID_ARG: Connect ETM event and task to the channel failed because of invalid argument

    - ESP_FAIL: Connect ETM event and task to the channel failed because of other reasons

esp_err_t esp_etm_del_event(esp_etm_event_handle_t event)

  Delete ETM event.

  Note

  Although the ETM event comes from various peripherals, we provide the same user API to delete the event handle seamlessly.

  Parameters:

    event -- [in] ETM event handle obtained from a driver/peripheral, e.g. `xxx_new_etm_event`

  Returns:

    - ESP_OK: Delete ETM event successfully

    - ESP_ERR_INVALID_ARG: Delete ETM event failed because of invalid argument

    - ESP_FAIL: Delete ETM event failed because of other reasons

esp_err_t esp_etm_del_task(esp_etm_task_handle_t task)

  Delete ETM task.

  Note

  Although the ETM task comes from various peripherals, we provide the same user API to delete the task handle seamlessly.

  Parameters:

    task -- [in] ETM task handle obtained from a driver/peripheral, e.g. `xxx_new_etm_task`

  Returns:

    - ESP_OK: Delete ETM task successfully

    - ESP_ERR_INVALID_ARG: Delete ETM task failed because of invalid argument

    - ESP_FAIL: Delete ETM task failed because of other reasons

esp_err_t esp_etm_dump(FILE *out_stream)

  Dump ETM channel usages to the given IO stream.

  Parameters:

    out_stream -- [in] IO stream (e.g. stdout)

  Returns:

    - ESP_OK: Dump ETM channel usages successfully

    - ESP_ERR_INVALID_ARG: Dump ETM channel usages failed because of invalid argument

    - ESP_FAIL: Dump ETM channel usages failed because of other reasons

### Structures

struct esp_etm_channel_config_t

  ETM channel configuration.

  Public Members

  struct esp_etm_channel_config_t::etm_chan_flags flags

    ETM channel flags

  struct etm_chan_flags

    Extra configuration flags for ETM channel.

    Public Members

    uint32_t allow_pd

      If set, driver allows the power domain to be powered off when system enters sleep mode. This can save power, but at the expense of more RAM being consumed to save register context.

### Type Definitions

typedef struct esp_etm_channel_t *esp_etm_channel_handle_t

  ETM channel handle.

typedef struct esp_etm_event_t *esp_etm_event_handle_t

  ETM event handle.

typedef struct esp_etm_task_t *esp_etm_task_handle_t

  ETM task handle.

### Header File

- components/esp_driver_gpio/include/driver/gpio_etm.h

- This header file can be included with:

  >     #include "driver/gpio_etm.h"

- This header file is a part of the API provided by the `esp_driver_gpio` component. To declare that your component depends on `esp_driver_gpio`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_driver_gpio

  > or

  >     PRIV_REQUIRES esp_driver_gpio

### Functions

esp_err_t gpio_new_etm_event(const gpio_etm_event_config_t *config, esp_etm_event_handle_t *ret_event, ...)

  Create an ETM event object for the GPIO peripheral.

  Note

  The created ETM event object can be deleted later by calling `esp_etm_del_event`

  Note

  The newly created ETM event object is not bind to any GPIO, you need to call `gpio_etm_event_bind_gpio` to bind the wanted GPIO

  Note

  Every success call to this function will acquire a free GPIO ETM event channel

  Parameters:

    - config -- [in] GPIO ETM event configuration

    - ret_event -- [out] Returned ETM event handle

    - ... -- [out] Other returned ETM event handles if any (the order of the returned event handles is aligned with the array order in field `edges` in `gpio_etm_event_config_t`)

  Returns:

    - ESP_OK: Create ETM event successfully

    - ESP_ERR_INVALID_ARG: Create ETM event failed because of invalid argument

    - ESP_ERR_NO_MEM: Create ETM event failed because of out of memory

    - ESP_ERR_NOT_FOUND: Create ETM event failed because all events are used up and no more free one

    - ESP_FAIL: Create ETM event failed because of other reasons

esp_err_t gpio_etm_event_bind_gpio(esp_etm_event_handle_t event, int gpio_num)

  Bind the GPIO with the ETM event.

  Note

  Calling this function multiple times with different GPIO number can override the previous setting immediately.

  Note

  Only GPIO ETM object can call this function

  Parameters:

    - event -- [in] ETM event handle that created by `gpio_new_etm_event`

    - gpio_num -- [in] GPIO number that can trigger the ETM event

  Returns:

    - ESP_OK: Set the GPIO for ETM event successfully

    - ESP_ERR_INVALID_ARG: Set the GPIO for ETM event failed because of invalid argument, e.g. GPIO is not input capable, ETM event is not of GPIO type

    - ESP_FAIL: Set the GPIO for ETM event failed because of other reasons

esp_err_t gpio_new_etm_task(const gpio_etm_task_config_t *config, esp_etm_task_handle_t *ret_task, ...)

  Create an ETM task object for the GPIO peripheral.

  Note

  The created ETM task object can be deleted later by calling `esp_etm_del_task`

  Note

  The GPIO ETM task works like a container, a newly created ETM task object doesn't have GPIO members to be managed. You need to call `gpio_etm_task_add_gpio` to put one or more GPIOs to the container.

  Note

  Every success call to this function will acquire a free GPIO ETM task channel

  Parameters:

    - config -- [in] GPIO ETM task configuration

    - ret_task -- [out] Returned ETM task handle

    - ... -- [out] Other returned ETM task handles if any (the order of the returned task handles is aligned with the array order in field `actions` in `gpio_etm_task_config_t`)

  Returns:

    - ESP_OK: Create ETM task successfully

    - ESP_ERR_INVALID_ARG: Create ETM task failed because of invalid argument

    - ESP_ERR_NO_MEM: Create ETM task failed because of out of memory

    - ESP_ERR_NOT_FOUND: Create ETM task failed because all tasks are used up and no more free one

    - ESP_FAIL: Create ETM task failed because of other reasons

esp_err_t gpio_etm_task_add_gpio(esp_etm_task_handle_t task, int gpio_num)

  Add GPIO to the ETM task.

  Note

  You can call this function multiple times to add more GPIOs

  Note

  Only GPIO ETM object can call this function

  Parameters:

    - task -- [in] ETM task handle that created by `gpio_new_etm_task`

    - gpio_num -- [in] GPIO number that can be controlled by the ETM task

  Returns:

    - ESP_OK: Add GPIO to the ETM task successfully

    - ESP_ERR_INVALID_ARG: Add GPIO to the ETM task failed because of invalid argument, e.g. GPIO is not output capable, ETM task is not of GPIO type

    - ESP_ERR_INVALID_STATE: Add GPIO to the ETM task failed because the GPIO is used by other ETM task already

    - ESP_FAIL: Add GPIO to the ETM task failed because of other reasons

esp_err_t gpio_etm_task_rm_gpio(esp_etm_task_handle_t task, int gpio_num)

  Remove the GPIO from the ETM task.

  Note

  Before deleting the ETM task, you need to remove all the GPIOs from the ETM task by this function

  Note

  Only GPIO ETM object can call this function

  Parameters:

    - task -- [in] ETM task handle that created by `gpio_new_etm_task`

    - gpio_num -- [in] GPIO number that to be remove from the ETM task

  Returns:

    - ESP_OK: Remove the GPIO from the ETM task successfully

    - ESP_ERR_INVALID_ARG: Remove the GPIO from the ETM task failed because of invalid argument

    - ESP_ERR_INVALID_STATE: Remove the GPIO from the ETM task failed because the GPIO is not controlled by this ETM task

    - ESP_FAIL: Remove the GPIO from the ETM task failed because of other reasons

### Structures

struct gpio_etm_event_config_t

  GPIO ETM event configuration.

  If more than one kind of ETM edge event want to be triggered on the same GPIO pin, you can configure them together. It helps to save GPIO ETM event channel resources for other GPIOs.

  Public Members

  gpio_etm_event_edge_t edge

    Which kind of edge can trigger the ETM event module

  gpio_etm_event_edge_t edges[GPIO_ETM_EVENT_EDGE_TYPES]

    Array of kinds of edges to trigger the ETM event module on the same GPIO

struct gpio_etm_task_config_t

  GPIO ETM task configuration.

  If multiple actions wants to be added to the same GPIO pin, you have to configure all the GPIO ETM tasks together.

  Public Members

  gpio_etm_task_action_t action

    Action to take by the ETM task module

  gpio_etm_task_action_t actions[GPIO_ETM_TASK_ACTION_TYPES]

    Array of actions to take by the ETM task module on the same GPIO

### Macros

GPIO_ETM_EVENT_EDGE_TYPES

  GPIO ETM edge events are POS/NEG/ANY

GPIO_ETM_TASK_ACTION_TYPES

  GPIO ETM action tasks are SET/CLEAR/TOGGLE

### Enumerations

enum gpio_etm_event_edge_t

  GPIO edges that can be used as ETM event.

  Values:

  enumerator GPIO_ETM_EVENT_EDGE_POS

    A rising edge on the GPIO will generate an ETM event signal

  enumerator GPIO_ETM_EVENT_EDGE_NEG

    A falling edge on the GPIO will generate an ETM event signal

  enumerator GPIO_ETM_EVENT_EDGE_ANY

    Any edge on the GPIO can generate an ETM event signal

enum gpio_etm_task_action_t

  GPIO actions that can be taken by the ETM task.

  Values:

  enumerator GPIO_ETM_TASK_ACTION_SET

    Set the GPIO level to high

  enumerator GPIO_ETM_TASK_ACTION_CLR

    Clear the GPIO level to low

  enumerator GPIO_ETM_TASK_ACTION_TOG

    Toggle the GPIO level

### Header File

- components/esp_system/include/esp_systick_etm.h

- This header file can be included with:

  >     #include "esp_systick_etm.h"

### Functions

esp_err_t esp_systick_new_etm_alarm_event(int core_id, esp_etm_event_handle_t *out_event)

  Get the ETM event handle of systick hardware's alarm/heartbeat event.

  Note

  The created ETM event object can be deleted later by calling `esp_etm_del_event`

  Parameters:

    - core_id -- [in] CPU core ID

    - out_event -- [out] Returned ETM event handle

  Returns:

    - ESP_OK Success

    - ESP_ERR_INVALID_ARG Parameter error

[1]

Different ESP chip series might have different numbers of ETM channels. For more details, please refer to ESP32-C5 Technical Reference Manual > Chapter Event Task Matrix (ETM) [PDF]. The driver does not forbid you from applying for more channels, but it will return an error when all available hardware resources are used up. Please always check the return value when doing channel allocation (i.e., `esp_etm_new_channel()`).

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.