# Digital Signature (DS)

[中文]

The Digital Signature (DS) module provides hardware acceleration of signing messages based on RSA. It uses pre-encrypted parameters to calculate a signature. The parameters are encrypted using HMAC as a key-derivation function. In turn, the HMAC uses eFuses as the input key.

On ESP32-C5, the Digital Signature (DS) module can also use a key stored in the Key Manager instead of an eFuse key block. The AES encryption key can be directly deployed in the Key Manager with the type `ESP_KEY_MGR_DS_KEY`. Refer to Key Manager for more details.

The whole process happens in hardware so that neither the decryption key for the RSA parameters nor the input key for the HMAC key derivation function can be seen by the software while calculating the signature.

For more detailed information on the hardware involved in the signature calculation and the registers used, see ESP32-C5 Technical Reference Manual > Digital Signature (DS) [PDF].

## Private Key Parameters

The private key parameters for the RSA signature are stored in flash. To prevent unauthorized access, they are AES-encrypted. The HMAC module is used as a key-derivation function to calculate the AES encryption key for the private key parameters. In turn, the HMAC module uses a key from the eFuses key block which can be read-protected to prevent unauthorized access as well.

Upon signature calculation invocation, the software only specifies which eFuse key to use, the corresponding eFuse key purpose, the location of the encrypted RSA parameters, and the message.

## Key Generation

Both the HMAC key and the RSA private key have to be created and stored before the DS peripheral can be used. This needs to be done in software on the ESP32-C5 or alternatively on a host. For this context, ESP-IDF provides `esp_efuse_write_block()` to set the HMAC key and `esp_hmac_calculate()` to encrypt the private RSA key parameters.

You can find instructions on how to calculate and assemble the private key parameters in ESP32-C5 Technical Reference Manual > Digital Signature (DS) [PDF].

## Signature Calculation with ESP-IDF

For more detailed information on the workflow and the registers used, see ESP32-C5 Technical Reference Manual > Digital Signature (DS) [PDF].

Three parameters need to be prepared to calculate the digital signature:

1. The eFuse key block ID which is used as the key for the HMAC

2. The location of the encrypted private key parameters

3. The message to be signed

Low-level API (plain RSA)

Since the signature calculation takes some time, there are two possible API versions to use in ESP-IDF. The first one is `esp_ds_sign()` and simply blocks until the calculation is finished. If software needs to do something else during the calculation, `esp_ds_start_sign()` can be called, followed by periodic calls to `esp_ds_is_busy()` to check when the calculation has finished. Once the calculation has finished, `esp_ds_finish_sign()` can be called to get the resulting signature.

The APIs `esp_ds_sign()` and `esp_ds_start_sign()` calculate a plain RSA signature with the help of the DS peripheral. This signature must be converted to an appropriate format (e.g., PKCS#1 v1.5 or PSS) for use in TLS or other protocols.

Note

This is only the basic DS building block; the message length is fixed. To create signatures of arbitrary messages, the input is normally a hash of the actual message, padded up to the required length.

PSA Crypto driver

The DS peripheral is also exposed via the PSA Crypto RSA DS driver, so you can use standard PSA APIs for signing (PKCS#1 v1.5 or PSS) and RSA decryption (PKCS#1 v1.5 or OAEP). Enable `CONFIG_MBEDTLS_HARDWARE_RSA_DS_PERIPHERAL` in `Component config` > `mbedTLS`. For using the DS peripheral with ESP-TLS (e.g. TLS client authentication), see Digital Signature with ESP-TLS in the ESP-TLS documentation.

## Configure the DS Peripheral for a TLS Connection

The DS peripheral on ESP32-C5 chip must be configured before it can be used for a TLS connection. The configuration involves the following steps:

1. Randomly generate a 256-bit value called the `Initialization Vector` (IV).

2. Randomly generate a 256-bit value called the `HMAC_KEY`.

3. Calculate the encrypted private key parameters from the client private key (RSA) and the parameters generated in the above steps.

4. Then burn the 256-bit `HMAC_KEY` on the eFuse, which can only be read by the DS peripheral.

For more details, see ESP32-C5 Technical Reference Manual > Digital Signature (DS) [PDF].

To configure the DS peripheral for development purposes, you can use the esp-secure-cert-tool.

The encrypted private key parameters obtained after the DS peripheral configuration should be stored in flash. The application needs to read the DS data from flash (e.g. through the APIs provided by the esp_secure_cert_mgr component; see the component/README for more details). For using the DS peripheral with ESP-TLS, see Digital Signature with ESP-TLS.

## Using DS with PSA Crypto

To use the DS peripheral for signing or decryption in application code (outside of ESP-TLS), enable `CONFIG_MBEDTLS_HARDWARE_RSA_DS_PERIPHERAL`. Populate an `esp_ds_data_ctx_t` with the encrypted key data (`esp_ds_data_t`), the eFuse key block ID, and the RSA key length in bits. Ensure the `rsa_length` field of `esp_ds_data_t` is set when the key is created (e.g. via `esp_ds_encrypt_params()` or the DS provisioning tool). Then wrap the context in an `esp_rsa_ds_opaque_key_t`, import it as a PSA opaque key using `PSA_KEY_LIFETIME_ESP_RSA_DS_VOLATILE`, and call `psa_sign_hash()` or `psa_asymmetric_decrypt()`:

    #include "psa/crypto.h"
    #include "psa_crypto_driver_esp_rsa_ds.h"

    // ds_ctx points to esp_ds_data_ctx_t (e.g. from secure cert or NVS)
    esp_ds_data_ctx_t *ds_ctx = ...;
    esp_rsa_ds_opaque_key_t rsa_ds_opaque_key = {
        .ds_data_ctx = ds_ctx,
    };

    psa_key_attributes_t attrs = PSA_KEY_ATTRIBUTES_INIT;
    psa_set_key_type(&attrs, PSA_KEY_TYPE_RSA_KEY_PAIR);
    psa_set_key_bits(&attrs, ds_ctx->rsa_length_bits);
    psa_set_key_usage_flags(&attrs, PSA_KEY_USAGE_SIGN_HASH);
    psa_set_key_algorithm(&attrs, PSA_ALG_RSA_PKCS1V15_SIGN(PSA_ALG_SHA_256));
    psa_set_key_lifetime(&attrs, PSA_KEY_LIFETIME_ESP_RSA_DS_VOLATILE);

    psa_key_id_t key_id;
    psa_status_t status = psa_import_key(&attrs,
                                         (const uint8_t *)&rsa_ds_opaque_key,
                                         sizeof(rsa_ds_opaque_key),
                                         &key_id);
    psa_reset_key_attributes(&attrs);
    if (status != PSA_SUCCESS) {
        // handle error
    }

    // Sign a hash (e.g. SHA-256 of your message)
    uint8_t hash[32] = { ... };
    uint8_t signature[256];
    size_t sig_len;
    status = psa_sign_hash(key_id, PSA_ALG_RSA_PKCS1V15_SIGN(PSA_ALG_SHA_256),
                           hash, sizeof(hash), signature, sizeof(signature), &sig_len);

    psa_destroy_key(key_id);

## Example for SSL Mutual Authentication Using DS

The SSL mutual authentication example that previously lived under `examples/protocols/mqtt/ssl_ds` is now shipped with the standalone espressif/mqtt component. Follow the component documentation to fetch the SSL DS example and build it together with ESP-MQTT. The example continues to use `mqtt_client` (implemented by ESP-MQTT) to connect to `test.mosquitto.org` over mutual-authenticated TLS, with the TLS portion handled by ESP-TLS.

In case both the `esp_ds_data_ctx_t::efuse_key_id` and `esp_rsa_ds_opaque_key_t::key_recovery_info` are set, the ESP-DS PSA driver prefers using the Key Manager-based DS key over the eFuse-based DS key.

## API Reference

### Header File

- components/mbedtls/port/psa_driver/include/psa_crypto_driver_esp_rsa_ds_contexts.h

- This header file can be included with:

  >     #include "psa_crypto_driver_esp_rsa_ds_contexts.h"

- This header file is a part of the API provided by the `mbedtls` component. To declare that your component depends on `mbedtls`, add the following to your CMakeLists.txt:

  >     REQUIRES mbedtls

  > or

  >     PRIV_REQUIRES mbedtls

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.