# Memory Management for MMU Supported Memory

[中文]

## Introduction

ESP32-C5 Memory Management Unit (MMU) is relatively simple. It can do memory address translation between physical memory addresses and virtual memory addresses. So CPU can access physical memories via virtual addresses. There are multiple types of virtual memory addresses, which have different capabilities.

ESP-IDF provides a memory mapping driver that manages the relation between these physical memory addresses and virtual memory addresses, so as to achieve some features such as reading from SPI flash via a pointer.

Memory mapping driver is actually a capabilities-based virtual memory address allocator that allows applications to make virtual memory address allocations for different purposes. In the following chapters, we call this driver `esp_mmap` driver.

ESP-IDF also provides a memory synchronization driver which can be used for potential memory desynchronization scenarios.

## Physical Memory Types

Memory mapping driver currently supports mapping to following physical memory type(s):

- SPI flash

- PSRAM

## Virtual Memory Capabilities

- `MMU_MEM_CAP_EXEC`: This capability indicates that the virtual memory address has the execute permission. Note this permission scope is within the MMU hardware.

- `MMU_MEM_CAP_READ`: This capability indicates that the virtual memory address has the read permission. Note this permission scope is within the MMU hardware.

- `MMU_MEM_CAP_WRITE`: This capability indicates that the virtual memory address has the write permission. Note this permission scope is within the MMU hardware.

- `MMU_MEM_CAP_32BIT`: This capability indicates that the virtual memory address allows for 32 bits or multiples of 32 bits access.

- `MMU_MEM_CAP_8BIT`: This capability indicates that the virtual memory address allows for 8 bits or multiples of 8 bits access.

You can call `esp_mmu_map_get_max_consecutive_free_block_size()` to know the largest consecutive mappable block size with certain capabilities.

## Memory Management Drivers

### Driver Concept

#### Terminology

The virtual memory pool is made up with one or multiple virtual memory regions, see below figure:

- A virtual memory pool stands for the whole virtual address range that can be mapped to physical memory.

- A virtual memory region is a range of virtual address with same attributes.

- A virtual memory block is a piece of virtual address range that is dynamically mapped.

- A slot is the virtual address range between two virtual memory blocks.

- A physical memory block is a piece of physical address range that is to-be-mapped or already mapped to a virtual memory block.

- Dynamical mapping is done by calling `esp_mmap` driver API `esp_mmu_map()`. This API maps the given physical memory block to a virtual memory block which is allocated by the `esp_mmap` driver.

#### Relation Between Memory Blocks

When mapping a physical memory block A, block A can have one of the following relations with another previously mapped physical memory block B:

- Enclosed: block A is completely enclosed within block B, see figure below:

- Identical: block A is completely the same as block B, see figure below:

  Note that `esp_mmap` driver considers the identical scenario the same as the enclosed scenario.

- Overlapped: block A is overlapped with block B, see figure below:

  There is a special condition, when block A entirely encloses block B, see figure below:

  Note that `esp_mmap` driver considers this scenario the same as the overlapped scenario.

### Driver Behaviour

#### Memory Map

You can call `esp_mmu_map()` to do a dynamical mapping. This API can allocate a certain size of virtual memory block according to the virtual memory capabilities you selected, then map this virtual memory block to the physical memory block as you requested. The `esp_mmap` driver supports mapping to one or more types of physical memory, so you should specify the physical memory target when mapping.

By default, physical memory blocks and virtual memory blocks are one-to-one mapped. This means, when calling `esp_mmu_map()`:

- If it is the enclosed scenario, this API will return an `ESP_ERR_INVALID_STATE`. The `out_ptr` will be assigned to the start virtual memory address of the previously mapped one which encloses the to-be-mapped one.

- If it is the identical scenario, this API will behaves exactly the same as the enclosed scenario.

- If it is the overlapped scenario, this API will by default return an `ESP_ERR_INVALID_ARG`. This means, `esp_mmap` driver by default does not allow mapping a physical memory address to multiple virtual memory addresses.

Specially, you can use `ESP_MMU_MMAP_FLAG_PADDR_SHARED`. This flag stands for one-to-multiple mapping between a physical address and multiple virtual addresses:

- If it is the overlapped scenario, this API will allocate a new virtual memory block as requested, then map to the given physical memory block.

#### Memory Unmap

You can call `esp_mmu_unmap()` to unmap a previously mapped memory block. This API returns an `ESP_ERR_NOT_FOUND` if you are trying to unmap a virtual memory block that is not mapped to any physical memory block yet.

#### Memory Address Conversion

The `esp_mmap` driver provides two helper APIs to do the conversion between virtual memory address and physical memory address：

- `esp_mmu_vaddr_to_paddr()` converts virtual address to physical address.

- `esp_mmu_paddr_to_vaddr()` converts physical address to virtual address.

#### Memory Synchronization

MMU supported physical memories can be accessed by one or multiple methods.

SPI flash can be accessed by SPI1 (ESP-IDF `esp_flash` driver APIs), or by pointers. ESP-IDF `esp_flash` driver APIs have already considered the memory synchronization, so users do not need to worry about this.

PSRAM can be accessed by pointers, hardware guarantees the data consistency when PSRAM is only accessed via pointers.

PSRAM can also be accessed by EDMA. Data desynchronization may happen because hardware does not guarantee the data consistency under such condition. You should call `esp_cache_msync()` to synchronize the Cache and the PSRAM.

See Memory Synchronization for more details.

## Thread Safety

Following APIs in `esp_mmu_map.h` are not guaranteed to be thread-safe:

- `esp_mmu_map_dump_mapped_blocks()`

APIs in `esp_cache.h` are guaranteed to be thread-safe.

## API Reference

### API Reference - ESP MMAP Driver

#### Header File

- components/esp_mm/include/esp_mmu_map.h

- This header file can be included with:

  >     #include "esp_mmu_map.h"

- This header file is a part of the API provided by the `esp_mm` component. To declare that your component depends on `esp_mm`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_mm

  > or

  >     PRIV_REQUIRES esp_mm

#### Functions

esp_err_t esp_mmu_map(esp_paddr_t paddr_start, size_t size, mmu_target_t target, mmu_mem_caps_t caps, int flags, void **out_ptr)

  Map a physical memory block to external virtual address block, with given capabilities.

  Parameters:

    - paddr_start -- [in] Start address of the physical memory block

    - size -- [in] Size to be mapped. Size will be rounded up by to the nearest multiple of MMU page size

    - target -- [in] Physical memory target you're going to map to, see `mmu_target_t`

    - caps -- [in] Memory capabilities, see `mmu_mem_caps_t`

    - flags -- [in] Mmap flags

    - out_ptr -- [out] Start address of the mapped virtual memory

  Returns:

    - ESP_OK

    - ESP_ERR_INVALID_ARG: Invalid argument, see printed logs

    - ESP_ERR_NOT_SUPPORTED: Only on ESP32, PSRAM is not a supported physical memory target

    - ESP_ERR_NOT_FOUND: No enough size free block to use

    - ESP_ERR_NO_MEM: Out of memory, this API will allocate some heap memory for internal usage

    - ESP_ERR_INVALID_STATE: Paddr is mapped already, this API will return corresponding `vaddr_start + new_block_offset` as per the previously mapped block. Only to-be-mapped paddr block is totally enclosed by a previously mapped block will lead to this error. (Identical scenario will behave similarly) new_block_start new_block_end |-----— New Block -----—| |------------— Block ------------—| block_start block_end

esp_err_t esp_mmu_unmap(void *ptr)

  Unmap a previously mapped virtual memory block.

  Parameters:

    ptr -- [in] Start address of the virtual memory

  Returns:

    - ESP_OK

    - ESP_ERR_INVALID_ARG: Null pointer

    - ESP_ERR_NOT_FOUND: Vaddr is not in external memory, or it's not mapped yet

esp_err_t esp_mmu_map_get_max_consecutive_free_block_size(mmu_mem_caps_t caps, mmu_target_t target, size_t *out_len)

  Get largest consecutive free external virtual memory block size, with given capabilities and given physical target.

  Parameters:

    - caps -- [in] Bitwise OR of MMU_MEM_CAP_* flags indicating the memory block

    - target -- [in] Physical memory target you're going to map to, see `mmu_target_t`.

    - out_len -- [out] Largest free block length, in bytes.

  Returns:

    - ESP_OK

    - ESP_ERR_INVALID_ARG: Invalid arguments, could be null pointer

esp_err_t esp_mmu_map_dump_mapped_blocks(FILE *stream)

  Dump all the previously mapped blocks

  Note

  This API shall not be called from an ISR.

  Note

  This API does not guarantee thread safety

  Parameters:

    stream -- stream to print information to; use stdout or stderr to print to the console; use fmemopen/open_memstream to print to a string buffer.

  Returns:

    - ESP_OK

esp_err_t esp_mmu_vaddr_to_paddr(void *vaddr, esp_paddr_t *out_paddr, mmu_target_t *out_target)

  Convert virtual address to physical address.

  Parameters:

    - vaddr -- [in] Virtual address

    - out_paddr -- [out] Physical address

    - out_target -- [out] Physical memory target, see `mmu_target_t`

  Returns:

    - ESP_OK

    - ESP_ERR_INVALID_ARG: Null pointer, or vaddr is not within external memory

    - ESP_ERR_NOT_FOUND: Vaddr is not mapped yet

esp_err_t esp_mmu_paddr_to_vaddr(esp_paddr_t paddr, mmu_target_t target, mmu_vaddr_t type, void **out_vaddr)

  Convert physical address to virtual address.

  Parameters:

    - paddr -- [in] Physical address

    - target -- [in] Physical memory target, see `mmu_target_t`

    - type -- [in] Virtual address type, could be either instruction or data

    - out_vaddr -- [out] Virtual address

  Returns:

    - ESP_OK

    - ESP_ERR_INVALID_ARG: Null pointer

    - ESP_ERR_NOT_FOUND: Paddr is not mapped yet

esp_err_t esp_mmu_paddr_find_caps(const esp_paddr_t paddr, mmu_mem_caps_t *out_caps)

  If the physical address is mapped, this API will provide the capabilities of the virtual address where the physical address is mapped to.

  Note

  : Only return value is ESP_OK(which means physically address is successfully mapped), then caps you get make sense.

  Note

  This API only check one page (see CONFIG_MMU_PAGE_SIZE), starting from the `paddr`

  Parameters:

    - paddr -- [in] Physical address

    - out_caps -- [out] Bitwise OR of MMU_MEM_CAP_* flags indicating the capabilities of a virtual address where the physical address is mapped to.

  Returns:

    - ESP_OK: Physical address successfully mapped.

    - ESP_ERR_INVALID_ARG: Null pointer

    - ESP_ERR_NOT_FOUND: Physical address is not mapped successfully.

#### Macros

ESP_MMU_MMAP_FLAG_PADDR_SHARED

  Share this mapping.

  MMU Memory Mapping Driver APIs for MMU supported memory

  Driver Backgrounds:

  Memory Pool || Memory Region 0 | Memory Region 1 | ... || Block 0 | Slot 0 | Block 1 | Block 2 | ... | Slot 1 (final slot) | ... |

  - A memory pool stands for the whole virtual address range that can be mapped to physical memory

  - A memory region is a range of virtual address with same attributes

  - A block is a piece of vaddr range that is dynamically mapped.

  - A Slot is the vaddr range between 2 blocks. MMAP flags

  - If this flag is set, a paddr block can be mapped to multiple vaddr blocks.

    1. This happens when:

       - the to-be-mapped paddr block is overlapped with an already mapped paddr block.

       - the to-be-mapped paddr block encloses an already mapped paddr block.

    2. If the to-be-mapped paddr block is enclosed by an already mapped paddr block, no new mapping will happen, return ESP_ERR_INVALID_STATE. The out pointer will be the already mapped paddr corresponding vaddr.

    3. If the to-be-mapped paddr block is identical with an already mapped paddr block, no new mapping will happen, return ESP_ERR_INVALID_STATE. The out pointer will be the corresponding vaddr.

  - If this flag isn't set, overlapped, enclosed or same to-be-mapped paddr block will lead to ESP_ERR_INVALID_ARG.

#### Type Definitions

typedef uint32_t esp_paddr_t

  Physical memory type.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.