# Peripherals API

[中文]

- Analog to Digital Converter (ADC)
- Clock Tree
- Digital To Analog Converter (DAC)
- GPIO & RTC GPIO
- General Purpose Timer (GPTimer)
- Inter-Integrated Circuit (I2C)
- Inter-IC Sound (I2S)
- LCD
- LED Control (LEDC)
- Motor Control Pulse Width Modulator (MCPWM)
- Pulse Counter (PCNT)
- Remote Control Transceiver (RMT)
- SD Pull-up Requirements
- SDMMC Host Driver
- SD SPI Host Driver
- SDIO Card Slave Driver
- Sigma-Delta Modulation (SDM)
- SPI Flash API
- SPI Master Driver
- SPI Slave Driver
- Capacitive Touch Sensor
- Two-Wire Automotive Interface (TWAI)
- Universal Asynchronous Receiver/Transmitter (UART)

Code examples for this API section are provided in the peripherals directory of ESP-IDF examples.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.