# Attestation

## Overview

Attestation is the process of securely providing information about a device to external parties through a cryptographically secured token. It enables IoT devices, especially those without user interfaces or in remote locations, to introduce themselves securely to networks and IoT platforms by offering attestation information.

Thus, the attestation service is employed by the device to communicate evidence regarding its credentials and operational state to a remote relying party. The collected information is structured into the Entity Attestation Token (EAT) format.

To ensure security, the EAT is cryptographically protected. The remote relying party can then verify the authenticity of the EAT and make decisions about engaging with the device based on its contents.

Note

- Support for Attestation can be toggled using the option CONFIG_SECURE_TEE_ATTESTATION (enabled by default).

## Attestation Flow

ESP-TEE Attestation Flow

1. The Relying Party sends an Attestation Request (AR) to the device REE with some challenge or nonce (usually a random number).

2. The device REE forwards the request to the device TEE attestation service through the secure service call interface.

3. The TEE assembles the Entity Attestation Token (EAT) (the attestation evidence) by gathering all the relevant claim information as outlined in the EAT claim table. It then generates a signature on the claim data, appending it to the token.

4. The evidence is transmitted back to the remote attestation service (verifier) through the device REE and the relying party. In certain cases, the Relying Party itself may act as the attestation service.

5. The attestation service assesses the received evidence and, upon successful verification, compares the EAT claim data with the available reference values.

6. The relying party determines the trustworthiness of the device based on the attestation result and its predefined policy. Subsequently, it communicates this determination to the device.

## Entity Attestation Token

The Entity Attestation Token (EAT) is a small blob of data that contains claims and is cryptographically signed. The cryptographic signing secures the token, so the means to convey the token does not need to provide any security.

When an attestation request is sent to the device, it generates the EAT in the predefined JSON format as given below. The token contains all the necessary information about the hardware and software entities on device. Here, an ECDSA key-pair from the TEE secure storage is used for signing the EAT, utilizing the slot ID mentioned in the attestation request. The EAT contains the compressed ECDSA public key as well as the `R` and `S` components of the signature.

> ESP-TEE: Attestation Evidence

### EAT: Header

Claim | Description | Comments
--- | --- | ---
Magic | Identifies the commencement of the EAT |
Encryption Algorithm | Specifies encryption algorithm details if the EAT is encrypted |
Signing Algorithm | Specifies signing algorithm details if the EAT is signed | Currently, only `ecdsa_secp256r1_sha256` is supported
Key ID | Identifies the key to be utilized by the device for encryption and signing | TEE secure storage key ID (string)

### EAT: Claim Table

Claim | Description | Comments
--- | --- | ---
Authentication Challenge | Challenge data provided by the caller to protect against replay attacks. This is typically a cryptographic nonce (random value) or a hash of data that includes a nonce. When using a data hash, the caller must ensure replay protection by incorporating a nonce into the hashed data. |
Client ID | Relying Party identification |
Device ID | Device identification (should be unique) | SHA256 digest of the device MAC address
Device Version | SoC H/W revision from eFuse |
Instance ID | Instance identification | Public-key hash (SHA256) from the current secure storage slot for the active session
Certification Reference | PSA certification ID |
Device State | Development/Production Mode |
Software Measurement | Details of the active firmware components - for e.g. app version, ESP-IDF version, digest, etc. There will be one entry of this type in the EAT for each firmware in the device. |

### EAT: Software Measurement

Key | Description | Comments
--- | --- | ---
Version | Entity image version | Not applicable to the bootloader
ESP-IDF Version |  | Not applicable to the bootloader
Secure Version | For firmware anti-rollback support | Applicable only to the REE application
Digest: Type |  | Currently, only `SHA256` is supported
Digest: Calculated Value |  |
Digest: Validation | Whether the calculated digest matches the one embedded in the firmware image |
Secure Boot signature verification status |  |
Secure Padding status |  | For more details, refer here.

### Sample EAT in JSON format

    {
      "header": {
        "magic": "44fef7cc",
        "encr_alg": "",
        "sign_alg": "ecdsa_secp256r1_sha256",
        "key_id": "tee_att_key0"
      },
      "eat": {
        "auth_challenge":"dcb9b53143ad6b081dad1a05c7ebda4e314d388762215799cf24ed52e9387678"
        "client_id": 262974944,
        "device_ver": 1,
        "device_id": "e8cddb2a7f9a5a7c61735d6dda26e4bd153c6d772a9be6f26bd321dfe25e0ac8",
        "instance_id": "1adba85e0df997fd961f25a9e312430cef162b5c69466cd5b172f1e65ac7360c",
        "psa_cert_ref": "0716053550477-10100",
        "device_status": 255,
        "sw_claims": {
          "tee": {
            "type": 1,
            "ver": "v0.3.0",
            "idf_ver": "v5.1.2-139-g07d83a7ced",
            "secure_ver": 0,
            "part_chip_rev": {
              "min": 0,
              "max": 99
            },
            "part_digest": {
              "type": 0,
              "calc_digest": "f732e7f285b7de7ac3167a867711eddbf17a2a05513d35e41cd1ebf2e0958b2e",
              "digest_validated": true,
              "sign_verified": true,
              "secure_padding": true
            }
          },
          "app": {
            "type": 2,
            "ver": "v0.1.0",
            "idf_ver": "v5.1.2-139-g07d83a7ced",
            "secure_ver": 0,
            "part_chip_rev": {
              "min": 0,
              "max": 99
            },
            "part_digest": {
              "type": 0,
              "calc_digest": "21e114fd30b9234c501525990dfab71d00348c531bb64224feff9deb32e66f9f",
              "digest_validated": true,
              "sign_verified": true,
              "secure_padding": true
            }
          },
          "bootloader": {
            "type": 0,
            "ver": "",
            "idf_ver": "",
            "secure_ver": -1,
            "part_chip_rev": {
              "min": 0,
              "max": 99
            },
            "part_digest": {
              "type": 0,
              "calc_digest": "516148649a7f670b894391ded9d64a0e8604c5cec9a1eeb0014d2549cdaa4725",
              "digest_validated": true,
              "sign_verified": true
            }
          }
        }
      },
      "public_key": {
        "compressed": "02a45c6c94c4be7722bd2513f4ccbc4daa369747e6e96e0f9f7a2eba055dee6d46"
      },
      "sign": {
        "r": "37bcc8ed9c15a4712c18fe20b257992e5d9ec273b6261675f247667b4575495b",
        "s": "28ce15da73880f7d5ee303948769b197077208f1f242aaee448e9ed23f9085fa"
      }
    }

## Application Example

The tee_attestation example demonstrates how to generate an entity attestation token containing validation details for all active firmware components (bootloader, TEE, and REE app).

## API Reference

### Header File

- components/mbedtls/port/include/psa/initial_attestation.h

- This header file can be included with:

  >     #include "psa/initial_attestation.h"

- This header file is a part of the API provided by the `mbedtls` component. To declare that your component depends on `mbedtls`, add the following to your CMakeLists.txt:

  >     REQUIRES mbedtls

  > or

  >     PRIV_REQUIRES mbedtls

### Functions

psa_status_t psa_initial_attest_get_token(const uint8_t *auth_challenge, size_t challenge_size, uint8_t *token_buf, size_t token_buf_size, size_t *token_size)

  Generate an entity attestation token.

  Generates an attestation token containing device identity and security claims, signed and encoded in the JSON format.

  Parameters:

    - auth_challenge -- Pointer to a buffer containing the challenge data from the verifier

    - challenge_size -- Size of the challenge in bytes. Must be 32, 48, or 64 bytes

    - token_buf -- Pointer to a buffer where the attestation token will be written

    - token_buf_size -- Size of the token buffer in bytes

    - token_size -- On success, will be set to the actual size of the generated token

  Returns:

    psa_status_t PSA_SUCCESS on success, PSA_ERROR_INVALID_ARGUMENT if parameters are invalid, PSA_ERROR_BUFFER_TOO_SMALL if token_buf is too small, PSA_ERROR_NOT_SUPPORTED if the requested challenge size is not supported, or another error code on failure

psa_status_t psa_initial_attest_get_token_size(size_t challenge_size, size_t *token_size)

  Get the size of the attestation token that would be generated.

  This can be used to allocate an appropriately sized buffer before calling psa_initial_attest_get_token().

  Parameters:

    - challenge_size -- Size of the challenge in bytes. Must be 32, 48, or 64 bytes

    - token_size -- On success, will be set to the size of the token that would be generated

  Returns:

    psa_status_t PSA_SUCCESS on success, PSA_ERROR_INVALID_ARGUMENT if challenge_size is invalid, PSA_ERROR_NOT_SUPPORTED if the requested challenge size is not supported, or another error code on failure

### Macros

PSA_INITIAL_ATTEST_API_VERSION_MAJOR

  Major version of this implementation of the Attestation API

PSA_INITIAL_ATTEST_API_VERSION_MINOR

  Minor version of this implementation of the Attestation API

PSA_INITIAL_ATTEST_MAX_TOKEN_SIZE

  Maximum size of an attestation token in bytes

PSA_INITIAL_ATTEST_CHALLENGE_SIZE_32

PSA_INITIAL_ATTEST_CHALLENGE_SIZE_48

PSA_INITIAL_ATTEST_CHALLENGE_SIZE_64

PSA_INITIAL_ATTEST_CHALLENGE_SIZE_MAX

  Maximum supported challenge size

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.