# Wi-Fi MAC Protocols

[中文]

## Wi-Fi HT20/40

## Wi-Fi QoS

ESP32-C61 supports all the mandatory features required in WFA Wi-Fi QoS Certification.

Four ACs (Access Category) are defined in Wi-Fi specification, and each AC has its own priority to access the Wi-Fi channel. Moreover, a map rule is defined to map the QoS priority of other protocol, e.g., 802.11D or TCP/IP precedence is mapped to Wi-Fi AC.

The table below describes how the IP Precedences are mapped to Wi-Fi ACs in ESP32-C61. It also indicates whether the AMPDU is supported for this AC. The table is sorted from high to low priority. That is to say, the AC_VO has the highest priority.

IP Precedence | Wi-Fi AC | Support AMPDU?
--- | --- | ---
6, 7 | AC_VO (Voice) | No
4, 5 | AC_VI (Video) | Yes
3, 0 | AC_BE (Best Effort) | Yes
1, 2 | AC_BK (Background) | Yes

The application can make use of the QoS feature by configuring the IP precedence via socket option IP_TOS. Here is an example to make the socket to use VI queue:

    const int ip_precedence_vi = 4;
    const int ip_precedence_offset = 5;
    int priority = (ip_precedence_vi << ip_precedence_offset);
    setsockopt(socket_id, IPPROTO_IP, IP_TOS, &priority, sizeof(priority));

Theoretically, the higher priority AC has better performance than the lower priority AC. However, it is not always true. Here are some suggestions about how to use the Wi-Fi QoS:

> - Some really important application traffic can be put into the AC_VO queue. But avoid using the AC_VO queue for heavy traffic, as it may impact the management frames which also use this queue. Eventually, it is worth noting that the AC_VO queue does not support AMPDU, and its performance with heavy traffic is no better than other queues.

> - Avoid using more than two precedences supported by different AMPDUs, e.g., when socket A uses precedence 0, socket B uses precedence 1, and socket C uses precedence 2. This can be a bad design because it may need much more memory. To be specific, the Wi-Fi driver may generate a Block Ack session for each precedence and it needs more memory if the Block Ack session is set up.

## Wi-Fi Aggregate MAC Protocol Data Unit (AMPDU)

ESP32-C61 supports both receiving and transmitting AMPDU, and the AMPDU can greatly improve the Wi-Fi throughput.

Generally, the AMPDU should be enabled. Disabling AMPDU is usually for debugging purposes.

## Wi-Fi AMSDU

ESP32-C61 supports receiving and transmitting AMSDU. AMSDU TX is disabled by default, since enable AMSDU TX need more memory. Select CONFIG_ESP_WIFI_AMSDU_TX_ENABLED to enable AMSDU Tx feature, it depends on CONFIG_SPIRAM.

## Wi-Fi Fragment

ESP32-C61 supports Wi-Fi receiving and transmitting fragment.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.