# Storage

[中文]

## Removed VFS SDMMC Deprecated API

Deprecated `esp_vfs_fat_sdmmc_unmount` function is now removed. Please use `esp_vfs_fat_sdcard_unmount` instead.

## VFS

- Deleted deprecated UART-VFS functions (`esp_vfs_dev_uart_*`) located in the `vfs` component. Please use API from UART driver instead: `uart_vfs_dev_*`.

- Deleted deprecated USB-Serial-JTAG-VFS functions (`esp_vfs_dev_usb_serial_jtag_*`) located in the `vfs` component. Please use API from USB-Serial-JTAG driver instead: `usb_serial_jtag_vfs_*`.

- `esp_vfs_register_fd_range` is now considered private and its signature was changed to match the new VFS API style. Projects that still rely on this internal helper must include `esp_private/socket.h` and should be aware that the API may change without notice.

- Legacy VFS APIs (such as `esp_vfs_register`) that operate on `esp_vfs_t` instead of `esp_vfs_fs_ops_t` are deprecated and will be removed in the next major release. Switch to the new `esp_vfs_fs_ops_t`-based APIs.

## `esp_vfs_console`

The `esp_vfs_console` component has been renamed to `esp_stdio`. This component did not have any public functions, so in normal circumstances, there is no need to update your code. If you for any reason had declared a dependency on this component, it can be deleted, as the new `esp_stdio` is a common component that is added to all components by default.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.