# Pulse Counter (PCNT)

## Introduction

The PCNT (Pulse Counter) module is designed to count the number of rising and/or falling edges of input signals. The ESP32-H2 contains multiple pulse counter units in the module. [1] Each unit is in effect an independent counter with multiple channels, where each channel can increment/decrement the counter on a rising/falling edge. Furthermore, each channel can be configured separately.

PCNT channels can react to signals of edge type and level type, however for simple applications, detecting the edge signal is usually sufficient. PCNT channels can be configured react to both pulse edges (i.e., rising and falling edge), and can be configured to increase, decrease or do nothing to the unit's counter on each edge. The level signal is the so-called control signal, which is used to control the counting mode of the edge signals that are attached to the same channel. By combining the usage of both edge and level signals, a PCNT unit can act as a quadrature decoder.

Besides that, PCNT unit is equipped with a separate glitch filter, which is helpful to remove noise from the signal.

Typically, a PCNT module can be used in scenarios like:

- Calculate periodic signal's frequency by counting the pulse numbers within a time slice

- Decode quadrature signals into speed and direction

## Functional Overview

Description of the PCNT functionality is divided into the following sections:

- Resource Allocation - covers how to allocate PCNT units and channels with properly set of configurations. It also covers how to recycle the resources when they finished working.

- Set Up Channel Actions - covers how to configure the PCNT channel to behave on different signal edges and levels.

- Watch Points - describes how to configure PCNT watch points (i.e., tell PCNT unit to trigger an event when the count reaches a certain value).

- Watch Step - describes how to configure PCNT watch step (i.e., tell PCNT unit to trigger an event when the count increment reaches a certain value).

- Register Event Callbacks - describes how to hook your specific code to the watch point event callback function.

- Set Glitch Filter - describes how to enable and set the timing parameters for the internal glitch filter.

- Enable and Disable Unit - describes how to enable and disable the PCNT unit.

- Unit IO Control - describes IO control functions of PCNT unit, like enable glitch filter, start and stop unit, get and clear count value.

- Power Management - describes what functionality will prevent the chip from going into low power mode.

- IRAM Safe - describes tips on how to make the PCNT interrupt and IO control functions work better along with a disabled cache.

- Thread Safety - lists which APIs are guaranteed to be thread safe by the driver.

- Kconfig Options - lists the supported Kconfig options that can be used to make a different effect on driver behavior.

### Resource Allocation

The PCNT unit and channel are represented by `pcnt_unit_handle_t` and `pcnt_channel_handle_t` respectively. All available units and channels are maintained by the driver in a resource pool, so you do not need to know the exact underlying instance ID.

#### Install PCNT Unit

To install a PCNT unit, there is a configuration structure that needs to be given in advance: `pcnt_unit_config_t`:

- `pcnt_unit_config_t::low_limit` and `pcnt_unit_config_t::high_limit` specify the range for the internal hardware counter. The counter will reset to zero automatically when it crosses either the high or low limit.

- `pcnt_unit_config_t::accum_count` sets whether to create an internal accumulator for the counter. This is helpful when you want to extend the counter's width, which by default is 16 bit at most, defined in the hardware. See also Compensate Overflow Loss for how to use this feature to compensate the overflow loss.

- `pcnt_unit_config_t::en_step_notify_up` Configure whether to enable watch step to count in the positive direction.

- `pcnt_unit_config_t::en_step_notify_down` Configure whether to enable watch step to count in the negative direction.

- `pcnt_unit_config_t::intr_priority` sets the priority of the interrupt. If it is set to `0`, the driver will allocate an interrupt with a default priority. Otherwise, the driver will use the given priority.

Note

Since all PCNT units share the same interrupt source, when installing multiple PCNT units make sure that the interrupt priority `pcnt_unit_config_t::intr_priority` is the same for each unit.

Unit allocation and initialization is done by calling a function `pcnt_new_unit()` with `pcnt_unit_config_t` as an input parameter. The function will return a PCNT unit handle only when it runs correctly. Specifically, when there are no more free PCNT units in the pool (i.e., unit resources have been used up), then this function will return `ESP_ERR_NOT_FOUND` error.

If a previously created PCNT unit is no longer needed, it is recommended to recycle the resource by calling `pcnt_del_unit()`. Which in return allows the underlying unit hardware to be used for other purposes. Before deleting a PCNT unit, one should ensure the following prerequisites:

- The unit is in the init state, in other words, the unit is either disabled by `pcnt_unit_disable()` or not enabled yet.

- The attached PCNT channels are all removed by `pcnt_del_channel()`.

    #define EXAMPLE_PCNT_HIGH_LIMIT 100
    #define EXAMPLE_PCNT_LOW_LIMIT  -100

    pcnt_unit_config_t unit_config = {
        .high_limit = EXAMPLE_PCNT_HIGH_LIMIT,
        .low_limit = EXAMPLE_PCNT_LOW_LIMIT,
    };
    pcnt_unit_handle_t pcnt_unit = NULL;
    ESP_ERROR_CHECK(pcnt_new_unit(&unit_config, &pcnt_unit));

#### Install PCNT Channel

To install a PCNT channel, you must initialize a `pcnt_chan_config_t` structure in advance, and then call `pcnt_new_channel()`. The configuration fields of the `pcnt_chan_config_t` structure are described below:

- `pcnt_chan_config_t::edge_gpio_num` and `pcnt_chan_config_t::level_gpio_num` specify the GPIO numbers used by edge type signal and level type signal. Please note, either of them can be assigned to `-1` if it is not actually used, and thus it will become a virtual IO. For some simple pulse counting applications where one of the level/edge signals is fixed (i.e., never changes), you can reclaim a GPIO by setting the signal as a virtual IO on channel allocation. Setting the level/edge signal as a virtual IO causes that signal to be internally routed to a fixed High/Low logic level, thus allowing you to save a GPIO for other purposes.

- `pcnt_chan_config_t::virt_edge_io_level` and `pcnt_chan_config_t::virt_level_io_level` specify the virtual IO level for edge and level input signal, to ensure a deterministic state for such control signal. Please note, they are only valid when either `pcnt_chan_config_t::edge_gpio_num` or `pcnt_chan_config_t::level_gpio_num` is assigned to `-1`.

- `pcnt_chan_config_t::invert_edge_input` and `pcnt_chan_config_t::invert_level_input` are used to decide whether to invert the input signals before they going into PCNT hardware. The invert is done by GPIO matrix instead of PCNT hardware.

Channel allocating and initialization is done by calling a function `pcnt_new_channel()` with the above `pcnt_chan_config_t` as an input parameter plus a PCNT unit handle returned from `pcnt_new_unit()`. This function will return a PCNT channel handle if it runs correctly. Specifically, when there are no more free PCNT channel within the unit (i.e., channel resources have been used up), then this function will return `ESP_ERR_NOT_FOUND` error. Note that, when install a PCNT channel for a specific unit, one should ensure the unit is in the init state, otherwise this function will return `ESP_ERR_INVALID_STATE` error.

If a previously created PCNT channel is no longer needed, it is recommended to recycle the resources by calling `pcnt_del_channel()`. Which in return allows the underlying channel hardware to be used for other purposes.

    #define EXAMPLE_CHAN_GPIO_A 0
    #define EXAMPLE_CHAN_GPIO_B 2

    pcnt_chan_config_t chan_config = {
        .edge_gpio_num = EXAMPLE_CHAN_GPIO_A,
        .level_gpio_num = EXAMPLE_CHAN_GPIO_B,
    };
    pcnt_channel_handle_t pcnt_chan = NULL;
    ESP_ERROR_CHECK(pcnt_new_channel(pcnt_unit, &chan_config, &pcnt_chan));

Note

In PCNT, the GPIOs involved can be reconfigured for pull-up or pull-down after initializing PCNT using functions such as `gpio_pullup_en()` and `gpio_pullup_dis()`.

### Set Up Channel Actions

The PCNT will increase/decrease/hold its internal count value when the input pulse signal toggles. You can set different actions for edge signal and/or level signal.

- `pcnt_channel_set_edge_action()` function is to set specific actions for rising and falling edge of the signal attached to the `pcnt_chan_config_t::edge_gpio_num`. Supported actions are listed in `pcnt_channel_edge_action_t`.

- `pcnt_channel_set_level_action()` function is to set specific actions for high and low level of the signal attached to the `pcnt_chan_config_t::level_gpio_num`. Supported actions are listed in `pcnt_channel_level_action_t`. This function is not mandatory if the `pcnt_chan_config_t::level_gpio_num` is set to `-1` when allocating PCNT channel by `pcnt_new_channel()`.

    // decrease the counter on rising edge, increase the counter on falling edge
    ESP_ERROR_CHECK(pcnt_channel_set_edge_action(pcnt_chan, PCNT_CHANNEL_EDGE_ACTION_DECREASE, PCNT_CHANNEL_EDGE_ACTION_INCREASE));
    // keep the counting mode when the control signal is high level, and reverse the counting mode when the control signal is low level
    ESP_ERROR_CHECK(pcnt_channel_set_level_action(pcnt_chan, PCNT_CHANNEL_LEVEL_ACTION_KEEP, PCNT_CHANNEL_LEVEL_ACTION_INVERSE));

### Watch Points

Each PCNT unit can be configured to watch several different values that you are interested in. The value to be watched is also called Watch Point. The watch point itself can not exceed the range set in `pcnt_unit_config_t` by `pcnt_unit_config_t::low_limit` and `pcnt_unit_config_t::high_limit`. When the counter reaches either watch point, a watch event will be triggered and notify you by interrupt if any watch event callback has ever registered in `pcnt_unit_register_event_callbacks()`. See Register Event Callbacks for how to register event callbacks.

The watch point can be added and removed by `pcnt_unit_add_watch_point()` and `pcnt_unit_remove_watch_point()`. The commonly-used watch points are: zero cross, maximum/minimum count and other threshold values. The number of available watch point is limited, `pcnt_unit_add_watch_point()` will return error `ESP_ERR_NOT_FOUND` if it can not find any free hardware resource to save the watch point. You can not add the same watch point for multiple times, otherwise it will return error `ESP_ERR_INVALID_STATE`.

It is recommended to remove the unused watch point by `pcnt_unit_remove_watch_point()` to recycle the watch point resources.

    // add zero across watch point
    ESP_ERROR_CHECK(pcnt_unit_add_watch_point(pcnt_unit, 0));
    // add high limit watch point
    ESP_ERROR_CHECK(pcnt_unit_add_watch_point(pcnt_unit, EXAMPLE_PCNT_HIGH_LIMIT));

### Watch Step

PCNT unit can be configured to watch a specific value increment (can be positive or negative) that you are interested in. The function of watching value increment is also called Watch Step. To install watch step requires enabling `pcnt_unit_config_t::en_step_notify_up` or `pcnt_unit_config_t::en_step_notify_down`. The step interval itself can not exceed the range set in `pcnt_unit_config_t` by `pcnt_unit_config_t::low_limit` and `pcnt_unit_config_t::high_limit`.When the counter increment reaches step interval, a watch event will be triggered and notify you by interrupt if any watch event callback has ever registered in `pcnt_unit_register_event_callbacks()`. See Register Event Callbacks for how to register event callbacks.

The watch step can be added and removed by `pcnt_unit_add_watch_step()` and `pcnt_unit_remove_watch_step()`. The parameter `step_interval` can be positive(step forward, e.g., [N]->[N+1]->[N+2]->...) or negative(step backward, e.g., [N]->[N-1]->[N-2]->...). The same direction can only add one watch step, otherwise it will return error `ESP_ERR_INVALID_STATE`.

Note

Due to hardware limitations, some chips may only support adding one direction of watch step. Please check the return value of `pcnt_unit_add_watch_step()` for more details.

It is recommended to remove the unused watch step by `pcnt_unit_remove_watch_step()` to recycle the watch step resources.

Note

When a watch step and a watch point are triggered at the same time (i.e. at the same absolute point), the callback function only gets called by once.

The step increment will be reset to 0 when the count reaches the high/low limit value. Please do not rely too much on the exact step interval.

    // add positive direction watch step with 100 step intervals
    ESP_ERROR_CHECK(pcnt_unit_add_watch_step(pcnt_unit, 100));

### Register Event Callbacks

When PCNT unit reaches any enabled watch point, specific event will be generated and notify the CPU by interrupt. If you have some function that want to get executed when event happens, you should hook your function to the interrupt service routine by calling `pcnt_unit_register_event_callbacks()`. All supported event callbacks are listed in the `pcnt_event_callbacks_t`:

- `pcnt_event_callbacks_t::on_reach` sets a callback function for watch point event. As this function is called within the ISR context, you must ensure that the function does not attempt to block (e.g., by making sure that only FreeRTOS APIs with `ISR` suffix are called from within the function). The function prototype is declared in `pcnt_watch_cb_t`.

You can save their own context to `pcnt_unit_register_event_callbacks()` as well, via the parameter `user_ctx`. This user data will be directly passed to the callback functions.

In the callback function, the driver will fill in the event data of specific event. For example, the watch point event or watch step event data is declared as `pcnt_watch_event_data_t`:

- `pcnt_watch_event_data_t::watch_point_value` saves the count value when the event triggered.

- `pcnt_watch_event_data_t::zero_cross_mode` saves how the PCNT unit crosses the zero point in the latest time. The possible zero cross modes are listed in the `pcnt_unit_zero_cross_mode_t`. Usually different zero cross mode means different counting direction and counting step size.

Registering callback function results in lazy installation of interrupt service, thus this function should only be called before the unit is enabled by `pcnt_unit_enable()`. Otherwise, it can return `ESP_ERR_INVALID_STATE` error.

    static bool example_pcnt_on_reach(pcnt_unit_handle_t unit, const pcnt_watch_event_data_t *edata, void *user_ctx)
    {
        BaseType_t high_task_wakeup;
        QueueHandle_t queue = (QueueHandle_t)user_ctx;
        // send watch point to queue, from this interrupt callback
        xQueueSendFromISR(queue, &(edata->watch_point_value), &high_task_wakeup);
        // return whether a high priority task has been waken up by this function
        return (high_task_wakeup == pdTRUE);
    }

    pcnt_event_callbacks_t cbs = {
        .on_reach = example_pcnt_on_reach,
    };
    QueueHandle_t queue = xQueueCreate(10, sizeof(int));
    ESP_ERROR_CHECK(pcnt_unit_register_event_callbacks(pcnt_unit, &cbs, queue));

### Set Glitch Filter

The PCNT unit features filters to ignore possible short glitches in the signals. The parameters that can be configured for the glitch filter are listed in `pcnt_glitch_filter_config_t`:

- `pcnt_glitch_filter_config_t::max_glitch_ns` sets the maximum glitch width, in nano seconds. If a signal pulse's width is smaller than this value, then it will be treated as noise and will not increase/decrease the internal counter.

You can enable the glitch filter for PCNT unit by calling `pcnt_unit_set_glitch_filter()` with the filter configuration provided above. Particularly, you can disable the glitch filter later by calling `pcnt_unit_set_glitch_filter()` with a `NULL` filter configuration.

This function should be called when the unit is in the init state. Otherwise, it will return `ESP_ERR_INVALID_STATE` error.

Note

The glitch filter operates using the APB clock. To ensure the counter does not miss any pulses, the maximum glitch width should be longer than one APB_CLK cycle (typically 12.5 ns if APB is 80 MHz). Since the APB frequency can change with Dynamic Frequency Scaling (DFS), the filter may not function as expected in such cases. Therefore, the driver installs a power management lock for each PCNT unit. For more details on the power management strategy used in the PCNT driver, please refer to Power Management.

    pcnt_glitch_filter_config_t filter_config = {
        .max_glitch_ns = 1000,
    };
    ESP_ERROR_CHECK(pcnt_unit_set_glitch_filter(pcnt_unit, &filter_config));

### Enable and Disable Unit

Before doing IO control to the PCNT unit, you need to enable it first, by calling `pcnt_unit_enable()`. Internally, this function:

- switches the PCNT driver state from init to enable.

- enables the interrupt service if it has been lazy installed in `pcnt_unit_register_event_callbacks()`.

- acquires a proper power management lock if it has been installed. See also Power Management for more information.

On the contrary, calling `pcnt_unit_disable()` will do the opposite, that is, put the PCNT driver back to the init state, disable the interrupts service and release the power management lock.

### Unit IO Control

#### Start/Stop and Clear

Calling `pcnt_unit_start()` makes the PCNT unit start to work, increase or decrease counter according to pulse signals. On the contrary, calling `pcnt_unit_stop()` will stop the PCNT unit but retain current count value. Instead, clearing counter can only be done by calling `pcnt_unit_clear_count()`.

Note, `pcnt_unit_start()` and `pcnt_unit_stop()` should be called when the unit has been enabled by `pcnt_unit_enable()`. Otherwise, it will return `ESP_ERR_INVALID_STATE` error.

#### Get Count Value

You can read current count value at any time by calling `pcnt_unit_get_count()`. The returned count value is a signed integer, where the sign can be used to reflect the direction.

    int pulse_count = 0;
    ESP_ERROR_CHECK(pcnt_unit_get_count(pcnt_unit, &pulse_count));

#### Compensate Overflow Loss

The internal hardware counter will be cleared to zero automatically when it reaches high or low limit. If you want to compensate for that count loss and extend the counter's bit-width, you can:

1. Enable `pcnt_unit_config_t::accum_count` when installing the PCNT unit.

2. Add the high/low limit as the Watch Points.

3. Now, the returned count value from the `pcnt_unit_get_count()` function not only reflects the hardware's count value, but also accumulates the high/low overflow loss to it.

Note

`pcnt_unit_clear_count()` resets the accumulated count value as well.

Note

When enabling the count overflow compensation, it is recommended to use as large a high/low count limit as possible, as it can avoid frequent interrupt triggering, improve system performance, and avoid compensation failure due to multiple overflows.

### Power Management

When power management is enabled (i.e., CONFIG_PM_ENABLE is on), the system adjusts the APB frequency before entering light sleep, which can cause the PCNT glitch filter to misinterpret valid signals as noise.

To prevent this, the driver can acquire a power management lock of type `ESP_PM_APB_FREQ_MAX`, ensuring the APB frequency remains constant. This lock is acquired when the PCNT unit is enabled via `pcnt_unit_enable()` and released when the unit is disabled via `pcnt_unit_disable()`.

### IRAM Safe

By default, the PCNT interrupt will be deferred when the Cache is disabled for reasons like writing/erasing Flash. Thus the alarm interrupt will not get executed in time, which is not expected in a real-time application.

There is a Kconfig option CONFIG_PCNT_ISR_IRAM_SAFE that:

1. Enables the interrupt being serviced even when cache is disabled

2. Places all functions that used by the ISR into IRAM [2]

3. Places driver object into DRAM (in case it is mapped to PSRAM by accident)

This allows the interrupt to run while the cache is disabled but comes at the cost of increased IRAM consumption.

There is another Kconfig option CONFIG_PCNT_CTRL_FUNC_IN_IRAM that can put commonly used IO control functions into IRAM as well. So that these functions can also be executable when the cache is disabled. These IO control functions are as follows:

- `pcnt_unit_start()`

- `pcnt_unit_stop()`

- `pcnt_unit_clear_count()`

- `pcnt_unit_get_count()`

### Thread Safety

The factory functions `pcnt_new_unit()` and `pcnt_new_channel()` are guaranteed to be thread safe by the driver, which means, you can call them from different RTOS tasks without protection by extra locks.

The following functions are allowed to run under ISR context, the driver uses a critical section to prevent them being called concurrently in both task and ISR.

- `pcnt_unit_start()`

- `pcnt_unit_stop()`

- `pcnt_unit_clear_count()`

- `pcnt_unit_get_count()`

Other functions that take the `pcnt_unit_handle_t` and `pcnt_channel_handle_t` as the first positional parameter, are not treated as thread safe. This means you should avoid calling them from multiple tasks.

### Kconfig Options

- CONFIG_PCNT_CTRL_FUNC_IN_IRAM controls where to place the PCNT control functions (IRAM or Flash), see IRAM Safe for more information.

- CONFIG_PCNT_ISR_IRAM_SAFE controls whether the default ISR handler can work when cache is disabled, see IRAM Safe for more information.

- CONFIG_PCNT_ENABLE_DEBUG_LOG is used to enabled the debug log output. Enabling this option increases the firmware binary size.

## Application Examples

- peripherals/pcnt/rotary_encoder demonstrates how to use the PCNT peripheral to decode the differential signals generated from a common rotary encoder, EC11, and how to configure the rotary encoder to wake the system from light-sleep.

## API Reference

### Header File

- components/esp_driver_pcnt/include/driver/pulse_cnt.h

- This header file can be included with:

  >     #include "driver/pulse_cnt.h"

- This header file is a part of the API provided by the `esp_driver_pcnt` component. To declare that your component depends on `esp_driver_pcnt`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_driver_pcnt

  > or

  >     PRIV_REQUIRES esp_driver_pcnt

### Functions

esp_err_t pcnt_new_unit(const pcnt_unit_config_t *config, pcnt_unit_handle_t *ret_unit)

  Create a new PCNT unit, and return the handle.

  Note

  The newly created PCNT unit is put in the init state.

  Parameters:

    - config -- [in] PCNT unit configuration

    - ret_unit -- [out] Returned PCNT unit handle

  Returns:

    - ESP_OK: Create PCNT unit successfully

    - ESP_ERR_INVALID_ARG: Create PCNT unit failed because of invalid argument (e.g. high/low limit value out of the range)

    - ESP_ERR_NO_MEM: Create PCNT unit failed because out of memory

    - ESP_ERR_NOT_FOUND: Create PCNT unit failed because all PCNT units are used up and no more free one

    - ESP_FAIL: Create PCNT unit failed because of other error

esp_err_t pcnt_del_unit(pcnt_unit_handle_t unit)

  Delete the PCNT unit handle.

  Note

  A PCNT unit can't be in the enable state when this function is invoked. See also `pcnt_unit_disable()` for how to disable a unit.

  Parameters:

    unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

  Returns:

    - ESP_OK: Delete the PCNT unit successfully

    - ESP_ERR_INVALID_ARG: Delete the PCNT unit failed because of invalid argument

    - ESP_ERR_INVALID_STATE: Delete the PCNT unit failed because the unit is not in init state or some PCNT channel is still in working

    - ESP_FAIL: Delete the PCNT unit failed because of other error

esp_err_t pcnt_unit_set_glitch_filter(pcnt_unit_handle_t unit, const pcnt_glitch_filter_config_t *config)

  Set glitch filter for PCNT unit.

  Note

  This function should be called when the PCNT unit is in the init state (i.e. before calling `pcnt_unit_enable()`)

  Parameters:

    - unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

    - config -- [in] PCNT filter configuration, set config to NULL means disabling the filter function

  Returns:

    - ESP_OK: Set glitch filter successfully

    - ESP_ERR_INVALID_ARG: Set glitch filter failed because of invalid argument (e.g. glitch width is too big)

    - ESP_ERR_INVALID_STATE: Set glitch filter failed because the unit is not in the init state

    - ESP_FAIL: Set glitch filter failed because of other error

esp_err_t pcnt_unit_enable(pcnt_unit_handle_t unit)

  Enable the PCNT unit.

  Note

  This function will transit the unit state from init to enable.

  Note

  This function will enable the interrupt service, if it's lazy installed in `pcnt_unit_register_event_callbacks()`.

  Note

  This function will acquire the PM lock if it's lazy installed in `pcnt_unit_set_glitch_filter()`.

  Note

  Enable a PCNT unit doesn't mean to start it. See also `pcnt_unit_start()` for how to start the PCNT counter.

  Parameters:

    unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

  Returns:

    - ESP_OK: Enable PCNT unit successfully

    - ESP_ERR_INVALID_ARG: Enable PCNT unit failed because of invalid argument

    - ESP_ERR_INVALID_STATE: Enable PCNT unit failed because the unit is already enabled

    - ESP_FAIL: Enable PCNT unit failed because of other error

esp_err_t pcnt_unit_disable(pcnt_unit_handle_t unit)

  Disable the PCNT unit.

  Note

  This function will do the opposite work to the `pcnt_unit_enable()`

  Note

  Disable a PCNT unit doesn't mean to stop it. See also `pcnt_unit_stop()` for how to stop the PCNT counter.

  Parameters:

    unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

  Returns:

    - ESP_OK: Disable PCNT unit successfully

    - ESP_ERR_INVALID_ARG: Disable PCNT unit failed because of invalid argument

    - ESP_ERR_INVALID_STATE: Disable PCNT unit failed because the unit is not enabled yet

    - ESP_FAIL: Disable PCNT unit failed because of other error

esp_err_t pcnt_unit_start(pcnt_unit_handle_t unit)

  Start the PCNT unit, the counter will start to count according to the edge and/or level input signals.

  Note

  This function should be called when the unit is in the enable state (i.e. after calling `pcnt_unit_enable()`)

  Note

  This function is allowed to run within ISR context

  Note

  This function will be placed into IRAM if `CONFIG_PCNT_CTRL_FUNC_IN_IRAM` is on, so that it's allowed to be executed when Cache is disabled

  Parameters:

    unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

  Returns:

    - ESP_OK: Start PCNT unit successfully

    - ESP_ERR_INVALID_ARG: Start PCNT unit failed because of invalid argument

    - ESP_ERR_INVALID_STATE: Start PCNT unit failed because the unit is not enabled yet

    - ESP_FAIL: Start PCNT unit failed because of other error

esp_err_t pcnt_unit_stop(pcnt_unit_handle_t unit)

  Stop PCNT from counting.

  Note

  This function should be called when the unit is in the enable state (i.e. after calling `pcnt_unit_enable()`)

  Note

  The stop operation won't clear the counter. Also see `pcnt_unit_clear_count()` for how to clear pulse count value.

  Note

  This function is allowed to run within ISR context

  Note

  This function will be placed into IRAM if `CONFIG_PCNT_CTRL_FUNC_IN_IRAM`, so that it is allowed to be executed when Cache is disabled

  Parameters:

    unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

  Returns:

    - ESP_OK: Stop PCNT unit successfully

    - ESP_ERR_INVALID_ARG: Stop PCNT unit failed because of invalid argument

    - ESP_ERR_INVALID_STATE: Stop PCNT unit failed because the unit is not enabled yet

    - ESP_FAIL: Stop PCNT unit failed because of other error

esp_err_t pcnt_unit_clear_count(pcnt_unit_handle_t unit)

  Clear PCNT pulse count value to zero.

  Note

  It's recommended to call this function after adding a watch point by `pcnt_unit_add_watch_point()`, so that the newly added watch point is effective immediately.

  Note

  This function is allowed to run within ISR context

  Note

  This function will be placed into IRAM if `CONFIG_PCNT_CTRL_FUNC_IN_IRAM`, so that it's allowed to be executed when Cache is disabled

  Parameters:

    unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

  Returns:

    - ESP_OK: Clear PCNT pulse count successfully

    - ESP_ERR_INVALID_ARG: Clear PCNT pulse count failed because of invalid argument

    - ESP_FAIL: Clear PCNT pulse count failed because of other error

esp_err_t pcnt_unit_get_count(pcnt_unit_handle_t unit, int *value)

  Get PCNT count value.

  Note

  This function is allowed to run within ISR context

  Note

  This function will be placed into IRAM if `CONFIG_PCNT_CTRL_FUNC_IN_IRAM`, so that it's allowed to be executed when Cache is disabled

  Parameters:

    - unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

    - value -- [out] Returned count value

  Returns:

    - ESP_OK: Get PCNT pulse count successfully

    - ESP_ERR_INVALID_ARG: Get PCNT pulse count failed because of invalid argument

    - ESP_FAIL: Get PCNT pulse count failed because of other error

esp_err_t pcnt_unit_register_event_callbacks(pcnt_unit_handle_t unit, const pcnt_event_callbacks_t *cbs, void *user_data)

  Set event callbacks for PCNT unit.

  Note

  User registered callbacks are expected to be runnable within ISR context

  Note

  The first call to this function needs to be before the call to `pcnt_unit_enable`

  Note

  User can deregister a previously registered callback by calling this function and setting the callback member in the `cbs` structure to NULL.

  Parameters:

    - unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

    - cbs -- [in] Group of callback functions

    - user_data -- [in] User data, which will be passed to callback functions directly

  Returns:

    - ESP_OK: Set event callbacks successfully

    - ESP_ERR_INVALID_ARG: Set event callbacks failed because of invalid argument

    - ESP_ERR_INVALID_STATE: Set event callbacks failed because the unit is not in init state

    - ESP_FAIL: Set event callbacks failed because of other error

esp_err_t pcnt_unit_add_watch_point(pcnt_unit_handle_t unit, int watch_point)

  Add a watch point for PCNT unit, PCNT will generate an event when the counter value reaches the watch point value.

  Parameters:

    - unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

    - watch_point -- [in] Value to be watched

  Returns:

    - ESP_OK: Add watch point successfully

    - ESP_ERR_INVALID_ARG: Add watch point failed because of invalid argument (e.g. the value to be watched is out of the limitation set in `pcnt_unit_config_t`)

    - ESP_ERR_INVALID_STATE: Add watch point failed because the same watch point has already been added

    - ESP_ERR_NOT_FOUND: Add watch point failed because no more hardware watch point can be configured

    - ESP_FAIL: Add watch point failed because of other error

esp_err_t pcnt_unit_remove_watch_point(pcnt_unit_handle_t unit, int watch_point)

  Remove a watch point for PCNT unit.

  Parameters:

    - unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

    - watch_point -- [in] Watch point value

  Returns:

    - ESP_OK: Remove watch point successfully

    - ESP_ERR_INVALID_ARG: Remove watch point failed because of invalid argument

    - ESP_ERR_INVALID_STATE: Remove watch point failed because the watch point was not added by `pcnt_unit_add_watch_point()` yet

    - ESP_FAIL: Remove watch point failed because of other error

esp_err_t pcnt_unit_add_watch_step(pcnt_unit_handle_t unit, int step_interval)

  Add a step notify for PCNT unit, PCNT will generate an event when the incremental(can be positive or negative) of counter value reaches the step interval.

  Parameters:

    - unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

    - step_interval -- [in] PCNT step notify interval value. Positive value means step forward, negative value means step backward.

  Returns:

    - ESP_OK: Add step notify successfully

    - ESP_ERR_INVALID_ARG: Add step notify failed because of invalid argument (e.g. the value incremental to be watched is out of the limitation set in `pcnt_unit_config_t`)

    - ESP_ERR_INVALID_STATE: Add step notify failed because the step notify has already been added

    - ESP_FAIL: Add step notify failed because of other error

esp_err_t pcnt_unit_remove_all_watch_step(pcnt_unit_handle_t unit)

  Remove all step notify for PCNT unit.

  Parameters:

    unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

  Returns:

    - ESP_OK: Remove step notify successfully

    - ESP_ERR_INVALID_ARG: Remove step notify failed because of invalid argument

    - ESP_ERR_INVALID_STATE: Remove step notify failed because the step notify was not added by `pcnt_unit_add_watch_step()` yet

    - ESP_FAIL: Remove step notify failed because of other error

esp_err_t pcnt_unit_remove_single_watch_step(pcnt_unit_handle_t unit, int step_interval)

  Remove a step notify for PCNT unit.

  Parameters:

    - unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

    - step_interval -- [in] Step notify interval value

  Returns:

    - ESP_OK: Remove step notify successfully

    - ESP_ERR_INVALID_ARG: Remove step notify failed because of invalid argument

    - ESP_ERR_INVALID_STATE: Remove step notify failed because the step notify was not added by `pcnt_unit_add_watch_step()` yet

    - ESP_FAIL: Remove step notify failed because of other error

esp_err_t pcnt_new_channel(pcnt_unit_handle_t unit, const pcnt_chan_config_t *config, pcnt_channel_handle_t *ret_chan)

  Create PCNT channel for specific unit, each PCNT has several channels associated with it.

  Note

  This function should be called when the unit is in init state (i.e. before calling `pcnt_unit_enable()`)

  Parameters:

    - unit -- [in] PCNT unit handle created by `pcnt_new_unit()`

    - config -- [in] PCNT channel configuration

    - ret_chan -- [out] Returned channel handle

  Returns:

    - ESP_OK: Create PCNT channel successfully

    - ESP_ERR_INVALID_ARG: Create PCNT channel failed because of invalid argument

    - ESP_ERR_NO_MEM: Create PCNT channel failed because of insufficient memory

    - ESP_ERR_NOT_FOUND: Create PCNT channel failed because all PCNT channels are used up and no more free one

    - ESP_ERR_INVALID_STATE: Create PCNT channel failed because the unit is not in the init state

    - ESP_FAIL: Create PCNT channel failed because of other error

esp_err_t pcnt_del_channel(pcnt_channel_handle_t chan)

  Delete the PCNT channel.

  Parameters:

    chan -- [in] PCNT channel handle created by `pcnt_new_channel()`

  Returns:

    - ESP_OK: Delete the PCNT channel successfully

    - ESP_ERR_INVALID_ARG: Delete the PCNT channel failed because of invalid argument

    - ESP_FAIL: Delete the PCNT channel failed because of other error

esp_err_t pcnt_channel_set_edge_action(pcnt_channel_handle_t chan, pcnt_channel_edge_action_t pos_act, pcnt_channel_edge_action_t neg_act)

  Set channel actions when edge signal changes (e.g. falling or rising edge occurred). The edge signal is input from the `edge_gpio_num` configured in `pcnt_chan_config_t`. We use these actions to control when and how to change the counter value.

  Parameters:

    - chan -- [in] PCNT channel handle created by `pcnt_new_channel()`

    - pos_act -- [in] Action on posedge signal

    - neg_act -- [in] Action on negedge signal

  Returns:

    - ESP_OK: Set edge action for PCNT channel successfully

    - ESP_ERR_INVALID_ARG: Set edge action for PCNT channel failed because of invalid argument

    - ESP_FAIL: Set edge action for PCNT channel failed because of other error

esp_err_t pcnt_channel_set_level_action(pcnt_channel_handle_t chan, pcnt_channel_level_action_t high_act, pcnt_channel_level_action_t low_act)

  Set channel actions when level signal changes (e.g. signal level goes from high to low). The level signal is input from the `level_gpio_num` configured in `pcnt_chan_config_t`. We use these actions to control when and how to change the counting mode.

  Parameters:

    - chan -- [in] PCNT channel handle created by `pcnt_new_channel()`

    - high_act -- [in] Action on high level signal

    - low_act -- [in] Action on low level signal

  Returns:

    - ESP_OK: Set level action for PCNT channel successfully

    - ESP_ERR_INVALID_ARG: Set level action for PCNT channel failed because of invalid argument

    - ESP_FAIL: Set level action for PCNT channel failed because of other error

### Structures

struct pcnt_watch_event_data_t

  PCNT watch event data.

  Public Members

  int watch_point_value

    Watch point value that triggered the event

  pcnt_unit_zero_cross_mode_t zero_cross_mode

    Zero cross mode

struct pcnt_event_callbacks_t

  Group of supported PCNT callbacks.

  Note

  The callbacks are all running under ISR environment

  Note

  When CONFIG_PCNT_ISR_IRAM_SAFE is enabled, the callback itself and functions callbed by it should be placed in IRAM.

  Public Members

  pcnt_watch_cb_t on_reach

    Called when PCNT unit counter reaches any watch point or step notify

struct pcnt_unit_config_t

  PCNT unit configuration.

  Public Members

  pcnt_clock_source_t clk_src

    Clock source for PCNT unit

  int low_limit

    Low limitation of the count unit, should be lower than 0

  int high_limit

    High limitation of the count unit, should be higher than 0

  int intr_priority

    PCNT interrupt priority, if set to 0, the driver will try to allocate an interrupt with a relative low priority (1,2,3)

  uint32_t accum_count

    Whether to accumulate the count value when overflows at the high/low limit

  uint32_t en_step_notify_up

    Enable step notify in the positive direction

  uint32_t en_step_notify_down

    Enable step notify in the negative direction

  struct pcnt_unit_config_t flags

    Extra flags

struct pcnt_chan_config_t

  PCNT channel configuration.

  Public Members

  int edge_gpio_num

    GPIO number used by the edge signal. Set to -1 if unused

  int level_gpio_num

    GPIO number used by the level signal. Set to -1 if unused

  uint32_t invert_edge_input

    Invert the input edge signal

  uint32_t invert_level_input

    Invert the input level signal

  uint32_t virt_edge_io_level

    Virtual edge IO level, 0: low, 1: high. Only valid when edge_gpio_num is set to -1

  uint32_t virt_level_io_level

    Virtual level IO level, 0: low, 1: high. Only valid when level_gpio_num is set to -1

  struct pcnt_chan_config_t flags

    Channel config flags

struct pcnt_glitch_filter_config_t

  PCNT glitch filter configuration.

  Public Members

  uint32_t max_glitch_ns

    Pulse width smaller than this threshold will be treated as glitch and ignored, in the unit of ns

### Macros

_pcnt_unit_remove_all_watch_step(unit)

_pcnt_unit_remove_single_watch_step(unit, step_interval)

_pcnt_get_remove_func(_1, _2, FUNC, ...)

pcnt_unit_remove_watch_step(...)

### Type Definitions

typedef struct pcnt_unit_t *pcnt_unit_handle_t

  Type of PCNT unit handle.

typedef struct pcnt_chan_t *pcnt_channel_handle_t

  Type of PCNT channel handle.

typedef bool (*pcnt_watch_cb_t)(pcnt_unit_handle_t unit, const pcnt_watch_event_data_t *edata, void *user_ctx)

  PCNT watch event callback prototype.

  Note

  The callback function is invoked from an ISR context, so it should meet the restrictions of not calling any blocking APIs when implementing the callback. e.g. must use ISR version of FreeRTOS APIs.

  Param unit:

    [in] PCNT unit handle

  Param edata:

    [in] PCNT event data, fed by the driver

  Param user_ctx:

    [in] User data, passed from `pcnt_unit_register_event_callbacks()`

  Return:

    Whether a high priority task has been woken up by this function

### Header File

- components/esp_hal_pcnt/include/hal/pcnt_types.h

- This header file can be included with:

  >     #include "hal/pcnt_types.h"

- This header file is a part of the API provided by the `esp_hal_pcnt` component. To declare that your component depends on `esp_hal_pcnt`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_hal_pcnt

  > or

  >     PRIV_REQUIRES esp_hal_pcnt

### Type Definitions

typedef int pcnt_clock_source_t

  Default type.

### Enumerations

enum pcnt_channel_level_action_t

  PCNT channel action on control level.

  Values:

  enumerator PCNT_CHANNEL_LEVEL_ACTION_KEEP

    Keep current count mode

  enumerator PCNT_CHANNEL_LEVEL_ACTION_INVERSE

    Invert current count mode (increase -> decrease, decrease -> increase)

  enumerator PCNT_CHANNEL_LEVEL_ACTION_HOLD

    Hold current count value

enum pcnt_channel_edge_action_t

  PCNT channel action on signal edge.

  Values:

  enumerator PCNT_CHANNEL_EDGE_ACTION_HOLD

    Hold current count value

  enumerator PCNT_CHANNEL_EDGE_ACTION_INCREASE

    Increase count value

  enumerator PCNT_CHANNEL_EDGE_ACTION_DECREASE

    Decrease count value

enum pcnt_unit_zero_cross_mode_t

  PCNT unit zero cross mode.

  Values:

  enumerator PCNT_UNIT_ZERO_CROSS_POS_ZERO

    start from positive value, end to zero, i.e. +N->0

  enumerator PCNT_UNIT_ZERO_CROSS_NEG_ZERO

    start from negative value, end to zero, i.e. -N->0

  enumerator PCNT_UNIT_ZERO_CROSS_NEG_POS

    start from negative value, end to positive value, i.e. -N->+M

  enumerator PCNT_UNIT_ZERO_CROSS_POS_NEG

    start from positive value, end to negative value, i.e. +N->-M

  enumerator PCNT_UNIT_ZERO_CROSS_INVALID

    invalid zero cross mode

enum pcnt_step_direction_t

  PCNT step direction.

  Values:

  enumerator PCNT_STEP_FORWARD

    step forward, e.g., [N]->[N+1]->[N+2]->...

  enumerator PCNT_STEP_BACKWARD

    step backward, e.g., [N]->[N-1]->[N-2]->...

[1]

Different ESP chip series might have different number of PCNT units and channels. Please refer to the [TRM] for details. The driver does not forbid you from applying for more PCNT units and channels, but it returns error when all available hardware resources are used up. Please always check the return value when doing resource allocation (e.g., `pcnt_new_unit()`).

[2]

`pcnt_event_callbacks_t::on_reach` callback and the functions invoked by itself should also be placed in IRAM, you need to take care of them by themselves.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.