# I2C Interfaced LCD

[中文]

1. Create I2C bus. Please refer to I2C API doc for more details.

   >     i2c_master_bus_handle_t i2c_bus = NULL;
   >     i2c_master_bus_config_t bus_config = {
   >         .clk_source = I2C_CLK_SRC_DEFAULT,
   >         .glitch_ignore_cnt = 7,
   >         .i2c_port = I2C_BUS_PORT,
   >         .sda_io_num = EXAMPLE_PIN_NUM_SDA,
   >         .scl_io_num = EXAMPLE_PIN_NUM_SCL,
   >         .flags.enable_internal_pullup = true,
   >     };
   >     ESP_ERROR_CHECK(i2c_new_master_bus(&bus_config, &i2c_bus));

2. Allocate an LCD IO device handle from the I2C bus. In this step, you need to provide the following information:

   > - `esp_lcd_panel_io_i2c_config_t::dev_addr` sets the I2C device address of the LCD controller chip. The LCD driver uses this address to communicate with the LCD controller chip.

   > - `esp_lcd_panel_io_i2c_config_t::scl_speed_hz` sets the I2C clock frequency in Hz. The value should not exceed the range recommended in the LCD spec.

   > - `esp_lcd_panel_io_i2c_config_t::lcd_cmd_bits` and `esp_lcd_panel_io_i2c_config_t::lcd_param_bits` set the bit width of the command and parameter recognized by the LCD controller chip. This is chip specific, you should refer to your LCD spec in advance.

   >     esp_lcd_panel_io_handle_t io_handle = NULL;
   >     esp_lcd_panel_io_i2c_config_t io_config = {
   >         .dev_addr = EXAMPLE_I2C_HW_ADDR,
   >         .scl_speed_hz = EXAMPLE_LCD_PIXEL_CLOCK_HZ,
   >         .control_phase_bytes = 1, // refer to LCD spec
   >         .dc_bit_offset = 6,       // refer to LCD spec
   >         .lcd_cmd_bits = EXAMPLE_LCD_CMD_BITS,
   >         .lcd_param_bits = EXAMPLE_LCD_CMD_BITS,
   >     };
   >     ESP_ERROR_CHECK(esp_lcd_new_panel_io_i2c(i2c_bus, &io_config, &io_handle));

3. Install the LCD controller driver. The LCD controller driver is responsible for sending the commands and parameters to the LCD controller chip. In this step, you need to specify the I2C IO device handle that allocated in the last step, and some panel specific configurations:

   > - `esp_lcd_panel_dev_config_t::reset_gpio_num` sets the LCD's hardware reset GPIO number. If the LCD does not have a hardware reset pin, set this to `-1`.

   > - `esp_lcd_panel_dev_config_t::bits_per_pixel` sets the bit width of the pixel color data. The LCD driver uses this value to calculate the number of bytes to send to the LCD controller chip.

   >     esp_lcd_panel_handle_t panel_handle = NULL;
   >     esp_lcd_panel_dev_config_t panel_config = {
   >         .bits_per_pixel = 1,
   >         .reset_gpio_num = EXAMPLE_PIN_NUM_RST,
   >     };
   >     ESP_ERROR_CHECK(esp_lcd_new_panel_ssd1306(io_handle, &panel_config, &panel_handle));

## API Reference

### Header File

- components/esp_lcd/include/esp_lcd_io_i2c.h

- This header file can be included with:

  >     #include "esp_lcd_io_i2c.h"

- This header file is a part of the API provided by the `esp_lcd` component. To declare that your component depends on `esp_lcd`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_lcd

  > or

  >     PRIV_REQUIRES esp_lcd

### Functions

esp_err_t esp_lcd_new_panel_io_i2c(i2c_master_bus_handle_t bus, const esp_lcd_panel_io_i2c_config_t *io_config, esp_lcd_panel_io_handle_t *ret_io)

  Create LCD panel IO handle, for I2C interface in new implementation.

  Note

  Please don't call this function in your project directly. Please call `esp_lcd_new_panel_to_i2c` instead.

  Parameters:

    - bus -- [in] I2C bus handle, (in i2c_master_dev_handle_t)

    - io_config -- [in] IO configuration, for I2C interface

    - ret_io -- [out] Returned IO handle

  Returns:

    - ESP_ERR_INVALID_ARG if parameter is invalid

    - ESP_ERR_NO_MEM if out of memory

    - ESP_OK on success

### Structures

struct esp_lcd_panel_io_i2c_config_t

  Panel IO configuration structure, for I2C interface.

  Public Members

  uint32_t dev_addr

    I2C device address

  uint32_t scl_speed_hz

    I2C LCD SCL frequency (hz)

  size_t control_phase_bytes

    I2C LCD panel will encode control information (e.g. D/C selection) into control phase, in several bytes

  uint8_t dc_bit_offset

    Offset of the D/C selection bit in control phase

  int lcd_cmd_bits

    Bit-width of LCD command

  int lcd_param_bits

    Bit-width of LCD parameter

  esp_lcd_panel_io_color_trans_done_cb_t on_color_trans_done

    Callback invoked when color data transfer has finished

  void *user_ctx

    User private data, passed directly to on_color_trans_done's user_ctx

  unsigned int dc_low_on_data

    If this flag is enabled, DC line = 0 means transfer data, DC line = 1 means transfer command; vice versa

  unsigned int disable_control_phase

    If this flag is enabled, the control phase isn't used

  struct esp_lcd_panel_io_i2c_config_t flags

    Extra flags to fine-tune the I2C device

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.