警告

This document is not updated for ESP32H4 yet, so some of the content may not be correct.

This warning was automatically inserted due to the source file being in the add_warnings_pages list.

# Bluetooth® Device APIs

## Overview

Bluetooth device reference APIs.

## API Reference

### Header File

- components/bt/host/bluedroid/api/include/api/esp_bt_device.h

- This header file can be included with:

  >     #include "esp_bt_device.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_bt_dev_register_callback(esp_bt_dev_cb_t callback)

  register callback function. This function should be called after esp_bluedroid_enable() completes successfully

  返回:

    - ESP_OK : Succeed

    - ESP_FAIL: others

const uint8_t *esp_bt_dev_get_address(void)

  Get bluetooth device address. Must use after "esp_bluedroid_enable".

  返回:

    bluetooth device address (six bytes), or NULL if bluetooth stack is not enabled

esp_err_t esp_bt_dev_coex_status_config(esp_bt_dev_coex_type_t type, esp_bt_dev_coex_op_t op, uint8_t status)

  Config bluetooth device coexis status. This function should be called after esp_bluedroid_enable() completes successfully.

  参数:

    - type -- [in] : coexist type to operate on

    - op -- [in] : clear or set coexist status

    - status -- [in] : coexist status to be configured

  返回:

    - ESP_OK : Succeed

    - ESP_ERR_INVALID_ARG : if name is NULL pointer or empty, or string length out of limit

    - ESP_ERR_INVALID_STATE : if bluetooth stack is not yet enabled

    - ESP_FAIL : others

esp_err_t esp_bt_config_file_path_get(char *file_path)

  This function is used to get the path name of the Bluetooth bond keys saved in the NVS module.

  参数:

    file_path -- [out] buffer to store the config file path, max length NVS_KEY_NAME_MAX_SIZE

  返回:

    - ESP_OK: success

esp_err_t esp_bt_config_file_path_update(const char *file_path)

  This function is used to update the path name of bluetooth bond keys saved in the NVS module and need to be called before esp_bluedroid_init_with_cfg().

  参数:

    file_path -- [in] the name of config file path, the length of file_path should be less than NVS_NS_NAME_MAX_SIZE

  返回:

    - ESP_OK: success

    - other: failed

### Unions

union esp_bt_dev_cb_param_t
  #include <esp_bt_device.h>

  BT device callback parameters.

  Public Members

  struct esp_bt_dev_cb_param_t::name_res_param name_res

    discovery result parameter struct

  struct name_res_param
    #include <esp_bt_device.h>

    ESP_BT_DEV_NAME_RES_EVT.

    Public Members

    esp_bt_status_t status

      Status of getting device name

    char *name

      Name of Bluetooth device

### Macros

ESP_BT_DEV_COEX_BLE_ST_MESH_CONFIG

ESP_BT_DEV_COEX_BLE_ST_MESH_TRAFFIC

ESP_BT_DEV_COEX_BLE_ST_MESH_STANDBY

ESP_BT_DEV_COEX_BT_ST_A2DP_STREAMING

ESP_BT_DEV_COEX_BT_ST_A2DP_PAUSED

ESP_BT_DEV_COEX_OP_CLEAR

ESP_BT_DEV_COEX_OP_SET

### Type Definitions

typedef uint8_t esp_bt_dev_coex_op_t

typedef void (*esp_bt_dev_cb_t)(esp_bt_dev_cb_event_t event, esp_bt_dev_cb_param_t *param)

  bluetooth device callback function type

  Param event:

    : Event type

  Param param:

    : Pointer to callback parameter

### Enumerations

enum esp_bt_dev_coex_type_t

  Bluetooth device coex type.

  Values:

  enumerator ESP_BT_DEV_COEX_TYPE_BLE
  enumerator ESP_BT_DEV_COEX_TYPE_BT

enum esp_bt_dev_cb_event_t

  BT device callback events.

  Values:

  enumerator ESP_BT_DEV_NAME_RES_EVT

    Device name result event

  enumerator ESP_BT_DEV_EVT_MAX

此文档对您有帮助吗？

- 反馈已收到，谢谢！
- 如果您有其他意见，欢迎填写乐鑫文档反馈表。

- 我们重视您的反馈。
- 您可以填写乐鑫文档反馈表告诉我们如何改进该文档。