# LCD

[English]

## 简介

ESP 系列芯片可以发出市场上常见的 LCD（如 SPI LCD、I2C LCD、并行 LCD (Intel 8080)、RGB/SRGB LCD、MIPI DSI LCD 等）所需的各种时序。`esp_lcd` 组件为上述各类 LCD 提供了一个统一的抽象驱动框架。

LCD 通常由两个主要平面组成：

- 控制平面：通过该平面，可以读取、写入 LCD 设备控制器的内部寄存器。主机通常使用该平面来初始化 LCD 电源或进行伽玛校正等。

- 数据平面：数据平面负责向 LCD 设备传输像素数据。

## 功能概述

在 `esp_lcd` 的上下文中，数据平面和控制平面都由 `esp_lcd_panel_handle_t` 数据类型表示。

在某些 LCD 中，上述两个平面可能会合并为一个平面。此时，像素数据通过控制平面传输，实现类似数据平面的功能。这在 SPI LCD 和 I2C LCD 中很常见。

此外，还有一些 LCD 不需要单独的控制平面。例如，某些 RGB LCD 在上电后会自动执行必要的初始化过程，主机只需通过数据平面不断刷新像素数据即可。但要注意，并非所有 RGB LCD 都完全不需要控制平面。部分 LCD 设备同时支持多种接口，需要主机通过控制平面（例如基于 SPI 接口）发送特定命令以启用 RGB 模式。

本文将讨论如何为不同类型的 LCD 创建控制平面和数据平面。

- SPI 接口的 LCD
- I2C 接口的 LCD
- 并行 IO 模拟 SPI 或 I80 接口的 LCD

备注

ESP-IDF 仓库中自带的 LCD 设备控制器驱动程序数量有限（例如，ST7789 驱动程序是开箱即用的）。更多驱动程序可通过 乐鑫组件注册表 获取。

## LCD 控制面板操作

- `esp_lcd_panel_reset()` 可以重置 LCD 控制面板。

- `esp_lcd_panel_init()` 执行基本的控制面板初始化。有关特定制造商的初始化设置，请参阅 添加特定制造商的初始化设置。

- 通过组合使用 `esp_lcd_panel_swap_xy()` 和 `esp_lcd_panel_mirror()`，可以实现 LCD 屏幕旋转和 LCD 屏幕镜像功能。

- `esp_lcd_panel_disp_on_off()` 可以通过切断从帧 buffer 到 LCD 屏幕的输出路径来打开或关闭 LCD 屏幕。请注意，这与控制 LCD 背光不同，`esp_lcd` 驱动程序无法控制 LCD 背光。

- `esp_lcd_panel_disp_sleep()` 可以通过进入睡眠模式减少 LCD 屏幕的功耗，而内部的帧 buffer 仍然保留。

## LCD 数据面板操作

- `esp_lcd_panel_reset()` 可以重置 LCD 数据面板。

- `esp_lcd_panel_init()` 执行基本的数据面板初始化。

- `esp_lcd_panel_draw_bitmap()` 可以将绘制 buffer 刷新到 LCD 屏幕上，其中目标绘制窗口是可配置的。请注意，使用该函数需要确保绘制 buffer 是一维数组，且每行像素数据之间没有跨距。

- `esp_lcd_panel_draw_bitmap_2d()` 可以绘制部分位图到 LCD 屏幕上，源窗口和目标绘制窗口都是可配置的。请注意，此时绘制 buffer 可以是二维数组，也可以是每行像素数据之间没有跨距的一维数组。

## 高级帧 Buffer 调试

对于高级调试场景，ESP-IDF 可以在 GDB 会话中加载 `idf-drivers-gdb` Python 包。该包提供 `framebuffer_display` 命令，可以从目标芯片读取 LCD 帧 buffer 内存，并在主机侧渲染。

当屏幕显示不符合预期时，该命令可用于判断帧 buffer 内容本身是否已经异常，或者问题是否更可能来自 LCD 接口时序、GPIO 路由、面板初始化或颜色格式配置。

有关安装方式、支持的像素格式、命令语法、示例和排障建议，请参阅 idf-drivers-gdb 包文档。

## 添加特定制造商的初始化设置

在 ESP-IDF 中，LCD 控制器驱动程序（例如 st7789）在函数 `esp_lcd_panel_init()` 中只提供了基本的控制面板初始化设置，大部分设置使用默认值。部分 LCD 模组需要进行一系列特定制造商的配置（通常包含伽玛配置、电压配置等）才能正常显示。若想添加特定制造商的初始化设置，请参照以下步骤：

    esp_lcd_panel_reset(panel_handle);
    esp_lcd_panel_init(panel_handle);
    // 进行额外的配置，例如伽玛控制
    // 使用底层 IO 句柄
    // 请咨询制造商来获取特殊命令和相应的值
    esp_lcd_panel_io_tx_param(io_handle, GAMMA_CMD, (uint8_t[]) {
           GAMMA_ARRAY
        }, N);
    // 打开显示屏
    esp_lcd_panel_disp_on_off(panel_handle, true);

## 应用示例

- peripherals/lcd/tjpgd 演示了如何解码 JPEG 图像并在 SPI 接口的 LCD 上显示图像，同时周期性地旋转图像。

- peripherals/lcd/spi_lcd_touch 演示了如何在相同的 SPI 总线上驱动 LCD 和触摸面板，并使用 LVGL 库显示简单的图形用户界面。

- peripherals/lcd/i2c_oled 演示了如何使用 esp_lcd 组件中的 SSD1306 面板驱动来简化移植 LVGL 库，并在 OLED 屏幕上显示滚动文本。

- peripherals/lcd/parlio_simulate 演示了如何使用 Parallel IO 外设驱动 SPI 或 I80 接口的屏幕。

## API 参考

### Header File

- components/esp_hal_lcd/include/hal/lcd_types.h

- This header file can be included with:

  >     #include "hal/lcd_types.h"

- This header file is a part of the API provided by the `esp_hal_lcd` component. To declare that your component depends on `esp_hal_lcd`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_hal_lcd

  > or

  >     PRIV_REQUIRES esp_hal_lcd

### Type Definitions

typedef int lcd_clock_source_t

### Enumerations

enum lcd_rgb_data_endian_t

  RGB data endian.

  Values:

  enumerator LCD_RGB_DATA_ENDIAN_BIG

    RGB data endian: MSB first

  enumerator LCD_RGB_DATA_ENDIAN_LITTLE

    RGB data endian: LSB first

enum lcd_color_format_t

  LCD color type, in FourCC format.

  Values:

  enumerator LCD_COLOR_FMT_GRAY8

    8-bit gray scale

  enumerator LCD_COLOR_FMT_RGB565

    RGB565.

  enumerator LCD_COLOR_FMT_RGB888

    RGB888.

  enumerator LCD_COLOR_FMT_YUV422_YUYV

    YUV422 packed in YUYV order.

  enumerator LCD_COLOR_FMT_YUV422_YVYU

    YUV422 packed in YVYU order.

  enumerator LCD_COLOR_FMT_YUV422_VYUY

    YUV422 packed in VYUY order.

  enumerator LCD_COLOR_FMT_YUV422_UYVY

    YUV422 packed in UYVY order.

  enumerator LCD_COLOR_FMT_YUV420_OUYY_EVYY

    YUV420 packed in OUYY/EVYY order.

enum lcd_color_range_t

  LCD color range.

  Values:

  enumerator LCD_COLOR_RANGE_LIMIT

    Limited color range

  enumerator LCD_COLOR_RANGE_FULL

    Full color range

enum lcd_yuv_conv_std_t

  The standard used for conversion between RGB and YUV.

  Values:

  enumerator LCD_YUV_CONV_STD_BT601

    YUV<->RGB conversion standard: BT.601

  enumerator LCD_YUV_CONV_STD_BT709

    YUV<->RGB conversion standard: BT.709

### Header File

- components/esp_lcd/include/esp_lcd_types.h

- This header file can be included with:

  >     #include "esp_lcd_types.h"

- This header file is a part of the API provided by the `esp_lcd` component. To declare that your component depends on `esp_lcd`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_lcd

  > or

  >     PRIV_REQUIRES esp_lcd

### Structures

struct esp_lcd_video_timing_t

  Timing parameters for the video data transmission.

  Public Members

  uint32_t h_size

    Horizontal resolution, i.e. the number of pixels in a line

  uint32_t v_size

    Vertical resolution, i.e. the number of lines in the frame

  uint32_t hsync_pulse_width

    Horizontal sync width, in pixel clock

  uint32_t hsync_back_porch

    Horizontal back porch, number of pixel clock between hsync and start of line active data

  uint32_t hsync_front_porch

    Horizontal front porch, number of pixel clock between the end of active data and the next hsync

  uint32_t vsync_pulse_width

    Vertical sync width, in number of lines

  uint32_t vsync_back_porch

    Vertical back porch, number of invalid lines between vsync and start of frame

  uint32_t vsync_front_porch

    Vertical front porch, number of invalid lines between the end of frame and the next vsync

struct esp_lcd_panel_io_event_data_t

  Type of LCD panel IO event data.

struct esp_lcd_panel_io_callbacks_t

  Type of LCD panel IO callbacks.

  Public Members

  esp_lcd_panel_io_color_trans_done_cb_t on_color_trans_done

    Callback invoked when color data transfer has finished

struct esp_lcd_color_conv_yuv_config_t

  Configuration of LCD color conversion: YUV <-> RGB.

  Public Members

  lcd_color_range_t in_color_range

    Color range of the input color

  lcd_color_range_t out_color_range

    Color range of the output color

  lcd_yuv_conv_std_t conv_std

    YUV conversion standard: BT601, BT709

struct esp_lcd_draw_bitmap_hook_data_t

  Type of draw bitmap hook data.

  Public Members

  void *dst_data

    Destination buffer (usually frame buffer)

  int dst_x_size

    Destination bitmap width

  int dst_y_size

    Destination bitmap height

  int dst_x_start

    Destination start x coordinate

  int dst_y_start

    Destination start y coordinate

  int dst_x_end

    Destination end x coordinate (exclusive)

  int dst_y_end

    Destination end y coordinate (exclusive)

  const void *src_data

    Source bitmap data

  int src_x_size

    Source bitmap width

  int src_y_size

    Source bitmap height

  int src_x_start

    Source start x coordinate

  int src_y_start

    Source start y coordinate

  int src_x_end

    Source end x coordinate (exclusive)

  int src_y_end

    Source end y coordinate (exclusive)

  int bits_per_pixel

    Bits per pixel

  bool (*on_hook_end)(esp_lcd_panel_handle_t panel)

    Callback to be invoked by an asynchronous hook after the custom draw operation completes. This notifies the panel driver to finish the draw transaction. If a color transfer done callback has been registered, it also invokes that callback

struct esp_lcd_panel_hooks_t

  Type of LCD panel hooks.

  Public Members

  esp_lcd_panel_draw_bitmap_hook_t draw_bitmap_hook

    Draw bitmap hook function

### Type Definitions

typedef struct esp_lcd_panel_io_t *esp_lcd_panel_io_handle_t

  Type of LCD panel IO handle

typedef struct esp_lcd_panel_t *esp_lcd_panel_handle_t

  Type of LCD panel handle

typedef bool (*esp_lcd_panel_io_color_trans_done_cb_t)(esp_lcd_panel_io_handle_t panel_io, esp_lcd_panel_io_event_data_t *edata, void *user_ctx)

  Declare the prototype of the function that will be invoked when panel IO finishes transferring color data.

  Param panel_io:

    [in] LCD panel IO handle, which is created by factory API like `esp_lcd_new_panel_io_spi()`

  Param edata:

    [in] Panel IO event data, fed by driver

  Param user_ctx:

    [in] User data, passed from `esp_lcd_panel_io_xxx_config_t`

  Return:

    Whether a high priority task has been waken up by this function

typedef esp_err_t (*esp_lcd_panel_draw_bitmap_hook_t)(esp_lcd_panel_handle_t panel, const esp_lcd_draw_bitmap_hook_data_t *hook_data, void *hook_ctx)

  draw bitmap hook function type for custom pixel processing operations

  This hook allows users to implement custom operations like scaling, rotation, color space conversion, etc. using hardware accelerators like PPA or DMA2D.

  备注

  For asynchronous operations, the hook should call hook_data->on_hook_end() after the operation is complete. The panel driver does not wait for a previous draw to finish; the hook must handle synchronization itself. The simplest approach is to serialize draws. To queue multiple transactions (e.g. via PPA), keep per-transaction hook_data, keep source buffers valid until completion, and handle overlapping destinations carefully.

  Param panel:

    [in] LCD panel handle

  Param hook_data:

    [in] Hook data

  Param hook_ctx:

    [in] Hook context

  Return:

    - ESP_OK on success

    - Other error codes on failure

### Enumerations

enum lcd_rgb_element_order_t

  RGB element order.

  Values:

  enumerator LCD_RGB_ELEMENT_ORDER_RGB

    RGB element order: RGB

  enumerator LCD_RGB_ELEMENT_ORDER_BGR

    RGB element order: BGR

### Header File

- components/esp_lcd/include/esp_lcd_panel_io.h

- This header file can be included with:

  >     #include "esp_lcd_panel_io.h"

- This header file is a part of the API provided by the `esp_lcd` component. To declare that your component depends on `esp_lcd`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_lcd

  > or

  >     PRIV_REQUIRES esp_lcd

### Functions

esp_err_t esp_lcd_panel_io_rx_param(esp_lcd_panel_io_handle_t io, int lcd_cmd, void *param, size_t param_size)

  Transmit LCD command and receive corresponding parameters.

  备注

  Commands sent by this function are short, so they are sent using polling transactions. The function does not return before the command transfer is completed. If any queued transactions sent by `esp_lcd_panel_io_tx_color()` are still pending when this function is called, this function will wait until they are finished and the queue is empty before sending the command(s).

  参数:

    - io -- [in] LCD panel IO handle, which is created by other factory API like `esp_lcd_new_panel_io_spi()`

    - lcd_cmd -- [in] The specific LCD command, set to -1 if no command needed

    - param -- [out] Buffer for the command data

    - param_size -- [in] Size of `param` buffer

  返回:

    - ESP_ERR_INVALID_ARG if parameter is invalid

    - ESP_ERR_NOT_SUPPORTED if read is not supported by transport

    - ESP_OK on success

esp_err_t esp_lcd_panel_io_tx_param(esp_lcd_panel_io_handle_t io, int lcd_cmd, const void *param, size_t param_size)

  Transmit LCD command and corresponding parameters.

  备注

  Commands sent by this function are short, so they are sent using polling transactions. The function does not return before the command transfer is completed. If any queued transactions sent by `esp_lcd_panel_io_tx_color()` are still pending when this function is called, this function will wait until they are finished and the queue is empty before sending the command(s).

  参数:

    - io -- [in] LCD panel IO handle, which is created by other factory API like `esp_lcd_new_panel_io_spi()`

    - lcd_cmd -- [in] The specific LCD command, set to -1 if no command needed

    - param -- [in] Buffer that holds the command specific parameters, set to NULL if no parameter is needed for the command

    - param_size -- [in] Size of `param` in memory, in bytes, set to zero if no parameter is needed for the command

  返回:

    - ESP_ERR_INVALID_ARG if parameter is invalid

    - ESP_OK on success

esp_err_t esp_lcd_panel_io_tx_color(esp_lcd_panel_io_handle_t io, int lcd_cmd, const void *color, size_t color_size)

  Transmit LCD RGB data.

  备注

  This function will package the command and RGB data into a transaction, and push into a queue. The real transmission is performed in the background (DMA+interrupt). The caller should take care of the lifecycle of the `color` buffer. Recycling of color buffer should be done in the callback `on_color_trans_done()`.

  参数:

    - io -- [in] LCD panel IO handle, which is created by factory API like `esp_lcd_new_panel_io_spi()`

    - lcd_cmd -- [in] The specific LCD command, set to -1 if no command needed

    - color -- [in] Buffer that holds the RGB color data

    - color_size -- [in] Size of `color` in memory, in bytes

  返回:

    - ESP_ERR_INVALID_ARG if parameter is invalid

    - ESP_OK on success

esp_err_t esp_lcd_panel_io_del(esp_lcd_panel_io_handle_t io)

  Destroy LCD panel IO handle (deinitialize panel and free all corresponding resource)

  参数:

    io -- [in] LCD panel IO handle, which is created by factory API like `esp_lcd_new_panel_io_spi()`

  返回:

    - ESP_ERR_INVALID_ARG if parameter is invalid

    - ESP_OK on success

esp_err_t esp_lcd_panel_io_register_event_callbacks(esp_lcd_panel_io_handle_t io, const esp_lcd_panel_io_callbacks_t *cbs, void *user_ctx)

  Register LCD panel IO callbacks.

  参数:

    - io -- [in] LCD panel IO handle, which is created by factory API like `esp_lcd_new_panel_io_spi()`

    - cbs -- [in] structure with all LCD panel IO callbacks

    - user_ctx -- [in] User private data, passed directly to callback's user_ctx

  返回:

    - ESP_ERR_INVALID_ARG if parameter is invalid

    - ESP_OK on success

### Header File

- components/esp_lcd/include/esp_lcd_panel_ops.h

- This header file can be included with:

  >     #include "esp_lcd_panel_ops.h"

- This header file is a part of the API provided by the `esp_lcd` component. To declare that your component depends on `esp_lcd`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_lcd

  > or

  >     PRIV_REQUIRES esp_lcd

### Functions

esp_err_t esp_lcd_panel_reset(esp_lcd_panel_handle_t panel)

  Reset LCD panel.

  备注

  Panel reset must be called before attempting to initialize the panel using `esp_lcd_panel_init()`.

  参数:

    panel -- [in] LCD panel handle, which is created by other factory API like `esp_lcd_new_panel_st7789()`

  返回:

    - ESP_OK on success

esp_err_t esp_lcd_panel_init(esp_lcd_panel_handle_t panel)

  Initialize LCD panel.

  备注

  Before calling this function, make sure the LCD panel has finished the `reset` stage by `esp_lcd_panel_reset()`.

  参数:

    panel -- [in] LCD panel handle, which is created by other factory API like `esp_lcd_new_panel_st7789()`

  返回:

    - ESP_OK on success

esp_err_t esp_lcd_panel_del(esp_lcd_panel_handle_t panel)

  Deinitialize the LCD panel.

  参数:

    panel -- [in] LCD panel handle, which is created by other factory API like `esp_lcd_new_panel_st7789()`

  返回:

    - ESP_OK on success

esp_err_t esp_lcd_panel_draw_bitmap(esp_lcd_panel_handle_t panel, int x_start, int y_start, int x_end, int y_end, const void *color_data)

  Draw bitmap on LCD panel.

  参数:

    - panel -- [in] LCD panel handle, which is created by other factory API like `esp_lcd_new_panel_st7789()`

    - x_start -- [in] Start pixel index in the target frame buffer, on x-axis (x_start is included)

    - y_start -- [in] Start pixel index in the target frame buffer, on y-axis (y_start is included)

    - x_end -- [in] End pixel index in the target frame buffer, on x-axis (x_end is not included)

    - y_end -- [in] End pixel index in the target frame buffer, on y-axis (y_end is not included)

    - color_data -- [in] RGB color data that will be dumped to the specific window range

  返回:

    - ESP_OK on success

esp_err_t esp_lcd_panel_draw_bitmap_2d(esp_lcd_panel_handle_t panel, int x_start, int y_start, int x_end, int y_end, const void *color_data, size_t src_x_size, size_t src_y_size, int src_x_start, int src_y_start, int src_x_end, int src_y_end)

  Draw partial source bitmap on LCD panel.

  This function allows drawing a portion of a source bitmap to a specific area on the LCD panel.

  参数:

    - panel -- [in] LCD panel handle, which is created by other factory API like `esp_lcd_new_panel_st7789()`

    - x_start -- [in] Start pixel index in the target frame buffer, on x-axis (x_start is included)

    - y_start -- [in] Start pixel index in the target frame buffer, on y-axis (y_start is included)

    - x_end -- [in] End pixel index in the target frame buffer, on x-axis (x_end is not included)

    - y_end -- [in] End pixel index in the target frame buffer, on y-axis (y_end is not included)

    - color_data -- [in] Source bitmap data

    - src_x_size -- [in] Size of the source bitmap in the x-axis

    - src_y_size -- [in] Size of the source bitmap in the y-axis

    - src_x_start -- [in] Start pixel index in the source bitmap, on x-axis (src_x_start is included)

    - src_y_start -- [in] Start pixel index in the source bitmap, on y-axis (src_y_start is included)

    - src_x_end -- [in] End pixel index in the source bitmap, on x-axis (src_x_end is not included)

    - src_y_end -- [in] End pixel index in the source bitmap, on y-axis (src_y_end is not included)

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if parameters are invalid

    - ESP_ERR_NOT_SUPPORTED if this function is not supported by the panel

esp_err_t esp_lcd_panel_mirror(esp_lcd_panel_handle_t panel, bool mirror_x, bool mirror_y)

  Mirror the LCD panel on specific axis.

  备注

  Combined with `esp_lcd_panel_swap_xy()`, one can realize screen rotation

  参数:

    - panel -- [in] LCD panel handle, which is created by other factory API like `esp_lcd_new_panel_st7789()`

    - mirror_x -- [in] Whether the panel will be mirrored about the x axis

    - mirror_y -- [in] Whether the panel will be mirrored about the y axis

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_SUPPORTED if this function is not supported by the panel

esp_err_t esp_lcd_panel_swap_xy(esp_lcd_panel_handle_t panel, bool swap_axes)

  Swap/Exchange x and y axis.

  备注

  Combined with `esp_lcd_panel_mirror()`, one can realize screen rotation

  参数:

    - panel -- [in] LCD panel handle, which is created by other factory API like `esp_lcd_new_panel_st7789()`

    - swap_axes -- [in] Whether to swap the x and y axis

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_SUPPORTED if this function is not supported by the panel

esp_err_t esp_lcd_panel_set_gap(esp_lcd_panel_handle_t panel, int x_gap, int y_gap)

  Set extra gap in x and y axis.

  The gap is the space (in pixels) between the left/top sides of the LCD panel and the first row/column respectively of the actual contents displayed.

  备注

  Setting a gap is useful when positioning or centering a frame that is smaller than the LCD.

  参数:

    - panel -- [in] LCD panel handle, which is created by other factory API like `esp_lcd_new_panel_st7789()`

    - x_gap -- [in] Extra gap on x axis, in pixels

    - y_gap -- [in] Extra gap on y axis, in pixels

  返回:

    - ESP_OK on success

esp_err_t esp_lcd_panel_invert_color(esp_lcd_panel_handle_t panel, bool invert_color_data)

  Invert the color (bit-wise invert the color data line)

  参数:

    - panel -- [in] LCD panel handle, which is created by other factory API like `esp_lcd_new_panel_st7789()`

    - invert_color_data -- [in] Whether to invert the color data

  返回:

    - ESP_OK on success

esp_err_t esp_lcd_panel_disp_on_off(esp_lcd_panel_handle_t panel, bool on_off)

  Turn on or off the display.

  参数:

    - panel -- [in] LCD panel handle, which is created by other factory API like `esp_lcd_new_panel_st7789()`

    - on_off -- [in] True to turns on display, False to turns off display

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_SUPPORTED if this function is not supported by the panel

esp_err_t esp_lcd_panel_disp_sleep(esp_lcd_panel_handle_t panel, bool sleep)

  Enter or exit sleep mode.

  参数:

    - panel -- [in] LCD panel handle, which is created by other factory API like `esp_lcd_new_panel_st7789()`

    - sleep -- [in] True to enter sleep mode, False to wake up

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_SUPPORTED if this function is not supported by the panel

esp_err_t esp_lcd_panel_set_brightness(esp_lcd_panel_handle_t panel, int brightness)

  Set the brightness of the display.

  参数:

    - panel -- [in] LCD panel handle, which is created by other factory API like `esp_lcd_new_panel_st7789()`

    - brightness -- [in] Brightness value (range depends on panel implementation, typically 0-255, 0-1023, or 0-100)

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_SUPPORTED if this function is not supported by the panel

### Header File

- components/esp_lcd/include/esp_lcd_panel_vendor.h

- This header file can be included with:

  >     #include "esp_lcd_panel_vendor.h"

- This header file is a part of the API provided by the `esp_lcd` component. To declare that your component depends on `esp_lcd`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_lcd

  > or

  >     PRIV_REQUIRES esp_lcd

此文档对您有帮助吗？

- 反馈已收到，谢谢！
- 如果您有其他意见，欢迎填写乐鑫文档反馈表。

- 我们重视您的反馈。
- 您可以填写乐鑫文档反馈表告诉我们如何改进该文档。