# 时钟树

[English]

ESP32-P4 的时钟子系统用于从一系列根时钟中提取并分配系统/模块时钟。时钟树驱动程序负责维护系统时钟的基本功能，并管理模块时钟间的复杂关系。

本文档首先介绍了根时钟和模块时钟，随后介绍了可供用户调用的时钟树 API，调用这些 API，可以监测模块时钟的运行状态。

## 简介

本节列出了 ESP32-P4 支持的根时钟和模块时钟的定义，这些定义通常用于驱动程序配置，有助于为外设选择合适的时钟源。

### 根时钟

根时钟会产生可靠的时钟信号，经各种门、复用器、分频器或倍频器传递，这些时钟信号最终成为 CPU 内核、Wi-Fi、蓝牙、RTC 及外设等功能模块的时钟源。

ESP32-P4 的根时钟列在 `soc_root_clk_t` 中：

> - 内部 17.5 MHz RC 振荡器 (RC_FAST)

>   > 此 RC 振荡器可产生约 17.5 MHz 的时钟信号输出，标识为 `RC_FAST_CLK`。

>   > 在运行时，通过校准，可以计算 `RC_FAST_CLK` 的实际频率。

> - 外部 40 MHz 晶振 (XTAL)

> - 内部 136 kHz RC 振荡器 (RC_SLOW)

>   > 此 RC 振荡器产生约 136 kHz 的时钟信号输出，标识为 `RC_SLOW_CLK`。在运行时，通过校准，可以计算该时钟信号的实际频率。

> - 外部 32 kHz 晶振 - 可选 (XTAL32K)

>   > `XTAL32K_CLK` 的时钟源是连接到 `XTAL_32K_P` 和 `XTAL_32K_N` 管脚的 32 kHz 晶振。

>   > 通过校准，可以计算 `XTAL32K_CLK` 的实际频率。

与晶振产生的信号相比，从 RC 振荡器电路产生的信号通常精度较低，且容易受环境影响。因此，ESP32-P4 为 `RTC_SLOW_CLK` 提供了几种时钟源选项，可以根据对系统时间精度和对功耗的要求选择。更多详情，请参阅 RTC 定时器时钟源。

### 模块时钟

ESP32-P4 的可用模块时钟在 `soc_module_clk_t` 中列出，每个模块时钟都有其唯一 ID。查阅文档中的枚举值，即可获取各模块时钟的详细信息。

## 使用 API

时钟树驱动程序提供了一个一体化接口，可以获取模块时钟的频率，即 `esp_clk_tree_src_get_freq_hz()`。通过该函数，你可以在任何时刻，通过提供时钟名称 `soc_module_clk_t` 和指定返回频率值的精度级别 `esp_clk_tree_src_freq_precision_t`，获取时钟频率。

## API 参考

### Header File

- components/soc/esp32p4/include/soc/clk_tree_defs.h

- This header file can be included with:

  >     #include "soc/clk_tree_defs.h"

### Macros

SOC_CLK_RC_FAST_FREQ_APPROX

  Approximate RC_FAST_CLK frequency in Hz

SOC_CLK_RC_SLOW_FREQ_APPROX

  Approximate RC_SLOW_CLK frequency in Hz

SOC_CLK_RC32K_FREQ_APPROX

  Approximate RC32K_CLK frequency in Hz

SOC_CLK_XTAL32K_FREQ_APPROX

  Approximate XTAL32K_CLK frequency in Hz

SOC_GPTIMER_CLKS

  Array initializer for all supported clock sources of GPTimer.

  The following code can be used to iterate all possible clocks:

      soc_periph_gptimer_clk_src_t gptimer_clks[] = (soc_periph_gptimer_clk_src_t)SOC_GPTIMER_CLKS;
      for (size_t i = 0; i< sizeof(gptimer_clks) / sizeof(gptimer_clks[0]); i++) {
          soc_periph_gptimer_clk_src_t clk = gptimer_clks[i];
      // Test GPTimer with the clock `clk`
      }

SOC_RMT_CLKS

  Array initializer for all supported clock sources of RMT.

SOC_UART_CLKS

  Array initializer for all supported clock sources of UART.

SOC_LP_UART_CLKS

  Array initializer for all supported clock sources of LP_UART.

SOC_MCPWM_TIMER_CLKS

  Array initializer for all supported clock sources of MCPWM Timer.

SOC_MCPWM_CAPTURE_CLKS

  Array initializer for all supported clock sources of MCPWM Capture Timer.

SOC_MCPWM_CARRIER_CLKS

  Array initializer for all supported clock sources of MCPWM Carrier.

SOC_I2S_CLKS

  Array initializer for all supported clock sources of I2S.

SOC_LP_I2S_CLKS

  Array initializer for all supported clock sources of LP I2S.

SOC_LCD_CLKS

  Array initializer for all supported clock sources of LCD.

SOC_CAM_CLKS

  Array initializer for all supported clock sources of CAM.

SOC_MIPI_CSI_PHY_CLKS

  Array initializer for all supported clock sources of MIPI CSI PHY interface.

SOC_MIPI_DSI_DPI_CLKS

  Array initializer for all supported clock sources of MIPI DSI DPI interface.

MIPI_DSI_PHY_CLK_SRC_RC_FAST

  For backward compatibility, old macro definitions are kept. Remove it in the next major release (esp-idf v7.0)

MIPI_DSI_PHY_CLK_SRC_PLL_F25M

MIPI_DSI_PHY_CLK_SRC_PLL_F20M

MIPI_DSI_PHY_CLK_SRC_DEFAULT

SOC_I2C_CLKS

  Array initializer for all supported clock sources of I2C.

SOC_LP_I2C_CLKS

  Array initializer for all supported clock sources of LP_I2C.

SOC_SPI_CLKS

  Array initializer for all supported clock sources of SPI.

SOC_PSRAM_CLKS

  Array initializer for all supported clock sources of PSRAM.

SOC_FLASH_CLKS

  Array initializer for all supported clock sources of FLASH.

SOC_ISP_CLKS

  Array initializer for all supported clock sources of ISP.

SOC_SDM_CLKS

  Array initializer for all supported clock sources of SDM.

SOC_GLITCH_FILTER_CLKS

  Array initializer for all supported clock sources of Glitch Filter.

SOC_ANA_CMPR_CLKS

  Array initializer for all supported clock sources of Analog Comparator.

SOC_TWAI_CLKS

  Array initializer for all supported clock sources of TWAI.

SOC_ADC_DIGI_CLKS

  Array initializer for all supported clock sources of ADC digital controller.

SOC_ADC_RTC_CLKS

  Array initializer for all supported clock sources of ADC RTC controller.

SOC_LP_ADC_CLKS

  Array initializer for all supported clock sources of LP_ADC.

SOC_MWDT_CLKS

  Array initializer for all supported clock sources of MWDT.

SOC_LEDC_CLKS

  Array initializer for all supported clock sources of LEDC.

SOC_PARLIO_CLKS

  Array initializer for all supported clock sources of PARLIO.

SOC_SDMMC_CLKS

  Array initializer for all supported clock sources of SDMMC.

SOC_TEMP_SENSOR_CLKS

  Array initializer for all supported clock sources of Temperature Sensor.

SOC_I3C_MASTER_CLKS

  Array initializer for all supported clock sources of I3C master.

SOC_EMAC_PTP_CLK

  Array initializer for all supported clock sources of EMAC PTP.

### Enumerations

enum soc_root_clk_t

  Root clock.

  Values:

  enumerator SOC_ROOT_CLK_INT_RC_FAST

    Internal 17.5MHz RC oscillator

  enumerator SOC_ROOT_CLK_INT_RC_SLOW

    Internal 136kHz RC oscillator

  enumerator SOC_ROOT_CLK_EXT_XTAL

    External 40MHz crystal

  enumerator SOC_ROOT_CLK_EXT_XTAL32K

    External 32kHz crystal

  enumerator SOC_ROOT_CLK_INT_RC32K

    Internal 32kHz RC oscillator

  enumerator SOC_ROOT_CLK_EXT_OSC_SLOW

    External slow clock signal at pin1

enum soc_cpu_clk_src_t

  CPU_CLK mux inputs, which are the supported clock sources for the CPU_CLK.

  备注

  Enum values are matched with the register field values on purpose

  Values:

  enumerator SOC_CPU_CLK_SRC_XTAL

    Select XTAL_CLK as CPU_CLK source

  enumerator SOC_CPU_CLK_SRC_CPLL

    Select CPLL_CLK as CPU_CLK source (CPLL_CLK is the output of 40MHz crystal oscillator frequency multiplier, can be 320/360/400MHz)

  enumerator SOC_CPU_CLK_SRC_PLL

    Alias name for `SOC_CPU_CLK_SRC_CPLL`

  enumerator SOC_CPU_CLK_SRC_RC_FAST

    Select RC_FAST_CLK as CPU_CLK source

  enumerator SOC_CPU_CLK_SRC_INVALID

    Invalid CPU_CLK source

enum soc_rtc_slow_clk_src_t

  RTC_SLOW_CLK mux inputs, which are the supported clock sources for the RTC_SLOW_CLK.

  备注

  Enum values are matched with the register field values on purpose

  Values:

  enumerator SOC_RTC_SLOW_CLK_SRC_RC_SLOW

    Select RC_SLOW_CLK as RTC_SLOW_CLK source

  enumerator SOC_RTC_SLOW_CLK_SRC_XTAL32K

    Select XTAL32K_CLK as RTC_SLOW_CLK source

  enumerator SOC_RTC_SLOW_CLK_SRC_RC32K

    Select RC32K_CLK as RTC_SLOW_CLK source

  enumerator SOC_RTC_SLOW_CLK_SRC_INVALID

    Invalid RTC_SLOW_CLK source

enum soc_rtc_fast_clk_src_t

  RTC_FAST_CLK mux inputs, which are the supported clock sources for the RTC_FAST_CLK.

  备注

  Enum values are matched with the register field values on purpose

  Values:

  enumerator SOC_RTC_FAST_CLK_SRC_RC_FAST

    Select RC_FAST_CLK as RTC_FAST_CLK source

  enumerator SOC_RTC_FAST_CLK_SRC_XTAL

    Select XTAL_CLK as RTC_FAST_CLK source

  enumerator SOC_RTC_FAST_CLK_SRC_LP_PLL

    Select LP_PLL_CLK as RTC_FAST_CLK source (LP_PLL_CLK is a 8MHz clock sourced from RC32K or XTAL32K)

  enumerator SOC_RTC_FAST_CLK_SRC_INVALID

    Invalid RTC_FAST_CLK source

  enumerator SOC_RTC_FAST_CLK_SRC_DEFAULT

    XTAL_CLK is the default clock source for RTC_FAST_CLK

  enumerator SOC_RTC_FAST_CLK_SRC_XTAL_DIV

    Alias name for `SOC_RTC_FAST_CLK_SRC_XTAL`

enum soc_lp_pll_clk_src_t

  LP_PLL_CLK mux inputs, which are the supported clock sources for the LP_PLL_CLK.

  备注

  Enum values are matched with the register field values on purpose

  Values:

  enumerator SOC_LP_PLL_CLK_SRC_RC32K

    Select RC32K_CLK as LP_PLL_CLK source

  enumerator SOC_LP_PLL_CLK_SRC_XTAL32K

    Select XTAL32K_CLK as LP_PLL_CLK source

  enumerator SOC_LP_PLL_CLK_SRC_INVALID

    Invalid LP_PLL_CLK source

enum soc_xtal_freq_t

  Possible main XTAL frequency options on the target.

  备注

  Enum values equal to the frequency value in MHz

  备注

  Not all frequency values listed here are supported in IDF. Please check SOC_XTAL_SUPPORT_XXX in soc_caps.h for the supported ones.

  Values:

  enumerator SOC_XTAL_FREQ_40M

    40MHz XTAL

enum soc_module_clk_t

  Supported clock sources for modules (CPU, peripherals, RTC, etc.)

  备注

  enum starts from 1, to save 0 for special purpose

  Values:

  enumerator SOC_MOD_CLK_CPU

    CPU_CLK can be sourced from XTAL, CPLL, or RC_FAST by configuring soc_cpu_clk_src_t

  enumerator SOC_MOD_CLK_RTC_FAST

    RTC_FAST_CLK can be sourced from XTAL, RC_FAST, or LP_PLL by configuring soc_rtc_fast_clk_src_t

  enumerator SOC_MOD_CLK_RTC_SLOW

    RTC_SLOW_CLK can be sourced from RC_SLOW, XTAL32K, or RC32K by configuring soc_rtc_slow_clk_src_t

  enumerator SOC_MOD_CLK_PLL_F20M

    PLL_F20M_CLK is derived from SPLL (clock gating + default divider 24), its default frequency is 20MHz

  enumerator SOC_MOD_CLK_PLL_F25M

    PLL_F25M_CLK is derived from MPLL (clock gating + configurable divider), it will have a frequency of 25MHz

  enumerator SOC_MOD_CLK_PLL_F50M

    PLL_F50M_CLK is derived from MPLL (clock gating + configurable divider 10), it will have a frequency of 50MHz

  enumerator SOC_MOD_CLK_PLL_F80M

    PLL_F80M_CLK is derived from SPLL (clock gating + default divider 6), its default frequency is 80MHz

  enumerator SOC_MOD_CLK_PLL_F160M

    PLL_F160M_CLK is derived from SPLL (clock gating + default divider 3), its default frequency is 160MHz

  enumerator SOC_MOD_CLK_PLL_F240M

    PLL_F240M_CLK is derived from SPLL (clock gating + default divider 2), its default frequency is 240MHz

  enumerator SOC_MOD_CLK_CPLL

    CPLL is from 40MHz XTAL oscillator frequency multipliers

  enumerator SOC_MOD_CLK_SPLL

    SPLL is from 40MHz XTAL oscillator frequency multipliers, its default frequency is 480MHz

  enumerator SOC_MOD_CLK_MPLL

    MPLL is from 40MHz XTAL oscillator frequency multipliers

  enumerator SOC_MOD_CLK_SDIO_PLL

    SDIO PLL is from 40MHz XTAL oscillator frequency multipliers, its default frequency is 200MHz

  enumerator SOC_MOD_CLK_XTAL32K

    XTAL32K_CLK comes from the external 32kHz crystal, passing a clock gating to the peripherals

  enumerator SOC_MOD_CLK_RC_FAST

    RC_FAST_CLK comes from the internal 20MHz rc oscillator, passing a clock gating to the peripherals

  enumerator SOC_MOD_CLK_XTAL

    XTAL_CLK comes from the external 40MHz crystal

  enumerator SOC_MOD_CLK_APLL

    Audio PLL is sourced from PLL, and its frequency is configurable through APLL configuration registers

  enumerator SOC_MOD_CLK_XTAL_D2

    XTAL_D2_CLK comes from the external 40MHz crystal, passing a div of 2 to the LP peripherals

  enumerator SOC_MOD_CLK_LP_PLL

    LP_PLL is from 32kHz XTAL oscillator frequency multipliers, it has a fixed frequency of 8MHz

  enumerator SOC_MOD_CLK_LP_DYN_FAST

    LP_DYN_FAST can be derived from RTC_SLOW_CLK or RTC_FAST_CLK depending on the chip’s power mode: Only in LP_SLEEP mode, select RTC_SLOW_CLK as the clock source; In other non-LP_SLEEP mode, select RTC_FAST_CLK as the clock source;

  enumerator SOC_MOD_CLK_LP_PERI

    LP_PERI_CLK is derived from LP_DYN_FAST (configurable divider)

  enumerator SOC_MOD_CLK_INVALID

    Indication of the end of the available module clock sources

enum soc_periph_systimer_clk_src_t

  Type of SYSTIMER clock source.

  Values:

  enumerator SYSTIMER_CLK_SRC_XTAL

    SYSTIMER source clock is XTAL

  enumerator SYSTIMER_CLK_SRC_RC_FAST

    SYSTIMER source clock is RC_FAST

  enumerator SYSTIMER_CLK_SRC_DEFAULT

    SYSTIMER source clock default choice is XTAL

enum soc_periph_gptimer_clk_src_t

  Type of GPTimer clock source.

  Values:

  enumerator GPTIMER_CLK_SRC_PLL_F80M

    Select PLL_F80M as the source clock

  enumerator GPTIMER_CLK_SRC_RC_FAST

    Select RC_FAST as the source clock

  enumerator GPTIMER_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator GPTIMER_CLK_SRC_DEFAULT

    Select PLL_F80M as the default choice

enum soc_periph_tg_clk_src_legacy_t

  Type of Timer Group clock source, reserved for the legacy timer group driver.

  Values:

  enumerator TIMER_SRC_CLK_PLL_F80M

    Timer group clock source is PLL_F80M

  enumerator TIMER_SRC_CLK_XTAL

    Timer group clock source is XTAL

  enumerator TIMER_SRC_CLK_DEFAULT

    Timer group clock source default choice is PLL_F80M

enum soc_periph_rmt_clk_src_t

  Type of RMT clock source.

  Values:

  enumerator RMT_CLK_SRC_PLL_F80M

    Select PLL_F80M as the source clock

  enumerator RMT_CLK_SRC_RC_FAST

    Select RC_FAST as the source clock

  enumerator RMT_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator RMT_CLK_SRC_DEFAULT

    Select PLL_F80M as the default choice

enum soc_periph_rmt_clk_src_legacy_t

  Type of RMT clock source, reserved for the legacy RMT driver.

  Values:

  enumerator RMT_BASECLK_PLL_F80M

    RMT source clock is PLL_F80M

  enumerator RMT_BASECLK_XTAL

    RMT source clock is XTAL

  enumerator RMT_BASECLK_DEFAULT

    RMT source clock default choice is PLL_F80M

enum soc_periph_uart_clk_src_legacy_t

  Type of UART clock source, reserved for the legacy UART driver.

  Values:

  enumerator UART_SCLK_PLL_F80M

    UART source clock is PLL_F80M

  enumerator UART_SCLK_RTC

    UART source clock is RC_FAST

  enumerator UART_SCLK_XTAL

    UART source clock is XTAL

  enumerator UART_SCLK_DEFAULT

    UART source clock default choice is PLL_F80M

enum soc_periph_lp_uart_clk_src_t

  Type of LP_UART clock source.

  Values:

  enumerator LP_UART_SCLK_LP_FAST

    LP_UART source clock is LP(RTC)_FAST

  enumerator LP_UART_SCLK_XTAL_D2

    LP_UART source clock is XTAL_D2

  enumerator LP_UART_SCLK_DEFAULT

    LP_UART source clock default choice is LP(RTC)_FAST

enum soc_periph_mcpwm_timer_clk_src_t

  Type of MCPWM timer clock source.

  Values:

  enumerator MCPWM_TIMER_CLK_SRC_PLL160M

    Select PLL_F160M as the source clock

  enumerator MCPWM_TIMER_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator MCPWM_TIMER_CLK_SRC_DEFAULT

    Select PLL_F160M as the default choice

enum soc_periph_mcpwm_capture_clk_src_t

  Type of MCPWM capture clock source.

  Values:

  enumerator MCPWM_CAPTURE_CLK_SRC_PLL160M

    Select PLL_F160M as the source clock

  enumerator MCPWM_CAPTURE_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator MCPWM_CAPTURE_CLK_SRC_DEFAULT

    Select PLL_F160M as the default choice

enum soc_periph_mcpwm_carrier_clk_src_t

  Type of MCPWM carrier clock source.

  Values:

  enumerator MCPWM_CARRIER_CLK_SRC_PLL160M

    Select PLL_F160M as the source clock

  enumerator MCPWM_CARRIER_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator MCPWM_CARRIER_CLK_SRC_DEFAULT

    Select PLL_F160M as the default choice

enum soc_periph_i2s_clk_src_t

  I2S clock source enum.

  Values:

  enumerator I2S_CLK_SRC_DEFAULT

    Auto select maximum clock source asdefault source clock

  enumerator I2S_CLK_SRC_PLL_160M

    Select PLL_F160M as the source clock (only supported on P4 hw_ver3)

  enumerator I2S_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator I2S_CLK_SRC_APLL

    Select APLL as the source clock

  enumerator I2S_CLK_SRC_EXTERNAL

    Select external clock as source clock

enum soc_periph_lp_i2s_clk_src_t

  LP I2S clock source enum.

  Values:

  enumerator LP_I2S_CLK_SRC_DEFAULT

    Select LP_PERI as the default source clock

  enumerator LP_I2S_CLK_SRC_LP_PERI

    Select LP_PERI as the source clock

  enumerator LP_I2S_CLK_SRC_XTAL_D2

    LP_I2S source clock is XTAL_D2

enum soc_periph_lcd_clk_src_t

  Type of LCD clock source.

  Values:

  enumerator LCD_CLK_SRC_PLL160M

    Select PLL_F160M as the source clock

  enumerator LCD_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator LCD_CLK_SRC_APLL

    Select APLL as the source clock

  enumerator LCD_CLK_SRC_DEFAULT

    Select PLL_F160M as the default choice

enum soc_periph_cam_clk_src_t

  Type of CAM clock source.

  Values:

  enumerator CAM_CLK_SRC_PLL160M

    Select PLL_F160M as the source clock

  enumerator CAM_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator CAM_CLK_SRC_APLL

    Select APLL as the source clock

  enumerator CAM_CLK_SRC_DEFAULT

    Select PLL_F160M as the default choice

enum soc_periph_mipi_csi_phy_clk_src_t

  Type of MIPI CSI PHY clock source.

  Values:

  enumerator MIPI_CSI_PHY_CLK_SRC_RC_FAST

    Select RC_FAST as MIPI CSI PHY source clock

  enumerator MIPI_CSI_PHY_CLK_SRC_PLL_F25M

    Select PLL_F25M as MIPI CSI PHY source clock

  enumerator MIPI_CSI_PHY_CLK_SRC_PLL_F20M

    Select PLL_F20M as MIPI CSI PHY source clock

  enumerator MIPI_CSI_PHY_CLK_SRC_DEFAULT

    Select PLL_F20M as default clock

enum soc_periph_mipi_dsi_dpi_clk_src_t

  Type of MIPI DSI DPI clock source.

  Values:

  enumerator MIPI_DSI_DPI_CLK_SRC_XTAL

    Select XTAL as MIPI DSI DPI source clock

  enumerator MIPI_DSI_DPI_CLK_SRC_PLL_F160M

    Select PLL_F160M as MIPI DSI DPI source clock

  enumerator MIPI_DSI_DPI_CLK_SRC_PLL_F240M

    Select PLL_F240M as MIPI DSI DPI source clock

  enumerator MIPI_DSI_DPI_CLK_SRC_APLL

    Select APLL as MIPI DSI DPI source clock

  enumerator MIPI_DSI_DPI_CLK_SRC_DEFAULT

    Select PLL_F240M as default clock

enum soc_periph_mipi_dsi_phy_cfg_clk_src_t

  Type of MIPI DSI PHY configuration clock source.

  Values:

  enumerator MIPI_DSI_PHY_CFG_CLK_SRC_RC_FAST

    Select RC_FAST as MIPI DSI PHY configuration source clock

  enumerator MIPI_DSI_PHY_CFG_CLK_SRC_PLL_F25M

    Select PLL_F25M as MIPI DSI PHY configuration source clock

  enumerator MIPI_DSI_PHY_CFG_CLK_SRC_PLL_F20M

    Select PLL_F20M as MIPI DSI PHY configuration source clock

  enumerator MIPI_DSI_PHY_CFG_CLK_SRC_DEFAULT

    Select PLL_F20M as default clock

enum soc_periph_mipi_dsi_phy_pllref_clk_src_t

  Type of MIPI DSI PHY PLL reference clock source.

  Values:

  enumerator MIPI_DSI_PHY_PLLREF_CLK_SRC_RC_FAST

    Select RC_FAST as MIPI DSI PHY PLL reference clock

  enumerator MIPI_DSI_PHY_PLLREF_CLK_SRC_PLL_F25M

    Select PLL_F25M as MIPI DSI PHY PLL reference clock

  enumerator MIPI_DSI_PHY_PLLREF_CLK_SRC_PLL_F20M

    Select PLL_F20M as MIPI DSI PHY PLL reference clock

  enumerator MIPI_DSI_PHY_PLLREF_CLK_SRC_DEFAULT_LEGACY

    Select PLL_F20M as default clock

  enumerator MIPI_DSI_PHY_PLLREF_CLK_SRC_XTAL

    Select XTAL as MIPI DSI PHY PLL reference clock

  enumerator MIPI_DSI_PHY_PLLREF_CLK_SRC_APLL

    Select APLL as MIPI DSI PHY PLL reference clock

  enumerator MIPI_DSI_PHY_PLLREF_CLK_SRC_CPLL

    Select CPLL as MIPI DSI PHY PLL reference clock

  enumerator MIPI_DSI_PHY_PLLREF_CLK_SRC_SPLL

    Select SPLL as MIPI DSI PHY PLL reference clock

  enumerator MIPI_DSI_PHY_PLLREF_CLK_SRC_MPLL

    Select MPLL as MIPI DSI PHY PLL reference clock

  enumerator MIPI_DSI_PHY_PLLREF_CLK_SRC_DEFAULT

    Select XTAL as default clock

enum soc_periph_i2c_clk_src_t

  Type of I2C clock source.

  Values:

  enumerator I2C_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator I2C_CLK_SRC_RC_FAST

    Select RC_FAST as the source clock

  enumerator I2C_CLK_SRC_DEFAULT

    Select XTAL as the default source clock

enum soc_periph_lp_i2c_clk_src_t

  Type of LP_I2C clock source.

  Values:

  enumerator LP_I2C_SCLK_LP_FAST

    LP_I2C source clock is RTC_FAST

  enumerator LP_I2C_SCLK_XTAL_D2

    LP_I2C source clock is XTAL_D2

  enumerator LP_I2C_SCLK_DEFAULT

    LP_I2C source clock default choice is RTC_FAST

enum soc_periph_spi_clk_src_t

  Type of SPI clock source.

  Values:

  enumerator SPI_CLK_SRC_XTAL

    Select XTAL as SPI source clock

  enumerator SPI_CLK_SRC_RC_FAST

    Select RC_FAST_20M as SPI source clock

  enumerator SPI_CLK_SRC_SPLL

    Select SPLL as SPI source clock

  enumerator SPI_CLK_SRC_DEFAULT

    Select SPLL as default source clock

enum soc_periph_psram_clk_src_t

  Type of PSRAM clock source.

  Values:

  enumerator PSRAM_CLK_SRC_DEFAULT

    Select SOC_MOD_CLK_SPLL as PSRAM source clock

  enumerator PSRAM_CLK_SRC_XTAL

    Select SOC_MOD_CLK_XTAL as PSRAM source clock

  enumerator PSRAM_CLK_SRC_CPLL

    Select SOC_MOD_CLK_CPLL as PSRAM source clock

  enumerator PSRAM_CLK_SRC_SPLL

    Select SOC_MOD_CLK_SPLL as PSRAM source clock

  enumerator PSRAM_CLK_SRC_MPLL

    Select SOC_MOD_CLK_MPLL as PSRAM source clock

enum soc_periph_flash_clk_src_t

  Type of FLASH clock source.

  Values:

  enumerator FLASH_CLK_SRC_DEFAULT

    Select SOC_MOD_CLK_SPLL as FLASH source clock

  enumerator FLASH_CLK_SRC_XTAL

    Select SOC_MOD_CLK_XTAL as FLASH source clock

  enumerator FLASH_CLK_SRC_CPLL

    Select SOC_MOD_CLK_CPLL as FLASH source clock

  enumerator FLASH_CLK_SRC_SPLL

    Select SOC_MOD_CLK_SPLL as FLASH source clock

enum soc_periph_isp_clk_src_t

  Type of ISP clock source.

  Values:

  enumerator ISP_CLK_SRC_DEFAULT

    Select SOC_MOD_CLK_PLL_F160M as ISP source clock

  enumerator ISP_CLK_SRC_XTAL

    Select SOC_MOD_CLK_XTAL as ISP source clock

  enumerator ISP_CLK_SRC_PLL160

    Select SOC_MOD_CLK_PLL_F160M as ISP source clock

  enumerator ISP_CLK_SRC_PLL240

    Select SOC_MOD_CLK_PLL_F240M as ISP source clock

enum soc_periph_sdm_clk_src_t

  Sigma Delta Modulator clock source.

  Values:

  enumerator SDM_CLK_SRC_XTAL

    Select XTAL clock as the source clock

  enumerator SDM_CLK_SRC_PLL_F80M

    Select PLL_F80M clock as the source clock

  enumerator SDM_CLK_SRC_DEFAULT

    Select PLL_F80M clock as the default clock choice

enum soc_periph_glitch_filter_clk_src_t

  Glitch filter clock source.

  Values:

  enumerator GLITCH_FILTER_CLK_SRC_XTAL

    Select XTAL clock as the source clock

  enumerator GLITCH_FILTER_CLK_SRC_PLL_F80M

    Select PLL_F80M clock as the source clock

  enumerator GLITCH_FILTER_CLK_SRC_DEFAULT

    Select PLL_F80M clock as the default clock choice

enum soc_periph_ana_cmpr_clk_src_t

  Analog Comparator clock source.

  Values:

  enumerator ANA_CMPR_CLK_SRC_XTAL

    Select XTAL clock as the source clock

  enumerator ANA_CMPR_CLK_SRC_PLL_F80M

    Select PLL_F80M clock as the source clock

  enumerator ANA_CMPR_CLK_SRC_DEFAULT

    Select PLL_F80M as the default clock choice

enum soc_periph_twai_clk_src_t

  TWAI clock source.

  Values:

  enumerator TWAI_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator TWAI_CLK_SRC_DEFAULT

    Select XTAL as the default clock choice

enum soc_periph_adc_digi_clk_src_t

  ADC digital controller clock source.

  Values:

  enumerator ADC_DIGI_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator ADC_DIGI_CLK_SRC_RC_FAST

    Select RC_FAST as the source clock

  enumerator ADC_DIGI_CLK_SRC_PLL_F80M

    Select PLL_F80M as the source clock

  enumerator ADC_DIGI_CLK_SRC_DEFAULT

    Select PLL_F80M as the default clock choice

enum soc_periph_adc_rtc_clk_src_t

  ADC RTC controller clock source.

  Values:

  enumerator ADC_RTC_CLK_SRC_RC_FAST

    Select RC_FAST as the source clock

  enumerator ADC_RTC_CLK_SRC_DEFAULT

    Select RC_FAST as the default clock choice

enum soc_periph_lp_adc_clk_src_t

  LP ADC controller clock source.

  Values:

  enumerator LP_ADC_CLK_SRC_LP_DYN_FAST

    Select LP_DYN_FAST as the source clock

enum soc_periph_mwdt_clk_src_t

  MWDT clock source.

  Values:

  enumerator MWDT_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator MWDT_CLK_SRC_PLL_F80M

    Select PLL fixed 80 MHz as the source clock

  enumerator MWDT_CLK_SRC_RC_FAST

    Select RTC fast as the source clock

  enumerator MWDT_CLK_SRC_DEFAULT

    Select XTAL 40 MHz as the default clock choice

enum soc_periph_ledc_clk_src_legacy_t

  Type of LEDC clock source, reserved for the legacy LEDC driver.

  Values:

  enumerator LEDC_AUTO_CLK

    LEDC source clock will be automatically selected based on the giving resolution and duty parameter when init the timer

  enumerator LEDC_USE_XTAL_CLK

    Select XTAL as the source clock

  enumerator LEDC_USE_PLL_DIV_CLK

    Select PLL_F80M clock as the source clock

  enumerator LEDC_USE_RC_FAST_CLK

    Select RC_FAST as the source clock

enum soc_periph_parlio_clk_src_t

  PARLIO clock source.

  Values:

  enumerator PARLIO_CLK_SRC_XTAL

    Select XTAL as the source clock

  enumerator PARLIO_CLK_SRC_RC_FAST

    Select RC_FAST as the source clock

  enumerator PARLIO_CLK_SRC_PLL_F160M

    Select PLL_F160M as the source clock

  enumerator PARLIO_CLK_SRC_EXTERNAL

    Select EXTERNAL clock as the source clock

  enumerator PARLIO_CLK_SRC_DEFAULT

    Select PLL_F160M as the default clock choice

enum soc_periph_sdmmc_clk_src_t

  Type of SDMMC clock source.

  Values:

  enumerator SDMMC_CLK_SRC_DEFAULT

    Select PLL_160M as the default choice

  enumerator SDMMC_CLK_SRC_PLL160M

    Select PLL_160M as the source clock

  enumerator SDMMC_CLK_SRC_SDIO_200M

enum soc_periph_temperature_sensor_clk_src_t

  Type of Temp Sensor clock source.

  Values:

  enumerator TEMPERATURE_SENSOR_CLK_SRC_LP_PERI

    Select LP_PERI as the source clock

  enumerator TEMPERATURE_SENSOR_CLK_SRC_DEFAULT

    Select LP_PERI as the default choice

enum soc_periph_i3c_master_clk_src_t

  Values:

  enumerator I3C_MASTER_CLK_SRC_XTAL
  enumerator I3C_MASTER_CLK_SRC_PLL_F160M
  enumerator I3C_MASTER_CLK_SRC_DEFAULT

enum soc_periph_emac_ptp_clk_src_t

  Values:

  enumerator EMAC_PTP_CLK_SRC_XTAL
  enumerator EMAC_PTP_CLK_SRC_PLL_F80M
  enumerator EMAC_PTP_CLK_SRC_DEFAULT

enum soc_clkout_sig_id_t

  Values:

  enumerator CLKOUT_SIG_MPLL

    MPLL is from 40MHz XTAL oscillator frequency multipliers

  enumerator CLKOUT_SIG_SPLL

    SPLL is from 40MHz XTAL oscillator frequency multipliers, its default frequency is 480MHz

  enumerator CLKOUT_SIG_CPLL

    CPLL_CLK is the output of 40MHz crystal oscillator frequency multiplier, can be 320/360/400MHz

  enumerator CLKOUT_SIG_XTAL

    External 40MHz crystal

  enumerator CLKOUT_SIG_RC_FAST

    Internal 17.5MHz RC oscillator

  enumerator CLKOUT_SIG_RC_SLOW

    Internal 136kHz RC oscillator

  enumerator CLKOUT_SIG_RC_32K

    Internal 32kHz RC oscillator

  enumerator CLKOUT_SIG_XTAL32K

    External 32kHz crystal clock

  enumerator CLKOUT_SIG_I2S0

    I2S0 clock, depends on the i2s driver configuration

  enumerator CLKOUT_SIG_I2S1

    I2S1 clock, depends on the i2s driver configuration

  enumerator CLKOUT_SIG_I2S2

    I2S2 clock, depends on the i2s driver configuration

  enumerator CLKOUT_SIG_CPU

    CPU clock

  enumerator CLKOUT_SIG_MEM

    MEM clock

  enumerator CLKOUT_SIG_SYS

    SYS clock

  enumerator CLKOUT_SIG_APB

    APB clock

  enumerator CLKOUT_SIG_PLL_F80M

    From PLL, usually be 80MHz

  enumerator CLKOUT_SIG_INVALID

### Header File

- components/esp_hw_support/include/esp_clk_tree.h

- This header file can be included with:

  >     #include "esp_clk_tree.h"

### Functions

esp_err_t esp_clk_tree_src_get_freq_hz(soc_module_clk_t clk_src, esp_clk_tree_src_freq_precision_t precision, uint32_t *freq_value)

  Get frequency of module clock source.

  参数:

    - clk_src -- [in] Clock source available to modules, in soc_module_clk_t

    - precision -- [in] Degree of precision, one of esp_clk_tree_src_freq_precision_t values This arg only applies to the clock sources that their frequencies can vary: SOC_MOD_CLK_RTC_FAST, SOC_MOD_CLK_RTC_SLOW, SOC_MOD_CLK_RC_FAST, SOC_MOD_CLK_RC_FAST_D256, SOC_MOD_CLK_XTAL32K For other clock sources, this field is ignored.

    - freq_value -- [out] Frequency of the clock source, in Hz

  返回:

    - ESP_OK Success

    - ESP_ERR_INVALID_ARG Parameter error

    - ESP_FAIL Calibration failed

### Enumerations

enum esp_clk_tree_src_freq_precision_t

  Degree of precision of frequency value to be returned by esp_clk_tree_src_get_freq_hz()

  Values:

  enumerator ESP_CLK_TREE_SRC_FREQ_PRECISION_CACHED
  enumerator ESP_CLK_TREE_SRC_FREQ_PRECISION_APPROX
  enumerator ESP_CLK_TREE_SRC_FREQ_PRECISION_EXACT
  enumerator ESP_CLK_TREE_SRC_FREQ_PRECISION_INVALID

此文档对您有帮助吗？

- 反馈已收到，谢谢！
- 如果您有其他意见，欢迎填写乐鑫文档反馈表。

- 我们重视您的反馈。
- 您可以填写乐鑫文档反馈表告诉我们如何改进该文档。