# Wi-Fi Expansion

[中文]

ESP32-H2 does not support Wi-Fi functionality natively, but it is possible to use the same Wi-Fi API and features using Wi-Fi expansion.

## ESP32-H2 esp_wifi_remote

The principle of Wi-Fi Expansion operation is to add another ESP32 series, Wi-Fi capable, target connected to the ESP32-H2 in a pre-defined way. Your project could then include the esp_wifi_remote component using:

    idf.py add-dependency esp_wifi_remote

Please follow the instructions described in the component documentation which is linked in the above paragraph.

To explore the Wi‑Fi Expansion functionality on ESP32-H2, you can:

- Start with the built‑in MQTT over TLS example `examples/protocols/mqtt` (or the MQTT 5.0 variant `examples/protocols/mqtt5`) and choose Wi‑Fi connection in the project configuration menu;

此文档对您有帮助吗？

- 反馈已收到，谢谢！
- 如果您有其他意见，欢迎填写乐鑫文档反馈表。

- 我们重视您的反馈。
- 您可以填写乐鑫文档反馈表告诉我们如何改进该文档。