:orphan:

ESP 主机主要功能支持状态
========================

:link_to_translation:`en:[English]`

本文档介绍了乐鑫低功耗蓝牙主机 ESP-Bluedroid 和 ESP-NimBLE 主要功能的支持状态。
如果你计划将低功耗蓝牙控制器和主机跑在 {IDF_TARGET_NAME} 上，主机的功能支持可能会受限于控制器的功能支持状态，
请参阅 :doc:`{IDF_TARGET_NAME} 主要功能支持状态 <ble-feature-support-status>` 。

|supported_def| **该功能已完成开发和内部测试。** [1]_

|experimental_def| **该功能已完成开发，正在进行内部测试。**
你可以探索这些功能以进行评估和反馈，但应注意可能出现的问题。

|developing_def| **该功能目前正在积极开发中， 预计在 YYYY/MM 月底之前支持。**
请关注此表以获得该功能的最新进展。
如果确实有紧急的开发需求，请联系 `乐鑫客户支持团队 <https://www.espressif.com/zh-hans/contact-us/sales-questions>`__ 以了解是否可以进行功能试用。

|unsupported_def| **该功能在该蓝牙主机上不支持。** 如果你有相关需求，请优先选择其他支持该功能的乐鑫蓝牙主机。
如果当前的乐鑫产品都不支持此功能，请联系 `乐鑫客户支持团队 <https://www.espressif.com/zh-hans/contact-us/sales-questions>`__ ，我们的研发团队会对你的需求进行内部可行性评估。

|NA_def| 具有此标签的功能可能为以下类型：
    - **Controller-only 功能**：该功能仅存在于 HCI 层之下，且无法通过主机API配置或启用，例如 Advertising Channel Index 。
      此类功能不需要蓝牙主机的支持。

.. list-table::
    :width: 100%
    :widths: auto
    :header-rows: 1

    * - .. centered:: 核心协议
      - .. centered:: 主要功能
      - .. centered:: ESP-Bluedroid 主机
      - .. centered:: ESP-NimBLE 主机
    * - .. centered:: |4.2|
      - LE Data Packet Length Extension
      - |supported|
      - |supported|
    * -
      - LE Secure Connections
      - |supported|
      - |supported|
    * -
      - Link Layer Privacy
      - |supported|
      - |supported|
    * -
      - Link Layer Extended Filter Policies
      - |supported|
      - |supported|
    * - .. centered:: |5.0|
      - 2 Msym/s PHY for LE
      - |supported|
      - |supported|
    * -
      - LE Long Range (Coded PHY S=2/S=8)
      - |supported|
      - |supported|
    * -
      - High Duty Cycle Non-Connectable Advertising
      - |supported|
      - |supported|
    * -
      - LE Advertising Extensions
      - |supported|
      - |supported|
    * -
      - LE Channel Selection Algorithm #2
      - |supported|
      - |supported|
    * - .. centered:: |5.1|
      - Angle of Arrival (AoA)/Angle of Departure (AoD)
      - |unsupported|
      - |developing202412|
    * -
      - GATT Caching
      - |experimental|
      - |experimental|
    * -
      - Randomized Advertising Channel Indexing
      - |NA|
      - |NA|
    * -
      - Periodic Advertising Sync Transfer
      - |supported|
      - |supported|
    * - .. centered:: |5.2|
      - LE Isochronous Channels (BIS/CIS)
      - |unsupported|
      - |unsupported|
    * -
      - Enhanced Attribute Protocol
      - |unsupported|
      - |developing202412|
    * -
      - LE Power Control
      - |unsupported|
      - |supported|
    * - .. centered:: |5.3|
      - AdvDataInfo in Periodic Advertising
      - |supported|
      - |supported|
    * -
      - LE Enhanced Connection Update (Connection Subrating)
      - |unsupported|
      - |supported|
    * -
      - LE Channel Classification
      - |supported|
      - |supported|
    * - .. centered:: |5.4|
      - Advertising Coding Selection
      - |unsupported|
      - |supported|
    * -
      - Encrypted Advertising Data
      - |unsupported|
      - |experimental|
    * -
      - LE GATT Security Levels Characteristic
      - |unsupported|
      - |developing202412|
    * -
      - Periodic Advertising with Responses
      - |unsupported|
      - |developing202412|

.. [1]
   如果想了解支持功能的 Bluetooth SIG 认证状态，
   请查阅 `SIG 蓝牙产品数据库 <https://qualification.bluetooth.com/Listings/Search>`__ 。

请注意，本文档不构成对客户的约束性承诺。
以上所列出来的功能支持状态信息仅供参考，可能会在不通知的情况下发生更改。
建议联系 `乐鑫客户支持团队 <https://www.espressif.com/zh-hans/contact-us/sales-questions>`__ 以获取最新信息，并确认功能是否适合你的特定需求。


.. |supported| image:: ../../../_static/ble/feature_status/supported.svg
   :class: align-center
.. |developing202412| image:: ../../../_static/ble/feature_status/developing202412.svg
   :class: align-center
.. |unsupported| image:: ../../../_static/ble/feature_status/unsupported.svg
   :class: align-center
.. |experimental| image:: ../../../_static/ble/feature_status/experimental.svg
   :class: align-center
.. |NA| image:: ../../../_static/ble/feature_status/NA.svg
   :class: align-center
.. |supported_def| image:: ../../../_static/ble/feature_status/supported.svg
.. |developing_def| image:: ../../../_static/ble/feature_status/developingYYYYMM.svg
.. |unsupported_def| image:: ../../../_static/ble/feature_status/unsupported.svg
.. |experimental_def| image:: ../../../_static/ble/feature_status/experimental.svg
.. |NA_def| image:: ../../../_static/ble/feature_status/NA.svg
.. |4.2| replace:: `4.2 <https://www.bluetooth.com/specifications/specs/core-specification-4-2/>`__
.. |5.0| replace:: `5.0 <https://www.bluetooth.com/specifications/specs/core-specification-5-0/>`__
.. |5.1| replace:: `5.1 <https://www.bluetooth.com/specifications/specs/core-specification-5-1/>`__
.. |5.2| replace:: `5.2 <https://www.bluetooth.com/specifications/specs/core-specification-5-2/>`__
.. |5.3| replace:: `5.3 <https://www.bluetooth.com/specifications/specs/core-specification-5-3/>`__
.. |5.4| replace:: `5.4 <https://www.bluetooth.com/specifications/specs/core-specification-5-4/>`__
