# ULP RISC-V 协处理器编程

[English]

ULP RISC-V 协处理器是 ULP 的一种变体，用于 ESP32-S2。与 ULP FSM 类似，ULP RISC-V 协处理器可以在主 CPU 处于低功耗模式时执行传感器读数等任务。其与 ULP FSM 的主要区别在于，ULP RISC-V 可以通过标准 GNU 工具使用 C 语言进行编程。ULP RISC-V 可以访问 RTC_SLOW_MEM 内存区域及 `RTC_CNTL`、`RTC_IO`、`SARADC` 等外设的寄存器。RISC-V 处理器是一种 32 位定点处理器，指令集基于 RV32IMC，包括硬件乘除法和压缩指令。

## 安装 ULP RISC-V 工具链

ULP RISC-V 协处理器代码以 C 语言（或汇编语言）编写，使用基于 GCC 的 RISC-V 工具链进行编译。

如果依照 快速入门指南 中的介绍安装好了 ESP-IDF 及其 CMake 构建系统，那么 ULP RISC-V 工具链已经被默认安装到了你的开发环境中。

备注

在早期版本的 ESP-IDF 中，RISC-V 工具链具有不同的名称：`riscv-none-embed-gcc`。

## 编译 ULP RISC-V 代码

要将 ULP RISC-V 代码编译为某组件的一部分，必须执行以下步骤：

1. ULP RISC-V 代码以 C 语言或汇编语言编写（必须使用 `.S` 扩展名），必须放在组件目录中一个独立的目录中，例如 `ulp/`。

备注

当注册组件时（通过 `idf_component_register`），该目录不应被添加至 `SRC_DIRS` 参数，因为目前该步骤需用于 ULP FSM。如何正确添加 ULP 源文件，请见以下步骤。

2. 注册后从组件 CMakeLists.txt 中调用 `ulp_embed_binary` 示例如下:

       ...
       idf_component_register()

       set(ulp_app_name ulp_${COMPONENT_NAME})
       set(ulp_sources "ulp/ulp_c_source_file.c" "ulp/ulp_assembly_source_file.S")
       set(ulp_exp_dep_srcs "ulp_c_source_file.c")

       ulp_embed_binary(${ulp_app_name} "${ulp_sources}" "${ulp_exp_dep_srcs}")

> `ulp_embed_binary` 的第一个参数指定生成的 ULP 二进制文件名。生成的其他文件，如 ELF 文件、.map 文件、头文件和链接器导出文件等也可使用此名称。第二个参数指定 ULP 源文件。最后，第三个参数指定组件源文件列表，其中包括生成的头文件。此列表用以正确构建依赖，并确保在构建过程中先生成后编译包含头文件的源文件。请参考下文，查看为 ULP 应用程序生成的头文件等相关概念。

3. 使用常规方法（例如 `idf.py app`）编译应用程序。

   在内部，构建系统将按照以下步骤编译 ULP 程序：

   1. 通过 C 编译器和汇编器运行每个源文件。 此步骤在组件编译目录中生成目标文件（ `.obj.c` 或 `.obj.S`，取决于处理的源文件）。

   2. 通过 C 预处理器运行链接器脚本模版。 模版位于 `components/ulp/ld` 目录中。

   3. 将目标文件链接到 ELF 输出文件 (`ulp_app_name.elf`)。此步骤生成的 .map 文件默认用于调试 (`ulp_app_name.map`)。

   4. 将 ELF 文件中的内容转储为二进制文件 (`ulp_app_name.bin`)，以便嵌入到应用程序中。

   5. 使用 `riscv32-esp-elf-nm` 在 ELF 文件中 生成全局符号列表 (`ulp_app_name.sym`)。

   6. 创建 LD 导出脚本和头文件 （`ulp_app_name.ld` 和 `ulp_app_name.h`），包含来自 `ulp_app_name.sym` 的符号。此步骤可借助 `esp32ulp_mapgen.py` 工具来完成。

   7. 将生成的二进制文件添加到要嵌入应用程序的二进制文件列表中。

## 访问 ULP RISC-V 程序变量

在 ULP RISC-V 程序中定义的全局符号也可以在主程序中使用。

例如，ULP RISC-V 程序可以定义 `measurement_count` 变量，此变量可以定义程序从深度睡眠中唤醒芯片之前需要进行的 ADC 测量的次数。

    volatile int measurement_count;

    int some_function()
    {
        //读取测量计数，后续需使用
        int temp = measurement_count;

        ...do something.
    }

构建系统生成定义 ULP 编程中全局符号的 `${ULP_APP_NAME}.h` 和 `${ULP_APP_NAME}.ld` 文件，使主程序能够访问全局 ULP RISC-V 程序变量。上述两个文件包含 ULP RISC-V 程序中定义的所有全局符号，且这些符号均以 `ulp_` 开头。

头文件包含对此类符号的声明：

    extern uint32_t ulp_measurement_count;

注意，所有符号（包括变量、数组、函数）均被声明为 `uint32_t`。函数和数组需要先获取符号地址，再转换为适当的类型。

生成的链接器文本定义了符号在 RTC_SLOW_MEM 中的位置:

    PROVIDE ( ulp_measurement_count = 0x50000060 );

要从主程序访问 ULP RISC-V 程序变量，需使用 `include` 语句包含生成的头文件。这样，就可以像访问常规变量一样访问 ULP RISC-V 程序变量。

    #include "ulp_app_name.h"

    void init_ulp_vars() {
        ulp_measurement_count = 64;
    }

### 互斥

如果想要互斥地访问被主程序和 ULP 程序共享的变量，则可以通过 ULP RISC-V Lock API 来实现：

> - `ulp_riscv_lock_acquire()`

> - `ulp_riscv_lock_release()`

ULP 中的所有硬件指令都不支持互斥，所以 Lock API 需通过一种软件算法（Peterson 算法 ）来实现互斥。

注意，只能从主程序的单个线程中调用这些锁，如果多个线程同时调用，将无法启用互斥功能。

## 启动 ULP RISC-V 程序

要运行 ULP RISC-V 程序，主程序需要调用 `ulp_riscv_load_binary()` 函数，将 ULP 程序加载到 RTC 内存中，然后调用 `ulp_riscv_run()` 函数，启动 ULP RISC-V 程序。

注意，必须在 menuconfig 中启用 `CONFIG_ULP_COPROC_ENABLED` 和 `CONFIG_ULP_COPROC_TYPE_RISCV` 选项，以便正常运行 ULP RISC-V 程序。`RTC slow memory reserved for coprocessor` 选项设置的值必须足够存储 ULP RISC-V 代码和数据。如果应用程序组件包含多个 ULP 程序，RTC 内存必须足以容纳最大的程序。

每个 ULP RISC-V 程序均以二进制 BLOB 的形式嵌入到 ESP-IDF 应用程序中。应用程序可以引用此 BLOB，并以下面的方式加载此 BLOB（假设 ULP_APP_NAME 已被定义为 `ulp_app_name`）：

    extern const uint8_t bin_start[] asm("_binary_ulp_app_name_bin_start");
    extern const uint8_t bin_end[]   asm("_binary_ulp_app_name_bin_end");

    void start_ulp_program() {
        ESP_ERROR_CHECK( ulp_riscv_load_binary( bin_start,
            (bin_end - bin_start)) );
    }

一旦上述程序加载到 RTC 内存后，应用程序即可调用 `ulp_riscv_run()` 函数启动此程序：

    ESP_ERROR_CHECK( ulp_riscv_run() );

## ULP RISC-V 程序流

ULP RISC-V 协处理器由定时器启动，调用 `ulp_riscv_run()` 即可启动定时器。定时器为 RTC_SLOW_CLK 的 Tick 事件计数（默认情况下，Tick 由内部 90 kHz RC 振荡器产生）。Tick 数值使用 `RTC_CNTL_ULP_CP_TIMER_1_REG` 寄存器设置。启用 ULP 时，使用 `RTC_CNTL_ULP_CP_TIMER_1_REG` 设置定时器 Tick 数值。

此应用程序可以调用 `ulp_set_wakeup_period()` 函数来设置 ULP 定时器周期值 (RTC_CNTL_ULP_CP_TIMER_1_REG)。

一旦定时器数到 `RTC_CNTL_ULP_CP_TIMER_1_REG` 寄存器中设置的 Tick 数，ULP RISC-V 协处理器就会启动，并调用 `ulp_riscv_run()` 的入口点开始运行程序。

程序保持运行，直至 `RTC_CNTL_COCPU_CTRL_REG` 寄存器中的 `RTC_CNTL_COCPU_DONE` 字段被置位或因非法处理器状态出现陷阱。一旦程序停止，ULP RISC-V 协处理器会关闭电源，定时器再次启动。

如需禁用定时器（有效防止 ULP 程序再次运行），请清除 `RTC_CNTL_STATE0_REG` 寄存器中的 `RTC_CNTL_ULP_CP_SLP_TIMER_EN` 位，此项操作可在 ULP 代码或主程序中进行。

## ULP RISC-V 外设支持

为了增强性能，ULP RISC-V 协处理器可以访问在低功耗 (RTC) 电源域中运行的外设。当主 CPU 处于睡眠模式时，ULP RISC-V 协处理器可与这些外设进行交互，并在满足唤醒条件时唤醒主 CPU。以下为所支持的外设类型。

### RTC I2C

RTC I2C 控制器提供了在 RTC 电源域中作为 I2C 主机的功能。ULP RISC-V 协处理器可以使用该控制器对 I2C 从机设备进行读写操作。如要使用 RTC I2C 外设，需在初始化 ULP RISC-V 内核并在其进入睡眠模式之前，先在主内核上运行的应用程序中调用 `ulp_riscv_i2c_master_init()` 函数。

初始化 RTC I2C 控制器之后，请务必先用 `ulp_riscv_i2c_master_set_slave_addr()` API 将 I2C 从机设备地址编入程序，再执行读写操作。

备注

RTC I2C 外设首先将检查 `ulp_riscv_i2c_master_set_slave_reg_addr()` API 是否将从机子寄存器地址编入程序。如未编入，I2C 外设将以 `SENS_SAR_I2C_CTRL_REG[18:11]` 作为后续读写操作的子寄存器地址。这可能会导致 RTC I2C 外设与某些无需对子寄存器进行配置的 I2C 设备或传感器不兼容。

备注

在主 CPU 访问 RTC I2C 外设和 ULP RISC-V 内核访问 RTC I2C 外设之间，未提供硬件原子操作的正确性保护，因此请勿让两个内核同时访问外设。

如果基于 RTC I2C 的 ULP RISC-V 程序未按预期运行，可以进行以下完整性检查排查问题：

> - SDA/SCL 管脚选择问题：SDA 管脚只能配置为 GPIO1 或 GPIO3，SCL 管脚只能配置为 GPIO0 或 GPIO2。请确保管脚配置正确。

> - I2C 时序参数问题：RTC I2C 总线时序配置受到 I2C 标准总线规范限制，任何违反标准 I2C 总线规范的时序参数都会导致错误。了解有关时序参数的详细信息，请阅读 标准 I2C 总线规范。

> - 如果 I2C 从机设备或传感器不需要子寄存器地址进行配置，它可能与 RTC I2C 外设不兼容。请参考前文注意事项。

> - 如果 RTC 驱动程序在主 CPU 上运行时出现 `Write Failed!` 或 `Read Failed!` 的错误日志，检查是否出现以下情况：

>   > - I2C 从机设备或传感器与乐鑫 SoC 上的标准 I2C 主机设备一起正常工作，说明 I2C 从机设备本身没有问题。

>   > - 如果 RTC I2C 中断状态日志报告 `TIMEOUT` 错误或 `ACK` 错误，则通常表示 I2C 设备未响应 RTC I2C 控制器发出的 `START` 条件。如果 I2C 从机设备未正确连接到控制器管脚或处于异常状态，则可能会发生这种情况。在进行后续操作之前，请确保 I2C 从机设备状态良好且连接正确。

>   > - 如果 RTC I2C 中断日志没有报告任何错误状态，则可能表示驱动程序接收 I2C 从机设备数据时速度较慢。这可能是由于 RTC I2C 控制器没有 TX/RX FIFO 来存储多字节数据，而是依赖于使用中断状态轮询机制来进行单字节传输。通过在外设的初始化配置参数中设置 SCL 低周期和 SCL 高周期，可以尽量提高外设 SCL 时钟的运行速度，在一定程度上缓解这一问题。

- 调试问题的方法还包括确保 RTC I2C 控制器 仅 在主 CPU 上运行， 没有 ULP RISC-V 代码干扰，并且没有激活 任何 睡眠模式。这是确保 RTC I2C 外设正常工作的基本配置。通过这种方式，可以排除由 ULP 或睡眠模式可能引起的任何潜在问题。

## ULP RISC-V 中断处理

ULP RISC-V 内核支持来自特定内部和外部事件的中断处理。设计上，ULP RISC-V 内核可以处理以下来源的中断：

ULP RISC-V 中断源
中断源 | 类型 | IRQ
--- | --- | ---
内部定时器中断 | 内部中断 | 0
EBREAK、ECALL 或非法指令 | 内部中断 | 1
非对齐内存访问 | 内部中断 | 2
RTC 外设中断源 | 外部中断 | 31

可通过特殊的 32 位寄存器 Q0-Q3 和自定义的 R-type 指令启用中断处理。更多信息，请参阅 ESP32-S2 技术参考手册 > 超低功耗协处理器 > ULP-RISC-V > ULP-RISC-V 中断 [PDF]。

系统启动时，默认启用所有中断。触发中断时，处理器将跳转到 IRQ 向量。IRQ 向量随即保存寄存器上下文，并调用全局中断分发器。ULP RISC-V 驱动程序实现了一个 弱 中断分发器 `_ulp_riscv_interrupt_handler()`，充当处理所有中断的中心点。该全局分发器用于调用由 `ulp_riscv_intr_alloc()` 分配的相应中断处理程序。

ULP RISC-V 的中断处理尚在开发中，还不支持针对内部中断源的中断处理。目前支持两个 RTC 外设中断源，即软件触发的中断和 RTC IO 触发的中断，不支持嵌套中断。如果需要自定义中断处理，可以通过定义 `_ulp_riscv_interrupt_handler()` 来覆盖默认的全局中断调度器。

## 调试 ULP RISC-V 程序

在对 ULP RISC-V 进行配置时，若程序未按预期运行，有时很难找出的原因。因为其内核的简单性，许多标准的调试方法如 JTAG 或 `printf` 无法使用。

以下方法可以调试 ULP RISC-V 程序：

> - 通过共享变量查看程序状态：如 访问 ULP RISC-V 程序变量 中所述，主 CPU 以及 ULP 内核都可以轻松访问 RTC 内存中的全局变量。通过 ULP 向该变量中写入状态信息，然后通过主 CPU 读取状态信息，有助于了解 ULP 内核的状态。该方法的缺点在于它要求主 CPU 一直处于唤醒状态，但现实情况可能并非如此。有时，保持主 CPU 处于唤醒状态还可能会掩盖一些问题，因为某些问题可能仅在特定电源域断电时才会出现。

> - 使用 bit-banged UART 驱动程序打印：ULP RISC-V 组件中有一个低速 bit-banged UART TX 驱动程序，可用于打印独立于主 CPU 状态的信息。有关如何使用此驱动程序的示例，请参阅 system/ulp/ulp_riscv/uart_print。

> - 陷阱信号：ULP RISC-V 有一个硬件陷阱，将在特定条件下触发，例如非法指令。这将导致主 CPU 被 `ESP_SLEEP_WAKEUP_COCPU_TRAP_TRIG` 唤醒。

## 应用示例

- 主 CPU 处于 Deep-sleep 状态时，ULP RISC-V 协处理器轮询 GPIO：system/ulp/ulp_riscv/gpio。

- ULP RISC-V 协处理器使用 bit-banged UART 驱动程序打印：system/ulp/ulp_riscv/uart_print.

- 主 CPU 处于 Deep-sleep 状态时，ULP RISC-V 协处理器读取外部温度传感器：system/ulp/ulp_riscv/ds18b20_onewire。

- 主 CPU 处于 Deep-sleep 状态时，ULP RISC-V 协处理器读取外部 I2C 温度和湿度传感器 (BMP180)，达到阈值时唤醒主 CPU：system/ulp/ulp_riscv/i2c.

- 使用 ULP RISC-V 协处理器处理软件中断和 RTC IO 中断：system/ulp/ulp_riscv/interrupts.

## API 参考

### Header File

- components/ulp/ulp_riscv/include/ulp_riscv.h

- This header file can be included with:

  >     #include "ulp_riscv.h"

- This header file is a part of the API provided by the `ulp` component. To declare that your component depends on `ulp`, add the following to your CMakeLists.txt:

  >     REQUIRES ulp

  > or

  >     PRIV_REQUIRES ulp

### Functions

esp_err_t ulp_riscv_isr_register(intr_handler_t fn, void *arg, uint32_t mask)

  Register ULP signal ISR.

  备注

  The ISR routine will only be active if the main CPU is not in deepsleep

  参数:

    - fn -- ISR callback function

    - arg -- ISR callback function arguments

    - mask -- Bit mask to enable the required ULP RISC-V interrupt signals

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if callback function is NULL or if the interrupt bits are invalid

    - ESP_ERR_NO_MEM if heap memory cannot be allocated for the interrupt

    - other errors returned by esp_intr_alloc

esp_err_t ulp_riscv_isr_deregister(intr_handler_t fn, void *arg, uint32_t mask)

  Deregister ULP signal ISR.

  参数:

    - fn -- ISR callback function

    - arg -- ISR callback function arguments

    - mask -- Bit mask to enable the required ULP RISC-V interrupt signals

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if callback function is NULL or if the interrupt bits are invalid

    - ESP_ERR_INVALID_STATE if a handler matching both callback function and its arguments isn't registered

esp_err_t ulp_riscv_config_and_run(ulp_riscv_cfg_t *cfg)

  Configure the ULP and run the program loaded into RTC memory.

  参数:

    cfg -- pointer to the config struct

  返回:

    ESP_OK on success

esp_err_t ulp_riscv_run(void)

  Configure the ULP with default settings and run the program loaded into RTC memory.

  返回:

    ESP_OK on success

esp_err_t ulp_riscv_load_binary(const uint8_t *program_binary, size_t program_size_bytes)

  Load ULP-RISC-V program binary into RTC memory.

  Different than ULP FSM, the binary program has no special format, it is the ELF file generated by RISC-V toolchain converted to binary format using objcopy.

  Linker script in components/ulp/ld/ulp_riscv.ld produces ELF files which correspond to this format. This linker script produces binaries with load_addr == 0.

  参数:

    - program_binary -- pointer to program binary

    - program_size_bytes -- size of the program binary

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_SIZE if program_size_bytes is more than 8KiB

void ulp_riscv_timer_stop(void)

  Stop the ULP timer.

  备注

  This will stop the ULP from waking up if halted, but will not abort any program currently executing on the ULP.

void ulp_riscv_timer_resume(void)

  Resumes the ULP timer.

  备注

  This will resume an already configured timer, but does no other configuration

void ulp_riscv_halt(void)

  Halts the program currently running on the ULP-RISC-V.

  备注

  Program will restart at the next ULP timer trigger if timer is still running. If you want to stop the ULP from waking up then call ulp_riscv_timer_stop() first.

void ulp_riscv_reset(void)

  Resets the ULP-RISC-V core from the main CPU.

  备注

  This will reset the ULP core from the main CPU. It is intended to be used when the ULP is in a bad state and cannot run as intended due to a corrupt firmware or any other reason. The main core can reset the ULP core with this API and then re-initilialize the ULP.

### Structures

struct ulp_riscv_cfg_t

  ULP riscv init parameters.

  Public Members

  ulp_riscv_wakeup_source_t wakeup_source

    ULP wakeup source

### Macros

ULP_RISCV_DEFAULT_CONFIG()

ULP_RISCV_SW_INT

ULP_RISCV_TRAP_INT

### Enumerations

enum ulp_riscv_wakeup_source_t

  Values:

  enumerator ULP_RISCV_WAKEUP_SOURCE_TIMER
  enumerator ULP_RISCV_WAKEUP_SOURCE_GPIO

### Header File

- components/ulp/ulp_riscv/shared/include/ulp_riscv_lock_shared.h

- This header file can be included with:

  >     #include "ulp_riscv_lock_shared.h"

- This header file is a part of the API provided by the `ulp` component. To declare that your component depends on `ulp`, add the following to your CMakeLists.txt:

  >     REQUIRES ulp

  > or

  >     PRIV_REQUIRES ulp

### Structures

struct ulp_riscv_lock_t

  Structure representing a lock shared between ULP and main CPU.

  Public Members

  bool critical_section_flag_ulp

    ULP wants to enter the critical sections

  bool critical_section_flag_main_cpu

    Main CPU wants to enter the critical sections

  ulp_riscv_lock_turn_t turn

    Which CPU is allowed to enter the critical section

### Enumerations

enum ulp_riscv_lock_turn_t

  Enum representing which processor is allowed to enter the critical section.

  Values:

  enumerator ULP_RISCV_LOCK_TURN_ULP

    ULP's turn to enter the critical section

  enumerator ULP_RISCV_LOCK_TURN_MAIN_CPU

    Main CPU's turn to enter the critical section

### Header File

- components/ulp/ulp_riscv/include/ulp_riscv_lock.h

- This header file can be included with:

  >     #include "ulp_riscv_lock.h"

- This header file is a part of the API provided by the `ulp` component. To declare that your component depends on `ulp`, add the following to your CMakeLists.txt:

  >     REQUIRES ulp

  > or

  >     PRIV_REQUIRES ulp

### Functions

void ulp_riscv_lock_acquire(ulp_riscv_lock_t *lock)

  Locks are based on the Peterson's algorithm, https://en.wikipedia.org/wiki/Peterson%27s_algorithm.

  Acquire the lock, preventing the ULP from taking until released. Spins until lock is acquired.

  备注

  The lock is only designed for being used by a single thread on the main CPU, it is not safe to try to acquire it from multiple threads.

  参数:

    lock -- Pointer to lock struct, shared with ULP

void ulp_riscv_lock_release(ulp_riscv_lock_t *lock)

  Release the lock.

  参数:

    lock -- Pointer to lock struct, shared with ULP

### Header File

- components/ulp/ulp_riscv/include/ulp_riscv_i2c.h

- This header file can be included with:

  >     #include "ulp_riscv_i2c.h"

- This header file is a part of the API provided by the `ulp` component. To declare that your component depends on `ulp`, add the following to your CMakeLists.txt:

  >     REQUIRES ulp

  > or

  >     PRIV_REQUIRES ulp

### Functions

void ulp_riscv_i2c_master_set_slave_addr(uint8_t slave_addr)

  Set the I2C slave device address.

  参数:

    slave_addr -- I2C slave address (7 bit)

void ulp_riscv_i2c_master_set_slave_reg_addr(uint8_t slave_reg_addr)

  Set the I2C slave device sub register address.

  备注

  The RTC I2C peripheral always expects a slave sub register address to be programmed. If it is not, the I2C peripheral uses the SENS_SAR_I2C_CTRL_REG[18:11] as the sub register address for the subsequent read or write operation.

  参数:

    slave_reg_addr -- I2C slave sub register address

void ulp_riscv_i2c_master_read_from_device(uint8_t *data_rd, size_t size)

  Read from I2C slave device.

  备注

  The I2C slave device address must be configured at least once before invoking this API.

  参数:

    - data_rd -- Buffer to hold data to be read

    - size -- Size of data to be read in bytes

void ulp_riscv_i2c_master_write_to_device(uint8_t *data_wr, size_t size)

  Write to I2C slave device.

  备注

  The I2C slave device address must be configured at least once before invoking this API.

  参数:

    - data_wr -- Buffer which holds the data to be written

    - size -- Size of data to be written in bytes

esp_err_t ulp_riscv_i2c_master_init(const ulp_riscv_i2c_cfg_t *cfg)

  Initialize and configure the RTC I2C for use by ULP RISC-V Currently RTC I2C can only be used in master mode.

  参数:

    cfg -- Configuration parameters

  返回:

    esp_err_t ESP_OK when successful

### Structures

struct ulp_riscv_i2c_pin_cfg_t

  ULP RISC-V RTC I2C pin config.

  Public Members

  uint32_t sda_io_num

    GPIO pin for SDA signal. Only GPIO#1 or GPIO#3 can be used as the SDA pin.

  uint32_t scl_io_num

    GPIO pin for SCL signal. Only GPIO#0 or GPIO#2 can be used as the SCL pin.

  bool sda_pullup_en

    SDA line enable internal pullup. Can be configured if external pullup is not used.

  bool scl_pullup_en

    SCL line enable internal pullup. Can be configured if external pullup is not used.

struct ulp_riscv_i2c_timing_cfg_t

  ULP RISC-V RTC I2C timing config.

  Public Members

  float scl_low_period

    SCL low period in micro seconds

  float scl_high_period

    SCL high period in micro seconds

  float sda_duty_period

    Period between the SDA switch and the falling edge of SCL in micro seconds

  float scl_start_period

    Waiting time after the START condition in micro seconds

  float scl_stop_period

    Waiting time before the END condition in micro seconds

  float i2c_trans_timeout

    I2C transaction timeout in micro seconds

struct ulp_riscv_i2c_cfg_t

  ULP RISC-V RTC I2C init parameters.

  Public Members

  ulp_riscv_i2c_pin_cfg_t i2c_pin_cfg

    RTC I2C pin configuration

  ulp_riscv_i2c_timing_cfg_t i2c_timing_cfg

    RTC I2C timing configuration

### Macros

ULP_RISCV_I2C_DEFAULT_GPIO_CONFIG()

ULP_RISCV_I2C_FAST_MODE_CONFIG()

ULP_RISCV_I2C_STANDARD_MODE_CONFIG()

ULP_RISCV_I2C_DEFAULT_CONFIG()

提供有关此文档的反馈