# ESP 本地控制

[English]

## 概述

通过 ESP-IDF 的 ESP 本地控制 (esp_local_ctrl) 组件，可使用 HTTPS 或 BLE 协议控制 ESP 设备。通过一系列可配置的处理程序，该组件允许你对应用程序定义的读/写 属性 进行访问。

通过 BLE 传输协议初始化 esp_local_ctrl 的过程如下：

>     esp_local_ctrl_config_t config = {
>         .transport = ESP_LOCAL_CTRL_TRANSPORT_BLE,
>         .transport_config = {
>             .ble = & (protocomm_ble_config_t) {
>                 .device_name  = SERVICE_NAME,
>                 .service_uuid = {
>                     /* LSB <---------------------------------------
>                     * ---------------------------------------> MSB */
>                     0x21, 0xd5, 0x3b, 0x8d, 0xbd, 0x75, 0x68, 0x8a,
>                     0xb4, 0x42, 0xeb, 0x31, 0x4a, 0x1e, 0x98, 0x3d
>                 }
>             }
>         },
>         .proto_sec = {
>             .version = PROTOCOM_SEC0,
>             .custom_handle = NULL,
>             .sec_params = NULL,
>         },
>         .handlers = {
>             /* User defined handler functions */
>             .get_prop_values = get_property_values,
>             .set_prop_values = set_property_values,
>             .usr_ctx         = NULL,
>             .usr_ctx_free_fn = NULL
>         },
>         /* Maximum number of properties that may be set */
>         .max_properties = 10
>     };

>     /* Start esp_local_ctrl service */
>     ESP_ERROR_CHECK(esp_local_ctrl_start(&config));

同样，对于 HTTP 传输：

>     /* Set the configuration */
>     httpd_ssl_config_t https_conf = HTTPD_SSL_CONFIG_DEFAULT();

>     /* Load server certificate */
>     extern const unsigned char servercert_start[] asm("_binary_servercert_pem_start");
>     extern const unsigned char servercert_end[]   asm("_binary_servercert_pem_end");
>     https_conf.servercert = servercert_start;
>     https_conf.servercert_len = servercert_end - servercert_start;

>     /* Load server private key */
>     extern const unsigned char prvtkey_pem_start[] asm("_binary_prvtkey_pem_start");
>     extern const unsigned char prvtkey_pem_end[]   asm("_binary_prvtkey_pem_end");
>     https_conf.prvtkey_pem = prvtkey_pem_start;
>     https_conf.prvtkey_len = prvtkey_pem_end - prvtkey_pem_start;

>     esp_local_ctrl_config_t config = {
>         .transport = ESP_LOCAL_CTRL_TRANSPORT_HTTPD,
>         .transport_config = {
>             .httpd = &https_conf
>         },
>         .proto_sec = {
>             .version = PROTOCOM_SEC0,
>             .custom_handle = NULL,
>             .sec_params = NULL,
>         },
>         .handlers = {
>             /* User defined handler functions */
>             .get_prop_values = get_property_values,
>             .set_prop_values = set_property_values,
>             .usr_ctx         = NULL,
>             .usr_ctx_free_fn = NULL
>         },
>         /* Maximum number of properties that may be set */
>         .max_properties = 10
>     };

>     /* Start esp_local_ctrl service */
>     ESP_ERROR_CHECK(esp_local_ctrl_start(&config));

你可以利用以下选项设置 ESP 本地控制的传输安全性：

1. `PROTOCOM_SEC2`: 指定使用基于 SRP6a 的密钥交换和基于 AES-GCM 的端到端加密。这一选项通过增强的 PAKE 协议（即 SRP6a）提供了强大的安全保障，是最受欢迎的选项。

2. `PROTOCOM_SEC1`: 指定使用基于 Curve25519 的密钥交换和基于 AES-CTR 的端到端加密。

3. `PROTOCOM_SEC0`: 指定以明文（无安全性）方式交换数据。

4. `PROTOCOM_SEC_CUSTOM`: 自定义安全需求。注意，使用这一选项时，必须提供 `protocomm_security_t *` 类型的 `custom_handle`。

备注

相应的安全方案需通过项目配置菜单启用。要了解详情，请参考 Protocol Communication 中关于启用 protocomm 安全版本的章节。

## 创建属性

启用 esp_local_ctrl 后，可以为其添加属性。每个属性必须具有唯一的名称 `name` （字符串），还需具有类型 `type` （如枚举）、标记 `flags` （位域）和大小 `size`。

如果希望属性值的长度可变（例如，字符串或字节流），则 `size` 值应保持为 0。对于有固定长度属性值的数据类型，如整型、浮点型等，将 `size` 字段设置为正确的值，有助于 esp_local_ctrl 对接收到的写入请求的参数进行内部检查。

`type` 和 `flags` 字段的含义取决于具体的应用程序，它们可以是枚举、位域、甚至整型。可以使用 `type` 表示属性，用 `flags` 指定属性的特征。

例如，以下属性被用作时间戳。此处假设应用程序定义了 `TYPE_TIMESTAMP` 和 `READONLY` 来设置此处的 `type` 和 `flags` 字段：

>     /* Create a timestamp property */
>     esp_local_ctrl_prop_t timestamp = {
>         .name        = "timestamp",
>         .type        = TYPE_TIMESTAMP,
>         .size        = sizeof(int32_t),
>         .flags       = READONLY,
>         .ctx         = func_get_time,
>         .ctx_free_fn = NULL
>     };

>     /* Now register the property */
>     esp_local_ctrl_add_property(&timestamp);

另外，此示例中还设置了一个 ctx 字段，指向自定义的 `func_get_time()`，用于在属性的 get/set 处理程序中检索时间戳。

以下为 `get_prop_values()` 处理程序的一个示例，用于检索时间戳：

>     static esp_err_t get_property_values(size_t props_count,
>                                          const esp_local_ctrl_prop_t *props,
>                                          esp_local_ctrl_prop_val_t *prop_values,
>                                          void *usr_ctx)
>     {
>         for (uint32_t i = 0; i < props_count; i++) {
>             ESP_LOGI(TAG, "Reading %s", props[i].name);
>             if (props[i].type == TYPE_TIMESTAMP) {
>                 /* Obtain the timer function from ctx */
>                 int32_t (*func_get_time)(void) = props[i].ctx;

>                 /* Use static variable for saving the value. This is essential because the value has to be valid even after this function returns. Alternative is to use dynamic allocation and set the free_fn field */
>                 static int32_t ts = func_get_time();
>                 prop_values[i].data = &ts;
>             }
>         }
>         return ESP_OK;
>     }

以下为 `set_prop_values()` 应用程序的一个示例,注意此示例是如何为只读属性限制写入操作：

>     static esp_err_t set_property_values(size_t props_count,
>                                          const esp_local_ctrl_prop_t *props,
>                                          const esp_local_ctrl_prop_val_t *prop_values,
>                                          void *usr_ctx)
>     {
>         for (uint32_t i = 0; i < props_count; i++) {
>             if (props[i].flags & READONLY) {
>                 ESP_LOGE(TAG, "Cannot write to read-only property %s", props[i].name);
>                 return ESP_ERR_INVALID_ARG;
>             } else {
>                 ESP_LOGI(TAG, "Setting %s", props[i].name);

>                 /* For keeping it simple, lets only log the incoming data */
>                 ESP_LOG_BUFFER_HEX_LEVEL(TAG, prop_values[i].data,
>                                          prop_values[i].size, ESP_LOG_INFO);
>             }
>         }
>         return ESP_OK;
>     }

完整示例请参见 protocols/esp_local_ctrl。该示例演示了如何通过 HTTPS 传输设置一个安全的 `esp_local_ctrl` 服务，以便在本地网络中控制设备。

## 客户端实现

在客户端的实现过程中，首先，通过支持的传输模式与设备建立 protocomm 会话，然后发送并接收 esp_local_ctrl 服务能够处理的 protobuf 信息。 esp_local_ctrl 服务会将这些信息转换为请求，并发起相应的处理程序 (set/get)。接着，为每个处理程序生成的响应会被再次打包到一条 protobuf 信息中，传输回客户端。

以下是 esp_local_ctrl 服务能够处理的各种 protobuf 信息：

1. `get_prop_count` : 返回服务支持的属性总数。

2. `get_prop_values` : 接受一个索引数组，并返回这些索引相对应的属性信息（名称、类型、标志）和属性值。

3. `set_prop_values` : 接受一个索引数组和一个新值数组，用于设置索引对应的属性值。

注意，在多个会话中，一个属性的索引可能相同，也可能不同。因此，客户端必须用唯一的属性名称来识别属性。每次建立新会话时，客户端都应首先调用 `get_prop_count`，然后调用 `get_prop_values`，为所有属性建立从索引到名称的映射。为一组属性调用 `set_prop_values` 时，必须先用创建的映射将名称转换为索引。如前所述，每次使用同一设备建立新会话时，客户端必须刷新该映射。

下面列出了 esp_local_ctrl 服务提供的各种 protocomm 端点：

ESP本地控制服务提供的端点
端点名称 (BLE + GATT 服务器) | URI (HTTPS 服务器 + mDNS) | 描述
--- | --- | ---
esp_local_ctrl/version | https://<mdns-hostname>.local/esp_local_ctrl/version | 检索版本字符串
esp_local_ctrl/control | https://<mdns-hostname>.local/esp_local_ctrl/control | 发送或接收控制信息

## API 参考

### Header File

- components/esp_local_ctrl/include/esp_local_ctrl.h

- This header file can be included with:

  >     #include "esp_local_ctrl.h"

- This header file is a part of the API provided by the `esp_local_ctrl` component. To declare that your component depends on `esp_local_ctrl`, add the following to your CMakeLists.txt:

  >     REQUIRES esp_local_ctrl

  > or

  >     PRIV_REQUIRES esp_local_ctrl

### Functions

const esp_local_ctrl_transport_t *esp_local_ctrl_get_transport_ble(void)

  Function for obtaining BLE transport mode.

const esp_local_ctrl_transport_t *esp_local_ctrl_get_transport_httpd(void)

  Function for obtaining HTTPD transport mode.

esp_err_t esp_local_ctrl_start(const esp_local_ctrl_config_t *config)

  Start local control service.

  参数

    config -- [in] Pointer to configuration structure

  返回

    - ESP_OK : Success

    - ESP_FAIL : Failure

esp_err_t esp_local_ctrl_stop(void)

  Stop local control service.

esp_err_t esp_local_ctrl_add_property(const esp_local_ctrl_prop_t *prop)

  Add a new property.

  This adds a new property and allocates internal resources for it. The total number of properties that could be added is limited by configuration option `max_properties`

  参数

    prop -- [in] Property description structure

  返回

    - ESP_OK : Success

    - ESP_FAIL : Failure

esp_err_t esp_local_ctrl_remove_property(const char *name)

  Remove a property.

  This finds a property by name, and releases the internal resources which are associated with it.

  参数

    name -- [in] Name of the property to remove

  返回

    - ESP_OK : Success

    - ESP_ERR_NOT_FOUND : Failure

const esp_local_ctrl_prop_t *esp_local_ctrl_get_property(const char *name)

  Get property description structure by name.

  This API may be used to get a property's context structure `esp_local_ctrl_prop_t` when its name is known

  参数

    name -- [in] Name of the property to find

  返回

    - Pointer to property

    - NULL if not found

esp_err_t esp_local_ctrl_set_handler(const char *ep_name, protocomm_req_handler_t handler, void *user_ctx)

  Register protocomm handler for a custom endpoint.

  This API can be called by the application to register a protocomm handler for an endpoint after the local control service has started.

  备注

  In case of BLE transport the names and uuids of all custom endpoints must be provided beforehand as a part of the `protocomm_ble_config_t` structure set in `esp_local_ctrl_config_t`, and passed to `esp_local_ctrl_start()`.

  参数

    - ep_name -- [in] Name of the endpoint

    - handler -- [in] Endpoint handler function

    - user_ctx -- [in] User data

  返回

    - ESP_OK : Success

    - ESP_FAIL : Failure

### Unions

union esp_local_ctrl_transport_config_t
  #include <esp_local_ctrl.h>

  Transport mode (BLE / HTTPD) configuration.

  Public Members

  esp_local_ctrl_transport_config_ble_t *ble

    This is same as `protocomm_ble_config_t`. See `protocomm_ble.h` for available configuration parameters.

  esp_local_ctrl_transport_config_httpd_t *httpd

    This is same as `httpd_ssl_config_t`. See `esp_https_server.h` for available configuration parameters.

### Structures

struct esp_local_ctrl_prop

  Property description data structure, which is to be populated and passed to the `esp_local_ctrl_add_property()` function.

  Once a property is added, its structure is available for read-only access inside `get_prop_values()` and `set_prop_values()` handlers.

  Public Members

  char *name

    Unique name of property

  uint32_t type

    Type of property. This may be set to application defined enums

  size_t size

    Size of the property value, which:

    - if zero, the property can have values of variable size

    - if non-zero, the property can have values of fixed size only, therefore, checks are performed internally by esp_local_ctrl when setting the value of such a property

  uint32_t flags

    Flags set for this property. This could be a bit field. A flag may indicate property behavior, e.g. read-only / constant

  void *ctx

    Pointer to some context data relevant for this property. This will be available for use inside the `get_prop_values` and `set_prop_values` handlers as a part of this property structure. When set, this is valid throughout the lifetime of a property, till either the property is removed or the esp_local_ctrl service is stopped.

  void (*ctx_free_fn)(void *ctx)

    Function used by esp_local_ctrl to internally free the property context when `esp_local_ctrl_remove_property()` or `esp_local_ctrl_stop()` is called.

struct esp_local_ctrl_prop_val

  Property value data structure. This gets passed to the `get_prop_values()` and `set_prop_values()` handlers for the purpose of retrieving or setting the present value of a property.

  Public Members

  void *data

    Pointer to memory holding property value

  size_t size

    Size of property value

  void (*free_fn)(void *data)

    This may be set by the application in `get_prop_values()` handler to tell `esp_local_ctrl` to call this function on the data pointer above, for freeing its resources after sending the `get_prop_values` response.

struct esp_local_ctrl_handlers

  Handlers for receiving and responding to local control commands for getting and setting properties.

  Public Members

  esp_err_t (*get_prop_values)(size_t props_count, const esp_local_ctrl_prop_t props[], esp_local_ctrl_prop_val_t prop_values[], void *usr_ctx)

    Handler function to be implemented for retrieving current values of properties.

    备注

    If any of the properties have fixed sizes, the size field of corresponding element in `prop_values` need to be set

    Param props_count

      [in] Total elements in the props array

    Param props

      [in] Array of properties, the current values for which have been requested by the client

    Param prop_values

      [out] Array of empty property values, the elements of which need to be populated with the current values of those properties specified by props argument

    Param usr_ctx

      [in] This provides value of the `usr_ctx` field of `esp_local_ctrl_handlers_t` structure

    Return

      Returning different error codes will convey the corresponding protocol level errors to the client :

      - ESP_OK : Success

      - ESP_ERR_INVALID_ARG : InvalidArgument

      - ESP_ERR_INVALID_STATE : InvalidProto

      - All other error codes : InternalError

  esp_err_t (*set_prop_values)(size_t props_count, const esp_local_ctrl_prop_t props[], const esp_local_ctrl_prop_val_t prop_values[], void *usr_ctx)

    Handler function to be implemented for changing values of properties.

    备注

    If any of the properties have variable sizes, the size field of the corresponding element in `prop_values` must be checked explicitly before making any assumptions on the size.

    Param props_count

      [in] Total elements in the props array

    Param props

      [in] Array of properties, the values for which the client requests to change

    Param prop_values

      [in] Array of property values, the elements of which need to be used for updating those properties specified by props argument

    Param usr_ctx

      [in] This provides value of the `usr_ctx` field of `esp_local_ctrl_handlers_t` structure

    Return

      Returning different error codes will convey the corresponding protocol level errors to the client :

      - ESP_OK : Success

      - ESP_ERR_INVALID_ARG : InvalidArgument

      - ESP_ERR_INVALID_STATE : InvalidProto

      - All other error codes : InternalError

  void *usr_ctx

    Context pointer to be passed to above handler functions upon invocation. This is different from the property level context, as this is valid throughout the lifetime of the `esp_local_ctrl` service, and freed only when the service is stopped.

  void (*usr_ctx_free_fn)(void *usr_ctx)

    Pointer to function which will be internally invoked on `usr_ctx` for freeing the context resources when `esp_local_ctrl_stop()` is called.

struct esp_local_ctrl_proto_sec_cfg

  Protocom security configs

  Public Members

  esp_local_ctrl_proto_sec_t version

    This sets protocom security version, sec0/sec1 or custom If custom, user must provide handle via `proto_sec_custom_handle` below

  void *custom_handle

    Custom security handle if security is set custom via `proto_sec` above This handle must follow `protocomm_security_t` signature

  const void *pop

    Proof of possession to be used for local control. Could be NULL.

  const void *sec_params

    Pointer to security params (NULL if not needed). This is not needed for protocomm security 0 This pointer should hold the struct of type esp_local_ctrl_security1_params_t for protocomm security 1 and esp_local_ctrl_security2_params_t for protocomm security 2 respectively. Could be NULL.

struct esp_local_ctrl_config

  Configuration structure to pass to `esp_local_ctrl_start()`

  Public Members

  const esp_local_ctrl_transport_t *transport

    Transport layer over which service will be provided

  esp_local_ctrl_transport_config_t transport_config

    Transport layer over which service will be provided

  esp_local_ctrl_proto_sec_cfg_t proto_sec

    Security version and POP

  esp_local_ctrl_handlers_t handlers

    Register handlers for responding to get/set requests on properties

  size_t max_properties

    This limits the number of properties that are available at a time

### Macros

ESP_LOCAL_CTRL_TRANSPORT_BLE

ESP_LOCAL_CTRL_TRANSPORT_HTTPD

### Type Definitions

typedef struct esp_local_ctrl_prop esp_local_ctrl_prop_t

  Property description data structure, which is to be populated and passed to the `esp_local_ctrl_add_property()` function.

  Once a property is added, its structure is available for read-only access inside `get_prop_values()` and `set_prop_values()` handlers.

typedef struct esp_local_ctrl_prop_val esp_local_ctrl_prop_val_t

  Property value data structure. This gets passed to the `get_prop_values()` and `set_prop_values()` handlers for the purpose of retrieving or setting the present value of a property.

typedef struct esp_local_ctrl_handlers esp_local_ctrl_handlers_t

  Handlers for receiving and responding to local control commands for getting and setting properties.

typedef struct esp_local_ctrl_transport esp_local_ctrl_transport_t

  Transport mode (BLE / HTTPD) over which the service will be provided.

  This is forward declaration of a private structure, implemented internally by `esp_local_ctrl`.

typedef struct protocomm_ble_config esp_local_ctrl_transport_config_ble_t

  Configuration for transport mode BLE.

  This is a forward declaration for `protocomm_ble_config_t`. To use this, application must set CONFIG_BT_ENABLED and include `protocomm_ble.h`.

typedef struct httpd_config esp_local_ctrl_transport_config_httpd_t

  Configuration for transport mode HTTPD.

  This is a forward declaration for `httpd_ssl_config_t` (for HTTPS) or `httpd_config_t` (for HTTP)

typedef enum esp_local_ctrl_proto_sec esp_local_ctrl_proto_sec_t

  Security types for esp_local_control.

typedef protocomm_security1_params_t esp_local_ctrl_security1_params_t

typedef protocomm_security2_params_t esp_local_ctrl_security2_params_t

typedef struct esp_local_ctrl_proto_sec_cfg esp_local_ctrl_proto_sec_cfg_t

  Protocom security configs

typedef struct esp_local_ctrl_config esp_local_ctrl_config_t

  Configuration structure to pass to `esp_local_ctrl_start()`

### Enumerations

enum esp_local_ctrl_proto_sec

  Security types for esp_local_control.

  Values:

  enumerator PROTOCOM_SEC0
  enumerator PROTOCOM_SEC1
  enumerator PROTOCOM_SEC2
  enumerator PROTOCOM_SEC_CUSTOM

此文档对您有帮助吗？

- 反馈已收到，谢谢！
- 如果您有其他意见，欢迎填写乐鑫文档反馈表。

- 我们重视您的反馈。
- 您可以填写乐鑫文档反馈表告诉我们如何改进该文档。