# ESP-BLE-MESH

备注

The current ESP-BLE-MESH v1.1 related code is a preview version, so the Mesh Protocol v1.1 related Structures, MACROs, and APIs involved in the code may be changed.

With various features of ESP-BLE-MESH, users can create a managed flooding mesh network for several scenarios, such as lighting, sensor and etc.

For an ESP32 to join and work on a ESP-BLE-MESH network, it must be provisioned firstly. By provisioning, the ESP32, as an unprovisioned device, will join the ESP-BLE-MESH network and become a ESP-BLE-MESH node, communicating with other nodes within or beyond the radio range.

Apart from ESP-BLE-MESH nodes, inside ESP-BLE-MESH network, there is also ESP32 that works as ESP-BLE-MESH provisioner, which could provision unprovisioned devices into ESP-BLE-MESH nodes and configure the nodes with various features.

For information how to start using ESP32 and ESP-BLE-MESH, please see the Section 快速入门. If you are interested in information on ESP-BLE-MESH architecture, including some details of software implementation, please see Section ESP-BLE-MESH 架构.

## Application Examples and Demos

Please refer to Sections 示例 and 演示视频.

## API Reference

ESP-BLE-MESH APIs are divided into the following parts:

- ESP-BLE-MESH Definitions

- ESP-BLE-MESH Core API Reference

- ESP-BLE-MESH Models API Reference

- ESP-BLE-MESH (v1.1) Core API Reference

## ESP-BLE-MESH Definitions

This section contains only one header file, which lists the following items of ESP-BLE-MESH.

- ID of all the models and related message opcodes

- Structs of model, element and Composition Data

- Structs of used by ESP-BLE-MESH Node/Provisioner for provisioning

- Structs used to transmit/receive messages

- Event types and related event parameters

### Header File

- components/bt/esp_ble_mesh/api/esp_ble_mesh_defs.h

- This header file can be included with:

  >     #include "esp_ble_mesh_defs.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Unions

union esp_ble_mesh_prov_cb_param_t
  #include <esp_ble_mesh_defs.h>

  BLE Mesh Node/Provisioner callback parameters union.

  Public Members

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_prov_register_comp_param prov_register_comp

    Event parameter of ESP_BLE_MESH_PROV_REGISTER_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_set_unprov_dev_name_comp_param node_set_unprov_dev_name_comp

    Event parameter of ESP_BLE_MESH_NODE_SET_UNPROV_DEV_NAME_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_prov_enable_comp_param node_prov_enable_comp

    Event parameter of ESP_BLE_MESH_NODE_PROV_ENABLE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_prov_disable_comp_param node_prov_disable_comp

    Event parameter of ESP_BLE_MESH_NODE_PROV_DISABLE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_link_open_evt_param node_prov_link_open

    Event parameter of ESP_BLE_MESH_NODE_PROV_LINK_OPEN_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_link_close_evt_param node_prov_link_close

    Event parameter of ESP_BLE_MESH_NODE_PROV_LINK_CLOSE_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_output_num_evt_param node_prov_output_num

    Event parameter of ESP_BLE_MESH_NODE_PROV_OUTPUT_NUMBER_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_output_str_evt_param node_prov_output_str

    Event parameter of ESP_BLE_MESH_NODE_PROV_OUTPUT_STRING_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_input_evt_param node_prov_input

    Event parameter of ESP_BLE_MESH_NODE_PROV_INPUT_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provision_complete_evt_param node_prov_complete

    Event parameter of ESP_BLE_MESH_NODE_PROV_COMPLETE_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provision_reset_param node_prov_reset

    Event parameter of ESP_BLE_MESH_NODE_PROV_RESET_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_set_oob_pub_key_comp_param node_prov_set_oob_pub_key_comp

    Event parameter of ESP_BLE_MESH_NODE_PROV_SET_OOB_PUB_KEY_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_input_number_comp_param node_prov_input_num_comp

    Event parameter of ESP_BLE_MESH_NODE_PROV_INPUT_NUM_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_input_string_comp_param node_prov_input_str_comp

    Event parameter of ESP_BLE_MESH_NODE_PROV_INPUT_STR_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_identity_enable_comp_param node_proxy_identity_enable_comp

    Event parameter of ESP_BLE_MESH_NODE_PROXY_IDENTITY_ENABLE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_gatt_enable_comp_param node_proxy_gatt_enable_comp

    Event parameter of ESP_BLE_MESH_NODE_PROXY_GATT_ENABLE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_gatt_disable_comp_param node_proxy_gatt_disable_comp

    Event parameter of ESP_BLE_MESH_NODE_PROXY_GATT_DISABLE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_private_identity_enable_comp_param node_private_proxy_identity_enable_comp

    Event parameter of ESP_BLE_MESH_NODE_PRIVATE_PROXY_IDENTITY_ENABLE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_private_identity_disable_comp_param node_private_proxy_identity_disable_comp

    Event parameter of ESP_BLE_MESH_NODE_PRIVATE_PROXY_IDENTITY_DISABLE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_node_add_local_net_key_comp_param node_add_net_key_comp

    Event parameter of ESP_BLE_MESH_NODE_ADD_LOCAL_NET_KEY_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_node_add_local_app_key_comp_param node_add_app_key_comp

    Event parameter of ESP_BLE_MESH_NODE_ADD_LOCAL_APP_KEY_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_node_bind_local_mod_app_comp_param node_bind_app_key_to_model_comp

    Event parameter of ESP_BLE_MESH_NODE_BIND_APP_KEY_TO_MODEL_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_recv_unprov_adv_pkt_param provisioner_recv_unprov_adv_pkt

    Event parameter of ESP_BLE_MESH_PROVISIONER_RECV_UNPROV_ADV_PKT_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_prov_enable_comp_param provisioner_prov_enable_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_ENABLE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_prov_disable_comp_param provisioner_prov_disable_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_DISABLE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_link_open_evt_param provisioner_prov_link_open

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_LINK_OPEN_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_prov_read_oob_pub_key_evt_param provisioner_prov_read_oob_pub_key

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_READ_OOB_PUB_KEY_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_prov_input_evt_param provisioner_prov_input

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_INPUT_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_prov_output_evt_param provisioner_prov_output

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_OUTPUT_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_link_close_evt_param provisioner_prov_link_close

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_LINK_CLOSE_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_prov_comp_param provisioner_prov_complete

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_COMPLETE_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_cert_based_prov_start_evt_param provisioner_cert_based_prov_start

    Event parameter of ESP_BLE_MESH_PROVISIONER_CERT_BASED_PROV_START_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_recv_prov_records_list_evt_param recv_provisioner_records_list

    Event parameter of ESP_BLE_MESH_PROVISIONER_RECV_PROV_RECORDS_LIST_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_prov_record_recv_comp_evt_param provisioner_prov_record_recv_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_RECORD_RECV_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_send_prov_records_get_evt_param provisioner_send_records_get

    Event parameter of ESP_BLE_MESH_PROVISIONER_SEND_PROV_RECORDS_GET_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_send_prov_record_req_evt_param provisioner_send_record_req

    Event parameter of ESP_BLE_MESH_PROVISIONER_SEND_PROV_RECORD_REQUEST_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_send_prov_invite_evt_param provisioner_send_prov_invite

    Event parameter of ESP_BLE_MESH_PROVISIONER_SEND_PROV_INVITE_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_send_link_close_evt_param provisioner_send_link_close

    Event parameter of ESP_BLE_MESH_PROVISIONER_SEND_LINK_CLOSE_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_add_unprov_dev_comp_param provisioner_add_unprov_dev_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_ADD_UNPROV_DEV_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_prov_dev_with_addr_comp_param provisioner_prov_dev_with_addr_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_DEV_WITH_ADDR_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_delete_dev_comp_param provisioner_delete_dev_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_DELETE_DEV_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_set_dev_uuid_match_comp_param provisioner_set_dev_uuid_match_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_SET_DEV_UUID_MATCH_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_set_prov_data_info_comp_param provisioner_set_prov_data_info_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_SET_PROV_DATA_INFO_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_set_static_oob_val_comp_param provisioner_set_static_oob_val_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_SET_STATIC_OOB_VALUE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_set_primary_elem_addr_comp_param provisioner_set_primary_elem_addr_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_SET_PRIMARY_ELEM_ADDR_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_prov_read_oob_pub_key_comp_param provisioner_prov_read_oob_pub_key_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_READ_OOB_PUB_KEY_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_prov_input_num_comp_param provisioner_prov_input_num_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_INPUT_NUMBER_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_prov_input_str_comp_param provisioner_prov_input_str_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_PROV_INPUT_STRING_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_set_node_name_comp_param provisioner_set_node_name_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_SET_NODE_NAME_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_add_local_app_key_comp_param provisioner_add_app_key_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_ADD_LOCAL_APP_KEY_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_update_local_app_key_comp_param provisioner_update_app_key_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_UPDATE_LOCAL_APP_KEY_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_bind_local_mod_app_comp_param provisioner_bind_app_key_to_model_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_BIND_APP_KEY_TO_MODEL_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_add_local_net_key_comp_param provisioner_add_net_key_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_ADD_LOCAL_NET_KEY_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_update_local_net_key_comp_param provisioner_update_net_key_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_UPDATE_LOCAL_NET_KEY_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_store_node_comp_data_comp_param provisioner_store_node_comp_data_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_STORE_NODE_COMP_DATA_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_delete_node_with_uuid_comp_param provisioner_delete_node_with_uuid_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_DELETE_NODE_WITH_UUID_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_delete_node_with_addr_comp_param provisioner_delete_node_with_addr_comp

    Event parameter of ESP_BLE_MESH_PROVISIONER_DELETE_NODE_WITH_ADDR_COMP_EVT

  int err_code

    Indicate the result of enabling/disabling to receive heartbeat messages by the Provisioner

    Indicate the result of setting the heartbeat filter type by the Provisioner

    Indicate the result of setting the heartbeat filter address by the Provisioner

    Indicate the result of directly erasing settings by the Provisioner

    Indicate the result of opening settings with index by the Provisioner

    Indicate the result of opening settings with user id by the Provisioner

    Indicate the result of closing settings with index by the Provisioner

    Indicate the result of closing settings with user id by the Provisioner

    Indicate the result of deleting settings with index by the Provisioner

    Indicate the result of deleting settings with user id by the Provisioner

    Indicate the result of Proxy Client send Solicitation PDU

  bool enable

    Indicate enabling or disabling receiving heartbeat messages

  struct esp_ble_mesh_prov_cb_param_t provisioner_enable_heartbeat_recv_comp

    ESP_BLE_MESH_PROVISIONER_ENABLE_HEARTBEAT_RECV_COMP_EVT.

    Event parameters of ESP_BLE_MESH_PROVISIONER_ENABLE_HEARTBEAT_RECV_COMP_EVT

  uint8_t type

    Type of the filter used for receiving heartbeat messages

  struct esp_ble_mesh_prov_cb_param_t provisioner_set_heartbeat_filter_type_comp

    ESP_BLE_MESH_PROVISIONER_SET_HEARTBEAT_FILTER_TYPE_COMP_EVT.

    Event parameters of ESP_BLE_MESH_PROVISIONER_SET_HEARTBEAT_FILTER_TYPE_COMP_EVT

  uint8_t op

    Operation (add, remove, clean)

  uint16_t hb_src

    Heartbeat source address

  uint16_t hb_dst

    Heartbeat destination address

  struct esp_ble_mesh_prov_cb_param_t provisioner_set_heartbeat_filter_info_comp

    ESP_BLE_MESH_PROVISIONER_SET_HEARTBEAT_FILTER_INFO_COMP_EVT.

    Event parameters of ESP_BLE_MESH_PROVISIONER_SET_HEARTBEAT_FILTER_INFO_COMP_EVT

  uint8_t init_ttl

    Heartbeat InitTTL

  uint8_t rx_ttl

    Heartbeat RxTTL

  uint8_t hops

    Heartbeat hops (InitTTL - RxTTL + 1)

  uint16_t feature

    Bit field of currently active features of the node

  int8_t rssi

    RSSI of the heartbeat message

  struct esp_ble_mesh_prov_cb_param_t provisioner_recv_heartbeat

    ESP_BLE_MESH_PROVISIONER_RECV_HEARTBEAT_MESSAGE_EVT.

    Event parameters of ESP_BLE_MESH_PROVISIONER_RECV_HEARTBEAT_MESSAGE_EVT

  struct esp_ble_mesh_prov_cb_param_t provisioner_direct_erase_settings_comp

    ESP_BLE_MESH_PROVISIONER_DIRECT_ERASE_SETTINGS_COMP_EVT.

    Event parameters of ESP_BLE_MESH_PROVISIONER_DIRECT_ERASE_SETTINGS_COMP_EVT

  uint8_t index

    Index of Provisioner settings

  struct esp_ble_mesh_prov_cb_param_t provisioner_open_settings_with_index_comp

    ESP_BLE_MESH_PROVISIONER_OPEN_SETTINGS_WITH_INDEX_COMP_EVT.

    Event parameter of ESP_BLE_MESH_PROVISIONER_OPEN_SETTINGS_WITH_INDEX_COMP_EVT

  char uid[ESP_BLE_MESH_SETTINGS_UID_SIZE + 1]

    Provisioner settings user id

  struct esp_ble_mesh_prov_cb_param_t provisioner_open_settings_with_uid_comp

    ESP_BLE_MESH_PROVISIONER_OPEN_SETTINGS_WITH_UID_COMP_EVT.

    Event parameters of ESP_BLE_MESH_PROVISIONER_OPEN_SETTINGS_WITH_UID_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t provisioner_close_settings_with_index_comp

    ESP_BLE_MESH_PROVISIONER_CLOSE_SETTINGS_WITH_INDEX_COMP_EVT.

    Event parameter of ESP_BLE_MESH_PROVISIONER_CLOSE_SETTINGS_WITH_INDEX_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t provisioner_close_settings_with_uid_comp

    ESP_BLE_MESH_PROVISIONER_CLOSE_SETTINGS_WITH_UID_COMP_EVT.

    Event parameters of ESP_BLE_MESH_PROVISIONER_CLOSE_SETTINGS_WITH_UID_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t provisioner_delete_settings_with_index_comp

    ESP_BLE_MESH_PROVISIONER_DELETE_SETTINGS_WITH_INDEX_COMP_EVT.

    Event parameter of ESP_BLE_MESH_PROVISIONER_DELETE_SETTINGS_WITH_INDEX_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t provisioner_delete_settings_with_uid_comp

    ESP_BLE_MESH_PROVISIONER_DELETE_SETTINGS_WITH_UID_COMP_EVT.

    Event parameters of ESP_BLE_MESH_PROVISIONER_DELETE_SETTINGS_WITH_UID_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_set_fast_prov_info_comp_param set_fast_prov_info_comp

    Event parameter of ESP_BLE_MESH_SET_FAST_PROV_INFO_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_set_fast_prov_action_comp_param set_fast_prov_action_comp

    Event parameter of ESP_BLE_MESH_SET_FAST_PROV_ACTION_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_heartbeat_msg_recv_param heartbeat_msg_recv

    Event parameter of ESP_BLE_MESH_HEARTBEAT_MESSAGE_RECV_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_lpn_enable_comp_param lpn_enable_comp

    Event parameter of ESP_BLE_MESH_LPN_ENABLE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_lpn_disable_comp_param lpn_disable_comp

    Event parameter of ESP_BLE_MESH_LPN_DISABLE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_lpn_poll_comp_param lpn_poll_comp

    Event parameter of ESP_BLE_MESH_LPN_POLL_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_lpn_friendship_establish_param lpn_friendship_establish

    Event parameter of ESP_BLE_MESH_LPN_FRIENDSHIP_ESTABLISH_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_lpn_friendship_terminate_param lpn_friendship_terminate

    Event parameter of ESP_BLE_MESH_LPN_FRIENDSHIP_TERMINATE_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_friend_friendship_establish_param frnd_friendship_establish

    Event parameter of ESP_BLE_MESH_FRIEND_FRIENDSHIP_ESTABLISH_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_friend_friendship_terminate_param frnd_friendship_terminate

    Event parameter of ESP_BLE_MESH_FRIEND_FRIENDSHIP_TERMINATE_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_client_recv_adv_pkt_param proxy_client_recv_adv_pkt

    Event parameter of ESP_BLE_MESH_PROXY_CLIENT_RECV_ADV_PKT_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_client_connected_param proxy_client_connected

    Event parameter of ESP_BLE_MESH_PROXY_CLIENT_CONNECTED_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_client_disconnected_param proxy_client_disconnected

    Event parameter of ESP_BLE_MESH_PROXY_CLIENT_DISCONNECTED_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_client_recv_filter_status_param proxy_client_recv_filter_status

    Event parameter of ESP_BLE_MESH_PROXY_CLIENT_RECV_FILTER_STATUS_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_client_connect_comp_param proxy_client_connect_comp

    Event parameter of ESP_BLE_MESH_PROXY_CLIENT_CONNECT_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_client_disconnect_comp_param proxy_client_disconnect_comp

    Event parameter of ESP_BLE_MESH_PROXY_CLIENT_DISCONNECT_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_client_set_filter_type_comp_param proxy_client_set_filter_type_comp

    Event parameter of ESP_BLE_MESH_PROXY_CLIENT_SET_FILTER_TYPE_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_client_add_filter_addr_comp_param proxy_client_add_filter_addr_comp

    Event parameter of ESP_BLE_MESH_PROXY_CLIENT_ADD_FILTER_ADDR_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_client_remove_filter_addr_comp_param proxy_client_remove_filter_addr_comp

    Event parameter of ESP_BLE_MESH_PROXY_CLIENT_REMOVE_FILTER_ADDR_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_client_directed_proxy_set_param proxy_client_directed_proxy_set_comp

    Event parameter of ESP_BLE_MESH_PROXY_CLIENT_DIRECTED_PROXY_SET_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_server_connected_param proxy_server_connected

    Event parameter of ESP_BLE_MESH_PROXY_SERVER_CONNECTED_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_proxy_server_disconnected_param proxy_server_disconnected

    Event parameter of ESP_BLE_MESH_PROXY_SERVER_DISCONNECTED_EVT

  uint16_t net_idx

    Corresponding NetKey Index

  uint16_t ssrc

    Solicitation SRC

  uint16_t dst

    Solicitation DST

  struct esp_ble_mesh_prov_cb_param_t proxy_client_send_solic_pdu_comp

    ESP_BLE_MESH_PROXY_CLIENT_SEND_SOLIC_PDU_COMP_EVT.

    Event parameter of ESP_BLE_MESH_PROXY_CLIENT_SEND_SOLIC_PDU_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_model_sub_group_addr_comp_param model_sub_group_addr_comp

    Event parameters of ESP_BLE_MESH_MODEL_SUBSCRIBE_GROUP_ADDR_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_model_unsub_group_addr_comp_param model_unsub_group_addr_comp

    Event parameters of ESP_BLE_MESH_MODEL_UNSUBSCRIBE_GROUP_ADDR_COMP_EVT

  struct esp_ble_mesh_prov_cb_param_t::ble_mesh_deinit_mesh_comp_param deinit_mesh_comp

    Event parameter of ESP_BLE_MESH_DEINIT_MESH_COMP_EVT

  struct ble_mesh_deinit_mesh_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_DEINIT_MESH_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of BLE Mesh deinitialization

  struct ble_mesh_friend_friendship_establish_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_FRIEND_FRIENDSHIP_ESTABLISH_EVT.

    Public Members

    uint16_t lpn_addr

      Low Power Node unicast address

  struct ble_mesh_friend_friendship_terminate_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_FRIEND_FRIENDSHIP_TERMINATE_EVT.

    Public Types

      This enum value is the reason of friendship termination on the friend node side

      Values:

      enumerator ESP_BLE_MESH_FRND_FRIENDSHIP_TERMINATE_ESTABLISH_FAIL

        Friend Offer has been sent, but Friend Offer is not received within 1 second, friendship fails to be established

      enumerator ESP_BLE_MESH_FRND_FRIENDSHIP_TERMINATE_POLL_TIMEOUT

        Friendship is established, PollTimeout timer expires and no Friend Poll/Sub Add/Sub Remove is received

      enumerator ESP_BLE_MESH_FRND_FRIENDSHIP_TERMINATE_RECV_FRND_REQ

        Receive Friend Request from existing Low Power Node

      enumerator ESP_BLE_MESH_FRND_FRIENDSHIP_TERMINATE_RECV_FRND_CLEAR

        Receive Friend Clear from other friend node

      enumerator ESP_BLE_MESH_FRND_FRIENDSHIP_TERMINATE_DISABLE

        Friend feature disabled or corresponding NetKey is deleted

    Public Members

    uint16_t lpn_addr

      Low Power Node unicast address

    enum esp_ble_mesh_prov_cb_param_t::ble_mesh_friend_friendship_terminate_param reason

      This enum value is the reason of friendship termination on the friend node side Friendship terminated reason

  struct ble_mesh_heartbeat_msg_recv_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_HEARTBEAT_MESSAGE_RECV_EVT.

    Public Members

    uint8_t hops

      Heartbeat hops (InitTTL - RxTTL + 1)

    uint16_t feature

      Bit field of currently active features of the node

  struct ble_mesh_input_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROV_INPUT_EVT.

    Public Members

    esp_ble_mesh_input_action_t action

      Action of Input OOB Authentication

    uint8_t size

      Size of Input OOB Authentication

  struct ble_mesh_input_number_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROV_INPUT_NUM_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of inputting number

  struct ble_mesh_input_string_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROV_INPUT_STR_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of inputting string

  struct ble_mesh_link_close_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROV_LINK_CLOSE_EVT.

    Public Members

    esp_ble_mesh_prov_bearer_t bearer

      Type of the bearer used when device link is closed

    uint8_t reason

      Reason of the closed provisioning link

  struct ble_mesh_link_open_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROV_LINK_OPEN_EVT.

    Public Members

    esp_ble_mesh_prov_bearer_t bearer

      Type of the bearer used when device link is open

  struct ble_mesh_lpn_disable_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_LPN_DISABLE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of disabling LPN functionality

  struct ble_mesh_lpn_enable_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_LPN_ENABLE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of enabling LPN functionality

  struct ble_mesh_lpn_friendship_establish_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_LPN_FRIENDSHIP_ESTABLISH_EVT.

    Public Members

    uint16_t friend_addr

      Friend Node unicast address

  struct ble_mesh_lpn_friendship_terminate_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_LPN_FRIENDSHIP_TERMINATE_EVT.

    Public Members

    uint16_t friend_addr

      Friend Node unicast address

  struct ble_mesh_lpn_poll_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_LPN_POLL_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of sending Friend Poll

  struct ble_mesh_model_sub_group_addr_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_MODEL_SUBSCRIBE_GROUP_ADDR_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of local model subscribing group address

    uint16_t element_addr

      Element address

    uint16_t company_id

      Company ID

    uint16_t model_id

      Model ID

    uint16_t group_addr

      Group Address

  struct ble_mesh_model_unsub_group_addr_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_MODEL_UNSUBSCRIBE_GROUP_ADDR_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of local model unsubscribing group address

    uint16_t element_addr

      Element address

    uint16_t company_id

      Company ID

    uint16_t model_id

      Model ID

    uint16_t group_addr

      Group Address

  struct ble_mesh_node_add_local_app_key_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_ADD_LOCAL_APP_KEY_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of adding local AppKey by the node

    uint16_t net_idx

      NetKey Index

    uint16_t app_idx

      AppKey Index

  struct ble_mesh_node_add_local_net_key_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_ADD_LOCAL_NET_KEY_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of adding local NetKey by the node

    uint16_t net_idx

      NetKey Index

  struct ble_mesh_node_bind_local_mod_app_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_BIND_APP_KEY_TO_MODEL_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of binding AppKey with model by the node

    uint16_t element_addr

      Element address

    uint16_t app_idx

      AppKey Index

    uint16_t company_id

      Company ID

    uint16_t model_id

      Model ID

  struct ble_mesh_output_num_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROV_OUTPUT_NUMBER_EVT.

    Public Members

    esp_ble_mesh_output_action_t action

      Action of Output OOB Authentication

    uint32_t number

      Number of Output OOB Authentication

  struct ble_mesh_output_str_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROV_OUTPUT_STRING_EVT.

    Public Members

    char string[8]

      String of Output OOB Authentication

  struct ble_mesh_prov_disable_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROV_DISABLE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of disabling BLE Mesh device

  struct ble_mesh_prov_enable_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROV_ENABLE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of enabling BLE Mesh device

  struct ble_mesh_prov_register_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROV_REGISTER_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of BLE Mesh initialization

  struct ble_mesh_provision_complete_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROV_COMPLETE_EVT.

    Public Members

    uint16_t net_idx

      NetKey Index

    uint8_t net_key[16]

      NetKey

    uint16_t addr

      Primary address

    uint8_t flags

      Flags

    uint32_t iv_index

      IV Index

  struct ble_mesh_provision_reset_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROV_RESET_EVT.

  struct ble_mesh_provisioner_add_local_app_key_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_ADD_LOCAL_APP_KEY_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of adding local AppKey by the Provisioner

    uint16_t net_idx

      NetKey Index

    uint16_t app_idx

      AppKey Index

  struct ble_mesh_provisioner_add_local_net_key_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_ADD_LOCAL_NET_KEY_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of adding local NetKey by the Provisioner

    uint16_t net_idx

      NetKey Index

  struct ble_mesh_provisioner_add_unprov_dev_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_ADD_UNPROV_DEV_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of adding device into queue by the Provisioner

  struct ble_mesh_provisioner_bind_local_mod_app_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_BIND_APP_KEY_TO_MODEL_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of binding AppKey with model by the Provisioner

    uint16_t element_addr

      Element address

    uint16_t app_idx

      AppKey Index

    uint16_t company_id

      Company ID

    uint16_t model_id

      Model ID

  struct ble_mesh_provisioner_cert_based_prov_start_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_CERT_BASED_PROV_START_EVT.

    Public Members

    uint16_t link_idx

      Index of the provisioning link

  struct ble_mesh_provisioner_delete_dev_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_DELETE_DEV_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of deleting device by the Provisioner

  struct ble_mesh_provisioner_delete_node_with_addr_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_DELETE_NODE_WITH_ADDR_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of deleting node with unicast address by the Provisioner

    uint16_t unicast_addr

      Node unicast address

  struct ble_mesh_provisioner_delete_node_with_uuid_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_DELETE_NODE_WITH_UUID_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of deleting node with uuid by the Provisioner

    uint8_t uuid[16]

      Node device uuid

  struct ble_mesh_provisioner_link_close_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_LINK_CLOSE_EVT.

    Public Members

    esp_ble_mesh_prov_bearer_t bearer

      Type of the bearer used when Provisioner link is closed

    uint8_t reason

      Reason of the closed provisioning link

  struct ble_mesh_provisioner_link_open_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_LINK_OPEN_EVT.

    Public Members

    esp_ble_mesh_prov_bearer_t bearer

      Type of the bearer used when Provisioner link is opened

  struct ble_mesh_provisioner_prov_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_COMPLETE_EVT.

    Public Members

    uint16_t node_idx

      Index of the provisioned device

    esp_ble_mesh_octet16_t device_uuid

      Device UUID of the provisioned device

    uint16_t unicast_addr

      Primary address of the provisioned device

    uint8_t element_num

      Element count of the provisioned device

    uint16_t netkey_idx

      NetKey Index of the provisioned device

  struct ble_mesh_provisioner_prov_dev_with_addr_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_DEV_WITH_ADDR_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of Provisioner starting to provision a device

  struct ble_mesh_provisioner_prov_disable_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_DISABLE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of disabling BLE Mesh Provisioner

  struct ble_mesh_provisioner_prov_enable_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_ENABLE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of enabling BLE Mesh Provisioner

  struct ble_mesh_provisioner_prov_input_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_INPUT_EVT.

    Public Members

    esp_ble_mesh_oob_method_t method

      Method of device Output OOB Authentication

    esp_ble_mesh_output_action_t action

      Action of device Output OOB Authentication

    uint8_t size

      Size of device Output OOB Authentication

    uint8_t link_idx

      Index of the provisioning link

  struct ble_mesh_provisioner_prov_input_num_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_INPUT_NUMBER_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of inputting number by the Provisioner

  struct ble_mesh_provisioner_prov_input_str_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_INPUT_STRING_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of inputting string by the Provisioner

  struct ble_mesh_provisioner_prov_output_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_OUTPUT_EVT.

    Public Members

    esp_ble_mesh_oob_method_t method

      Method of device Input OOB Authentication

    esp_ble_mesh_input_action_t action

      Action of device Input OOB Authentication

    uint8_t size

      Size of device Input OOB Authentication

    uint8_t link_idx

      Index of the provisioning link

    char string[8]

      String output by the Provisioner

    uint32_t number

      Number output by the Provisioner

    union esp_ble_mesh_prov_cb_param_t::ble_mesh_provisioner_prov_output_evt_param

      Union of output OOB

  struct ble_mesh_provisioner_prov_read_oob_pub_key_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_READ_OOB_PUB_KEY_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of setting OOB Public Key by the Provisioner

  struct ble_mesh_provisioner_prov_read_oob_pub_key_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_READ_OOB_PUB_KEY_EVT.

    Public Members

    uint8_t link_idx

      Index of the provisioning link

  struct ble_mesh_provisioner_prov_record_recv_comp_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_PROV_RECORD_RECV_COMP_EVT.

    Public Members

    uint8_t status

      Indicates whether or not the request was handled successfully

    uint16_t link_idx

      Index of the provisioning link

    uint16_t record_id

      Identifies the provisioning record for which the request is made

    uint16_t frag_offset

      The starting offset of the requested fragment in the provisioning record data

    uint16_t total_len

      Total length of the provisioning record data stored on the Provisionee

    uint8_t *record

      Provisioning record data fragment

  struct ble_mesh_provisioner_recv_prov_records_list_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_RECV_PROV_RECORDS_LIST_EVT.

    Public Members

    uint16_t link_idx

      Index of the provisioning link

    uint16_t len

      Length of message

    uint8_t *msg

      Lists the Record IDs of the provisioning records stored on the Provisionee

  struct ble_mesh_provisioner_recv_unprov_adv_pkt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_RECV_UNPROV_ADV_PKT_EVT.

    Public Members

    uint8_t dev_uuid[16]

      Device UUID of the unprovisioned device

    esp_ble_mesh_bd_addr_t addr

      Device address of the unprovisioned device

    esp_ble_mesh_addr_type_t addr_type

      Device address type

    uint16_t oob_info

      OOB Info of the unprovisioned device

    uint8_t adv_type

      Advertising type of the unprovisioned device

    esp_ble_mesh_prov_bearer_t bearer

      Bearer of the unprovisioned device

    int8_t rssi

      RSSI of the received advertising packet

  struct ble_mesh_provisioner_send_link_close_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_SEND_LINK_CLOSE_EVT.

    Public Members

    uint16_t link_idx

      Index of the provisioning link

    int err_code

      Indicate the result of send Link Close message

  struct ble_mesh_provisioner_send_prov_invite_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_SEND_PROV_INVITE_EVT.

    Public Members

    uint16_t link_idx

      Index of the provisioning link

    int err_code

      Indicate the result of send Provisioning Invite message

  struct ble_mesh_provisioner_send_prov_record_req_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_SEND_PROV_RECORD_REQUEST_EVT.

    Public Members

    int err_code

      Indicate the result of send Provisioning Record Request message

    uint16_t link_idx

      Index of the provisioning link

    uint16_t record_id

      Identifies the provisioning record for which the request is made

    uint16_t frag_offset

      The starting offset of the requested fragment in the provisioning record data

    uint16_t max_size

      The maximum size of the provisioning record fragment that the Provisioner can receive

  struct ble_mesh_provisioner_send_prov_records_get_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_SEND_PROV_RECORDS_GET_EVT.

    Public Members

    int err_code

      Indicate the result of send Provisioning Records List Get message

    uint16_t link_idx

      Index of the provisioning link

  struct ble_mesh_provisioner_set_dev_uuid_match_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_SET_DEV_UUID_MATCH_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of setting Device UUID match value by the Provisioner

  struct ble_mesh_provisioner_set_node_name_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_SET_NODE_NAME_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of setting provisioned device name by the Provisioner

    uint16_t node_index

      Index of the provisioned device

  struct ble_mesh_provisioner_set_primary_elem_addr_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_SET_PRIMARY_ELEM_ADDR_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of setting unicast address of primary element by the Provisioner

  struct ble_mesh_provisioner_set_prov_data_info_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_SET_PROV_DATA_INFO_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of setting provisioning info by the Provisioner

  struct ble_mesh_provisioner_set_static_oob_val_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_SET_STATIC_OOB_VALUE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of setting static oob value by the Provisioner

  struct ble_mesh_provisioner_store_node_comp_data_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_STORE_NODE_COMP_DATA_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of storing node composition data by the Provisioner

    uint16_t addr

      Node element address

  struct ble_mesh_provisioner_update_local_app_key_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_UPDATE_LOCAL_APP_KEY_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of updating local AppKey by the Provisioner

    uint16_t net_idx

      NetKey Index

    uint16_t app_idx

      AppKey Index

  struct ble_mesh_provisioner_update_local_net_key_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROVISIONER_UPDATE_LOCAL_NET_KEY_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of updating local NetKey by the Provisioner

    uint16_t net_idx

      NetKey Index

  struct ble_mesh_proxy_client_add_filter_addr_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROXY_CLIENT_ADD_FILTER_ADDR_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of Proxy Client add filter address

    uint8_t conn_handle

      Proxy connection handle

    uint16_t net_idx

      Corresponding NetKey Index

  struct ble_mesh_proxy_client_connect_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROXY_CLIENT_CONNECT_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of Proxy Client connect

    esp_ble_mesh_bd_addr_t addr

      Device address of the Proxy Server

    esp_ble_mesh_addr_type_t addr_type

      Device address type

    uint16_t net_idx

      Corresponding NetKey Index

  struct ble_mesh_proxy_client_connected_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROXY_CLIENT_CONNECTED_EVT.

    Public Members

    esp_ble_mesh_bd_addr_t addr

      Device address of the Proxy Server

    esp_ble_mesh_addr_type_t addr_type

      Device address type

    uint8_t conn_handle

      Proxy connection handle

    uint16_t net_idx

      Corresponding NetKey Index

  struct ble_mesh_proxy_client_directed_proxy_set_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROXY_CLIENT_DIRECTED_PROXY_CONTROL_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of Proxy Client directed proxy control address

    uint8_t conn_handle

      Proxy connection handle

    uint16_t net_idx

      Corresponding NetKey Index

  struct ble_mesh_proxy_client_disconnect_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROXY_CLIENT_DISCONNECT_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of Proxy Client disconnect

    uint8_t conn_handle

      Proxy connection handle

  struct ble_mesh_proxy_client_disconnected_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROXY_CLIENT_DISCONNECTED_EVT.

    Public Members

    esp_ble_mesh_bd_addr_t addr

      Device address of the Proxy Server

    esp_ble_mesh_addr_type_t addr_type

      Device address type

    uint8_t conn_handle

      Proxy connection handle

    uint16_t net_idx

      Corresponding NetKey Index

    uint8_t reason

      Proxy disconnect reason

  struct ble_mesh_proxy_client_recv_adv_pkt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROXY_CLIENT_RECV_ADV_PKT_EVT.

    Public Members

    esp_ble_mesh_bd_addr_t addr

      Device address

    esp_ble_mesh_addr_type_t addr_type

      Device address type

    uint16_t net_idx

      Network ID related NetKey Index

    uint8_t net_id[8]

      Network ID contained in the advertising packet

    int8_t rssi

      RSSI of the received advertising packet

  struct ble_mesh_proxy_client_recv_filter_status_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROXY_CLIENT_RECV_FILTER_STATUS_EVT.

    Public Members

    uint8_t conn_handle

      Proxy connection handle

    uint16_t server_addr

      Proxy Server primary element address

    uint16_t net_idx

      Corresponding NetKey Index

    uint8_t filter_type

      Proxy Server filter type(whitelist or blacklist)

    uint16_t list_size

      Number of addresses in the Proxy Server filter list

  struct ble_mesh_proxy_client_remove_filter_addr_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROXY_CLIENT_REMOVE_FILTER_ADDR_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of Proxy Client remove filter address

    uint8_t conn_handle

      Proxy connection handle

    uint16_t net_idx

      Corresponding NetKey Index

  struct ble_mesh_proxy_client_set_filter_type_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROXY_CLIENT_SET_FILTER_TYPE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of Proxy Client set filter type

    uint8_t conn_handle

      Proxy connection handle

    uint16_t net_idx

      Corresponding NetKey Index

  struct ble_mesh_proxy_gatt_disable_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROXY_GATT_DISABLE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of disabling Mesh Proxy Service

  struct ble_mesh_proxy_gatt_enable_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROXY_GATT_ENABLE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of enabling Mesh Proxy Service

  struct ble_mesh_proxy_identity_enable_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROXY_IDENTITY_ENABLE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of enabling Mesh Proxy advertising

  struct ble_mesh_proxy_private_identity_disable_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PRIVATE_PROXY_IDENTITY_DISABLE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of disabling Mesh Proxy private advertising

  struct ble_mesh_proxy_private_identity_enable_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PRIVATE_PROXY_IDENTITY_ENABLE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of enabling Mesh Proxy private advertising

  struct ble_mesh_proxy_server_connected_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROXY_SERVER_CONNECTED_EVT.

    Public Members

    uint8_t conn_handle

      Proxy connection handle

  struct ble_mesh_proxy_server_disconnected_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_PROXY_SERVER_DISCONNECTED_EVT.

    Public Members

    uint8_t conn_handle

      Proxy connection handle

    uint8_t reason

      Proxy disconnect reason

  struct ble_mesh_set_fast_prov_action_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_SET_FAST_PROV_ACTION_COMP_EVT.

    Public Members

    uint8_t status_action

      Indicate the result of setting action of fast provisioning

  struct ble_mesh_set_fast_prov_info_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_SET_FAST_PROV_INFO_COMP_EVT.

    Public Members

    uint8_t status_unicast

      Indicate the result of setting unicast address range of fast provisioning

    uint8_t status_net_idx

      Indicate the result of setting NetKey Index of fast provisioning

    uint8_t status_match

      Indicate the result of setting matching Device UUID of fast provisioning

  struct ble_mesh_set_oob_pub_key_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_PROV_SET_OOB_PUB_KEY_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of setting OOB Public Key

  struct ble_mesh_set_unprov_dev_name_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_NODE_SET_UNPROV_DEV_NAME_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of setting BLE Mesh device name

union esp_ble_mesh_server_state_value_t
  #include <esp_ble_mesh_defs.h>

  Server model state value union.

  Public Members

  uint8_t onoff

    The value of the Generic OnOff state

    The value of the Light LC Light OnOff state

  struct esp_ble_mesh_server_state_value_t gen_onoff

    The Generic OnOff state

  int16_t level

    The value of the Generic Level state

  struct esp_ble_mesh_server_state_value_t gen_level

    The Generic Level state

  uint8_t onpowerup

    The value of the Generic OnPowerUp state

  struct esp_ble_mesh_server_state_value_t gen_onpowerup

    The Generic OnPowerUp state

  uint16_t power

    The value of the Generic Power Actual state

  struct esp_ble_mesh_server_state_value_t gen_power_actual

    The Generic Power Actual state

  uint16_t lightness

    The value of the Light Lightness Actual state

    The value of the Light Lightness Linear state

    The value of the Light CTL Lightness state

    The value of the Light HSL Lightness state

    The value of the Light xyL Lightness state

  struct esp_ble_mesh_server_state_value_t light_lightness_actual

    The Light Lightness Actual state

  struct esp_ble_mesh_server_state_value_t light_lightness_linear

    The Light Lightness Linear state

  struct esp_ble_mesh_server_state_value_t light_ctl_lightness

    The Light CTL Lightness state

  uint16_t temperature

    The value of the Light CTL Temperature state

  int16_t delta_uv

    The value of the Light CTL Delta UV state

  struct esp_ble_mesh_server_state_value_t light_ctl_temp_delta_uv

    The Light CTL Temperature & Delta UV states

  uint16_t hue

    The value of the Light HSL Hue state

  uint16_t saturation

    The value of the Light HSL Saturation state

  struct esp_ble_mesh_server_state_value_t light_hsl

    The Light HSL composite state

  struct esp_ble_mesh_server_state_value_t light_hsl_lightness

    The Light HSL Lightness state

  struct esp_ble_mesh_server_state_value_t light_hsl_hue

    The Light HSL Hue state

  struct esp_ble_mesh_server_state_value_t light_hsl_saturation

    The Light HSL Saturation state

  struct esp_ble_mesh_server_state_value_t light_xyl_lightness

    The Light xyL Lightness state

  struct esp_ble_mesh_server_state_value_t light_lc_light_onoff

    The Light LC Light OnOff state

union esp_ble_mesh_model_cb_param_t
  #include <esp_ble_mesh_defs.h>

  BLE Mesh model callback parameters union.

  Public Members

  struct esp_ble_mesh_model_cb_param_t::ble_mesh_model_operation_evt_param model_operation

    Event parameter of ESP_BLE_MESH_MODEL_OPERATION_EVT

  struct esp_ble_mesh_model_cb_param_t::ble_mesh_model_send_comp_param model_send_comp

    Event parameter of ESP_BLE_MESH_MODEL_SEND_COMP_EVT

  struct esp_ble_mesh_model_cb_param_t::ble_mesh_model_publish_comp_param model_publish_comp

    Event parameter of ESP_BLE_MESH_MODEL_PUBLISH_COMP_EVT

  struct esp_ble_mesh_model_cb_param_t::ble_mesh_mod_recv_publish_msg_param client_recv_publish_msg

    Event parameter of ESP_BLE_MESH_CLIENT_MODEL_RECV_PUBLISH_MSG_EVT

  struct esp_ble_mesh_model_cb_param_t::ble_mesh_client_model_send_timeout_param client_send_timeout

    Event parameter of ESP_BLE_MESH_CLIENT_MODEL_SEND_TIMEOUT_EVT

  struct esp_ble_mesh_model_cb_param_t::ble_mesh_model_publish_update_evt_param model_publish_update

    Event parameter of ESP_BLE_MESH_MODEL_PUBLISH_UPDATE_EVT

  struct esp_ble_mesh_model_cb_param_t::ble_mesh_server_model_update_state_comp_param server_model_update_state

    Event parameter of ESP_BLE_MESH_SERVER_MODEL_UPDATE_STATE_COMP_EVT

  struct ble_mesh_client_model_send_timeout_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_CLIENT_MODEL_SEND_TIMEOUT_EVT.

    Public Members

    uint32_t opcode

      Opcode of the previously sent message

    esp_ble_mesh_model_t *model

      Pointer to the model which sends the previous message

    esp_ble_mesh_msg_ctx_t *ctx

      Pointer to the context of the previous message

  struct ble_mesh_mod_recv_publish_msg_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_CLIENT_MODEL_RECV_PUBLISH_MSG_EVT.

    Public Members

    uint32_t opcode

      Opcode of the unsolicited received message

    esp_ble_mesh_model_t *model

      Pointer to the model which receives the message

    esp_ble_mesh_msg_ctx_t *ctx

      Pointer to the context of the message

    uint16_t length

      Length of the received message

    uint8_t *msg

      Value of the received message

  struct ble_mesh_model_operation_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_MODEL_OPERATION_EVT.

    Public Members

    uint32_t opcode

      Opcode of the received message

    esp_ble_mesh_model_t *model

      Pointer to the model which receives the message

    esp_ble_mesh_msg_ctx_t *ctx

      Pointer to the context of the received message

    uint16_t length

      Length of the received message

    uint8_t *msg

      Value of the received message

  struct ble_mesh_model_publish_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_MODEL_PUBLISH_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of publishing a message

    esp_ble_mesh_model_t *model

      Pointer to the model which publishes the message

  struct ble_mesh_model_publish_update_evt_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_MODEL_PUBLISH_UPDATE_EVT.

    Public Members

    esp_ble_mesh_model_t *model

      Pointer to the model which is going to update its publish message

  struct ble_mesh_model_send_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_MODEL_SEND_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of sending a message

    uint32_t opcode

      Opcode of the message

    esp_ble_mesh_model_t *model

      Pointer to the model which sends the message

    esp_ble_mesh_msg_ctx_t *ctx

      Context of the message

  struct ble_mesh_server_model_update_state_comp_param
    #include <esp_ble_mesh_defs.h>

    ESP_BLE_MESH_SERVER_MODEL_UPDATE_STATE_COMP_EVT.

    Public Members

    int err_code

      Indicate the result of updating server model state

    esp_ble_mesh_model_t *model

      Pointer to the server model which state value is updated

    esp_ble_mesh_server_state_type_t type

      Type of the updated server state

### Structures

struct esp_ble_mesh_deinit_param_t

  BLE Mesh deinit parameters

  Public Members

  bool erase_flash

    Indicate if erasing flash when deinit mesh stack

struct esp_ble_mesh_scan_param_t

  Scan parameters

  Public Members

  uint16_t scan_interval

    Scan interval.

    Range: 0x0004 to 0x4000.

    Time = N * 0.625 ms. Time Range: 2.5 ms to 10.24 s

  uint16_t uncoded_scan_window

    Uncoded Scan window.

    Time scanned on uncoded PHY within a scan interval.

    Range: 0x0004 to 0x4000.

    Time = N * 0.625 ms. Time Range: 2.5 ms to 10.24 s

struct esp_ble_mesh_uar_t

  Format of Unicast Address Range

  Public Members

  uint16_t len_present

    Indicate the presence or absence of the RangeLength field

  uint16_t range_start

    15 least significant bits of the starting unicast address

  uint8_t range_length

    Number of addresses in the range (0x02 - 0xFF)

struct esp_ble_mesh_elem_t

  Abstraction that describes a BLE Mesh Element. This structure is associated with struct bt_mesh_elem in mesh_access.h

  Public Members

  uint16_t element_addr

    Element Address, assigned during provisioning.

  const uint16_t location

    Location Descriptor (GATT Bluetooth Namespace Descriptors)

  const uint8_t sig_model_count

    SIG Model count

  const uint8_t vnd_model_count

    Vendor Model count

  esp_ble_mesh_model_t *sig_models

    SIG Models

  esp_ble_mesh_model_t *vnd_models

    Vendor Models

struct esp_ble_mesh_model_pub_t

  Abstraction that describes a model publication context. This structure is associated with struct bt_mesh_model_pub in mesh_access.h

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the model to which the context belongs. Initialized by the stack.

  uint16_t publish_addr

    Publish Address.

  uint16_t app_idx

    Publish AppKey Index.

  uint16_t cred

    Friendship Credentials Flag.

  uint16_t send_rel

    Force reliable sending (segment acks)

  uint16_t send_szmic

    Size of TransMIC when publishing a Segmented Access message

  uint8_t ttl

    Publish Time to Live.

  uint8_t retransmit

    Retransmit Count & Interval Steps.

  uint8_t period

    Publish Period.

  uint8_t period_div

    Divisor for the Period.

  uint8_t fast_period

    Use FastPeriodDivisor

  uint8_t count

    Retransmissions left.

  uint32_t period_start

    Start of the current period.

  struct net_buf_simple *msg

    Publication buffer, containing the publication message.

    This will get correctly created when the publication context has been defined using the ESP_BLE_MESH_MODEL_PUB_DEFINE macro.

    ESP_BLE_MESH_MODEL_PUB_DEFINE(name, size);

  esp_ble_mesh_cb_t update

    Callback used to update publish message. Initialized by the stack.

  struct k_delayed_work timer

    Publish Period Timer. Initialized by the stack.

  uint8_t dev_role

    Role of the device that is going to publish messages

struct esp_ble_mesh_model_op_t

  Abstraction that describes a model operation context. This structure is associated with struct bt_mesh_model_op in mesh_access.h

  Public Members

  const uint32_t opcode

    Message opcode

  const size_t min_len

    Message minimum length

  esp_ble_mesh_cb_t param_cb

    Callback used to handle message. Initialized by the stack.

struct esp_ble_mesh_model_cbs_t

  Abstraction that describes a model callback structure. This structure is associated with struct bt_mesh_model_cb in mesh_access.h.

  Public Members

  esp_ble_mesh_cb_t init_cb

    Callback used during model initialization. Initialized by the stack.

struct esp_ble_mesh_model

  Abstraction that describes a Mesh Model instance. This structure is associated with struct bt_mesh_model in mesh_access.h

  Public Members

  const uint16_t model_id

    16-bit model identifier

  uint16_t company_id

    16-bit company identifier

  uint16_t model_id

    16-bit model identifier

  struct esp_ble_mesh_model vnd

    Structure encapsulating a model ID with a company ID

  union esp_ble_mesh_model

    Model ID

  uint8_t element_idx

    Internal information, mainly for persistent storage Belongs to Nth element

  uint8_t model_idx

    Is the Nth model in the element

  uint16_t flags

    Information about what has changed

  esp_ble_mesh_elem_t *element

    The Element to which this Model belongs

  esp_ble_mesh_model_pub_t *const pub

    Model Publication

  uint16_t keys[CONFIG_BLE_MESH_MODEL_KEY_COUNT]

    AppKey List

  uint16_t groups[CONFIG_BLE_MESH_MODEL_GROUP_COUNT]

    Subscription List (group or virtual addresses)

  esp_ble_mesh_model_op_t *op

    Model operation context

  esp_ble_mesh_model_cbs_t *cb

    Model callback structure

  void *user_data

    Model-specific user data

struct esp_ble_mesh_adv_cfg_t

  Enhanced configuration for Mesh messages with legacy advertising

  Public Members

  uint32_t adv_itvl

    Advertising interval in milliseconds. If set to 0, the Mesh protocol stack's xmit parameters are used. If set to another value (e.g., 10), the advertising interval will be 10 ms.

  uint8_t adv_cnt

    Number of advertising per packet. If set to 0, the Mesh protocol stack's xmit parameters are used. If set to another value (e.g., 3), the number of advertising per packet will be 3.

  uint8_t channel_map

    Advertising channel map. If set to 0, the protocol stack uses default channels. If set to another value (e.g., ESP_BLE_MESH_ADV_CHAN_37), the advertising channel map will be 0x01, the advertising packet will only advertise on channel 37.

struct esp_ble_mesh_msg_enh_params_t

  Enhanced message advertising parameters

  Public Members

  uint8_t adv_cfg_used

    Use custom advertising parameters (0: disabled, 1: enabled). When enabled, `adv_cfg` parameters override stack defaults.

  esp_ble_mesh_adv_cfg_t adv_cfg

    Standard advertising parameters

struct esp_ble_mesh_msg_ctx_t

  Message sending context. This structure is associated with struct bt_mesh_msg_ctx in mesh_access.h

  Public Members

  uint16_t net_idx

    NetKey Index of the subnet through which to send the message.

  uint16_t app_idx

    AppKey Index for message encryption.

  uint16_t addr

    Remote address.

  uint16_t recv_dst

    Destination address of a received message. Not used for sending.

  int8_t recv_rssi

    RSSI of a received message. Not used for sending.

  uint32_t recv_op

    Opcode of a received message. Not used for sending.

  uint8_t recv_ttl

    Received TTL value. Not used for sending.

  uint8_t recv_cred

    Security credentials of a received message. Not used for sending.

  uint8_t recv_tag

    Tag of a received message. Not used for sending.

  uint8_t send_rel

    Force sending reliably by using segment acknowledgement.

  uint8_t send_szmic

    Size of TransMIC when sending a Segmented Access message.

  uint8_t send_ttl

    TTL, or ESP_BLE_MESH_TTL_DEFAULT for default TTL.

  uint8_t send_cred

    Security credentials used for sending the message

  uint8_t send_tag

    Tag used for sending the message.

  esp_ble_mesh_model_t *model

    Model corresponding to the message, no need to be initialized before sending message

  bool srv_send

    Indicate if the message is sent by a node server model, no need to be initialized before sending message

  esp_ble_mesh_msg_enh_params_t enh

    Enhanced message advertising parameters

struct esp_ble_mesh_prov_t

  Provisioning properties & capabilities. This structure is associated with struct bt_mesh_prov in mesh_access.h

struct esp_ble_mesh_comp_t

  Node Composition data context. This structure is associated with struct bt_mesh_comp in mesh_access.h

  Public Members

  uint16_t cid

    16-bit SIG-assigned company identifier

  uint16_t pid

    16-bit vendor-assigned product identifier

  uint16_t vid

    16-bit vendor-assigned product version identifier

  size_t element_count

    Element count

  esp_ble_mesh_elem_t *elements

    A sequence of elements

struct esp_ble_mesh_unprov_dev_add_t

  Information of the device which is going to be added for provisioning.

  Public Members

  esp_ble_mesh_bd_addr_t addr

    Device address

  esp_ble_mesh_addr_type_t addr_type

    Device address type

  uint8_t uuid[16]

    Device UUID

  uint16_t oob_info

    Device OOB Info ADD_DEV_START_PROV_NOW_FLAG shall not be set if the bearer has both PB-ADV and PB-GATT enabled

  esp_ble_mesh_prov_bearer_t bearer

    Provisioning Bearer

struct esp_ble_mesh_device_delete_t

  Information of the device which is going to be deleted.

  Public Members

  esp_ble_mesh_bd_addr_t addr

    Device address

  esp_ble_mesh_addr_type_t addr_type

    Device address type

  uint8_t uuid[16]

    Device UUID

  union esp_ble_mesh_device_delete_t

    Union of Device information

  uint8_t flag

    BIT0: device address; BIT1: device UUID

struct esp_ble_mesh_prov_data_info_t

  Information of the provisioner which is going to be updated.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint8_t flags

    Flags

  uint32_t iv_index

    IV Index

  union esp_ble_mesh_prov_data_info_t

    Provisioning data

  uint8_t flag

    BIT0: net_idx; BIT1: flags; BIT2: iv_index

struct esp_ble_mesh_node_t

  Information of the provisioned node

  Public Members

  esp_ble_mesh_bd_addr_t addr

    Node device address

  esp_ble_mesh_addr_type_t addr_type

    Node device address type

  uint8_t dev_uuid[16]

    Device UUID

  uint16_t oob_info

    Node OOB information

  uint16_t unicast_addr

    Node unicast address

  uint8_t element_num

    Node element number

  uint16_t net_idx

    Node NetKey Index

  uint8_t flags

    Node key refresh flag and iv update flag

  uint32_t iv_index

    Node IV Index

  uint8_t dev_key[16]

    Node device key

  char name[ESP_BLE_MESH_NODE_NAME_MAX_LEN + 1]

    Node name

  uint16_t comp_length

    Length of Composition Data

  uint8_t *comp_data

    Value of Composition Data

struct esp_ble_mesh_fast_prov_info_t

  Context of fast provisioning which need to be set.

  Public Members

  uint16_t unicast_min

    Minimum unicast address used for fast provisioning

  uint16_t unicast_max

    Maximum unicast address used for fast provisioning

  uint16_t net_idx

    Netkey index used for fast provisioning

  uint8_t flags

    Flags used for fast provisioning

  uint32_t iv_index

    IV Index used for fast provisioning

  uint8_t offset

    Offset of the UUID to be compared

  uint8_t match_len

    Length of the UUID to be compared

  uint8_t match_val[16]

    Value of UUID to be compared

struct esp_ble_mesh_heartbeat_filter_info_t

  Context of Provisioner heartbeat filter information to be set

  Public Members

  uint16_t hb_src

    Heartbeat source address (unicast address)

  uint16_t hb_dst

    Heartbeat destination address (unicast address or group address)

struct esp_ble_mesh_client_op_pair_t

  BLE Mesh client models related definitions.

  Client model Get/Set message opcode and corresponding Status message opcode

  Public Members

  uint32_t cli_op

    The client message opcode

  uint32_t status_op

    The server status opcode corresponding to the client message opcode

struct esp_ble_mesh_client_t

  Client Model user data context.

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the client model. Initialized by the stack.

  uint32_t op_pair_size

    Size of the op_pair

  const esp_ble_mesh_client_op_pair_t *op_pair

    Table containing get/set message opcode and corresponding status message opcode

  uint32_t publish_status

    Callback used to handle the received unsolicited message. Initialized by the stack.

  void *internal_data

    Pointer to the internal data of client model

  void *vendor_data

    Pointer to the vendor data of client model

  uint8_t msg_role

    Role of the device (Node/Provisioner) that is going to send messages

struct esp_ble_mesh_client_common_param_t

  Common parameters of the messages sent by Client Model.

  Public Members

  esp_ble_mesh_opcode_t opcode

    Message opcode

  esp_ble_mesh_model_t *model

    Pointer to the client model structure

  esp_ble_mesh_msg_ctx_t ctx

    The context used to send message

  int32_t msg_timeout

    Timeout value (ms) to get response to the sent message Note: if using default timeout value in menuconfig, make sure to set this value to 0

  uint8_t msg_role

    Role of the device - Node/Provisioner

struct esp_ble_mesh_state_transition_t

  Parameters of the server model state transition

  Public Functions

  BLE_MESH_ATOMIC_DEFINE(flag, ESP_BLE_MESH_SERVER_FLAG_MAX)

    Flag used to indicate if the transition timer has been started internally.

    If the model which contains esp_ble_mesh_state_transition_t sets "set_auto_rsp" to ESP_BLE_MESH_SERVER_RSP_BY_APP, the handler of the timer shall be initialized by the users.

    And users can use this flag to indicate whether the timer is started or not.

  Public Members

  bool just_started

    Indicate if the state transition has just started

  uint8_t trans_time

    State transition time

  uint8_t remain_time

    Remaining time of state transition

  uint8_t delay

    Delay before starting state transition

  uint32_t quo_tt

    Duration of each divided transition step

  uint32_t counter

    Number of steps which the transition duration is divided

  uint32_t total_duration

    State transition total duration

  int64_t start_timestamp

    Time when the state transition is started

  struct k_delayed_work timer

    Timer used for state transition

struct esp_ble_mesh_last_msg_info_t

  Parameters of the server model received last same set message.

  Public Members

  uint8_t tid

    Transaction number of the last message

  uint16_t src

    Source address of the last message

  uint16_t dst

    Destination address of the last message

  int64_t timestamp

    Time when the last message is received

struct esp_ble_mesh_server_rsp_ctrl_t

  Parameters of the Server Model response control

  Public Members

  uint8_t get_auto_rsp

    BLE Mesh Server Response Option.

    1. If get_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, then the response of Client Get messages need to be replied by the application;

    2. If get_auto_rsp is set to ESP_BLE_MESH_SERVER_AUTO_RSP, then the response of Client Get messages will be replied by the server models;

    3. If set_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, then the response of Client Set messages need to be replied by the application;

    4. If set_auto_rsp is set to ESP_BLE_MESH_SERVER_AUTO_RSP, then the response of Client Set messages will be replied by the server models;

    5. If status_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, then the response of Server Status messages need to be replied by the application;

    6. If status_auto_rsp is set to ESP_BLE_MESH_SERVER_AUTO_RSP, then the response of Server Status messages will be replied by the server models; Response control for Client Get messages

  uint8_t set_auto_rsp

    Response control for Client Set messages

  uint8_t status_auto_rsp

    Response control for Server Status messages

### Macros

ESP_BLE_MESH_SDU_MAX_LEN

  < The maximum length of a BLE Mesh message, including Opcode, Payload and TransMIC

ESP_BLE_MESH_MIC_SHORT

  < Length of a short Mesh MIC. Length of a long Mesh MIC.

ESP_BLE_MESH_MIC_LONG

  The maximum length of a BLE Mesh provisioned node name

ESP_BLE_MESH_NODE_NAME_MAX_LEN

  The maximum length of a BLE Mesh unprovisioned device name

ESP_BLE_MESH_DEVICE_NAME_MAX_LEN

  The maximum length of settings user id

ESP_BLE_MESH_SETTINGS_UID_SIZE

  The default value of Random Update Interval Steps

ESP_BLE_MESH_RAND_UPDATE_INTERVAL_DEFAULT

  Invalid settings index

ESP_BLE_MESH_INVALID_SETTINGS_IDX

  Define the BLE Mesh octet 16 bytes size

ESP_BLE_MESH_OCTET16_LEN

ESP_BLE_MESH_OCTET8_LEN

ESP_BLE_MESH_CID_NVAL

  Special TTL value to request using configured default TTL

ESP_BLE_MESH_TTL_DEFAULT

  Maximum allowed TTL value

ESP_BLE_MESH_TTL_MAX

ESP_BLE_MESH_ADDR_UNASSIGNED

ESP_BLE_MESH_ADDR_ALL_NODES

ESP_BLE_MESH_ADDR_PROXIES

ESP_BLE_MESH_ADDR_FRIENDS

ESP_BLE_MESH_ADDR_RELAYS

ESP_BLE_MESH_KEY_UNUSED

ESP_BLE_MESH_KEY_DEV

ESP_BLE_MESH_KEY_PRIMARY

ESP_BLE_MESH_KEY_ANY

  Internal macros used to initialize array members

ESP_BLE_MESH_KEY_UNUSED_ELT_(IDX, _)

ESP_BLE_MESH_ADDR_UNASSIGNED_ELT_(IDX, _)

ESP_BLE_MESH_MODEL_KEYS_UNUSED

ESP_BLE_MESH_MODEL_GROUPS_UNASSIGNED

ESP_BLE_MESH_NET_PRIMARY

  < Primary Network Key index Relay state value

ESP_BLE_MESH_RELAY_DISABLED

ESP_BLE_MESH_RELAY_ENABLED

ESP_BLE_MESH_RELAY_NOT_SUPPORTED

  Beacon state value

ESP_BLE_MESH_BEACON_DISABLED

ESP_BLE_MESH_BEACON_ENABLED

ESP_BLE_MESH_PRIVATE_BEACON_DISABLE

ESP_BLE_MESH_PRIVATE_BEACON_ENABLE

  GATT Proxy state value

ESP_BLE_MESH_GATT_PROXY_DISABLED

ESP_BLE_MESH_GATT_PROXY_ENABLED

ESP_BLE_MESH_GATT_PROXY_NOT_SUPPORTED

ESP_BLE_MESH_PRIVATE_GATT_PROXY_DISABLED

ESP_BLE_MESH_PRIVATE_GATT_PROXY_ENABLED

ESP_BLE_MESH_PRIVATE_GATT_PROXY_NOT_SUPPORTED

ESP_BLE_MESH_PRIVATE_NODE_IDENTITY_DISABLED

ESP_BLE_MESH_PRIVATE_NODE_IDENTITY_ENABLED

ESP_BLE_MESH_PRIVATE_NODE_IDENTITY_NOT_SUPPORTED

  Friend state value

ESP_BLE_MESH_FRIEND_DISABLED

ESP_BLE_MESH_FRIEND_ENABLED

ESP_BLE_MESH_FRIEND_NOT_SUPPORTED

  Node identity state value

ESP_BLE_MESH_NODE_IDENTITY_STOPPED

ESP_BLE_MESH_NODE_IDENTITY_RUNNING

ESP_BLE_MESH_NODE_IDENTITY_NOT_SUPPORTED

  Subnet Bridge state value

ESP_BLE_MESH_SUBNET_BRIDGE_DISABLED

ESP_BLE_MESH_SUBNET_BRIDGE_ENABLED

  Supported features

ESP_BLE_MESH_FEATURE_RELAY

ESP_BLE_MESH_FEATURE_PROXY

ESP_BLE_MESH_FEATURE_FRIEND

ESP_BLE_MESH_FEATURE_LOW_POWER

ESP_BLE_MESH_FEATURE_ALL_SUPPORTED

ESP_BLE_MESH_ADDR_IS_UNICAST(addr)

ESP_BLE_MESH_ADDR_IS_GROUP(addr)

ESP_BLE_MESH_ADDR_IS_VIRTUAL(addr)

ESP_BLE_MESH_ADDR_IS_RFU(addr)

ESP_BLE_MESH_INVALID_NODE_INDEX

ESP_BLE_MESH_PROV_RECORD_MAX_ID

ESP_BLE_MESH_TRANSMIT(count, int_ms)

  Encode transmission count & interval steps.

  备注

  For example, ESP_BLE_MESH_TRANSMIT(2, 20) means that the message will be sent about 90ms(count is 3, step is 1, interval is 30 ms

  which includes 10ms of advertising interval random delay).

  参数:

    - count -- Number of retransmissions (first transmission is excluded).

    - int_ms -- Interval steps in milliseconds. Must be greater than 0 and a multiple of 10.

  返回:

    BLE Mesh transmit value that can be used e.g. for the default values of the Configuration Model data.

ESP_BLE_MESH_GET_TRANSMIT_COUNT(transmit)

  Decode transmit count from a transmit value.

  参数:

    - transmit -- Encoded transmit count & interval value.

  返回:

    Transmission count (actual transmissions equal to N + 1).

ESP_BLE_MESH_GET_TRANSMIT_INTERVAL(transmit)

  Decode transmit interval from a transmit value.

  参数:

    - transmit -- Encoded transmit count & interval value.

  返回:

    Transmission interval in milliseconds.

ESP_BLE_MESH_PUBLISH_TRANSMIT(count, int_ms)

  Encode Publish Retransmit count & interval steps.

  参数:

    - count -- Number of retransmissions (first transmission is excluded).

    - int_ms -- Interval steps in milliseconds. Must be greater than 0 and a multiple of 50.

  返回:

    BLE Mesh transmit value that can be used e.g. for the default values of the Configuration Model data.

ESP_BLE_MESH_GET_PUBLISH_TRANSMIT_COUNT(transmit)

  Decode Publish Retransmit count from a given value.

  参数:

    - transmit -- Encoded Publish Retransmit count & interval value.

  返回:

    Retransmission count (actual transmissions equal to N + 1).

ESP_BLE_MESH_GET_PUBLISH_TRANSMIT_INTERVAL(transmit)

  Decode Publish Retransmit interval from a given value.

  Callbacks which are not needed to be initialized by users (set with 0 and will be initialized internally)

  参数:

    - transmit -- Encoded Publish Retransmit count & interval value.

  返回:

    Transmission interval in milliseconds.

ESP_BLE_MESH_PROV_STATIC_OOB_MAX_LEN

  Maximum length of string used by Output OOB authentication

ESP_BLE_MESH_PROV_OUTPUT_OOB_MAX_LEN

  Maximum length of string used by Output OOB authentication

ESP_BLE_MESH_PROV_INPUT_OOB_MAX_LEN

  Macros used to define message opcode

ESP_BLE_MESH_MODEL_OP_1(b0)

ESP_BLE_MESH_MODEL_OP_2(b0, b1)

ESP_BLE_MESH_MODEL_OP_3(b0, cid)

  This macro is associated with BLE_MESH_MODEL_CB in mesh_access.h

ESP_BLE_MESH_SIG_MODEL(_id, _op, _pub, _user_data)

ESP_BLE_MESH_VENDOR_MODEL(_company, _id, _op, _pub, _user_data)

  < This macro is associated with BLE_MESH_MODEL_VND_CB in mesh_access.h

ESP_BLE_MESH_ELEMENT(_loc, _mods, _vnd_mods)

  Helper to define a BLE Mesh element within an array.

  In case the element has no SIG or Vendor models, the helper macro ESP_BLE_MESH_MODEL_NONE can be given instead.

  备注

  This macro is associated with BLE_MESH_ELEM in mesh_access.h

  参数:

    - _loc -- Location Descriptor.

    - _mods -- Array of SIG models.

    - _vnd_mods -- Array of vendor models.

ESP_BLE_MESH_PROV(uuid, sta_val, sta_val_len, out_size, out_act, in_size, in_act)

BT_OCTET32_LEN

BD_ADDR_LEN

ESP_BLE_MESH_ADDR_TYPE_PUBLIC

ESP_BLE_MESH_ADDR_TYPE_RANDOM

ESP_BLE_MESH_ADDR_TYPE_RPA_PUBLIC

ESP_BLE_MESH_ADDR_TYPE_RPA_RANDOM

ESP_BLE_MESH_DIRECTED_FORWARDING_DISABLED

ESP_BLE_MESH_DIRECTED_FORWARDING_ENABLED

ESP_BLE_MESH_DIRECTED_RELAY_DISABLED

ESP_BLE_MESH_DIRECTED_RELAY_ENABLED

ESP_BLE_MESH_DIRECTED_PROXY_IGNORE

ESP_BLE_MESH_DIRECTED_PROXY_USE_DEFAULT_IGNORE

ESP_BLE_MESH_DIRECTED_FRIEND_IGNORE

ESP_BLE_MESH_DIRECTED_PROXY_DISABLED

ESP_BLE_MESH_DIRECTED_PROXY_ENABLED

ESP_BLE_MESH_DIRECTED_PROXY_NOT_SUPPORTED

ESP_BLE_MESH_DIRECTED_PROXY_USE_DEF_DISABLED

ESP_BLE_MESH_DIRECTED_PROXY_USE_DEF_ENABLED

ESP_BLE_MESH_DIRECTED_PROXY_USE_DEF_NOT_SUPPORTED

ESP_BLE_MESH_DIRECTED_FRIEND_DISABLED

ESP_BLE_MESH_DIRECTED_FRIEND_ENABLED

ESP_BLE_MESH_DIRECTED_FRIEND_NOT_SUPPORTED

ESP_BLE_MESH_DIRECTED_PUB_POLICY_FLOODING

ESP_BLE_MESH_DIRECTED_PUB_POLICY_FORWARD

ESP_BLE_MESH_PROXY_USE_DIRECTED_DISABLED

ESP_BLE_MESH_PROXY_USE_DIRECTED_ENABLED

ESP_BLE_MESH_FLOODING_CRED

ESP_BLE_MESH_FRIENDSHIP_CRED

ESP_BLE_MESH_DIRECTED_CRED

ESP_BLE_MESH_TAG_SEND_SEGMENTED

ESP_BLE_MESH_TAG_IMMUTABLE_CRED

ESP_BLE_MESH_TAG_USE_DIRECTED

ESP_BLE_MESH_TAG_RELAY

ESP_BLE_MESH_TAG_FRIENDSHIP

ESP_BLE_MESH_SEG_SZMIC_SHORT

ESP_BLE_MESH_SEG_SZMIC_LONG

ESP_BLE_MESH_MODEL_PUB_DEFINE(_name, _msg_len, _role)

  Define a model publication context.

  参数:

    - _name -- Variable name given to the context.

    - _msg_len -- Length of the publication message.

    - _role -- Role of the device which contains the model.

ESP_BLE_MESH_MODEL_OP(_opcode, _min_len)

  Define a model operation context.

  参数:

    - _opcode -- Message opcode.

    - _min_len -- Message minimum length.

ESP_BLE_MESH_MODEL_OP_END

  Define the terminator for the model operation table. Each model operation struct array must use this terminator as the end tag of the operation unit.

ESP_BLE_MESH_MODEL_NONE

  Helper to define an empty model array. This structure is associated with BLE_MESH_MODEL_NONE in mesh_access.h

ESP_BLE_MESH_ADV_CFG_NULL

ESP_BLE_MESH_EXT_ADV_CFG_NULL

ESP_BLE_MESH_ADV_CFG_DEFAULT

ESP_BLE_MESH_EXT_ADV_CFG_DEFAULT

ADD_DEV_RM_AFTER_PROV_FLAG

  Device will be removed from queue after provisioned successfully

ADD_DEV_START_PROV_NOW_FLAG

  Start provisioning device immediately

ADD_DEV_FLUSHABLE_DEV_FLAG

  Device can be remove when queue is full and new device is going to added

DEL_DEV_ADDR_FLAG

DEL_DEV_UUID_FLAG

PROV_DATA_NET_IDX_FLAG

PROV_DATA_FLAGS_FLAG

PROV_DATA_IV_INDEX_FLAG

ESP_BLE_MESH_HEARTBEAT_FILTER_ACCEPTLIST

ESP_BLE_MESH_HEARTBEAT_FILTER_REJECTLIST

  Provisioner heartbeat filter operation

ESP_BLE_MESH_HEARTBEAT_FILTER_ADD

ESP_BLE_MESH_HEARTBEAT_FILTER_REMOVE

ESP_BLE_MESH_MODEL_ID_CONFIG_SRV

  BLE Mesh models related Model ID and Opcode definitions.

  < Foundation Models

ESP_BLE_MESH_MODEL_ID_CONFIG_CLI

ESP_BLE_MESH_MODEL_ID_HEALTH_SRV

ESP_BLE_MESH_MODEL_ID_HEALTH_CLI

ESP_BLE_MESH_MODEL_ID_RPR_SRV

ESP_BLE_MESH_MODEL_ID_RPR_CLI

ESP_BLE_MESH_MODEL_ID_DF_SRV

ESP_BLE_MESH_MODEL_ID_DF_CLI

ESP_BLE_MESH_MODEL_ID_BRC_SRV

ESP_BLE_MESH_MODEL_ID_BRC_CLI

ESP_BLE_MESH_MODEL_ID_PRB_SRV

ESP_BLE_MESH_MODEL_ID_PRB_CLI

ESP_BLE_MESH_MODEL_ID_ODP_SRV

ESP_BLE_MESH_MODEL_ID_ODP_CLI

ESP_BLE_MESH_MODEL_ID_SAR_SRV

ESP_BLE_MESH_MODEL_ID_SAR_CLI

ESP_BLE_MESH_MODEL_ID_AGG_SRV

ESP_BLE_MESH_MODEL_ID_AGG_CLI

ESP_BLE_MESH_MODEL_ID_LCD_SRV

ESP_BLE_MESH_MODEL_ID_LCD_CLI

ESP_BLE_MESH_MODEL_ID_SRPL_SRV

ESP_BLE_MESH_MODEL_ID_SRPL_CLI

  Models from the Mesh Model Specification

ESP_BLE_MESH_MODEL_ID_GEN_ONOFF_SRV

ESP_BLE_MESH_MODEL_ID_GEN_ONOFF_CLI

ESP_BLE_MESH_MODEL_ID_GEN_LEVEL_SRV

ESP_BLE_MESH_MODEL_ID_GEN_LEVEL_CLI

ESP_BLE_MESH_MODEL_ID_GEN_DEF_TRANS_TIME_SRV

ESP_BLE_MESH_MODEL_ID_GEN_DEF_TRANS_TIME_CLI

ESP_BLE_MESH_MODEL_ID_GEN_POWER_ONOFF_SRV

ESP_BLE_MESH_MODEL_ID_GEN_POWER_ONOFF_SETUP_SRV

ESP_BLE_MESH_MODEL_ID_GEN_POWER_ONOFF_CLI

ESP_BLE_MESH_MODEL_ID_GEN_POWER_LEVEL_SRV

ESP_BLE_MESH_MODEL_ID_GEN_POWER_LEVEL_SETUP_SRV

ESP_BLE_MESH_MODEL_ID_GEN_POWER_LEVEL_CLI

ESP_BLE_MESH_MODEL_ID_GEN_BATTERY_SRV

ESP_BLE_MESH_MODEL_ID_GEN_BATTERY_CLI

ESP_BLE_MESH_MODEL_ID_GEN_LOCATION_SRV

ESP_BLE_MESH_MODEL_ID_GEN_LOCATION_SETUP_SRV

ESP_BLE_MESH_MODEL_ID_GEN_LOCATION_CLI

ESP_BLE_MESH_MODEL_ID_GEN_ADMIN_PROP_SRV

ESP_BLE_MESH_MODEL_ID_GEN_MANUFACTURER_PROP_SRV

ESP_BLE_MESH_MODEL_ID_GEN_USER_PROP_SRV

ESP_BLE_MESH_MODEL_ID_GEN_CLIENT_PROP_SRV

ESP_BLE_MESH_MODEL_ID_GEN_PROP_CLI

ESP_BLE_MESH_MODEL_ID_SENSOR_SRV

ESP_BLE_MESH_MODEL_ID_SENSOR_SETUP_SRV

ESP_BLE_MESH_MODEL_ID_SENSOR_CLI

ESP_BLE_MESH_MODEL_ID_TIME_SRV

ESP_BLE_MESH_MODEL_ID_TIME_SETUP_SRV

ESP_BLE_MESH_MODEL_ID_TIME_CLI

ESP_BLE_MESH_MODEL_ID_SCENE_SRV

ESP_BLE_MESH_MODEL_ID_SCENE_SETUP_SRV

ESP_BLE_MESH_MODEL_ID_SCENE_CLI

ESP_BLE_MESH_MODEL_ID_SCHEDULER_SRV

ESP_BLE_MESH_MODEL_ID_SCHEDULER_SETUP_SRV

ESP_BLE_MESH_MODEL_ID_SCHEDULER_CLI

ESP_BLE_MESH_MODEL_ID_LIGHT_LIGHTNESS_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_LIGHTNESS_SETUP_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_LIGHTNESS_CLI

ESP_BLE_MESH_MODEL_ID_LIGHT_CTL_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_CTL_SETUP_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_CTL_CLI

ESP_BLE_MESH_MODEL_ID_LIGHT_CTL_TEMP_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_HSL_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_HSL_SETUP_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_HSL_CLI

ESP_BLE_MESH_MODEL_ID_LIGHT_HSL_HUE_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_HSL_SAT_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_XYL_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_XYL_SETUP_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_XYL_CLI

ESP_BLE_MESH_MODEL_ID_LIGHT_LC_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_LC_SETUP_SRV

ESP_BLE_MESH_MODEL_ID_LIGHT_LC_CLI

ESP_BLE_MESH_MODEL_ID_MBT_SRV

ESP_BLE_MESH_MODEL_ID_MBT_CLI

ESP_BLE_MESH_MODEL_OP_BEACON_GET

  Config Beacon Get

ESP_BLE_MESH_MODEL_OP_COMPOSITION_DATA_GET

  Config Composition Data Get

ESP_BLE_MESH_MODEL_OP_DEFAULT_TTL_GET

  Config Default TTL Get

ESP_BLE_MESH_MODEL_OP_GATT_PROXY_GET

  Config GATT Proxy Get

ESP_BLE_MESH_MODEL_OP_RELAY_GET

  Config Relay Get

ESP_BLE_MESH_MODEL_OP_MODEL_PUB_GET

  Config Model Publication Get

ESP_BLE_MESH_MODEL_OP_FRIEND_GET

  Config Friend Get

ESP_BLE_MESH_MODEL_OP_HEARTBEAT_PUB_GET

  Config Heartbeat Publication Get

ESP_BLE_MESH_MODEL_OP_HEARTBEAT_SUB_GET

  Config Heartbeat Subscription Get

ESP_BLE_MESH_MODEL_OP_NET_KEY_GET

  Config NetKey Get

ESP_BLE_MESH_MODEL_OP_APP_KEY_GET

  Config AppKey Get

ESP_BLE_MESH_MODEL_OP_NODE_IDENTITY_GET

  Config Node Identity Get

ESP_BLE_MESH_MODEL_OP_SIG_MODEL_SUB_GET

  Config SIG Model Subscription Get

ESP_BLE_MESH_MODEL_OP_VENDOR_MODEL_SUB_GET

  Config Vendor Model Subscription Get

ESP_BLE_MESH_MODEL_OP_SIG_MODEL_APP_GET

  Config SIG Model App Get

ESP_BLE_MESH_MODEL_OP_VENDOR_MODEL_APP_GET

  Config Vendor Model App Get

ESP_BLE_MESH_MODEL_OP_KEY_REFRESH_PHASE_GET

  Config Key Refresh Phase Get

ESP_BLE_MESH_MODEL_OP_LPN_POLLTIMEOUT_GET

  Config Low Power Node PollTimeout Get

ESP_BLE_MESH_MODEL_OP_NETWORK_TRANSMIT_GET

  Config Network Transmit Get

ESP_BLE_MESH_MODEL_OP_BEACON_SET

  Config Beacon Set

ESP_BLE_MESH_MODEL_OP_DEFAULT_TTL_SET

  Config Default TTL Set

ESP_BLE_MESH_MODEL_OP_GATT_PROXY_SET

  Config GATT Proxy Set

ESP_BLE_MESH_MODEL_OP_RELAY_SET

  Config Relay Set

ESP_BLE_MESH_MODEL_OP_MODEL_PUB_SET

  Config Model Publication Set

ESP_BLE_MESH_MODEL_OP_MODEL_SUB_ADD

  Config Model Subscription Add

ESP_BLE_MESH_MODEL_OP_MODEL_SUB_VIRTUAL_ADDR_ADD

  Config Model Subscription Virtual Address Add

ESP_BLE_MESH_MODEL_OP_MODEL_SUB_DELETE

  Config Model Subscription Delete

ESP_BLE_MESH_MODEL_OP_MODEL_SUB_VIRTUAL_ADDR_DELETE

  Config Model Subscription Virtual Address Delete

ESP_BLE_MESH_MODEL_OP_MODEL_SUB_OVERWRITE

  Config Model Subscription Overwrite

ESP_BLE_MESH_MODEL_OP_MODEL_SUB_VIRTUAL_ADDR_OVERWRITE

  Config Model Subscription Virtual Address Overwrite

ESP_BLE_MESH_MODEL_OP_NET_KEY_ADD

  Config NetKey Add

ESP_BLE_MESH_MODEL_OP_APP_KEY_ADD

  Config AppKey Add

ESP_BLE_MESH_MODEL_OP_MODEL_APP_BIND

  Config Model App Bind

ESP_BLE_MESH_MODEL_OP_NODE_RESET

  Config Node Reset

ESP_BLE_MESH_MODEL_OP_FRIEND_SET

  Config Friend Set

ESP_BLE_MESH_MODEL_OP_HEARTBEAT_PUB_SET

  Config Heartbeat Publication Set

ESP_BLE_MESH_MODEL_OP_HEARTBEAT_SUB_SET

  Config Heartbeat Subscription Set

ESP_BLE_MESH_MODEL_OP_NET_KEY_UPDATE

  Config NetKey Update

ESP_BLE_MESH_MODEL_OP_NET_KEY_DELETE

  Config NetKey Delete

ESP_BLE_MESH_MODEL_OP_APP_KEY_UPDATE

  Config AppKey Update

ESP_BLE_MESH_MODEL_OP_APP_KEY_DELETE

  Config AppKey Delete

ESP_BLE_MESH_MODEL_OP_NODE_IDENTITY_SET

  Config Node Identity Set

ESP_BLE_MESH_MODEL_OP_KEY_REFRESH_PHASE_SET

  Config Key Refresh Phase Set

ESP_BLE_MESH_MODEL_OP_MODEL_PUB_VIRTUAL_ADDR_SET

  Config Model Publication Virtual Address Set

ESP_BLE_MESH_MODEL_OP_MODEL_SUB_DELETE_ALL

  Config Model Subscription Delete All

ESP_BLE_MESH_MODEL_OP_MODEL_APP_UNBIND

  Config Model App Unbind

ESP_BLE_MESH_MODEL_OP_NETWORK_TRANSMIT_SET

  Config Network Transmit Set

ESP_BLE_MESH_MODEL_OP_BEACON_STATUS

ESP_BLE_MESH_MODEL_OP_COMPOSITION_DATA_STATUS

ESP_BLE_MESH_MODEL_OP_DEFAULT_TTL_STATUS

ESP_BLE_MESH_MODEL_OP_GATT_PROXY_STATUS

ESP_BLE_MESH_MODEL_OP_RELAY_STATUS

ESP_BLE_MESH_MODEL_OP_MODEL_PUB_STATUS

ESP_BLE_MESH_MODEL_OP_MODEL_SUB_STATUS

ESP_BLE_MESH_MODEL_OP_SIG_MODEL_SUB_LIST

ESP_BLE_MESH_MODEL_OP_VENDOR_MODEL_SUB_LIST

ESP_BLE_MESH_MODEL_OP_NET_KEY_STATUS

ESP_BLE_MESH_MODEL_OP_NET_KEY_LIST

ESP_BLE_MESH_MODEL_OP_APP_KEY_STATUS

ESP_BLE_MESH_MODEL_OP_APP_KEY_LIST

ESP_BLE_MESH_MODEL_OP_NODE_IDENTITY_STATUS

ESP_BLE_MESH_MODEL_OP_MODEL_APP_STATUS

ESP_BLE_MESH_MODEL_OP_SIG_MODEL_APP_LIST

ESP_BLE_MESH_MODEL_OP_VENDOR_MODEL_APP_LIST

ESP_BLE_MESH_MODEL_OP_NODE_RESET_STATUS

ESP_BLE_MESH_MODEL_OP_FRIEND_STATUS

ESP_BLE_MESH_MODEL_OP_KEY_REFRESH_PHASE_STATUS

ESP_BLE_MESH_MODEL_OP_HEARTBEAT_PUB_STATUS

ESP_BLE_MESH_MODEL_OP_HEARTBEAT_SUB_STATUS

ESP_BLE_MESH_MODEL_OP_LPN_POLLTIMEOUT_STATUS

ESP_BLE_MESH_MODEL_OP_NETWORK_TRANSMIT_STATUS

ESP_BLE_MESH_CFG_STATUS_SUCCESS

ESP_BLE_MESH_CFG_STATUS_INVALID_ADDRESS

ESP_BLE_MESH_CFG_STATUS_INVALID_MODEL

ESP_BLE_MESH_CFG_STATUS_INVALID_APPKEY

ESP_BLE_MESH_CFG_STATUS_INVALID_NETKEY

ESP_BLE_MESH_CFG_STATUS_INSUFFICIENT_RESOURCES

ESP_BLE_MESH_CFG_STATUS_KEY_INDEX_ALREADY_STORED

ESP_BLE_MESH_CFG_STATUS_INVALID_PUBLISH_PARAMETERS

ESP_BLE_MESH_CFG_STATUS_NOT_A_SUBSCRIBE_MODEL

ESP_BLE_MESH_CFG_STATUS_STORAGE_FAILURE

ESP_BLE_MESH_CFG_STATUS_FEATURE_NOT_SUPPORTED

ESP_BLE_MESH_CFG_STATUS_CANNOT_UPDATE

ESP_BLE_MESH_CFG_STATUS_CANNOT_REMOVE

ESP_BLE_MESH_CFG_STATUS_CANNOT_BIND

ESP_BLE_MESH_CFG_STATUS_TEMP_UNABLE_TO_CHANGE_STATE

ESP_BLE_MESH_CFG_STATUS_CANNOT_SET

ESP_BLE_MESH_CFG_STATUS_UNSPECIFIED_ERROR

ESP_BLE_MESH_CFG_STATUS_INVALID_BINDING

ESP_BLE_MESH_CFG_STATUS_INVALID_PATH_ENTRY

ESP_BLE_MESH_CFG_STATUS_CANNOT_GET

ESP_BLE_MESH_CFG_STATUS_OBSOLETE_INFO

ESP_BLE_MESH_CFG_STATUS_INVALID_BEARER

ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_GET

  Health Fault Get

ESP_BLE_MESH_MODEL_OP_HEALTH_PERIOD_GET

  Health Period Get

ESP_BLE_MESH_MODEL_OP_ATTENTION_GET

  Health Attention Get

ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_CLEAR

  Health Fault Clear

ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_CLEAR_UNACK

  Health Fault Clear Unacknowledged

ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_TEST

  Health Fault Test

ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_TEST_UNACK

  Health Fault Test Unacknowledged

ESP_BLE_MESH_MODEL_OP_HEALTH_PERIOD_SET

  Health Period Set

ESP_BLE_MESH_MODEL_OP_HEALTH_PERIOD_SET_UNACK

  Health Period Set Unacknowledged

ESP_BLE_MESH_MODEL_OP_ATTENTION_SET

  Health Attention Set

ESP_BLE_MESH_MODEL_OP_ATTENTION_SET_UNACK

  Health Attention Set Unacknowledged

ESP_BLE_MESH_MODEL_OP_HEALTH_CURRENT_STATUS

ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_STATUS

ESP_BLE_MESH_MODEL_OP_HEALTH_PERIOD_STATUS

ESP_BLE_MESH_MODEL_OP_ATTENTION_STATUS

ESP_BLE_MESH_MODEL_OP_GEN_ONOFF_GET

ESP_BLE_MESH_MODEL_OP_GEN_ONOFF_SET

ESP_BLE_MESH_MODEL_OP_GEN_ONOFF_SET_UNACK

ESP_BLE_MESH_MODEL_OP_GEN_ONOFF_STATUS

  Generic Level Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_LEVEL_GET

ESP_BLE_MESH_MODEL_OP_GEN_LEVEL_SET

ESP_BLE_MESH_MODEL_OP_GEN_LEVEL_SET_UNACK

ESP_BLE_MESH_MODEL_OP_GEN_LEVEL_STATUS

ESP_BLE_MESH_MODEL_OP_GEN_DELTA_SET

ESP_BLE_MESH_MODEL_OP_GEN_DELTA_SET_UNACK

ESP_BLE_MESH_MODEL_OP_GEN_MOVE_SET

ESP_BLE_MESH_MODEL_OP_GEN_MOVE_SET_UNACK

  Generic Default Transition Time Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_DEF_TRANS_TIME_GET

ESP_BLE_MESH_MODEL_OP_GEN_DEF_TRANS_TIME_SET

ESP_BLE_MESH_MODEL_OP_GEN_DEF_TRANS_TIME_SET_UNACK

ESP_BLE_MESH_MODEL_OP_GEN_DEF_TRANS_TIME_STATUS

  Generic Power OnOff Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_ONPOWERUP_GET

ESP_BLE_MESH_MODEL_OP_GEN_ONPOWERUP_STATUS

  Generic Power OnOff Setup Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_ONPOWERUP_SET

ESP_BLE_MESH_MODEL_OP_GEN_ONPOWERUP_SET_UNACK

  Generic Power Level Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_POWER_LEVEL_GET

ESP_BLE_MESH_MODEL_OP_GEN_POWER_LEVEL_SET

ESP_BLE_MESH_MODEL_OP_GEN_POWER_LEVEL_SET_UNACK

ESP_BLE_MESH_MODEL_OP_GEN_POWER_LEVEL_STATUS

ESP_BLE_MESH_MODEL_OP_GEN_POWER_LAST_GET

ESP_BLE_MESH_MODEL_OP_GEN_POWER_LAST_STATUS

ESP_BLE_MESH_MODEL_OP_GEN_POWER_DEFAULT_GET

ESP_BLE_MESH_MODEL_OP_GEN_POWER_DEFAULT_STATUS

ESP_BLE_MESH_MODEL_OP_GEN_POWER_RANGE_GET

ESP_BLE_MESH_MODEL_OP_GEN_POWER_RANGE_STATUS

  Generic Power Level Setup Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_POWER_DEFAULT_SET

ESP_BLE_MESH_MODEL_OP_GEN_POWER_DEFAULT_SET_UNACK

ESP_BLE_MESH_MODEL_OP_GEN_POWER_RANGE_SET

ESP_BLE_MESH_MODEL_OP_GEN_POWER_RANGE_SET_UNACK

  Generic Battery Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_BATTERY_GET

ESP_BLE_MESH_MODEL_OP_GEN_BATTERY_STATUS

  Generic Location Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_LOC_GLOBAL_GET

ESP_BLE_MESH_MODEL_OP_GEN_LOC_GLOBAL_STATUS

ESP_BLE_MESH_MODEL_OP_GEN_LOC_LOCAL_GET

ESP_BLE_MESH_MODEL_OP_GEN_LOC_LOCAL_STATUS

  Generic Location Setup Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_LOC_GLOBAL_SET

ESP_BLE_MESH_MODEL_OP_GEN_LOC_GLOBAL_SET_UNACK

ESP_BLE_MESH_MODEL_OP_GEN_LOC_LOCAL_SET

ESP_BLE_MESH_MODEL_OP_GEN_LOC_LOCAL_SET_UNACK

  Generic Manufacturer Property Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_MANUFACTURER_PROPERTIES_GET

ESP_BLE_MESH_MODEL_OP_GEN_MANUFACTURER_PROPERTIES_STATUS

ESP_BLE_MESH_MODEL_OP_GEN_MANUFACTURER_PROPERTY_GET

ESP_BLE_MESH_MODEL_OP_GEN_MANUFACTURER_PROPERTY_SET

ESP_BLE_MESH_MODEL_OP_GEN_MANUFACTURER_PROPERTY_SET_UNACK

ESP_BLE_MESH_MODEL_OP_GEN_MANUFACTURER_PROPERTY_STATUS

  Generic Admin Property Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_ADMIN_PROPERTIES_GET

ESP_BLE_MESH_MODEL_OP_GEN_ADMIN_PROPERTIES_STATUS

ESP_BLE_MESH_MODEL_OP_GEN_ADMIN_PROPERTY_GET

ESP_BLE_MESH_MODEL_OP_GEN_ADMIN_PROPERTY_SET

ESP_BLE_MESH_MODEL_OP_GEN_ADMIN_PROPERTY_SET_UNACK

ESP_BLE_MESH_MODEL_OP_GEN_ADMIN_PROPERTY_STATUS

  Generic User Property Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_USER_PROPERTIES_GET

ESP_BLE_MESH_MODEL_OP_GEN_USER_PROPERTIES_STATUS

ESP_BLE_MESH_MODEL_OP_GEN_USER_PROPERTY_GET

ESP_BLE_MESH_MODEL_OP_GEN_USER_PROPERTY_SET

ESP_BLE_MESH_MODEL_OP_GEN_USER_PROPERTY_SET_UNACK

ESP_BLE_MESH_MODEL_OP_GEN_USER_PROPERTY_STATUS

  Generic Client Property Message Opcode

ESP_BLE_MESH_MODEL_OP_GEN_CLIENT_PROPERTIES_GET

ESP_BLE_MESH_MODEL_OP_GEN_CLIENT_PROPERTIES_STATUS

ESP_BLE_MESH_MODEL_OP_SENSOR_DESCRIPTOR_GET

ESP_BLE_MESH_MODEL_OP_SENSOR_DESCRIPTOR_STATUS

ESP_BLE_MESH_MODEL_OP_SENSOR_GET

ESP_BLE_MESH_MODEL_OP_SENSOR_STATUS

ESP_BLE_MESH_MODEL_OP_SENSOR_COLUMN_GET

ESP_BLE_MESH_MODEL_OP_SENSOR_COLUMN_STATUS

ESP_BLE_MESH_MODEL_OP_SENSOR_SERIES_GET

ESP_BLE_MESH_MODEL_OP_SENSOR_SERIES_STATUS

  Sensor Setup Message Opcode

ESP_BLE_MESH_MODEL_OP_SENSOR_CADENCE_GET

ESP_BLE_MESH_MODEL_OP_SENSOR_CADENCE_SET

ESP_BLE_MESH_MODEL_OP_SENSOR_CADENCE_SET_UNACK

ESP_BLE_MESH_MODEL_OP_SENSOR_CADENCE_STATUS

ESP_BLE_MESH_MODEL_OP_SENSOR_SETTINGS_GET

ESP_BLE_MESH_MODEL_OP_SENSOR_SETTINGS_STATUS

ESP_BLE_MESH_MODEL_OP_SENSOR_SETTING_GET

ESP_BLE_MESH_MODEL_OP_SENSOR_SETTING_SET

ESP_BLE_MESH_MODEL_OP_SENSOR_SETTING_SET_UNACK

ESP_BLE_MESH_MODEL_OP_SENSOR_SETTING_STATUS

ESP_BLE_MESH_MODEL_OP_TIME_GET

ESP_BLE_MESH_MODEL_OP_TIME_SET

ESP_BLE_MESH_MODEL_OP_TIME_STATUS

ESP_BLE_MESH_MODEL_OP_TIME_ROLE_GET

ESP_BLE_MESH_MODEL_OP_TIME_ROLE_SET

ESP_BLE_MESH_MODEL_OP_TIME_ROLE_STATUS

ESP_BLE_MESH_MODEL_OP_TIME_ZONE_GET

ESP_BLE_MESH_MODEL_OP_TIME_ZONE_SET

ESP_BLE_MESH_MODEL_OP_TIME_ZONE_STATUS

ESP_BLE_MESH_MODEL_OP_TAI_UTC_DELTA_GET

ESP_BLE_MESH_MODEL_OP_TAI_UTC_DELTA_SET

ESP_BLE_MESH_MODEL_OP_TAI_UTC_DELTA_STATUS

  Scene Message Opcode

ESP_BLE_MESH_MODEL_OP_SCENE_GET

ESP_BLE_MESH_MODEL_OP_SCENE_RECALL

ESP_BLE_MESH_MODEL_OP_SCENE_RECALL_UNACK

ESP_BLE_MESH_MODEL_OP_SCENE_STATUS

ESP_BLE_MESH_MODEL_OP_SCENE_REGISTER_GET

ESP_BLE_MESH_MODEL_OP_SCENE_REGISTER_STATUS

  Scene Setup Message Opcode

ESP_BLE_MESH_MODEL_OP_SCENE_STORE

ESP_BLE_MESH_MODEL_OP_SCENE_STORE_UNACK

ESP_BLE_MESH_MODEL_OP_SCENE_DELETE

ESP_BLE_MESH_MODEL_OP_SCENE_DELETE_UNACK

  Scheduler Message Opcode

ESP_BLE_MESH_MODEL_OP_SCHEDULER_ACT_GET

ESP_BLE_MESH_MODEL_OP_SCHEDULER_ACT_STATUS

ESP_BLE_MESH_MODEL_OP_SCHEDULER_GET

ESP_BLE_MESH_MODEL_OP_SCHEDULER_STATUS

  Scheduler Setup Message Opcode

ESP_BLE_MESH_MODEL_OP_SCHEDULER_ACT_SET

ESP_BLE_MESH_MODEL_OP_SCHEDULER_ACT_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_LINEAR_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_LINEAR_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_LINEAR_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_LINEAR_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_LAST_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_LAST_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_DEFAULT_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_DEFAULT_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_RANGE_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_RANGE_STATUS

  Light Lightness Setup Message Opcode

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_DEFAULT_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_DEFAULT_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_RANGE_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_RANGE_SET_UNACK

  Light CTL Message Opcode

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_RANGE_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_RANGE_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_DEFAULT_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_DEFAULT_STATUS

  Light CTL Setup Message Opcode

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_DEFAULT_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_DEFAULT_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_RANGE_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_RANGE_SET_UNACK

  Light HSL Message Opcode

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_HUE_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_HUE_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_HUE_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_HUE_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_SATURATION_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_SATURATION_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_SATURATION_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_SATURATION_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_TARGET_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_TARGET_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_DEFAULT_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_DEFAULT_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_RANGE_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_RANGE_STATUS

  Light HSL Setup Message Opcode

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_DEFAULT_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_DEFAULT_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_RANGE_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_RANGE_SET_UNACK

  Light xyL Message Opcode

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_TARGET_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_TARGET_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_DEFAULT_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_DEFAULT_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_RANGE_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_RANGE_STATUS

  Light xyL Setup Message Opcode

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_DEFAULT_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_DEFAULT_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_RANGE_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_RANGE_SET_UNACK

  Light Control Message Opcode

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_MODE_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_MODE_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_MODE_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_MODE_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_OM_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_OM_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_OM_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_OM_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_LIGHT_ONOFF_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_LIGHT_ONOFF_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_LIGHT_ONOFF_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_LIGHT_ONOFF_STATUS

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_PROPERTY_GET

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_PROPERTY_SET

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_PROPERTY_SET_UNACK

ESP_BLE_MESH_MODEL_OP_LIGHT_LC_PROPERTY_STATUS

ESP_BLE_MESH_MODEL_STATUS_SUCCESS

ESP_BLE_MESH_MODEL_STATUS_CANNOT_SET_RANGE_MIN

ESP_BLE_MESH_MODEL_STATUS_CANNOT_SET_RANGE_MAX

ESP_BLE_MESH_SERVER_RSP_BY_APP

  Response need to be sent in the application

ESP_BLE_MESH_SERVER_AUTO_RSP

  Response will be sent internally

### Type Definitions

typedef uint8_t esp_ble_mesh_octet16_t[ESP_BLE_MESH_OCTET16_LEN]

  Define the BLE Mesh octet 8 bytes size

typedef uint8_t esp_ble_mesh_octet8_t[ESP_BLE_MESH_OCTET8_LEN]

  Invalid Company ID

typedef uint32_t esp_ble_mesh_cb_t

typedef uint8_t UINT8

typedef uint16_t UINT16

typedef uint32_t UINT32

typedef uint64_t UINT64

typedef UINT8 BT_OCTET32[BT_OCTET32_LEN]

typedef uint8_t BD_ADDR[BD_ADDR_LEN]

typedef uint8_t esp_ble_mesh_bd_addr_t[BD_ADDR_LEN]

typedef uint8_t esp_ble_mesh_addr_type_t

  BLE device address type.

typedef struct esp_ble_mesh_model esp_ble_mesh_model_t

typedef uint8_t esp_ble_mesh_dev_add_flag_t

typedef uint32_t esp_ble_mesh_opcode_config_client_get_t

  esp_ble_mesh_opcode_config_client_get_t belongs to esp_ble_mesh_opcode_t, this typedef is only used to locate the opcodes used by esp_ble_mesh_config_client_get_state. The following opcodes will only be used in the esp_ble_mesh_config_client_get_state function.

typedef uint32_t esp_ble_mesh_opcode_config_client_set_t

  esp_ble_mesh_opcode_config_client_set_t belongs to esp_ble_mesh_opcode_t, this typedef is only used to locate the opcodes used by esp_ble_mesh_config_client_set_state. The following opcodes will only be used in the esp_ble_mesh_config_client_set_state function.

typedef uint32_t esp_ble_mesh_opcode_config_status_t

  esp_ble_mesh_opcode_config_status_t belongs to esp_ble_mesh_opcode_t, this typedef is only used to locate the opcodes used by the Config Model messages The following opcodes are used by the BLE Mesh Config Server Model internally to respond to the Config Client Model's request messages.

typedef uint8_t esp_ble_mesh_cfg_status_t

  This typedef is only used to indicate the status code contained in some of the Configuration Server Model status message.

typedef uint32_t esp_ble_mesh_opcode_health_client_get_t

  esp_ble_mesh_opcode_health_client_get_t belongs to esp_ble_mesh_opcode_t, this typedef is only used to locate the opcodes used by esp_ble_mesh_health_client_get_state. The following opcodes will only be used in the esp_ble_mesh_health_client_get_state function.

typedef uint32_t esp_ble_mesh_opcode_health_client_set_t

  esp_ble_mesh_opcode_health_client_set_t belongs to esp_ble_mesh_opcode_t, this typedef is only used to locate the opcodes used by esp_ble_mesh_health_client_set_state. The following opcodes will only be used in the esp_ble_mesh_health_client_set_state function.

typedef uint32_t esp_ble_mesh_health_model_status_t

  esp_ble_mesh_health_model_status_t belongs to esp_ble_mesh_opcode_t, this typedef is only used to locate the opcodes used by the Health Model messages. The following opcodes are used by the BLE Mesh Health Server Model internally to respond to the Health Client Model's request messages.

typedef uint32_t esp_ble_mesh_generic_message_opcode_t

  esp_ble_mesh_generic_message_opcode_t belongs to esp_ble_mesh_opcode_t, this typedef is only used to locate the opcodes used by functions esp_ble_mesh_generic_client_get_state & esp_ble_mesh_generic_client_set_state. Generic OnOff Message Opcode

typedef uint32_t esp_ble_mesh_sensor_message_opcode_t

  esp_ble_mesh_sensor_message_opcode_t belongs to esp_ble_mesh_opcode_t, this typedef is only used to locate the opcodes used by functions esp_ble_mesh_sensor_client_get_state & esp_ble_mesh_sensor_client_set_state. Sensor Message Opcode

typedef uint32_t esp_ble_mesh_time_scene_message_opcode_t

  esp_ble_mesh_time_scene_message_opcode_t belongs to esp_ble_mesh_opcode_t, this typedef is only used to locate the opcodes used by functions esp_ble_mesh_time_scene_client_get_state & esp_ble_mesh_time_scene_client_set_state. Time Message Opcode

typedef uint32_t esp_ble_mesh_light_message_opcode_t

  esp_ble_mesh_light_message_opcode_t belongs to esp_ble_mesh_opcode_t, this typedef is only used to locate the opcodes used by functions esp_ble_mesh_light_client_get_state & esp_ble_mesh_light_client_set_state. Light Lightness Message Opcode

typedef uint32_t esp_ble_mesh_opcode_t

  End of defines of esp_ble_mesh_opcode_t

typedef uint8_t esp_ble_mesh_model_status_t

  This typedef is only used to indicate the status code contained in some of the server models (e.g. Generic Server Model) status message.

### Enumerations

enum esp_ble_mesh_cb_type_t

  Values:

  enumerator ESP_BLE_MESH_TYPE_PROV_CB
  enumerator ESP_BLE_MESH_TYPE_OUTPUT_NUM_CB
  enumerator ESP_BLE_MESH_TYPE_OUTPUT_STR_CB
  enumerator ESP_BLE_MESH_TYPE_INTPUT_CB
  enumerator ESP_BLE_MESH_TYPE_LINK_OPEN_CB
  enumerator ESP_BLE_MESH_TYPE_LINK_CLOSE_CB
  enumerator ESP_BLE_MESH_TYPE_COMPLETE_CB
  enumerator ESP_BLE_MESH_TYPE_RESET_CB

enum esp_ble_mesh_oob_method_t

  Values:

  enumerator ESP_BLE_MESH_NO_OOB
  enumerator ESP_BLE_MESH_STATIC_OOB
  enumerator ESP_BLE_MESH_OUTPUT_OOB
  enumerator ESP_BLE_MESH_INPUT_OOB

enum esp_ble_mesh_output_action_t

  Values:

  enumerator ESP_BLE_MESH_NO_OUTPUT
  enumerator ESP_BLE_MESH_BLINK
  enumerator ESP_BLE_MESH_BEEP
  enumerator ESP_BLE_MESH_VIBRATE
  enumerator ESP_BLE_MESH_DISPLAY_NUMBER
  enumerator ESP_BLE_MESH_DISPLAY_STRING

enum esp_ble_mesh_input_action_t

  Values:

  enumerator ESP_BLE_MESH_NO_INPUT
  enumerator ESP_BLE_MESH_PUSH
  enumerator ESP_BLE_MESH_TWIST
  enumerator ESP_BLE_MESH_ENTER_NUMBER
  enumerator ESP_BLE_MESH_ENTER_STRING

enum esp_ble_mesh_prov_bearer_t

  Values:

  enumerator ESP_BLE_MESH_PROV_ADV
  enumerator ESP_BLE_MESH_PROV_GATT

enum esp_ble_mesh_prov_oob_info_t

  Values:

  enumerator ESP_BLE_MESH_PROV_OOB_OTHER
  enumerator ESP_BLE_MESH_PROV_OOB_URI
  enumerator ESP_BLE_MESH_PROV_OOB_2D_CODE
  enumerator ESP_BLE_MESH_PROV_OOB_BAR_CODE
  enumerator ESP_BLE_MESH_PROV_OOB_NFC
  enumerator ESP_BLE_MESH_PROV_OOB_NUMBER
  enumerator ESP_BLE_MESH_PROV_OOB_STRING
  enumerator ESP_BLE_MESH_PROV_CERT_BASED
  enumerator ESP_BLE_MESH_PROV_RECORDS
  enumerator ESP_BLE_MESH_PROV_OOB_ON_BOX
  enumerator ESP_BLE_MESH_PROV_OOB_IN_BOX
  enumerator ESP_BLE_MESH_PROV_OOB_ON_PAPER
  enumerator ESP_BLE_MESH_PROV_OOB_IN_MANUAL
  enumerator ESP_BLE_MESH_PROV_OOB_ON_DEV

enum esp_ble_mesh_dev_role_t

  Values:

  enumerator ROLE_NODE
  enumerator ROLE_PROVISIONER
  enumerator ROLE_FAST_PROV

enum esp_ble_mesh_fast_prov_action_t

  Values:

  enumerator FAST_PROV_ACT_NONE
  enumerator FAST_PROV_ACT_ENTER
  enumerator FAST_PROV_ACT_SUSPEND
  enumerator FAST_PROV_ACT_EXIT
  enumerator FAST_PROV_ACT_MAX

enum esp_ble_mesh_proxy_filter_type_t

  Values:

  enumerator PROXY_FILTER_WHITELIST
  enumerator PROXY_FILTER_BLACKLIST

enum esp_ble_mesh_prov_cb_event_t

  Values:

  enumerator ESP_BLE_MESH_PROV_REGISTER_COMP_EVT

    Initialize BLE Mesh provisioning capabilities and internal data information completion event

  enumerator ESP_BLE_MESH_NODE_SET_UNPROV_DEV_NAME_COMP_EVT

    Set the unprovisioned device name completion event

  enumerator ESP_BLE_MESH_NODE_PROV_ENABLE_COMP_EVT

    Enable node provisioning functionality completion event

  enumerator ESP_BLE_MESH_NODE_PROV_DISABLE_COMP_EVT

    Disable node provisioning functionality completion event

  enumerator ESP_BLE_MESH_NODE_PROV_LINK_OPEN_EVT

    Establish a BLE Mesh link event

  enumerator ESP_BLE_MESH_NODE_PROV_LINK_CLOSE_EVT

    Close a BLE Mesh link event

  enumerator ESP_BLE_MESH_NODE_PROV_OOB_PUB_KEY_EVT

    Generate Node input OOB public key event

  enumerator ESP_BLE_MESH_NODE_PROV_OUTPUT_NUMBER_EVT

    Generate Node Output Number event

  enumerator ESP_BLE_MESH_NODE_PROV_OUTPUT_STRING_EVT

    Generate Node Output String event

  enumerator ESP_BLE_MESH_NODE_PROV_INPUT_EVT

    Event requiring the user to input a number or string

  enumerator ESP_BLE_MESH_NODE_PROV_COMPLETE_EVT

    Provisioning done event

  enumerator ESP_BLE_MESH_NODE_PROV_RESET_EVT

    Provisioning reset event

  enumerator ESP_BLE_MESH_NODE_PROV_SET_OOB_PUB_KEY_COMP_EVT

    Node set oob public key completion event

  enumerator ESP_BLE_MESH_NODE_PROV_INPUT_NUMBER_COMP_EVT

    Node input number completion event

  enumerator ESP_BLE_MESH_NODE_PROV_INPUT_STRING_COMP_EVT

    Node input string completion event

  enumerator ESP_BLE_MESH_NODE_PROXY_IDENTITY_ENABLE_COMP_EVT

    Enable BLE Mesh Proxy Identity advertising completion event

  enumerator ESP_BLE_MESH_NODE_PRIVATE_PROXY_IDENTITY_ENABLE_COMP_EVT

    Enable BLE Mesh Private Proxy Identity advertising completion event

  enumerator ESP_BLE_MESH_NODE_PRIVATE_PROXY_IDENTITY_DISABLE_COMP_EVT

    Disable BLE Mesh Private Proxy Identity advertising completion event

  enumerator ESP_BLE_MESH_NODE_PROXY_GATT_ENABLE_COMP_EVT

    Enable BLE Mesh GATT Proxy Service completion event

  enumerator ESP_BLE_MESH_NODE_PROXY_GATT_DISABLE_COMP_EVT

    Disable BLE Mesh GATT Proxy Service completion event

  enumerator ESP_BLE_MESH_NODE_ADD_LOCAL_NET_KEY_COMP_EVT

    Node add NetKey locally completion event

  enumerator ESP_BLE_MESH_NODE_ADD_LOCAL_APP_KEY_COMP_EVT

    Node add AppKey locally completion event

  enumerator ESP_BLE_MESH_NODE_BIND_APP_KEY_TO_MODEL_COMP_EVT

    Node bind AppKey to model locally completion event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_ENABLE_COMP_EVT

    Provisioner enable provisioning functionality completion event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_DISABLE_COMP_EVT

    Provisioner disable provisioning functionality completion event

  enumerator ESP_BLE_MESH_PROVISIONER_RECV_UNPROV_ADV_PKT_EVT

    Provisioner receives unprovisioned device beacon event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_READ_OOB_PUB_KEY_EVT

    Provisioner read unprovisioned device OOB public key event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_INPUT_EVT

    Provisioner input value for provisioning procedure event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_OUTPUT_EVT

    Provisioner output value for provisioning procedure event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_LINK_OPEN_EVT

    Provisioner establish a BLE Mesh link event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_LINK_CLOSE_EVT

    Provisioner close a BLE Mesh link event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_COMPLETE_EVT

    Provisioner provisioning done event

  enumerator ESP_BLE_MESH_PROVISIONER_CERT_BASED_PROV_START_EVT

    Provisioner initiate a certificate based provisioning

  enumerator ESP_BLE_MESH_PROVISIONER_RECV_PROV_RECORDS_LIST_EVT

    Provisioner receive provisioning records list event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_RECORD_RECV_COMP_EVT

    Provisioner receive provisioning record complete event

  enumerator ESP_BLE_MESH_PROVISIONER_SEND_PROV_RECORDS_GET_EVT

    Provisioner send provisioning records get to device event

  enumerator ESP_BLE_MESH_PROVISIONER_SEND_PROV_RECORD_REQUEST_EVT

    Provisioner send provisioning record request to device event

  enumerator ESP_BLE_MESH_PROVISIONER_SEND_PROV_INVITE_EVT

    Provisioner send provisioning invite to device event

  enumerator ESP_BLE_MESH_PROVISIONER_SEND_LINK_CLOSE_EVT

    Provisioner send link close to device event

  enumerator ESP_BLE_MESH_PROVISIONER_ADD_UNPROV_DEV_COMP_EVT

    Provisioner add a device to the list which contains devices that are waiting/going to be provisioned completion event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_DEV_WITH_ADDR_COMP_EVT

    Provisioner start to provision an unprovisioned device completion event

  enumerator ESP_BLE_MESH_PROVISIONER_DELETE_DEV_COMP_EVT

    Provisioner delete a device from the list, close provisioning link with the device completion event

  enumerator ESP_BLE_MESH_PROVISIONER_SET_DEV_UUID_MATCH_COMP_EVT

    Provisioner set the value to be compared with part of the unprovisioned device UUID completion event

  enumerator ESP_BLE_MESH_PROVISIONER_SET_PROV_DATA_INFO_COMP_EVT

    Provisioner set net_idx/flags/iv_index used for provisioning completion event

  enumerator ESP_BLE_MESH_PROVISIONER_SET_STATIC_OOB_VALUE_COMP_EVT

    Provisioner set static oob value used for provisioning completion event

  enumerator ESP_BLE_MESH_PROVISIONER_SET_PRIMARY_ELEM_ADDR_COMP_EVT

    Provisioner set unicast address of primary element completion event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_READ_OOB_PUB_KEY_COMP_EVT

    Provisioner read unprovisioned device OOB public key completion event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_INPUT_NUMBER_COMP_EVT

    Provisioner input number completion event

  enumerator ESP_BLE_MESH_PROVISIONER_PROV_INPUT_STRING_COMP_EVT

    Provisioner input string completion event

  enumerator ESP_BLE_MESH_PROVISIONER_SET_NODE_NAME_COMP_EVT

    Provisioner set node name completion event

  enumerator ESP_BLE_MESH_PROVISIONER_ADD_LOCAL_APP_KEY_COMP_EVT

    Provisioner add local app key completion event

  enumerator ESP_BLE_MESH_PROVISIONER_UPDATE_LOCAL_APP_KEY_COMP_EVT

    Provisioner update local app key completion event

  enumerator ESP_BLE_MESH_PROVISIONER_BIND_APP_KEY_TO_MODEL_COMP_EVT

    Provisioner bind local model with local app key completion event

  enumerator ESP_BLE_MESH_PROVISIONER_ADD_LOCAL_NET_KEY_COMP_EVT

    Provisioner add local network key completion event

  enumerator ESP_BLE_MESH_PROVISIONER_UPDATE_LOCAL_NET_KEY_COMP_EVT

    Provisioner update local network key completion event

  enumerator ESP_BLE_MESH_PROVISIONER_STORE_NODE_COMP_DATA_COMP_EVT

    Provisioner store node composition data completion event

  enumerator ESP_BLE_MESH_PROVISIONER_DELETE_NODE_WITH_UUID_COMP_EVT

    Provisioner delete node with uuid completion event

  enumerator ESP_BLE_MESH_PROVISIONER_DELETE_NODE_WITH_ADDR_COMP_EVT

    Provisioner delete node with unicast address completion event

  enumerator ESP_BLE_MESH_PROVISIONER_ENABLE_HEARTBEAT_RECV_COMP_EVT

    Provisioner start to receive heartbeat message completion event

  enumerator ESP_BLE_MESH_PROVISIONER_SET_HEARTBEAT_FILTER_TYPE_COMP_EVT

    Provisioner set the heartbeat filter type completion event

  enumerator ESP_BLE_MESH_PROVISIONER_SET_HEARTBEAT_FILTER_INFO_COMP_EVT

    Provisioner set the heartbeat filter information completion event

  enumerator ESP_BLE_MESH_PROVISIONER_RECV_HEARTBEAT_MESSAGE_EVT

    Provisioner receive heartbeat message event

  enumerator ESP_BLE_MESH_PROVISIONER_DIRECT_ERASE_SETTINGS_COMP_EVT

    Provisioner directly erase settings completion event

  enumerator ESP_BLE_MESH_PROVISIONER_OPEN_SETTINGS_WITH_INDEX_COMP_EVT

    Provisioner open settings with index completion event

  enumerator ESP_BLE_MESH_PROVISIONER_OPEN_SETTINGS_WITH_UID_COMP_EVT

    Provisioner open settings with user id completion event

  enumerator ESP_BLE_MESH_PROVISIONER_CLOSE_SETTINGS_WITH_INDEX_COMP_EVT

    Provisioner close settings with index completion event

  enumerator ESP_BLE_MESH_PROVISIONER_CLOSE_SETTINGS_WITH_UID_COMP_EVT

    Provisioner close settings with user id completion event

  enumerator ESP_BLE_MESH_PROVISIONER_DELETE_SETTINGS_WITH_INDEX_COMP_EVT

    Provisioner delete settings with index completion event

  enumerator ESP_BLE_MESH_PROVISIONER_DELETE_SETTINGS_WITH_UID_COMP_EVT

    Provisioner delete settings with user id completion event

  enumerator ESP_BLE_MESH_SET_FAST_PROV_INFO_COMP_EVT

    Set fast provisioning information (e.g. unicast address range, net_idx, etc.) completion event

  enumerator ESP_BLE_MESH_SET_FAST_PROV_ACTION_COMP_EVT

    Set fast provisioning action completion event

  enumerator ESP_BLE_MESH_HEARTBEAT_MESSAGE_RECV_EVT

    Receive Heartbeat message event

  enumerator ESP_BLE_MESH_LPN_ENABLE_COMP_EVT

    Enable Low Power Node completion event

  enumerator ESP_BLE_MESH_LPN_DISABLE_COMP_EVT

    Disable Low Power Node completion event

  enumerator ESP_BLE_MESH_LPN_POLL_COMP_EVT

    Low Power Node send Friend Poll completion event

  enumerator ESP_BLE_MESH_LPN_FRIENDSHIP_ESTABLISH_EVT

    Low Power Node establishes friendship event

  enumerator ESP_BLE_MESH_LPN_FRIENDSHIP_TERMINATE_EVT

    Low Power Node terminates friendship event

  enumerator ESP_BLE_MESH_FRIEND_FRIENDSHIP_ESTABLISH_EVT

    Friend Node establishes friendship event

  enumerator ESP_BLE_MESH_FRIEND_FRIENDSHIP_TERMINATE_EVT

    Friend Node terminates friendship event

  enumerator ESP_BLE_MESH_PROXY_CLIENT_RECV_ADV_PKT_EVT

    Proxy Client receives Network ID advertising packet event

  enumerator ESP_BLE_MESH_PROXY_CLIENT_CONNECTED_EVT

    Proxy Client establishes connection successfully event

  enumerator ESP_BLE_MESH_PROXY_CLIENT_DISCONNECTED_EVT

    Proxy Client terminates connection successfully event

  enumerator ESP_BLE_MESH_PROXY_CLIENT_RECV_FILTER_STATUS_EVT

    Proxy Client receives Proxy Filter Status event

  enumerator ESP_BLE_MESH_PROXY_CLIENT_CONNECT_COMP_EVT

    Proxy Client connect completion event

  enumerator ESP_BLE_MESH_PROXY_CLIENT_DISCONNECT_COMP_EVT

    Proxy Client disconnect completion event

  enumerator ESP_BLE_MESH_PROXY_CLIENT_SET_FILTER_TYPE_COMP_EVT

    Proxy Client set filter type completion event

  enumerator ESP_BLE_MESH_PROXY_CLIENT_ADD_FILTER_ADDR_COMP_EVT

    Proxy Client add filter address completion event

  enumerator ESP_BLE_MESH_PROXY_CLIENT_REMOVE_FILTER_ADDR_COMP_EVT

    Proxy Client remove filter address completion event

  enumerator ESP_BLE_MESH_PROXY_CLIENT_DIRECTED_PROXY_SET_COMP_EVT

    Proxy Client directed proxy set completion event

  enumerator ESP_BLE_MESH_PROXY_SERVER_CONNECTED_EVT

    Proxy Server establishes connection successfully event

  enumerator ESP_BLE_MESH_PROXY_SERVER_DISCONNECTED_EVT

    Proxy Server terminates connection successfully event

  enumerator ESP_BLE_MESH_PROXY_CLIENT_SEND_SOLIC_PDU_COMP_EVT

    Proxy Client send Solicitation PDU completion event

  enumerator ESP_BLE_MESH_MODEL_SUBSCRIBE_GROUP_ADDR_COMP_EVT

    Local model subscribes group address completion event

  enumerator ESP_BLE_MESH_MODEL_UNSUBSCRIBE_GROUP_ADDR_COMP_EVT

    Local model unsubscribes group address completion event

  enumerator ESP_BLE_MESH_DEINIT_MESH_COMP_EVT

    De-initialize BLE Mesh stack completion event

  enumerator ESP_BLE_MESH_PROV_EVT_MAX

enum esp_ble_mesh_server_state_type_t

  This enum value is the type of server model states

  Values:

  enumerator ESP_BLE_MESH_GENERIC_ONOFF_STATE
  enumerator ESP_BLE_MESH_GENERIC_LEVEL_STATE
  enumerator ESP_BLE_MESH_GENERIC_ONPOWERUP_STATE
  enumerator ESP_BLE_MESH_GENERIC_POWER_ACTUAL_STATE
  enumerator ESP_BLE_MESH_LIGHT_LIGHTNESS_ACTUAL_STATE
  enumerator ESP_BLE_MESH_LIGHT_LIGHTNESS_LINEAR_STATE
  enumerator ESP_BLE_MESH_LIGHT_CTL_LIGHTNESS_STATE
  enumerator ESP_BLE_MESH_LIGHT_CTL_TEMP_DELTA_UV_STATE
  enumerator ESP_BLE_MESH_LIGHT_HSL_STATE
  enumerator ESP_BLE_MESH_LIGHT_HSL_LIGHTNESS_STATE
  enumerator ESP_BLE_MESH_LIGHT_HSL_HUE_STATE
  enumerator ESP_BLE_MESH_LIGHT_HSL_SATURATION_STATE
  enumerator ESP_BLE_MESH_LIGHT_XYL_LIGHTNESS_STATE
  enumerator ESP_BLE_MESH_LIGHT_LC_LIGHT_ONOFF_STATE
  enumerator ESP_BLE_MESH_SERVER_MODEL_STATE_MAX

enum esp_ble_mesh_model_cb_event_t

  Values:

  enumerator ESP_BLE_MESH_MODEL_OPERATION_EVT

    User-defined models receive messages from peer devices (e.g. get, set, status, etc) event

  enumerator ESP_BLE_MESH_MODEL_SEND_COMP_EVT

    User-defined models send messages completion event

  enumerator ESP_BLE_MESH_MODEL_PUBLISH_COMP_EVT

    User-defined models publish messages completion event

  enumerator ESP_BLE_MESH_CLIENT_MODEL_RECV_PUBLISH_MSG_EVT

    User-defined client models receive publish messages event

  enumerator ESP_BLE_MESH_CLIENT_MODEL_SEND_TIMEOUT_EVT

    Timeout event for the user-defined client models that failed to receive response from peer server models

  enumerator ESP_BLE_MESH_MODEL_PUBLISH_UPDATE_EVT

    When a model is configured to publish messages periodically, this event will occur during every publish period

  enumerator ESP_BLE_MESH_SERVER_MODEL_UPDATE_STATE_COMP_EVT

    Server models update state value completion event

  enumerator ESP_BLE_MESH_MODEL_EVT_MAX

## ESP-BLE-MESH Core API Reference

This section contains ESP-BLE-MESH Core related APIs, which can be used to initialize ESP-BLE-MESH stack, provision, send/publish messages, etc.

This API reference covers six components:

- ESP-BLE-MESH Stack Initialization

- Reading of Local Data Information

- Low Power Operation (Updating)

- Send/Publish Messages, add Local AppKey, etc.

- ESP-BLE-MESH Node/Provisioner Provisioning

- ESP-BLE-MESH GATT Proxy Server

### ESP-BLE-MESH Stack Initialization

### Header File

- components/bt/esp_ble_mesh/api/core/include/esp_ble_mesh_common_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_common_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_init(esp_ble_mesh_prov_t *prov, esp_ble_mesh_comp_t *comp)

  Initialize BLE Mesh module. This API initializes provisioning capabilities and composition data information.

  备注

  After calling this API, the device needs to call esp_ble_mesh_prov_enable() to enable provisioning functionality again.

  参数:

    - prov -- [in] Pointer to the device provisioning capabilities. This pointer must remain valid during the lifetime of the BLE Mesh device.

    - comp -- [in] Pointer to the device composition data information. This pointer must remain valid during the lifetime of the BLE Mesh device.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_deinit(esp_ble_mesh_deinit_param_t *param)

  De-initialize BLE Mesh module.

  备注

  1. This function shall be invoked after esp_ble_mesh_client_model_deinit().

  2. This function is strictly forbidden to run in any BTC Task Context (e.g. registered Mesh Event Callback).

  参数:

    param -- [in] Pointer to the structure of BLE Mesh deinit parameters.

  返回:

    ESP_OK on success or error code otherwise.

### Reading of Local Data Information

### Header File

- components/bt/esp_ble_mesh/api/core/include/esp_ble_mesh_local_data_operation_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_local_data_operation_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

int32_t esp_ble_mesh_get_model_publish_period(esp_ble_mesh_model_t *model)

  Get the model publish period, the unit is ms.

  参数:

    model -- [in] Model instance pointer.

  返回:

    Publish period value on success, 0 or (negative) error code from errno.h on failure.

uint16_t esp_ble_mesh_get_primary_element_address(void)

  Get the address of the primary element.

  返回:

    Address of the primary element on success, or ESP_BLE_MESH_ADDR_UNASSIGNED on failure which means the device has not been provisioned.

uint16_t *esp_ble_mesh_is_model_subscribed_to_group(esp_ble_mesh_model_t *model, uint16_t group_addr)

  Check if the model has subscribed to the given group address. Note: E.g., once a status message is received and the destination address is a group address, the model uses this API to check if it is successfully subscribed to the given group address.

  参数:

    - model -- [in] Pointer to the model.

    - group_addr -- [in] Group address.

  返回:

    Pointer to the group address within the Subscription List of the model on success, or NULL on failure which means the model has not subscribed to the given group address. Note: With the pointer to the group address returned, you can reset the group address to 0x0000 in order to unsubscribe the model from the group.

esp_ble_mesh_elem_t *esp_ble_mesh_find_element(uint16_t element_addr)

  Find the BLE Mesh element pointer via the element address.

  参数:

    element_addr -- [in] Element address.

  返回:

    Pointer to the element on success, or NULL on failure.

uint8_t esp_ble_mesh_get_element_count(void)

  Get the number of elements that have been registered.

  返回:

    Number of elements.

esp_ble_mesh_model_t *esp_ble_mesh_find_vendor_model(const esp_ble_mesh_elem_t *element, uint16_t company_id, uint16_t model_id)

  Find the Vendor specific model with the given element, the company ID and the Vendor Model ID.

  参数:

    - element -- [in] Element to which the model belongs.

    - company_id -- [in] A 16-bit company identifier assigned by the Bluetooth SIG.

    - model_id -- [in] A 16-bit vendor-assigned model identifier.

  返回:

    Pointer to the Vendor Model on success, or NULL on failure which means the Vendor Model is not found.

esp_ble_mesh_model_t *esp_ble_mesh_find_sig_model(const esp_ble_mesh_elem_t *element, uint16_t model_id)

  Find the SIG model with the given element and Model id.

  参数:

    - element -- [in] Element to which the model belongs.

    - model_id -- [in] SIG model identifier.

  返回:

    Pointer to the SIG Model on success, or NULL on failure which means the SIG Model is not found.

const esp_ble_mesh_comp_t *esp_ble_mesh_get_composition_data(void)

  Get the Composition data which has been registered.

  返回:

    Pointer to the Composition data on success, or NULL on failure which means the Composition data is not initialized.

esp_err_t esp_ble_mesh_model_subscribe_group_addr(uint16_t element_addr, uint16_t company_id, uint16_t model_id, uint16_t group_addr)

  A local model of node or Provisioner subscribes a group address.

  备注

  This function shall not be invoked before node is provisioned or Provisioner is enabled.

  参数:

    - element_addr -- [in] Unicast address of the element to which the model belongs.

    - company_id -- [in] A 16-bit company identifier.

    - model_id -- [in] A 16-bit model identifier.

    - group_addr -- [in] The group address to be subscribed.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_model_unsubscribe_group_addr(uint16_t element_addr, uint16_t company_id, uint16_t model_id, uint16_t group_addr)

  A local model of node or Provisioner unsubscribes a group address.

  备注

  This function shall not be invoked before node is provisioned or Provisioner is enabled.

  参数:

    - element_addr -- [in] Unicast address of the element to which the model belongs.

    - company_id -- [in] A 16-bit company identifier.

    - model_id -- [in] A 16-bit model identifier.

    - group_addr -- [in] The subscribed group address.

  返回:

    ESP_OK on success or error code otherwise.

const uint8_t *esp_ble_mesh_node_get_local_net_key(uint16_t net_idx)

  This function is called by Node to get the local NetKey.

  参数:

    net_idx -- [in] NetKey index.

  返回:

    NetKey on success, or NULL on failure.

const uint8_t *esp_ble_mesh_node_get_local_app_key(uint16_t app_idx)

  This function is called by Node to get the local AppKey.

  参数:

    app_idx -- [in] AppKey index.

  返回:

    AppKey on success, or NULL on failure.

esp_err_t esp_ble_mesh_node_add_local_net_key(const uint8_t net_key[16], uint16_t net_idx)

  This function is called by Node to add a local NetKey.

  备注

  This function can only be called after the device is provisioned.

  参数:

    - net_key -- [in] NetKey to be added.

    - net_idx -- [in] NetKey Index.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_node_add_local_app_key(const uint8_t app_key[16], uint16_t net_idx, uint16_t app_idx)

  This function is called by Node to add a local AppKey.

  备注

  The net_idx must be an existing one. This function can only be called after the device is provisioned.

  参数:

    - app_key -- [in] AppKey to be added.

    - net_idx -- [in] NetKey Index.

    - app_idx -- [in] AppKey Index.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_node_bind_app_key_to_local_model(uint16_t element_addr, uint16_t company_id, uint16_t model_id, uint16_t app_idx)

  This function is called by Node to bind AppKey to model locally.

  备注

  If going to bind app_key with local vendor model, the company_id shall be set to 0xFFFF. This function can only be called after the device is provisioned.

  参数:

    - element_addr -- [in] Node local element address

    - company_id -- [in] Node local company id

    - model_id -- [in] Node local model id

    - app_idx -- [in] Node local appkey index

  返回:

    ESP_OK on success or error code otherwise.

Coexist with BLE

### Header File

- components/bt/esp_ble_mesh/api/core/include/esp_ble_mesh_ble_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_ble_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_ble_callback(esp_ble_mesh_ble_cb_t callback)

  Register BLE scanning callback.

  参数:

    callback -- [in] Pointer to the BLE scanning callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_start_ble_advertising(const esp_ble_mesh_ble_adv_param_t *param, const esp_ble_mesh_ble_adv_data_t *data)

  This function is called to start BLE advertising with the corresponding data and parameters while BLE Mesh is working at the same time.

  备注

  1. When this function is called, the BLE advertising packet will be posted to the BLE mesh adv queue in the mesh stack and waited to be sent.

  1. In the BLE advertising parameters, the "duration" means the time used for sending the BLE advertising packet each time, it shall not be smaller than the advertising interval. When the packet is sent successfully, it will be posted to the adv queue again after the "period" time if the "count" is bigger than 0. The "count" means how many durations the packet will be sent after it is sent successfully for the first time. And if the "count" is set to 0xFFFF, which means the packet will be sent infinitely.

  2. The "priority" means the priority of BLE advertising packet compared with BLE Mesh packets. Currently two options (i.e. low/high) are provided. If the "priority" is high, the BLE advertising packet will be posted to the front of adv queue. Otherwise it will be posted to the back of adv queue.

  参数:

    - param -- [in] Pointer to the BLE advertising parameters

    - data -- [in] Pointer to the BLE advertising data and scan response data

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_stop_ble_advertising(uint8_t index)

  This function is called to stop BLE advertising with the corresponding index.

  参数:

    index -- [in] Index of BLE advertising

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_start_ble_scanning(esp_ble_mesh_ble_scan_param_t *param)

  This function is called to start scanning normal BLE advertising packets and notifying the packets to the application layer.

  参数:

    param -- [in] Pointer to the BLE scanning parameters

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_stop_ble_scanning(void)

  This function is called to stop notifying normal BLE advertising packets to the application layer.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_scan_params_update(esp_ble_mesh_scan_param_t *scan_param)

  Update BLE Mesh scan parameters.

  备注

  1. This function shall be used after ESP BLE Mesh is initialized! Parameters `scan_interval` and `uncoded_scan_window` must both be multiples of 8.

  2. If the config BLE_MESH_USE_BLE_50 is enabled, within the scan_interval:

     - If uncoded_scan_window is not zero, the scan_interval is divided into two parts:

       - uncoded_scan_window: Used for performing uncoded scanning.

       - (scan_interval - uncoded_scan_window): The remaining time is used for coded scanning (coded_scan).

     - If uncoded_scan_window is set to 0, it means the entire scan_interval is used for coded scanning.

     - If uncoded_scan_window is equal to scan_interval, it means the entire scan_interval is used for uncoded scanning.

  参数:

    scan_param -- [in] Scan parameters

  返回:

    - ESP_OK: Success

    - ESP_FAIL: Invalid parameters or unable transfer this command to the stack

### Unions

union esp_ble_mesh_ble_cb_param_t
  #include <esp_ble_mesh_ble_api.h>

  BLE operation callback parameters

  Public Members

  int err_code

    Indicate the result of starting BLE advertising

    Indicate the result of stopping BLE advertising

    Indicate the result of starting BLE scanning

    Indicate the result of stopping BLE scanning

  uint8_t index

    Index of the BLE advertising

  struct esp_ble_mesh_ble_cb_param_t start_ble_advertising_comp

    ESP_BLE_MESH_START_BLE_ADVERTISING_COMP_EVT.

    Event parameters of ESP_BLE_MESH_START_BLE_ADVERTISING_COMP_EVT

  struct esp_ble_mesh_ble_cb_param_t stop_ble_advertising_comp

    ESP_BLE_MESH_STOP_BLE_ADVERTISING_COMP_EVT.

    Event parameters of ESP_BLE_MESH_STOP_BLE_ADVERTISING_COMP_EVT

  struct esp_ble_mesh_ble_cb_param_t start_ble_scan_comp

    ESP_BLE_MESH_START_BLE_SCANNING_COMP_EVT.

    Event parameters of ESP_BLE_MESH_START_BLE_SCANNING_COMP_EVT

  struct esp_ble_mesh_ble_cb_param_t stop_ble_scan_comp

    ESP_BLE_MESH_STOP_BLE_SCANNING_COMP_EVT.

    Event parameters of ESP_BLE_MESH_STOP_BLE_SCANNING_COMP_EVT

  esp_ble_mesh_ble_adv_rpt_t scan_ble_adv_pkt

    Event parameters of ESP_BLE_MESH_SCAN_BLE_ADVERTISING_PKT_EVT.

  struct esp_ble_mesh_ble_cb_param_t::ble_mesh_scan_params_update_comp_param scan_params_update_comp

    Event parameter of ESP_BLE_MESH_SCAN_PARAMS_UPDATE_COMP_EVT

  struct ble_mesh_scan_params_update_comp_param
    #include <esp_ble_mesh_ble_api.h>

    Event parameter of ESP_BLE_MESH_SCAN_PARAMS_UPDATE_COMP_EVT.

    Public Members

    int err_code

      Indicates the result of updating scan parameters

### Structures

struct esp_ble_mesh_ble_adv_rpt_t

  Context of BLE advertising report.

  Public Members

  uint8_t addr[6]

    Device address

  uint8_t addr_type

    Device address type

  uint8_t adv_type

    Advertising type

  uint8_t *data

    Advertising data

  uint16_t length

    Advertising data length

  int8_t rssi

    RSSI of the advertising packet

struct esp_ble_mesh_ble_adv_param_t

  Context of BLE advertising parameters.

  Public Members

  uint16_t interval

    BLE advertising interval

  uint8_t adv_type

    BLE advertising type

  uint8_t own_addr_type

    Own address type

  uint8_t peer_addr_type

    Peer address type

  uint8_t peer_addr[BD_ADDR_LEN]

    Peer address

  uint16_t duration

    Duration is milliseconds

  uint16_t period

    Period in milliseconds

  uint16_t count

    Number of advertising duration

  uint8_t priority

    Priority of BLE advertising packet

struct esp_ble_mesh_ble_adv_data_t

  Context of BLE advertising data.

  Public Members

  uint8_t adv_data_len

    Advertising data length

  uint8_t adv_data[31]

    Advertising data

  uint8_t scan_rsp_data_len

    Scan response data length

  uint8_t scan_rsp_data[31]

    Scan response data

struct esp_ble_mesh_ble_scan_param_t

  Context of BLE scanning parameters.

  Public Members

  uint32_t duration

    Duration used to scan normal BLE advertising packets

### Macros

ESP_BLE_MESH_BLE_ADV_INFINITE

  Count for sending BLE advertising packet infinitely This enum value is the priority of BLE advertising packet

### Type Definitions

typedef void (*esp_ble_mesh_ble_cb_t)(esp_ble_mesh_ble_cb_event_t event, esp_ble_mesh_ble_cb_param_t *param)

  BLE scanning callback function type.

  Param event:

    BLE scanning callback event type

  Param param:

    BLE scanning callback parameter

### Enumerations

enum esp_ble_mesh_ble_cb_event_t

  This enum value is the event of BLE operations

  Values:

  enumerator ESP_BLE_MESH_START_BLE_ADVERTISING_COMP_EVT

    Start BLE advertising completion event

  enumerator ESP_BLE_MESH_STOP_BLE_ADVERTISING_COMP_EVT

    Stop BLE advertising completion event

  enumerator ESP_BLE_MESH_START_BLE_SCANNING_COMP_EVT

    Start BLE scanning completion event

  enumerator ESP_BLE_MESH_STOP_BLE_SCANNING_COMP_EVT

    Stop BLE scanning completion event

  enumerator ESP_BLE_MESH_SCAN_BLE_ADVERTISING_PKT_EVT

    Scanning BLE advertising packets event

  enumerator ESP_BLE_MESH_SCAN_PARAMS_UPDATE_COMP_EVT

    Scan parameters update completion event

  enumerator ESP_BLE_MESH_BLE_EVT_MAX

enum esp_ble_mesh_ble_adv_priority_t

  Values:

  enumerator ESP_BLE_MESH_BLE_ADV_PRIO_LOW
  enumerator ESP_BLE_MESH_BLE_ADV_PRIO_HIGH

### Low Power Operation (Updating)

### Header File

- components/bt/esp_ble_mesh/api/core/include/esp_ble_mesh_low_power_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_low_power_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_lpn_enable(void)

  Enable BLE Mesh device LPN functionality.

  备注

  This API enables LPN functionality. Once called, the proper Friend Request will be sent.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_lpn_disable(bool force)

  Disable BLE Mesh device LPN functionality.

  参数:

    force -- [in] when disabling LPN functionality, use this flag to indicate whether directly clear corresponding information or just send friend clear to disable it if friendship has already been established.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_lpn_poll(void)

  LPN tries to poll messages from the Friend Node.

  备注

  The Friend Poll message is sent by a Low Power node to ask the Friend node to send a message that it has stored for the Low Power node. Users can call this API to send Friend Poll message manually. If this API is not invoked, the bottom layer of the Low Power node will send Friend Poll before the PollTimeout timer expires. If the corresponding Friend Update is received and MD is set to 0, which means there are no messages for the Low Power node, then the Low Power node will stop scanning.

  返回:

    ESP_OK on success or error code otherwise.

### Send/Publish Messages, Add Local AppKey, Etc.

### Header File

- components/bt/esp_ble_mesh/api/core/include/esp_ble_mesh_networking_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_networking_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_custom_model_callback(esp_ble_mesh_model_cb_t callback)

  Register BLE Mesh callback for user-defined models' operations. This callback can report the following events generated for the user-defined models:

  - Call back the messages received by user-defined client and server models to the application layer;

  - If users call esp_ble_mesh_server/client_model_send, this callback notifies the application layer of the send_complete event;

  - If user-defined client model sends a message that requires response, and the response message is received after the timer expires, the response message will be reported to the application layer as published by a peer device;

  - If the user-defined client model fails to receive the response message during a specified period of time, a timeout event will be reported to the application layer.

  备注

  The client models (i.e. Config Client model, Health Client model, Generic Client models, Sensor Client model, Scene Client model and Lighting Client models) that have been realized internally have their specific register functions. For example, esp_ble_mesh_register_config_client_callback is the register function for Config Client Model.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_model_msg_opcode_init(uint8_t *data, uint32_t opcode)

  Add the message opcode to the beginning of the model message before sending or publishing the model message.

  备注

  This API is only used to set the opcode of the message.

  参数:

    - data -- [in] Pointer to the message data.

    - opcode -- [in] The message opcode.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_client_model_init(esp_ble_mesh_model_t *model)

  Initialize the user-defined client model. All user-defined client models shall call this function to initialize the client model internal data. Node: Before calling this API, the op_pair_size and op_pair variables within the user_data(defined using esp_ble_mesh_client_t_) of the client model need to be initialized.

  参数:

    model -- [in] BLE Mesh Client model to which the message belongs.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_client_model_deinit(esp_ble_mesh_model_t *model)

  De-initialize the user-defined client model.

  备注

  This function shall be invoked before esp_ble_mesh_deinit() is called.

  参数:

    model -- [in] Pointer of the Client model.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_server_model_send_msg(esp_ble_mesh_model_t *model, esp_ble_mesh_msg_ctx_t *ctx, uint32_t opcode, uint16_t length, uint8_t *data)

  Send server model messages(such as server model status messages).

  参数:

    - model -- [in] BLE Mesh Server Model to which the message belongs.

    - ctx -- [in] Message context, includes keys, TTL, etc.

    - opcode -- [in] Message opcode.

    - length -- [in] Message length (exclude the message opcode).

    - data -- [in] Parameters of Access Payload (exclude the message opcode) to be sent.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_client_model_send_msg(esp_ble_mesh_model_t *model, esp_ble_mesh_msg_ctx_t *ctx, uint32_t opcode, uint16_t length, uint8_t *data, int32_t msg_timeout, bool need_rsp, esp_ble_mesh_dev_role_t device_role)

  Send client model message (such as model get, set, etc).

  参数:

    - model -- [in] BLE Mesh Client Model to which the message belongs.

    - ctx -- [in] Message context, includes keys, TTL, etc.

    - opcode -- [in] Message opcode.

    - length -- [in] Message length (exclude the message opcode).

    - data -- [in] Parameters of the Access Payload (exclude the message opcode) to be sent.

    - msg_timeout -- [in] Time to get response to the message (in milliseconds).

    - need_rsp -- [in] TRUE if the opcode requires the peer device to reply, FALSE otherwise.

    - device_role -- [in] Role of the device (Node/Provisioner) that sends the message.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_model_publish(esp_ble_mesh_model_t *model, uint32_t opcode, uint16_t length, uint8_t *data, esp_ble_mesh_dev_role_t device_role)

  Send a model publication message.

  备注

  Before calling this function, the user needs to ensure that the model publication message (esp_ble_mesh_model_pub_t::msg) contains a valid message to be sent. And if users want to update the publishing message, this API should be called in ESP_BLE_MESH_MODEL_PUBLISH_UPDATE_EVT with the message updated.

  参数:

    - model -- [in] Mesh (client) Model publishing the message.

    - opcode -- [in] Message opcode.

    - length -- [in] Message length (exclude the message opcode).

    - data -- [in] Parameters of the Access Payload (exclude the message opcode) to be sent.

    - device_role -- [in] Role of the device (node/provisioner) publishing the message of the type esp_ble_mesh_dev_role_t.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_server_model_update_state(esp_ble_mesh_model_t *model, esp_ble_mesh_server_state_type_t type, esp_ble_mesh_server_state_value_t *value)

  Update a server model state value. If the model publication state is set properly (e.g. publish address is set to a valid address), it will publish corresponding status message.

  备注

  Currently this API is used to update bound state value, not for all server model states.

  参数:

    - model -- [in] Server model which is going to update the state.

    - type -- [in] Server model state type.

    - value -- [in] Server model state value.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_node_local_reset(void)

  Reset the provisioning procedure of the local BLE Mesh node.

  备注

  All provisioning information in this node will be deleted and the node needs to be re-provisioned. The API function esp_ble_mesh_node_prov_enable() needs to be called to start a new provisioning procedure.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_set_node_name(uint16_t index, const char *name)

  This function is called to set the node (provisioned device) name.

  备注

  index is obtained from the parameters of ESP_BLE_MESH_PROVISIONER_PROV_COMPLETE_EVT.

  参数:

    - index -- [in] Index of the node in the node queue.

    - name -- [in] Name (end by '\0') to be set for the node.

  返回:

    ESP_OK on success or error code otherwise.

const char *esp_ble_mesh_provisioner_get_node_name(uint16_t index)

  This function is called to get the node (provisioned device) name.

  备注

  index is obtained from the parameters of ESP_BLE_MESH_PROVISIONER_PROV_COMPLETE_EVT.

  参数:

    index -- [in] Index of the node in the node queue.

  返回:

    Node name on success, or NULL on failure.

uint16_t esp_ble_mesh_provisioner_get_node_index(const char *name)

  This function is called to get the node (provisioned device) index.

  参数:

    name -- [in] Name of the node (end by '\0').

  返回:

    Node index on success, or an invalid value (0xFFFF) on failure.

esp_err_t esp_ble_mesh_provisioner_store_node_comp_data(uint16_t unicast_addr, uint8_t *data, uint16_t length)

  This function is called to store the Composition Data of the node.

  参数:

    - unicast_addr -- [in] Element address of the node

    - data -- [in] Pointer of Composition Data

    - length -- [in] Length of Composition Data

  返回:

    ESP_OK on success or error code otherwise.

esp_ble_mesh_node_t *esp_ble_mesh_provisioner_get_node_with_uuid(const uint8_t uuid[16])

  This function is called to get the provisioned node information with the node device uuid.

  参数:

    uuid -- [in] Device UUID of the node

  返回:

    Pointer of the node info struct or NULL on failure.

esp_ble_mesh_node_t *esp_ble_mesh_provisioner_get_node_with_addr(uint16_t unicast_addr)

  This function is called to get the provisioned node information with the node unicast address.

  参数:

    unicast_addr -- [in] Unicast address of the node

  返回:

    Pointer of the node info struct or NULL on failure.

esp_ble_mesh_node_t *esp_ble_mesh_provisioner_get_node_with_name(const char *name)

  This function is called to get the provisioned node information with the node name.

  参数:

    name -- [in] Name of the node (end by '\0').

  返回:

    Pointer of the node info struct or NULL on failure.

uint16_t esp_ble_mesh_provisioner_get_prov_node_count(void)

  This function is called by Provisioner to get provisioned node count.

  返回:

    Number of the provisioned nodes.

const esp_ble_mesh_node_t **esp_ble_mesh_provisioner_get_node_table_entry(void)

  This function is called by Provisioner to get the entry of the node table.

  备注

  After invoking the function to get the entry of nodes, users can use the "for" loop combined with the macro CONFIG_BLE_MESH_MAX_PROV_NODES to get each node's information. Before trying to read the node's information, users need to check if the node exists, i.e. if the *(esp_ble_mesh_node_t **node) is NULL. For example: `const esp_ble_mesh_node_t **entry = esp_ble_mesh_provisioner_get_node_table_entry(); for (int i = 0; i < CONFIG_BLE_MESH_MAX_PROV_NODES; i++) { const esp_ble_mesh_node_t *node = entry[i]; if (node) { ...... } }`

  返回:

    Pointer to the start of the node table.

esp_err_t esp_ble_mesh_provisioner_delete_node_with_uuid(const uint8_t uuid[16])

  This function is called to delete the provisioned node information with the node device uuid.

  参数:

    uuid -- [in] Device UUID of the node

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_delete_node_with_addr(uint16_t unicast_addr)

  This function is called to delete the provisioned node information with the node unicast address.

  参数:

    unicast_addr -- [in] Unicast address of the node

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_add_local_app_key(const uint8_t app_key[16], uint16_t net_idx, uint16_t app_idx)

  This function is called to add a local AppKey for Provisioner.

  备注

  app_key: If set to NULL, app_key will be generated internally. net_idx: Should be an existing one. app_idx: If it is going to be generated internally, it should be set to 0xFFFF, and the new app_idx will be reported via an event.

  参数:

    - app_key -- [in] The app key to be set for the local BLE Mesh stack.

    - net_idx -- [in] The network key index.

    - app_idx -- [in] The app key index.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_update_local_app_key(const uint8_t app_key[16], uint16_t net_idx, uint16_t app_idx)

  This function is used to update a local AppKey for Provisioner.

  参数:

    - app_key -- [in] Value of the AppKey.

    - net_idx -- [in] Corresponding NetKey Index.

    - app_idx -- [in] The AppKey Index

  返回:

    ESP_OK on success or error code otherwise.

const uint8_t *esp_ble_mesh_provisioner_get_local_app_key(uint16_t net_idx, uint16_t app_idx)

  This function is called by Provisioner to get the local app key value.

  参数:

    - net_idx -- [in] Network key index.

    - app_idx -- [in] Application key index.

  返回:

    App key on success, or NULL on failure.

esp_err_t esp_ble_mesh_provisioner_bind_app_key_to_local_model(uint16_t element_addr, uint16_t app_idx, uint16_t model_id, uint16_t company_id)

  This function is called by Provisioner to bind own model with proper app key.

  备注

  company_id: If going to bind app_key with local vendor model, company_id should be set to 0xFFFF.

  参数:

    - element_addr -- [in] Provisioner local element address

    - app_idx -- [in] Provisioner local appkey index

    - model_id -- [in] Provisioner local model id

    - company_id -- [in] Provisioner local company id

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_add_local_net_key(const uint8_t net_key[16], uint16_t net_idx)

  This function is called by Provisioner to add local network key.

  备注

  net_key: If set to NULL, net_key will be generated internally. net_idx: If it is going to be generated internally, it should be set to 0xFFFF, and the new net_idx will be reported via an event.

  参数:

    - net_key -- [in] The network key to be added to the Provisioner local BLE Mesh stack.

    - net_idx -- [in] The network key index.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_update_local_net_key(const uint8_t net_key[16], uint16_t net_idx)

  This function is called by Provisioner to update a local network key.

  参数:

    - net_key -- [in] Value of the NetKey.

    - net_idx -- [in] The NetKey Index.

  返回:

    ESP_OK on success or error code otherwise.

const uint8_t *esp_ble_mesh_provisioner_get_local_net_key(uint16_t net_idx)

  This function is called by Provisioner to get the local network key value.

  参数:

    net_idx -- [in] Network key index.

  返回:

    Network key on success, or NULL on failure.

esp_err_t esp_ble_mesh_provisioner_recv_heartbeat(bool enable)

  This function is called by Provisioner to enable or disable receiving heartbeat messages.

  备注

  If enabling receiving heartbeat message successfully, the filter will be an empty rejectlist by default, which means all heartbeat messages received by the Provisioner will be reported to the application layer.

  参数:

    enable -- [in] Enable or disable receiving heartbeat messages.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_set_heartbeat_filter_type(uint8_t type)

  This function is called by Provisioner to set the heartbeat filter type.

  备注

  1. If the filter type is not the same with the current value, then all the filter entries will be cleaned.

  1. If the previous type is rejectlist, and changed to acceptlist, then the filter will be an empty acceptlist, which means no heartbeat messages will be reported. Users need to add SRC or DST into the filter entry, then heartbeat messages from the SRC or to the DST will be reported.

  参数:

    type -- [in] Heartbeat filter type (acceptlist or rejectlist).

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_set_heartbeat_filter_info(uint8_t op, esp_ble_mesh_heartbeat_filter_info_t *info)

  This function is called by Provisioner to add or remove a heartbeat filter entry.

  1. If the operation is "REMOVE", the "hb_src" can be set to the SRC (can only be a unicast address) of heartbeat messages, and the "hb_dst" can be set to the DST (unicast address or group address), at least one of them needs to be set.

     - The filter entry with the same SRC or DST will be removed.

  备注

  1. If the operation is "ADD", the "hb_src" can be set to the SRC (can only be a unicast address) of heartbeat messages, and the "hb_dst" can be set to the DST (unicast address or group address), at least one of them needs to be set.

  - If only one of them is set, the filter entry will only use the configured SRC or DST to filter heartbeat messages.

  - If both of them are set, the SRC and DST will both be used to decide if a heartbeat message will be handled.

  - If SRC or DST already exists in some filter entry, then the corresponding entry will be cleaned firstly, then a new entry will be allocated to store the information.

  参数:

    - op -- [in] Add or REMOVE

    - info -- [in] Heartbeat filter entry information, including: hb_src - Heartbeat source address; hb_dst - Heartbeat destination address;

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_direct_erase_settings(void)

  This function is called by Provisioner to directly erase the mesh information from nvs namespace.

  备注

  This function can be invoked when the mesh stack is not initialized or has been de-initialized.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_open_settings_with_index(uint8_t index)

  This function is called by Provisioner to open a nvs namespace for storing mesh information.

  备注

  Before open another nvs namespace, the previously opened nvs namespace must be closed firstly.

  参数:

    index -- [in] Settings index.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_open_settings_with_uid(const char *uid)

  This function is called by Provisioner to open a nvs namespace for storing mesh information.

  备注

  Before open another nvs namespace, the previously opened nvs namespace must be closed firstly.

  参数:

    uid -- [in] Settings user id.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_close_settings_with_index(uint8_t index, bool erase)

  This function is called by Provisioner to close a nvs namespace which is opened previously for storing mesh information.

  备注

  1. Before closing the nvs namespace, it must be open.

  1. When the function is invoked, the Provisioner functionality will be disabled firstly, and: a) If the "erase" flag is set to false, the mesh information will be cleaned (e.g. removing NetKey, AppKey, nodes, etc) from the mesh stack. b) If the "erase" flag is set to true, the mesh information stored in the nvs namespace will also be erased besides been cleaned from the mesh stack.

  2. If Provisioner tries to work properly again, we can invoke the open function to open a new nvs namespace or a previously added one, and restore the mesh information from it if not erased.

  3. The working process shall be as following: a) Open settings A b) Start to provision and control nodes c) Close settings A d) Open settings B e) Start to provision and control other nodes f) Close settings B g) ......

  参数:

    - index -- [in] Settings index.

    - erase -- [in] Indicate if erasing mesh information.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_close_settings_with_uid(const char *uid, bool erase)

  This function is called by Provisioner to close a nvs namespace which is opened previously for storing mesh information.

  备注

  1. Before closing the nvs namespace, it must be open.

  1. When the function is invoked, the Provisioner functionality will be disabled firstly, and: a) If the "erase" flag is set to false, the mesh information will be cleaned (e.g. removing NetKey, AppKey, nodes, etc) from the mesh stack. b) If the "erase" flag is set to true, the mesh information stored in the nvs namespace will also be erased besides been cleaned from the mesh stack.

  2. If Provisioner tries to work properly again, we can invoke the open function to open a new nvs namespace or a previously added one, and restore the mesh information from it if not erased.

  3. The working process shall be as following: a) Open settings A b) Start to provision and control nodes c) Close settings A d) Open settings B e) Start to provision and control other nodes f) Close settings B g) ......

  参数:

    - uid -- [in] Settings user id.

    - erase -- [in] Indicate if erasing mesh information.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_delete_settings_with_index(uint8_t index)

  This function is called by Provisioner to erase the mesh information and settings user id from a nvs namespace.

  备注

  When this function is called, the nvs namespace must not be open. This function is used to erase the mesh information and settings user id which are not used currently.

  参数:

    index -- [in] Settings index.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_delete_settings_with_uid(const char *uid)

  This function is called by Provisioner to erase the mesh information and settings user id from a nvs namespace.

  备注

  When this function is called, the nvs namespace must not be open. This function is used to erase the mesh information and settings user id which are not used currently.

  参数:

    uid -- [in] Settings user id.

  返回:

    ESP_OK on success or error code otherwise.

const char *esp_ble_mesh_provisioner_get_settings_uid(uint8_t index)

  This function is called by Provisioner to get settings user id.

  参数:

    index -- [in] Settings index.

  返回:

    Setting user id on success or NULL on failure.

uint8_t esp_ble_mesh_provisioner_get_settings_index(const char *uid)

  This function is called by Provisioner to get settings index.

  参数:

    uid -- [in] Settings user id.

  返回:

    Settings index.

uint8_t esp_ble_mesh_provisioner_get_free_settings_count(void)

  This function is called by Provisioner to get the number of free settings user id.

  返回:

    Number of free settings user id.

const uint8_t *esp_ble_mesh_get_fast_prov_app_key(uint16_t net_idx, uint16_t app_idx)

  This function is called to get fast provisioning application key.

  参数:

    - net_idx -- [in] Network key index.

    - app_idx -- [in] Application key index.

  返回:

    Application key on success, or NULL on failure.

### Type Definitions

typedef void (*esp_ble_mesh_model_cb_t)(esp_ble_mesh_model_cb_event_t event, esp_ble_mesh_model_cb_param_t *param)

  : event, event code of user-defined model events; param, parameters of user-defined model events

### ESP-BLE-MESH Node/Provisioner Provisioning

### Header File

- components/bt/esp_ble_mesh/api/core/include/esp_ble_mesh_provisioning_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_provisioning_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_prov_callback(esp_ble_mesh_prov_cb_t callback)

  Register BLE Mesh provisioning callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

bool esp_ble_mesh_node_is_provisioned(void)

  Check if a device has been provisioned.

  返回:

    TRUE if the device is provisioned, FALSE if the device is unprovisioned.

esp_err_t esp_ble_mesh_node_prov_enable(esp_ble_mesh_prov_bearer_t bearers)

  Enable specific provisioning bearers to get the device ready for provisioning.

  备注

  PB-ADV: send unprovisioned device beacon. PB-GATT: send connectable advertising packets.

  参数:

    bearers -- Bit-wise OR of provisioning bearers.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_node_prov_disable(esp_ble_mesh_prov_bearer_t bearers)

  Disable specific provisioning bearers to make a device inaccessible for provisioning.

  参数:

    bearers -- Bit-wise OR of provisioning bearers.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_node_set_oob_pub_key(uint8_t pub_key_x[32], uint8_t pub_key_y[32], uint8_t private_key[32])

  Unprovisioned device set own oob public key & private key pair.

  备注

  In order to avoid suffering brute-forcing attack (CVE-2020-26559). The Bluetooth SIG recommends that potentially vulnerable mesh provisioners use an out-of-band mechanism to exchange the public keys. So as an unprovisioned device, it should use this function to input the Public Key exchanged through the out-of-band mechanism.

  参数:

    - pub_key_x -- [in] Unprovisioned device's Public Key X

    - pub_key_y -- [in] Unprovisioned device's Public Key Y

    - private_key -- [in] Unprovisioned device's Private Key

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_node_input_number(uint32_t number)

  Provide provisioning input OOB number.

  备注

  This is intended to be called if the user has received ESP_BLE_MESH_NODE_PROV_INPUT_EVT with ESP_BLE_MESH_ENTER_NUMBER as the action.

  参数:

    number -- [in] Number input by device.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_node_input_string(const char *string)

  Provide provisioning input OOB string.

  备注

  This is intended to be called if the user has received ESP_BLE_MESH_NODE_PROV_INPUT_EVT with ESP_BLE_MESH_ENTER_STRING as the action.

  参数:

    string -- [in] String input by device.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_set_unprovisioned_device_name(const char *name)

  Using this function, an unprovisioned device can set its own device name, which will be broadcasted in its advertising data.

  备注

  This API applicable to PB-GATT mode only by setting the name to the scan response data, it doesn't apply to PB-ADV mode.

  参数:

    name -- [in] Unprovisioned device name

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_read_oob_pub_key(uint8_t link_idx, uint8_t pub_key_x[32], uint8_t pub_key_y[32])

  Provisioner inputs unprovisioned device's oob public key.

  备注

  In order to avoid suffering brute-forcing attack (CVE-2020-26559). The Bluetooth SIG recommends that potentially vulnerable mesh provisioners use an out-of-band mechanism to exchange the public keys.

  参数:

    - link_idx -- [in] The provisioning link index

    - pub_key_x -- [in] Unprovisioned device's Public Key X

    - pub_key_y -- [in] Unprovisioned device's Public Key Y

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_input_string(const char *string, uint8_t link_idx)

  Provide provisioning input OOB string.

                This is intended to be called after the esp_ble_mesh_prov_t prov_input_num
                callback has been called with ESP_BLE_MESH_ENTER_STRING as the action.

  参数:

    - string -- [in] String input by Provisioner.

    - link_idx -- [in] The provisioning link index.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_input_number(uint32_t number, uint8_t link_idx)

  Provide provisioning input OOB number.

                This is intended to be called after the esp_ble_mesh_prov_t prov_input_num
                callback has been called with ESP_BLE_MESH_ENTER_NUMBER as the action.

  参数:

    - number -- [in] Number input by Provisioner.

    - link_idx -- [in] The provisioning link index.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_prov_enable(esp_ble_mesh_prov_bearer_t bearers)

  Enable one or more provisioning bearers.

  备注

  PB-ADV: Enable BLE scan. PB-GATT: Initialize corresponding BLE Mesh Proxy info.

  参数:

    bearers -- [in] Bit-wise OR of provisioning bearers.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_prov_disable(esp_ble_mesh_prov_bearer_t bearers)

  Disable one or more provisioning bearers.

  备注

  PB-ADV: Disable BLE scan. PB-GATT: Break any existing BLE Mesh Provisioning connections.

  参数:

    bearers -- [in] Bit-wise OR of provisioning bearers.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_add_unprov_dev(esp_ble_mesh_unprov_dev_add_t *add_dev, esp_ble_mesh_dev_add_flag_t flags)

  Add unprovisioned device info to the unprov_dev queue.

  备注

  : 1. Currently address type only supports public address and static random address.

  1. If device UUID and/or device address as well as address type already exist in the device queue, but the bearer is different from the existing one, add operation will also be successful and it will update the provision bearer supported by the device.

  2. For example, if the Provisioner wants to add an unprovisioned device info before receiving its unprovisioned device beacon or Mesh Provisioning advertising packets, the Provisioner can use this API to add the device info with each one or both of device UUID and device address added. When the Provisioner gets the device's advertising packets, it will start provisioning the device internally.

     - In this situation, the Provisioner can set bearers with each one or both of ESP_BLE_MESH_PROV_ADV and ESP_BLE_MESH_PROV_GATT enabled, and cannot set flags with ADD_DEV_START_PROV_NOW_FLAG enabled.

  3. Another example is when the Provisioner receives the unprovisioned device's beacon or Mesh Provisioning advertising packets, the advertising packets will be reported on to the application layer using the callback registered by the function esp_ble_mesh_register_prov_callback. And in the callback, the Provisioner can call this API to start provisioning the device.

     - If the Provisioner uses PB-ADV to provision, either one or both of device UUID and device address can be added, bearers shall be set with ESP_BLE_MESH_PROV_ADV enabled and the flags shall be set with ADD_DEV_START_PROV_NOW_FLAG enabled.

     - If the Provisioner uses PB-GATT to provision, both the device UUID and device address need to be added, bearers shall be set with ESP_BLE_MESH_PROV_GATT enabled, and the flags shall be set with ADD_DEV_START_PROV_NOW_FLAG enabled.

     - If the Provisioner just wants to store the unprovisioned device info when receiving its advertising packets and start to provision it the next time (e.g. after receiving its advertising packets again), then it can add the device info with either one or both of device UUID and device address included. Bearers can be set with either one or both of ESP_BLE_MESH_PROV_ADV and ESP_BLE_MESH_PROV_GATT enabled (recommend to enable the bearer which will receive its advertising packets, because if the other bearer is enabled, the Provisioner is not aware if the device supports the bearer), and flags cannot be set with ADD_DEV_START_PROV_NOW_FLAG enabled.

     - Note: ESP_BLE_MESH_PROV_ADV, ESP_BLE_MESH_PROV_GATT and ADD_DEV_START_PROV_NOW_FLAG can not be enabled at the same time.

  参数:

    - add_dev -- [in] Pointer to a struct containing the device information

    - flags -- [in] Flags indicate several operations on the device information

      - Remove device information from queue after device has been provisioned (BIT0)

      - Start provisioning immediately after device is added to queue (BIT1)

      - Device can be removed if device queue is full (BIT2)

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_prov_device_with_addr(const uint8_t uuid[16], esp_ble_mesh_bd_addr_t addr, esp_ble_mesh_addr_type_t addr_type, esp_ble_mesh_prov_bearer_t bearer, uint16_t oob_info, uint16_t unicast_addr)

  Provision an unprovisioned device and assign a fixed unicast address for it in advance.

  备注

  : 1. Currently address type only supports public address and static random address.

  1. Bearer must be equal to ESP_BLE_MESH_PROV_ADV or ESP_BLE_MESH_PROV_GATT, since Provisioner will start to provision a device immediately once this function is invoked. And the input bearer must be identical with the one within the parameters of the ESP_BLE_MESH_PROVISIONER_RECV_UNPROV_ADV_PKT_EVT event.

  2. If this function is used by a Provisioner to provision devices, the application should take care of the assigned unicast address and avoid overlap of the unicast addresses of different nodes.

  3. Recommend to use only one of the functions "esp_ble_mesh_provisioner_add_unprov_dev" and "esp_ble_mesh_provisioner_prov_device_with_addr" by a Provisioner.

  参数:

    - uuid -- [in] Device UUID of the unprovisioned device

    - addr -- [in] Device address of the unprovisioned device

    - addr_type -- [in] Device address type of the unprovisioned device

    - bearer -- [in] Provisioning bearer going to be used by Provisioner

    - oob_info -- [in] OOB info of the unprovisioned device

    - unicast_addr -- [in] Unicast address going to be allocated for the unprovisioned device

  返回:

    Zero on success or (negative) error code otherwise.

esp_err_t esp_ble_mesh_provisioner_delete_dev(esp_ble_mesh_device_delete_t *del_dev)

  Delete device from queue, and reset current provisioning link with the device.

  备注

  If the device is in the queue, remove it from the queue; if the device is being provisioned, terminate the provisioning procedure. Either one of the device address or device UUID can be used as input.

  参数:

    del_dev -- [in] Pointer to a struct containing the device information.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_set_dev_uuid_match(const uint8_t *match_val, uint8_t match_len, uint8_t offset, bool prov_after_match)

  This function is called by Provisioner to set the part of the device UUID to be compared before starting to provision.

  参数:

    - match_val -- [in] Value to be compared with the part of the device UUID.

    - match_len -- [in] Length of the compared match value.

    - offset -- [in] Offset of the device UUID to be compared (based on zero).

    - prov_after_match -- [in] Flag used to indicate whether provisioner should start to provision the device immediately if the part of the UUID matches.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_set_prov_data_info(esp_ble_mesh_prov_data_info_t *prov_data_info)

  This function is called by Provisioner to set provisioning data information before starting to provision.

  参数:

    prov_data_info -- [in] Pointer to a struct containing net_idx or flags or iv_index.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_set_static_oob_value(const uint8_t *value, uint8_t length)

  This function is called by Provisioner to set static oob value used for provisioning.

  AuthValues selected using a cryptographically secure random or pseudorandom number generator and having the maximum permitted entropy (128-bits) will be most difficult to brute-force. AuthValues with reduced entropy or generated in a predictable manner will not grant the same level of protection against this vulnerability. Selecting a new AuthValue with each provisioning attempt can also make it more difficult to launch a brute-force attack by requiring the attacker to restart the search with each provisioning attempt (CVE-2020-26556).

  备注

  The Bluetooth SIG recommends that mesh implementations enforce a randomly selected AuthValue using all of the available bits, where permitted by the implementation. A large entropy helps ensure that a brute-force of the AuthValue, even a static AuthValue, cannot normally be completed in a reasonable time (CVE-2020-26557).

  参数:

    - value -- [in] Pointer to the static oob value.

    - length -- [in] Length of the static oob value.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_provisioner_set_primary_elem_addr(uint16_t addr)

  This function is called by Provisioner to set own Primary element address.

  备注

  This API must be invoked when BLE Mesh initialization is completed successfully, and can be invoked before Provisioner functionality is enabled. Once this API is invoked successfully, the prov_unicast_addr value in the struct esp_ble_mesh_prov_t will be ignored, and Provisioner will use this address as its own primary element address. And if the unicast address going to assigned for the next unprovisioned device is smaller than the input address + element number of Provisioner, then the address for the next unprovisioned device will be recalculated internally.

  参数:

    addr -- [in] Unicast address of the Primary element of Provisioner.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_set_fast_prov_info(esp_ble_mesh_fast_prov_info_t *fast_prov_info)

  This function is called to set provisioning data information before starting fast provisioning.

  参数:

    fast_prov_info -- [in] Pointer to a struct containing unicast address range, net_idx, etc.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_set_fast_prov_action(esp_ble_mesh_fast_prov_action_t action)

  This function is called to start/suspend/exit fast provisioning.

  参数:

    action -- [in] fast provisioning action (i.e. enter, suspend, exit).

  返回:

    ESP_OK on success or error code otherwise.

### Type Definitions

typedef void (*esp_ble_mesh_prov_cb_t)(esp_ble_mesh_prov_cb_event_t event, esp_ble_mesh_prov_cb_param_t *param)

  : event, event code of provisioning events; param, parameters of provisioning events

typedef void (*esp_ble_mesh_prov_adv_cb_t)(const esp_ble_mesh_bd_addr_t addr, const esp_ble_mesh_addr_type_t addr_type, const uint8_t adv_type, const uint8_t *dev_uuid, uint16_t oob_info, esp_ble_mesh_prov_bearer_t bearer)

  Callback for Provisioner that received advertising packets from unprovisioned devices which are not in the unprovisioned device queue.

  Report on the unprovisioned device beacon and mesh provisioning service adv data to application.

  Param addr:

    [in] Pointer to the unprovisioned device address.

  Param addr_type:

    [in] Unprovisioned device address type.

  Param adv_type:

    [in] Adv packet type(ADV_IND or ADV_NONCONN_IND).

  Param dev_uuid:

    [in] Unprovisioned device UUID pointer.

  Param oob_info:

    [in] OOB information of the unprovisioned device.

  Param bearer:

    [in] Adv packet received from PB-GATT or PB-ADV bearer.

### ESP-BLE-MESH GATT Proxy Server

### Header File

- components/bt/esp_ble_mesh/api/core/include/esp_ble_mesh_proxy_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_proxy_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_proxy_identity_enable(void)

  Enable advertising with Node Identity.

  备注

  This API requires that GATT Proxy support be enabled. Once called, each subnet starts advertising using Node Identity for the next 60 seconds, and after 60s Network ID will be advertised. Under normal conditions, the BLE Mesh Proxy Node Identity and Network ID advertising will be enabled automatically by BLE Mesh stack after the device is provisioned.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_proxy_gatt_enable(void)

  Enable BLE Mesh GATT Proxy Service.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_proxy_gatt_disable(void)

  Disconnect the BLE Mesh GATT Proxy connection if there is any, and disable the BLE Mesh GATT Proxy Service.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_private_proxy_identity_enable(void)

  Enable advertising with Private Node Identity.

  备注

  This API requires that GATT Proxy support be enabled. Once called, each subnet starts advertising using Private Node Identity for the next 60 seconds, and after 60s Private Network ID will be advertised. Under normal conditions, the BLE Mesh Proxy Node Identity, Network ID advertising, Proxy Private Node Identity and Private Network ID advertising will be enabled automatically by BLE Mesh stack after the device is provisioned.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_private_proxy_identity_disable(void)

  Disable advertising with Private Node Identity.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_proxy_client_connect(esp_ble_mesh_bd_addr_t addr, esp_ble_mesh_addr_type_t addr_type, uint16_t net_idx)

  Proxy Client creates a connection with the Proxy Server.

  参数:

    - addr -- [in] Device address of the Proxy Server.

    - addr_type -- [in] Device address type(public or static random).

    - net_idx -- [in] NetKey Index related with Network ID in the Mesh Proxy advertising packet.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_proxy_client_disconnect(uint8_t conn_handle)

  Proxy Client terminates a connection with the Proxy Server.

  参数:

    conn_handle -- [in] Proxy connection handle.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_proxy_client_set_filter_type(uint8_t conn_handle, uint16_t net_idx, esp_ble_mesh_proxy_filter_type_t filter_type)

  Proxy Client sets the filter type of the Proxy Server.

  参数:

    - conn_handle -- [in] Proxy connection handle.

    - net_idx -- [in] Corresponding NetKey Index.

    - filter_type -- [in] whitelist or blacklist.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_proxy_client_add_filter_addr(uint8_t conn_handle, uint16_t net_idx, uint16_t *addr, uint16_t addr_num)

  Proxy Client adds address to the Proxy Server filter list.

  参数:

    - conn_handle -- [in] Proxy connection handle.

    - net_idx -- [in] Corresponding NetKey Index.

    - addr -- [in] Pointer to the filter address.

    - addr_num -- [in] Number of the filter address.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_proxy_client_remove_filter_addr(uint8_t conn_handle, uint16_t net_idx, uint16_t *addr, uint16_t addr_num)

  Proxy Client removes address from the Proxy Server filter list.

  参数:

    - conn_handle -- [in] Proxy connection handle.

    - net_idx -- [in] Corresponding NetKey Index.

    - addr -- [in] Pointer to the filter address.

    - addr_num -- [in] Number of the filter address.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_proxy_client_directed_proxy_set(uint8_t conn_handle, uint16_t net_idx, uint8_t use_directed)

  Proxy Client sets whether or not the Directed Proxy Server uses directed forwarding for Directed Proxy Client messages.

  参数:

    - conn_handle -- [in] Proxy connection handle.

    - net_idx -- [in] Corresponding NetKey Index.

    - use_directed -- [in] Whether or not to send message by directed forwarding.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_proxy_client_send_solic_pdu(uint8_t net_idx, uint16_t ssrc, uint16_t dst)

  Proxy Client sends Solicitation PDU.

  参数:

    - net_idx -- [in] Corresponding NetKey Index.

    - ssrc -- [in] Solicitation SRC, shall be one of its element address.

    - dst -- [in] Solicitation DST (TBD).

  返回:

    ESP_OK on success or error code otherwise.

### Macros

ESP_BLE_MESH_PROXY_CLI_DIRECTED_FORWARDING_ENABLE

ESP_BLE_MESH_PROXY_CLI_DIRECTED_FORWARDING_DISABLE

## ESP-BLE-MESH Models API Reference

This section contains ESP-BLE-MESH Model related APIs, event types, event parameters, etc.

There are six categories of models:

- Configuration Client/Server Models

- Health Client/Server Models

- Generic Client/Server Models

- Sensor Client/Server Models

- Time and Scenes Client/Server Models

- Lighting Client/Server Models

备注

Definitions related to Server Models are being updated, and will be released soon.

### Configuration Client/Server Models

### Header File

- components/bt/esp_ble_mesh/api/models/include/esp_ble_mesh_config_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_config_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_config_client_callback(esp_ble_mesh_cfg_client_cb_t callback)

  Register BLE Mesh Config Client Model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_config_server_callback(esp_ble_mesh_cfg_server_cb_t callback)

  Register BLE Mesh Config Server Model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_config_client_get_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_cfg_client_get_state_t *get_state)

  Get the value of Config Server Model states using the Config Client Model get messages.

  备注

  If you want to find the opcodes and corresponding meanings accepted by this API, please refer to esp_ble_mesh_opcode_config_client_get_t in esp_ble_mesh_defs.h

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - get_state -- [in] Pointer to a union, each kind of opcode corresponds to one structure inside. Shall not be set to NULL.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_config_client_set_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_cfg_client_set_state_t *set_state)

  Set the value of the Configuration Server Model states using the Config Client Model set messages.

  备注

  If you want to find the opcodes and corresponding meanings accepted by this API, please refer to esp_ble_mesh_opcode_config_client_set_t in esp_ble_mesh_defs.h

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - set_state -- [in] Pointer to a union, each kind of opcode corresponds to one structure inside. Shall not be set to NULL.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_cfg_client_get_state_t
  #include <esp_ble_mesh_config_model_api.h>

  For ESP_BLE_MESH_MODEL_OP_BEACON_GET ESP_BLE_MESH_MODEL_OP_COMPOSITION_DATA_GET ESP_BLE_MESH_MODEL_OP_DEFAULT_TTL_GET ESP_BLE_MESH_MODEL_OP_GATT_PROXY_GET ESP_BLE_MESH_MODEL_OP_RELAY_GET ESP_BLE_MESH_MODEL_OP_MODEL_PUB_GET ESP_BLE_MESH_MODEL_OP_FRIEND_GET ESP_BLE_MESH_MODEL_OP_HEARTBEAT_PUB_GET ESP_BLE_MESH_MODEL_OP_HEARTBEAT_SUB_GET the get_state parameter in the esp_ble_mesh_config_client_get_state function should not be set to NULL.

  Public Members

  esp_ble_mesh_cfg_model_pub_get_t model_pub_get

    For ESP_BLE_MESH_MODEL_OP_MODEL_PUB_GET.

  esp_ble_mesh_cfg_composition_data_get_t comp_data_get

    For ESP_BLE_MESH_MODEL_OP_COMPOSITION_DATA_GET.

  esp_ble_mesh_cfg_sig_model_sub_get_t sig_model_sub_get

    For ESP_BLE_MESH_MODEL_OP_SIG_MODEL_SUB_GET

  esp_ble_mesh_cfg_vnd_model_sub_get_t vnd_model_sub_get

    For ESP_BLE_MESH_MODEL_OP_VENDOR_MODEL_SUB_GET

  esp_ble_mesh_cfg_app_key_get_t app_key_get

    For ESP_BLE_MESH_MODEL_OP_APP_KEY_GET.

  esp_ble_mesh_cfg_node_identity_get_t node_identity_get

    For ESP_BLE_MESH_MODEL_OP_NODE_IDENTITY_GET.

  esp_ble_mesh_cfg_sig_model_app_get_t sig_model_app_get

    For ESP_BLE_MESH_MODEL_OP_SIG_MODEL_APP_GET

  esp_ble_mesh_cfg_vnd_model_app_get_t vnd_model_app_get

    For ESP_BLE_MESH_MODEL_OP_VENDOR_MODEL_APP_GET

  esp_ble_mesh_cfg_kr_phase_get_t kr_phase_get

    For ESP_BLE_MESH_MODEL_OP_KEY_REFRESH_PHASE_GET

  esp_ble_mesh_cfg_lpn_polltimeout_get_t lpn_pollto_get

    For ESP_BLE_MESH_MODEL_OP_LPN_POLLTIMEOUT_GET

union esp_ble_mesh_cfg_client_set_state_t
  #include <esp_ble_mesh_config_model_api.h>

  For ESP_BLE_MESH_MODEL_OP_BEACON_SET ESP_BLE_MESH_MODEL_OP_DEFAULT_TTL_SET ESP_BLE_MESH_MODEL_OP_GATT_PROXY_SET ESP_BLE_MESH_MODEL_OP_RELAY_SET ESP_BLE_MESH_MODEL_OP_MODEL_PUB_SET ESP_BLE_MESH_MODEL_OP_MODEL_SUB_ADD ESP_BLE_MESH_MODEL_OP_MODEL_SUB_VIRTUAL_ADDR_ADD ESP_BLE_MESH_MODEL_OP_MODEL_SUB_DELETE ESP_BLE_MESH_MODEL_OP_MODEL_SUB_VIRTUAL_ADDR_DELETE ESP_BLE_MESH_MODEL_OP_MODEL_SUB_OVERWRITE ESP_BLE_MESH_MODEL_OP_MODEL_SUB_VIRTUAL_ADDR_OVERWRITE ESP_BLE_MESH_MODEL_OP_NET_KEY_ADD ESP_BLE_MESH_MODEL_OP_APP_KEY_ADD ESP_BLE_MESH_MODEL_OP_MODEL_APP_BIND ESP_BLE_MESH_MODEL_OP_NODE_RESET ESP_BLE_MESH_MODEL_OP_FRIEND_SET ESP_BLE_MESH_MODEL_OP_HEARTBEAT_PUB_SET ESP_BLE_MESH_MODEL_OP_HEARTBEAT_SUB_SET the set_state parameter in the esp_ble_mesh_config_client_set_state function should not be set to NULL.

  Public Members

  esp_ble_mesh_cfg_beacon_set_t beacon_set

    For ESP_BLE_MESH_MODEL_OP_BEACON_SET

  esp_ble_mesh_cfg_default_ttl_set_t default_ttl_set

    For ESP_BLE_MESH_MODEL_OP_DEFAULT_TTL_SET

  esp_ble_mesh_cfg_friend_set_t friend_set

    For ESP_BLE_MESH_MODEL_OP_FRIEND_SET

  esp_ble_mesh_cfg_gatt_proxy_set_t gatt_proxy_set

    For ESP_BLE_MESH_MODEL_OP_GATT_PROXY_SET

  esp_ble_mesh_cfg_relay_set_t relay_set

    For ESP_BLE_MESH_MODEL_OP_RELAY_SET

  esp_ble_mesh_cfg_net_key_add_t net_key_add

    For ESP_BLE_MESH_MODEL_OP_NET_KEY_ADD

  esp_ble_mesh_cfg_app_key_add_t app_key_add

    For ESP_BLE_MESH_MODEL_OP_APP_KEY_ADD

  esp_ble_mesh_cfg_model_app_bind_t model_app_bind

    For ESP_BLE_MESH_MODEL_OP_MODEL_APP_BIND

  esp_ble_mesh_cfg_model_pub_set_t model_pub_set

    For ESP_BLE_MESH_MODEL_OP_MODEL_PUB_SET

  esp_ble_mesh_cfg_model_sub_add_t model_sub_add

    For ESP_BLE_MESH_MODEL_OP_MODEL_SUB_ADD

  esp_ble_mesh_cfg_model_sub_delete_t model_sub_delete

    For ESP_BLE_MESH_MODEL_OP_MODEL_SUB_DELETE

  esp_ble_mesh_cfg_model_sub_overwrite_t model_sub_overwrite

    For ESP_BLE_MESH_MODEL_OP_MODEL_SUB_OVERWRITE

  esp_ble_mesh_cfg_model_sub_va_add_t model_sub_va_add

    For ESP_BLE_MESH_MODEL_OP_MODEL_SUB_VIRTUAL_ADDR_ADD

  esp_ble_mesh_cfg_model_sub_va_delete_t model_sub_va_delete

    For ESP_BLE_MESH_MODEL_OP_MODEL_SUB_VIRTUAL_ADDR_DELETE

  esp_ble_mesh_cfg_model_sub_va_overwrite_t model_sub_va_overwrite

    For ESP_BLE_MESH_MODEL_OP_MODEL_SUB_VIRTUAL_ADDR_OVERWRITE

  esp_ble_mesh_cfg_heartbeat_pub_set_t heartbeat_pub_set

    For ESP_BLE_MESH_MODEL_OP_HEARTBEAT_PUB_SET

  esp_ble_mesh_cfg_heartbeat_sub_set_t heartbeat_sub_set

    For ESP_BLE_MESH_MODEL_OP_HEARTBEAT_SUB_SET

  esp_ble_mesh_cfg_model_pub_va_set_t model_pub_va_set

    For ESP_BLE_MESH_MODEL_OP_MODEL_PUB_VIRTUAL_ADDR_SET

  esp_ble_mesh_cfg_model_sub_delete_all_t model_sub_delete_all

    For ESP_BLE_MESH_MODEL_OP_MODEL_SUB_DELETE_ALL

  esp_ble_mesh_cfg_net_key_update_t net_key_update

    For ESP_BLE_MESH_MODEL_OP_NET_KEY_UPDATE

  esp_ble_mesh_cfg_net_key_delete_t net_key_delete

    For ESP_BLE_MESH_MODEL_OP_NET_KEY_DELETE

  esp_ble_mesh_cfg_app_key_update_t app_key_update

    For ESP_BLE_MESH_MODEL_OP_APP_KEY_UPDATE

  esp_ble_mesh_cfg_app_key_delete_t app_key_delete

    For ESP_BLE_MESH_MODEL_OP_APP_KEY_DELETE

  esp_ble_mesh_cfg_node_identity_set_t node_identity_set

    For ESP_BLE_MESH_MODEL_OP_NODE_IDENTITY_SET

  esp_ble_mesh_cfg_model_app_unbind_t model_app_unbind

    For ESP_BLE_MESH_MODEL_OP_MODEL_APP_UNBIND

  esp_ble_mesh_cfg_kr_phase_set_t kr_phase_set

    For ESP_BLE_MESH_MODEL_OP_KEY_REFRESH_PHASE_SET

  esp_ble_mesh_cfg_net_transmit_set_t net_transmit_set

    For ESP_BLE_MESH_MODEL_OP_NETWORK_TRANSMIT_SET

union esp_ble_mesh_cfg_client_common_cb_param_t
  #include <esp_ble_mesh_config_model_api.h>

  Configuration Client Model received message union.

  Public Members

  esp_ble_mesh_cfg_beacon_status_cb_t beacon_status

    The beacon status value

  esp_ble_mesh_cfg_comp_data_status_cb_t comp_data_status

    The composition data status value

  esp_ble_mesh_cfg_default_ttl_status_cb_t default_ttl_status

    The default_ttl status value

  esp_ble_mesh_cfg_gatt_proxy_status_cb_t gatt_proxy_status

    The gatt_proxy status value

  esp_ble_mesh_cfg_relay_status_cb_t relay_status

    The relay status value

  esp_ble_mesh_cfg_model_pub_status_cb_t model_pub_status

    The model publication status value

  esp_ble_mesh_cfg_model_sub_status_cb_t model_sub_status

    The model subscription status value

  esp_ble_mesh_cfg_net_key_status_cb_t netkey_status

    The netkey status value

  esp_ble_mesh_cfg_app_key_status_cb_t appkey_status

    The appkey status value

  esp_ble_mesh_cfg_mod_app_status_cb_t model_app_status

    The model app status value

  esp_ble_mesh_cfg_friend_status_cb_t friend_status

    The friend status value

  esp_ble_mesh_cfg_hb_pub_status_cb_t heartbeat_pub_status

    The heartbeat publication status value

  esp_ble_mesh_cfg_hb_sub_status_cb_t heartbeat_sub_status

    The heartbeat subscription status value

  esp_ble_mesh_cfg_net_trans_status_cb_t net_transmit_status

    The network transmit status value

  esp_ble_mesh_cfg_model_sub_list_cb_t model_sub_list

    The model subscription list value

  esp_ble_mesh_cfg_net_key_list_cb_t netkey_list

    The network key index list value

  esp_ble_mesh_cfg_app_key_list_cb_t appkey_list

    The application key index list value

  esp_ble_mesh_cfg_node_id_status_cb_t node_identity_status

    The node identity status value

  esp_ble_mesh_cfg_model_app_list_cb_t model_app_list

    The model application key index list value

  esp_ble_mesh_cfg_kr_phase_status_cb_t kr_phase_status

    The key refresh phase status value

  esp_ble_mesh_cfg_lpn_pollto_status_cb_t lpn_timeout_status

    The low power node poll timeout status value

union esp_ble_mesh_cfg_server_state_change_t
  #include <esp_ble_mesh_config_model_api.h>

  Configuration Server model state change value union.

  Public Members

  esp_ble_mesh_state_change_cfg_mod_pub_set_t mod_pub_set

    The recv_op in ctx can be used to decide which state is changed. Config Model Publication Set

  esp_ble_mesh_state_change_cfg_mod_pub_va_set_t mod_pub_va_set

    Config Model Publication Virtual Address Set

  esp_ble_mesh_state_change_cfg_model_sub_add_t mod_sub_add

    Config Model Subscription Add

  esp_ble_mesh_state_change_cfg_model_sub_delete_t mod_sub_delete

    Config Model Subscription Delete

  esp_ble_mesh_state_change_cfg_netkey_add_t netkey_add

    Config NetKey Add

  esp_ble_mesh_state_change_cfg_netkey_update_t netkey_update

    Config NetKey Update

  esp_ble_mesh_state_change_cfg_netkey_delete_t netkey_delete

    Config NetKey Delete

  esp_ble_mesh_state_change_cfg_appkey_add_t appkey_add

    Config AppKey Add

  esp_ble_mesh_state_change_cfg_appkey_update_t appkey_update

    Config AppKey Update

  esp_ble_mesh_state_change_cfg_appkey_delete_t appkey_delete

    Config AppKey Delete

  esp_ble_mesh_state_change_cfg_model_app_bind_t mod_app_bind

    Config Model App Bind

  esp_ble_mesh_state_change_cfg_model_app_unbind_t mod_app_unbind

    Config Model App Unbind

  esp_ble_mesh_state_change_cfg_kr_phase_set_t kr_phase_set

    Config Key Refresh Phase Set

union esp_ble_mesh_cfg_server_cb_value_t
  #include <esp_ble_mesh_config_model_api.h>

  Configuration Server model callback value union.

  Public Members

  esp_ble_mesh_cfg_server_state_change_t state_change

    ESP_BLE_MESH_CFG_SERVER_STATE_CHANGE_EVT

### Structures

struct esp_ble_mesh_cfg_srv_t

  Configuration Server Model context

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to Configuration Server Model

  uint8_t net_transmit

    Network Transmit state

  uint8_t relay

    Relay Mode state

  uint8_t relay_retransmit

    Relay Retransmit state

  uint8_t beacon

    Secure Network Beacon state

  uint8_t gatt_proxy

    GATT Proxy state

  uint8_t friend_state

    Friend state

  uint8_t default_ttl

    Default TTL

  struct k_delayed_work timer

    Heartbeat Publication timer

  uint16_t dst

    Destination address for Heartbeat messages

  uint16_t count

    Number of Heartbeat messages to be sent

    Number of Heartbeat messages received

  uint8_t period

    Period for sending Heartbeat messages

  uint8_t ttl

    TTL to be used when sending Heartbeat messages

  uint16_t feature

    Bit field indicating features that trigger Heartbeat messages when changed

  uint16_t net_idx

    NetKey Index used by Heartbeat Publication

  struct esp_ble_mesh_cfg_srv_t heartbeat_pub

    Heartbeat Publication

  int64_t expiry

    Timestamp when Heartbeat subscription period is expired

  uint16_t src

    Source address for Heartbeat messages

  uint8_t min_hops

    Minimum hops when receiving Heartbeat messages

  uint8_t max_hops

    Maximum hops when receiving Heartbeat messages

  esp_ble_mesh_cb_t heartbeat_recv_cb

    Optional heartbeat subscription tracking function

  struct esp_ble_mesh_cfg_srv_t heartbeat_sub

    Heartbeat Subscription

struct esp_ble_mesh_cfg_composition_data_get_t

  Parameters of Config Composition Data Get.

  Public Members

  uint8_t page

    Page number of the Composition Data.

struct esp_ble_mesh_cfg_model_pub_get_t

  Parameters of Config Model Publication Get.

  Public Members

  uint16_t element_addr

    The element address

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_sig_model_sub_get_t

  Parameters of Config SIG Model Subscription Get.

  Public Members

  uint16_t element_addr

    The element address

  uint16_t model_id

    The model id

struct esp_ble_mesh_cfg_vnd_model_sub_get_t

  Parameters of Config Vendor Model Subscription Get.

  Public Members

  uint16_t element_addr

    The element address

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_app_key_get_t

  Parameters of Config AppKey Get.

  Public Members

  uint16_t net_idx

    The network key index

struct esp_ble_mesh_cfg_node_identity_get_t

  Parameters of Config Node Identity Get.

  Public Members

  uint16_t net_idx

    The network key index

struct esp_ble_mesh_cfg_sig_model_app_get_t

  Parameters of Config SIG Model App Get.

  Public Members

  uint16_t element_addr

    The element address

  uint16_t model_id

    The model id

struct esp_ble_mesh_cfg_vnd_model_app_get_t

  Parameters of Config Vendor Model App Get.

  Public Members

  uint16_t element_addr

    The element address

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_kr_phase_get_t

  Parameters of Config Key Refresh Phase Get.

  Public Members

  uint16_t net_idx

    The network key index

struct esp_ble_mesh_cfg_lpn_polltimeout_get_t

  Parameters of Config Low Power Node PollTimeout Get.

  Public Members

  uint16_t lpn_addr

    The unicast address of the Low Power node

struct esp_ble_mesh_cfg_beacon_set_t

  Parameters of Config Beacon Set.

  Public Members

  uint8_t beacon

    New Secure Network Beacon state

struct esp_ble_mesh_cfg_default_ttl_set_t

  Parameters of Config Default TTL Set.

  Public Members

  uint8_t ttl

    The default TTL state value

struct esp_ble_mesh_cfg_friend_set_t

  Parameters of Config Friend Set.

  Public Members

  uint8_t friend_state

    The friend state value

struct esp_ble_mesh_cfg_gatt_proxy_set_t

  Parameters of Config GATT Proxy Set.

  Public Members

  uint8_t gatt_proxy

    The GATT Proxy state value

struct esp_ble_mesh_cfg_relay_set_t

  Parameters of Config Relay Set.

  Public Members

  uint8_t relay

    The relay value

  uint8_t relay_retransmit

    The relay retransmit value

struct esp_ble_mesh_cfg_net_key_add_t

  Parameters of Config NetKey Add.

  Public Members

  uint16_t net_idx

    The network key index

  uint8_t net_key[16]

    The network key value

struct esp_ble_mesh_cfg_app_key_add_t

  Parameters of Config AppKey Add.

  Public Members

  uint16_t net_idx

    The network key index

  uint16_t app_idx

    The app key index

  uint8_t app_key[16]

    The app key value

struct esp_ble_mesh_cfg_model_app_bind_t

  Parameters of Config Model App Bind.

  Public Members

  uint16_t element_addr

    The element address

  uint16_t model_app_idx

    Index of the app key to bind with the model

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_model_pub_set_t

  Parameters of Config Model Publication Set.

  Public Members

  uint16_t element_addr

    The element address

  uint16_t publish_addr

    Value of the publish address

  uint16_t publish_app_idx

    Index of the application key

  bool cred_flag

    Value of the Friendship Credential Flag

  uint8_t publish_ttl

    Default TTL value for the publishing messages

  uint8_t publish_period

    Period for periodic status publishing

  uint8_t publish_retransmit

    Number of retransmissions and number of 50-millisecond steps between retransmissions

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_model_sub_add_t

  Parameters of Config Model Subscription Add.

  Public Members

  uint16_t element_addr

    The element address

  uint16_t sub_addr

    The address to be added to the Subscription List

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_model_sub_delete_t

  Parameters of Config Model Subscription Delete.

  Public Members

  uint16_t element_addr

    The element address

  uint16_t sub_addr

    The address to be removed from the Subscription List

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_model_sub_overwrite_t

  Parameters of Config Model Subscription Overwrite.

  Public Members

  uint16_t element_addr

    The element address

  uint16_t sub_addr

    The address to be added to the Subscription List

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_model_sub_va_add_t

  Parameters of Config Model Subscription Virtual Address Add.

  Public Members

  uint16_t element_addr

    The element address

  uint8_t label_uuid[16]

    The Label UUID of the virtual address to be added to the Subscription List

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_model_sub_va_delete_t

  Parameters of Config Model Subscription Virtual Address Delete.

  Public Members

  uint16_t element_addr

    The element address

  uint8_t label_uuid[16]

    The Label UUID of the virtual address to be removed from the Subscription List

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_model_sub_va_overwrite_t

  Parameters of Config Model Subscription Virtual Address Overwrite.

  Public Members

  uint16_t element_addr

    The element address

  uint8_t label_uuid[16]

    The Label UUID of the virtual address to be added to the Subscription List

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_model_pub_va_set_t

  Parameters of Config Model Publication Virtual Address Set.

  Public Members

  uint16_t element_addr

    The element address

  uint8_t label_uuid[16]

    Value of the Label UUID publish address

  uint16_t publish_app_idx

    Index of the application key

  bool cred_flag

    Value of the Friendship Credential Flag

  uint8_t publish_ttl

    Default TTL value for the publishing messages

  uint8_t publish_period

    Period for periodic status publishing

  uint8_t publish_retransmit

    Number of retransmissions and number of 50-millisecond steps between retransmissions

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_model_sub_delete_all_t

  Parameters of Config Model Subscription Delete All.

  Public Members

  uint16_t element_addr

    The element address

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_net_key_update_t

  Parameters of Config NetKey Update.

  Public Members

  uint16_t net_idx

    The network key index

  uint8_t net_key[16]

    The network key value

struct esp_ble_mesh_cfg_net_key_delete_t

  Parameters of Config NetKey Delete.

  Public Members

  uint16_t net_idx

    The network key index

struct esp_ble_mesh_cfg_app_key_update_t

  Parameters of Config AppKey Update.

  Public Members

  uint16_t net_idx

    The network key index

  uint16_t app_idx

    The app key index

  uint8_t app_key[16]

    The app key value

struct esp_ble_mesh_cfg_app_key_delete_t

  Parameters of Config AppKey Delete.

  Public Members

  uint16_t net_idx

    The network key index

  uint16_t app_idx

    The app key index

struct esp_ble_mesh_cfg_node_identity_set_t

  Parameters of Config Node Identity Set.

  Public Members

  uint16_t net_idx

    The network key index

  uint8_t identity

    New Node Identity state

struct esp_ble_mesh_cfg_model_app_unbind_t

  Parameters of Config Model App Unbind.

  Public Members

  uint16_t element_addr

    The element address

  uint16_t model_app_idx

    Index of the app key to bind with the model

  uint16_t model_id

    The model id

  uint16_t company_id

    The company id, if not a vendor model, shall set to 0xFFFF

struct esp_ble_mesh_cfg_kr_phase_set_t

  Parameters of Config Key Refresh Phase Set.

  Public Members

  uint16_t net_idx

    The network key index

  uint8_t transition

    New Key Refresh Phase Transition

struct esp_ble_mesh_cfg_net_transmit_set_t

  Parameters of Config Network Transmit Set.

  Public Members

  uint8_t net_transmit

    Network Transmit State

struct esp_ble_mesh_cfg_heartbeat_pub_set_t

  Parameters of Config Model Heartbeat Publication Set.

  Public Members

  uint16_t dst

    Destination address for Heartbeat messages

  uint8_t count

    Number of Heartbeat messages to be sent

  uint8_t period

    Period for sending Heartbeat messages

  uint8_t ttl

    TTL to be used when sending Heartbeat messages

  uint16_t feature

    Bit field indicating features that trigger Heartbeat messages when changed

  uint16_t net_idx

    NetKey Index

struct esp_ble_mesh_cfg_heartbeat_sub_set_t

  Parameters of Config Model Heartbeat Subscription Set.

  Public Members

  uint16_t src

    Source address for Heartbeat messages

  uint16_t dst

    Destination address for Heartbeat messages

  uint8_t period

    Period for receiving Heartbeat messages

struct esp_ble_mesh_cfg_beacon_status_cb_t

  Parameter of Config Beacon Status

  Public Members

  uint8_t beacon

    Secure Network Beacon state value

struct esp_ble_mesh_cfg_comp_data_status_cb_t

  Parameters of Config Composition Data Status

  Public Members

  uint8_t page

    Page number of the Composition Data

  struct net_buf_simple *composition_data

    Pointer to Composition Data for the identified page

struct esp_ble_mesh_cfg_default_ttl_status_cb_t

  Parameter of Config Default TTL Status

  Public Members

  uint8_t default_ttl

    Default TTL state value

struct esp_ble_mesh_cfg_gatt_proxy_status_cb_t

  Parameter of Config GATT Proxy Status

  Public Members

  uint8_t gatt_proxy

    GATT Proxy state value

struct esp_ble_mesh_cfg_relay_status_cb_t

  Parameters of Config Relay Status

  Public Members

  uint8_t relay

    Relay state value

  uint8_t retransmit

    Relay retransmit value(number of retransmissions and number of 10-millisecond steps between retransmissions)

struct esp_ble_mesh_cfg_model_pub_status_cb_t

  Parameters of Config Model Publication Status

  Public Members

  uint8_t status

    Status Code for the request message

  uint16_t element_addr

    Address of the element

  uint16_t publish_addr

    Value of the publish address

  uint16_t app_idx

    Index of the application key

  bool cred_flag

    Value of the Friendship Credential Flag

  uint8_t ttl

    Default TTL value for the outgoing messages

  uint8_t period

    Period for periodic status publishing

  uint8_t transmit

    Number of retransmissions and number of 50-millisecond steps between retransmissions

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

struct esp_ble_mesh_cfg_model_sub_status_cb_t

  Parameters of Config Model Subscription Status

  Public Members

  uint8_t status

    Status Code for the request message

  uint16_t element_addr

    Address of the element

  uint16_t sub_addr

    Value of the address

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

struct esp_ble_mesh_cfg_net_key_status_cb_t

  Parameters of Config NetKey Status

  Public Members

  uint8_t status

    Status Code for the request message

  uint16_t net_idx

    Index of the NetKey

struct esp_ble_mesh_cfg_app_key_status_cb_t

  Parameters of Config AppKey Status

  Public Members

  uint8_t status

    Status Code for the request message

  uint16_t net_idx

    Index of the NetKey

  uint16_t app_idx

    Index of the application key

struct esp_ble_mesh_cfg_mod_app_status_cb_t

  Parameters of Config Model App Status

  Public Members

  uint8_t status

    Status Code for the request message

  uint16_t element_addr

    Address of the element

  uint16_t app_idx

    Index of the application key

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

struct esp_ble_mesh_cfg_friend_status_cb_t

  Parameter of Config Friend Status

  Public Members

  uint8_t friend_state

    Friend state value

struct esp_ble_mesh_cfg_hb_pub_status_cb_t

  Parameters of Config Heartbeat Publication Status

  Public Members

  uint8_t status

    Status Code for the request message

  uint16_t dst

    Destination address for Heartbeat messages

  uint8_t count

    Number of Heartbeat messages remaining to be sent

  uint8_t period

    Period for sending Heartbeat messages

  uint8_t ttl

    TTL to be used when sending Heartbeat messages

  uint16_t features

    Features that trigger Heartbeat messages when changed

  uint16_t net_idx

    Index of the NetKey

struct esp_ble_mesh_cfg_hb_sub_status_cb_t

  Parameters of Config Heartbeat Subscription Status

  Public Members

  uint8_t status

    Status Code for the request message

  uint16_t src

    Source address for Heartbeat messages

  uint16_t dst

    Destination address for Heartbeat messages

  uint8_t period

    Remaining Period for processing Heartbeat messages

  uint8_t count

    Number of Heartbeat messages received

  uint8_t min_hops

    Minimum hops when receiving Heartbeat messages

  uint8_t max_hops

    Maximum hops when receiving Heartbeat messages

struct esp_ble_mesh_cfg_net_trans_status_cb_t

  Parameters of Config Network Transmit Status

  Public Members

  uint8_t net_trans_count

    Number of transmissions for each Network PDU originating from the node

  uint8_t net_trans_step

    Maximum hops when receiving Heartbeat messages

struct esp_ble_mesh_cfg_model_sub_list_cb_t

  Parameters of Config SIG/Vendor Subscription List

  Public Members

  uint8_t status

    Status Code for the request message

  uint16_t element_addr

    Address of the element

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

  struct net_buf_simple *sub_addr

    A block of all addresses from the Subscription List

struct esp_ble_mesh_cfg_net_key_list_cb_t

  Parameter of Config NetKey List

  Public Members

  struct net_buf_simple *net_idx

    A list of NetKey Indexes known to the node

struct esp_ble_mesh_cfg_app_key_list_cb_t

  Parameters of Config AppKey List

  Public Members

  uint8_t status

    Status Code for the request message

  uint16_t net_idx

    NetKey Index of the NetKey that the AppKeys are bound to

  struct net_buf_simple *app_idx

    A list of AppKey indexes that are bound to the NetKey identified by NetKeyIndex

struct esp_ble_mesh_cfg_node_id_status_cb_t

  Parameters of Config Node Identity Status

  Public Members

  uint8_t status

    Status Code for the request message

  uint16_t net_idx

    Index of the NetKey

  uint8_t identity

    Node Identity state

struct esp_ble_mesh_cfg_model_app_list_cb_t

  Parameters of Config SIG/Vendor Model App List

  Public Members

  uint8_t status

    Status Code for the request message

  uint16_t element_addr

    Address of the element

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

  struct net_buf_simple *app_idx

    All AppKey indexes bound to the Model

struct esp_ble_mesh_cfg_kr_phase_status_cb_t

  Parameters of Config Key Refresh Phase Status

  Public Members

  uint8_t status

    Status Code for the request message

  uint16_t net_idx

    Index of the NetKey

  uint8_t phase

    Key Refresh Phase state

struct esp_ble_mesh_cfg_lpn_pollto_status_cb_t

  Parameters of Config Low Power Node PollTimeout Status

  Public Members

  uint16_t lpn_addr

    The unicast address of the Low Power node

  int32_t poll_timeout

    The current value of the PollTimeout timer of the Low Power node

struct esp_ble_mesh_cfg_client_cb_param_t

  Configuration Client Model callback parameters

  Public Members

  int error_code

    Appropriate error code

  esp_ble_mesh_client_common_param_t *params

    The client common parameters

  esp_ble_mesh_cfg_client_common_cb_param_t status_cb

    The config status message callback values

struct esp_ble_mesh_state_change_cfg_mod_pub_set_t

  Configuration Server model related context.

  Parameters of Config Model Publication Set

  Public Members

  uint16_t element_addr

    Element Address

  uint16_t pub_addr

    Publish Address

  uint16_t app_idx

    AppKey Index

  bool cred_flag

    Friendship Credential Flag

  uint8_t pub_ttl

    Publish TTL

  uint8_t pub_period

    Publish Period

  uint8_t pub_retransmit

    Publish Retransmit

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

struct esp_ble_mesh_state_change_cfg_mod_pub_va_set_t

  Parameters of Config Model Publication Virtual Address Set

  Public Members

  uint16_t element_addr

    Element Address

  uint8_t label_uuid[16]

    Label UUID

  uint16_t app_idx

    AppKey Index

  bool cred_flag

    Friendship Credential Flag

  uint8_t pub_ttl

    Publish TTL

  uint8_t pub_period

    Publish Period

  uint8_t pub_retransmit

    Publish Retransmit

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

struct esp_ble_mesh_state_change_cfg_model_sub_add_t

  Parameters of Config Model Subscription Add

  Public Members

  uint16_t element_addr

    Element Address

  uint16_t sub_addr

    Subscription Address

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

struct esp_ble_mesh_state_change_cfg_model_sub_delete_t

  Parameters of Config Model Subscription Delete

  Public Members

  uint16_t element_addr

    Element Address

  uint16_t sub_addr

    Subscription Address

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

struct esp_ble_mesh_state_change_cfg_netkey_add_t

  Parameters of Config NetKey Add

  Public Members

  uint16_t net_idx

    NetKey Index

  uint8_t net_key[16]

    NetKey

struct esp_ble_mesh_state_change_cfg_netkey_update_t

  Parameters of Config NetKey Update

  Public Members

  uint16_t net_idx

    NetKey Index

  uint8_t net_key[16]

    NetKey

struct esp_ble_mesh_state_change_cfg_netkey_delete_t

  Parameter of Config NetKey Delete

  Public Members

  uint16_t net_idx

    NetKey Index

struct esp_ble_mesh_state_change_cfg_appkey_add_t

  Parameters of Config AppKey Add

  Public Members

  uint16_t net_idx

    NetKey Index

  uint16_t app_idx

    AppKey Index

  uint8_t app_key[16]

    AppKey

struct esp_ble_mesh_state_change_cfg_appkey_update_t

  Parameters of Config AppKey Update

  Public Members

  uint16_t net_idx

    NetKey Index

  uint16_t app_idx

    AppKey Index

  uint8_t app_key[16]

    AppKey

struct esp_ble_mesh_state_change_cfg_appkey_delete_t

  Parameters of Config AppKey Delete

  Public Members

  uint16_t net_idx

    NetKey Index

  uint16_t app_idx

    AppKey Index

struct esp_ble_mesh_state_change_cfg_model_app_bind_t

  Parameters of Config Model App Bind

  Public Members

  uint16_t element_addr

    Element Address

  uint16_t app_idx

    AppKey Index

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

struct esp_ble_mesh_state_change_cfg_model_app_unbind_t

  Parameters of Config Model App Unbind

  Public Members

  uint16_t element_addr

    Element Address

  uint16_t app_idx

    AppKey Index

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

struct esp_ble_mesh_state_change_cfg_kr_phase_set_t

  Parameters of Config Key Refresh Phase Set

  Public Members

  uint16_t net_idx

    NetKey Index

  uint8_t kr_phase

    New Key Refresh Phase Transition

struct esp_ble_mesh_cfg_server_cb_param_t

  Configuration Server model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the server model structure

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received message

  esp_ble_mesh_cfg_server_cb_value_t value

    Value of the received configuration messages

### Macros

ESP_BLE_MESH_MODEL_CFG_SRV(srv_data)

  Define a new Config Server Model.

  备注

  The Config Server Model can only be included by a Primary Element.

  参数:

    - srv_data -- Pointer to a unique Config Server Model user_data.

  返回:

    New Config Server Model instance.

ESP_BLE_MESH_MODEL_CFG_CLI(cli_data)

  Define a new Config Client Model.

  备注

  The Config Client Model can only be included by a Primary Element.

  参数:

    - cli_data -- Pointer to a unique struct esp_ble_mesh_client_t.

  返回:

    New Config Client Model instance.

### Type Definitions

typedef void (*esp_ble_mesh_cfg_client_cb_t)(esp_ble_mesh_cfg_client_cb_event_t event, esp_ble_mesh_cfg_client_cb_param_t *param)

  Bluetooth Mesh Config Client and Server Model functions.

  Configuration Client Model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_cfg_server_cb_t)(esp_ble_mesh_cfg_server_cb_event_t event, esp_ble_mesh_cfg_server_cb_param_t *param)

  Configuration Server Model callback function type.

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_cfg_client_cb_event_t

  This enum value is the event of Configuration Client Model

  Values:

  enumerator ESP_BLE_MESH_CFG_CLIENT_GET_STATE_EVT
  enumerator ESP_BLE_MESH_CFG_CLIENT_SET_STATE_EVT
  enumerator ESP_BLE_MESH_CFG_CLIENT_PUBLISH_EVT
  enumerator ESP_BLE_MESH_CFG_CLIENT_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_CFG_CLIENT_EVT_MAX

enum esp_ble_mesh_cfg_server_cb_event_t

  This enum value is the event of Configuration Server model

  Values:

  enumerator ESP_BLE_MESH_CFG_SERVER_STATE_CHANGE_EVT
  enumerator ESP_BLE_MESH_CFG_SERVER_EVT_MAX

### Health Client/Server Models

### Header File

- components/bt/esp_ble_mesh/api/models/include/esp_ble_mesh_health_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_health_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_health_client_callback(esp_ble_mesh_health_client_cb_t callback)

  Register BLE Mesh Health Model callback, the callback will report Health Client & Server Model events.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_health_server_callback(esp_ble_mesh_health_server_cb_t callback)

  Register BLE Mesh Health Server Model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_health_client_get_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_health_client_get_state_t *get_state)

  This function is called to get the Health Server states using the Health Client Model get messages.

  备注

  If you want to find the opcodes and corresponding meanings accepted by this API, please refer to esp_ble_mesh_opcode_health_client_get_t in esp_ble_mesh_defs.h

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - get_state -- [in] Pointer to a union, each kind of opcode corresponds to one structure inside. Shall not be set to NULL.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_health_client_set_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_health_client_set_state_t *set_state)

  This function is called to set the Health Server states using the Health Client Model set messages.

  备注

  If you want to find the opcodes and corresponding meanings accepted by this API, please refer to esp_ble_mesh_opcode_health_client_set_t in esp_ble_mesh_defs.h

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - set_state -- [in] Pointer to a union, each kind of opcode corresponds to one structure inside. Shall not be set to NULL.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_health_server_fault_update(esp_ble_mesh_elem_t *element)

  This function is called by the Health Server Model to update the context of its Health Current status.

  参数:

    element -- [in] The element to which the Health Server Model belongs.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_health_client_get_state_t
  #include <esp_ble_mesh_health_model_api.h>

  For ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_GET ESP_BLE_MESH_MODEL_OP_ATTENTION_GET ESP_BLE_MESH_MODEL_OP_HEALTH_PERIOD_GET the get_state parameter in the esp_ble_mesh_health_client_get_state function should not be set to NULL.

  Public Members

  esp_ble_mesh_health_fault_get_t fault_get

    For ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_GET.

union esp_ble_mesh_health_client_set_state_t
  #include <esp_ble_mesh_health_model_api.h>

  For ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_CLEAR ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_CLEAR_UNACK ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_TEST ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_TEST_UNACK ESP_BLE_MESH_MODEL_OP_HEALTH_PERIOD_SET ESP_BLE_MESH_MODEL_OP_HEALTH_PERIOD_SET_UNACK ESP_BLE_MESH_MODEL_OP_ATTENTION_SET ESP_BLE_MESH_MODEL_OP_ATTENTION_SET_UNACK the set_state parameter in the esp_ble_mesh_health_client_set_state function should not be set to NULL.

  Public Members

  esp_ble_mesh_health_attention_set_t attention_set

    For ESP_BLE_MESH_MODEL_OP_ATTENTION_SET or ESP_BLE_MESH_MODEL_OP_ATTENTION_SET_UNACK.

  esp_ble_mesh_health_period_set_t period_set

    For ESP_BLE_MESH_MODEL_OP_HEALTH_PERIOD_SET or ESP_BLE_MESH_MODEL_OP_HEALTH_PERIOD_SET_UNACK.

  esp_ble_mesh_health_fault_test_t fault_test

    For ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_TEST or ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_TEST_UNACK.

  esp_ble_mesh_health_fault_clear_t fault_clear

    For ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_CLEAR or ESP_BLE_MESH_MODEL_OP_HEALTH_FAULT_CLEAR_UNACK.

union esp_ble_mesh_health_client_common_cb_param_t
  #include <esp_ble_mesh_health_model_api.h>

  Health Client Model received message union.

  Public Members

  esp_ble_mesh_health_current_status_cb_t current_status

    The health current status value

  esp_ble_mesh_health_fault_status_cb_t fault_status

    The health fault status value

  esp_ble_mesh_health_period_status_cb_t period_status

    The health period status value

  esp_ble_mesh_health_attention_status_cb_t attention_status

    The health attention status value

union esp_ble_mesh_health_server_cb_param_t
  #include <esp_ble_mesh_health_model_api.h>

  Health Server Model callback parameters union.

  Public Members

  esp_ble_mesh_health_fault_update_comp_cb_t fault_update_comp

    ESP_BLE_MESH_HEALTH_SERVER_FAULT_UPDATE_COMP_EVT

  esp_ble_mesh_health_fault_clear_cb_t fault_clear

    ESP_BLE_MESH_HEALTH_SERVER_FAULT_CLEAR_EVT

  esp_ble_mesh_health_fault_test_cb_t fault_test

    ESP_BLE_MESH_HEALTH_SERVER_FAULT_TEST_EVT

  esp_ble_mesh_health_attention_on_cb_t attention_on

    ESP_BLE_MESH_HEALTH_SERVER_ATTENTION_ON_EVT

  esp_ble_mesh_health_attention_off_cb_t attention_off

    ESP_BLE_MESH_HEALTH_SERVER_ATTENTION_OFF_EVT

### Structures

struct esp_ble_mesh_health_srv_cb_t

  ESP BLE Mesh Health Server callback

  Public Members

  esp_ble_mesh_cb_t fault_clear

    Clear health registered faults. Initialized by the stack.

  esp_ble_mesh_cb_t fault_test

    Run a specific health test. Initialized by the stack.

  esp_ble_mesh_cb_t attention_on

    Health attention on callback. Initialized by the stack.

  esp_ble_mesh_cb_t attention_off

    Health attention off callback. Initialized by the stack.

struct esp_ble_mesh_health_test_t

  ESP BLE Mesh Health Server test Context

  Public Members

  uint8_t id_count

    Number of Health self-test ID

  const uint8_t *test_ids

    Array of Health self-test IDs

  uint16_t company_id

    Company ID used to identify the Health Fault state

  uint8_t prev_test_id

    Current test ID of the health fault test

  uint8_t current_faults[ESP_BLE_MESH_HEALTH_FAULT_ARRAY_SIZE]

    Array of current faults

  uint8_t registered_faults[ESP_BLE_MESH_HEALTH_FAULT_ARRAY_SIZE]

    Array of registered faults

struct esp_ble_mesh_health_srv_t

  ESP BLE Mesh Health Server Model Context

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to Health Server Model

  esp_ble_mesh_health_srv_cb_t health_cb

    Health callback struct

  struct k_delayed_work attention_timer

    Attention Timer state

  bool attention_timer_start

    Attention Timer start flag

  esp_ble_mesh_health_test_t health_test

    Health Server fault test

struct esp_ble_mesh_health_fault_get_t

  Parameter of Health Fault Get

  Public Members

  uint16_t company_id

    Bluetooth assigned 16-bit Company ID

struct esp_ble_mesh_health_attention_set_t

  Parameter of Health Attention Set

  Public Members

  uint8_t attention

    Value of the Attention Timer state

struct esp_ble_mesh_health_period_set_t

  Parameter of Health Period Set

  Public Members

  uint8_t fast_period_divisor

    Divider for the Publish Period

struct esp_ble_mesh_health_fault_test_t

  Parameter of Health Fault Test

  Public Members

  uint16_t company_id

    Bluetooth assigned 16-bit Company ID

  uint8_t test_id

    ID of a specific test to be performed

struct esp_ble_mesh_health_fault_clear_t

  Parameter of Health Fault Clear

  Public Members

  uint16_t company_id

    Bluetooth assigned 16-bit Company ID

struct esp_ble_mesh_health_current_status_cb_t

  Parameters of Health Current Status

  Public Members

  uint8_t test_id

    ID of a most recently performed test

  uint16_t company_id

    Bluetooth assigned 16-bit Company ID

  struct net_buf_simple *fault_array

    FaultArray field contains a sequence of 1-octet fault values

struct esp_ble_mesh_health_fault_status_cb_t

  Parameters of Health Fault Status

  Public Members

  uint8_t test_id

    ID of a most recently performed test

  uint16_t company_id

    Bluetooth assigned 16-bit Company ID

  struct net_buf_simple *fault_array

    FaultArray field contains a sequence of 1-octet fault values

struct esp_ble_mesh_health_period_status_cb_t

  Parameter of Health Period Status

  Public Members

  uint8_t fast_period_divisor

    Divider for the Publish Period

struct esp_ble_mesh_health_attention_status_cb_t

  Parameter of Health Attention Status

  Public Members

  uint8_t attention

    Value of the Attention Timer state

struct esp_ble_mesh_health_client_cb_param_t

  Health Client Model callback parameters

  Public Members

  int error_code

    Appropriate error code

  esp_ble_mesh_client_common_param_t *params

    The client common parameters.

  esp_ble_mesh_health_client_common_cb_param_t status_cb

    The health message status callback values

struct esp_ble_mesh_health_fault_update_comp_cb_t

  Parameter of publishing Health Current Status completion event

  Public Members

  int error_code

    The result of publishing Health Current Status

  esp_ble_mesh_elem_t *element

    Pointer to the element which contains the Health Server Model

struct esp_ble_mesh_health_fault_clear_cb_t

  Parameters of Health Fault Clear event

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Health Server Model

  uint16_t company_id

    Bluetooth assigned 16-bit Company ID

struct esp_ble_mesh_health_fault_test_cb_t

  Parameters of Health Fault Test event

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Health Server Model

  uint8_t test_id

    ID of a specific test to be performed

  uint16_t company_id

    Bluetooth assigned 16-bit Company ID

struct esp_ble_mesh_health_attention_on_cb_t

  Parameter of Health Attention On event

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Health Server Model

  uint8_t time

    Duration of attention timer on (in seconds)

struct esp_ble_mesh_health_attention_off_cb_t

  Parameter of Health Attention Off event

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Health Server Model

### Macros

ESP_BLE_MESH_MODEL_HEALTH_SRV(srv, pub)

  Define a new Health Server Model.

  备注

  The Health Server Model can only be included by a Primary Element.

  参数:

    - srv -- Pointer to the unique struct esp_ble_mesh_health_srv_t.

    - pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

  返回:

    New Health Server Model instance.

ESP_BLE_MESH_MODEL_HEALTH_CLI(cli_data)

  Define a new Health Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Health Client Model.

  参数:

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Health Client Model instance.

ESP_BLE_MESH_HEALTH_PUB_DEFINE(_name, _max, _role)

  A helper to define a health publication context

  参数:

    - _name -- Name given to the publication context variable.

    - _max -- Maximum number of faults the element can have.

    - _role -- Role of the device which contains the model.

ESP_BLE_MESH_HEALTH_STANDARD_TEST

  SIG identifier of Health Fault Test. 0x01 ~ 0xFF: Vendor Specific Test.

ESP_BLE_MESH_NO_FAULT

  Fault values of Health Fault Test. 0x33 ~ 0x7F: Reserved for Future Use. 0x80 ~ 0xFF: Vendor Specific Warning/Error.

ESP_BLE_MESH_BATTERY_LOW_WARNING

ESP_BLE_MESH_BATTERY_LOW_ERROR

ESP_BLE_MESH_SUPPLY_VOLTAGE_TOO_LOW_WARNING

ESP_BLE_MESH_SUPPLY_VOLTAGE_TOO_LOW_ERROR

ESP_BLE_MESH_SUPPLY_VOLTAGE_TOO_HIGH_WARNING

ESP_BLE_MESH_SUPPLY_VOLTAGE_TOO_HIGH_ERROR

ESP_BLE_MESH_POWER_SUPPLY_INTERRUPTED_WARNING

ESP_BLE_MESH_POWER_SUPPLY_INTERRUPTED_ERROR

ESP_BLE_MESH_NO_LOAD_WARNING

ESP_BLE_MESH_NO_LOAD_ERROR

ESP_BLE_MESH_OVERLOAD_WARNING

ESP_BLE_MESH_OVERLOAD_ERROR

ESP_BLE_MESH_OVERHEAT_WARNING

ESP_BLE_MESH_OVERHEAT_ERROR

ESP_BLE_MESH_CONDENSATION_WARNING

ESP_BLE_MESH_CONDENSATION_ERROR

ESP_BLE_MESH_VIBRATION_WARNING

ESP_BLE_MESH_VIBRATION_ERROR

ESP_BLE_MESH_CONFIGURATION_WARNING

ESP_BLE_MESH_CONFIGURATION_ERROR

ESP_BLE_MESH_ELEMENT_NOT_CALIBRATED_WARNING

ESP_BLE_MESH_ELEMENT_NOT_CALIBRATED_ERROR

ESP_BLE_MESH_MEMORY_WARNING

ESP_BLE_MESH_MEMORY_ERROR

ESP_BLE_MESH_SELF_TEST_WARNING

ESP_BLE_MESH_SELF_TEST_ERROR

ESP_BLE_MESH_INPUT_TOO_LOW_WARNING

ESP_BLE_MESH_INPUT_TOO_LOW_ERROR

ESP_BLE_MESH_INPUT_TOO_HIGH_WARNING

ESP_BLE_MESH_INPUT_TOO_HIGH_ERROR

ESP_BLE_MESH_INPUT_NO_CHANGE_WARNING

ESP_BLE_MESH_INPUT_NO_CHANGE_ERROR

ESP_BLE_MESH_ACTUATOR_BLOCKED_WARNING

ESP_BLE_MESH_ACTUATOR_BLOCKED_ERROR

ESP_BLE_MESH_HOUSING_OPENED_WARNING

ESP_BLE_MESH_HOUSING_OPENED_ERROR

ESP_BLE_MESH_TAMPER_WARNING

ESP_BLE_MESH_TAMPER_ERROR

ESP_BLE_MESH_DEVICE_MOVED_WARNING

ESP_BLE_MESH_DEVICE_MOVED_ERROR

ESP_BLE_MESH_DEVICE_DROPPED_WARNING

ESP_BLE_MESH_DEVICE_DROPPED_ERROR

ESP_BLE_MESH_OVERFLOW_WARNING

ESP_BLE_MESH_OVERFLOW_ERROR

ESP_BLE_MESH_EMPTY_WARNING

ESP_BLE_MESH_EMPTY_ERROR

ESP_BLE_MESH_INTERNAL_BUS_WARNING

ESP_BLE_MESH_INTERNAL_BUS_ERROR

ESP_BLE_MESH_MECHANISM_JAMMED_WARNING

ESP_BLE_MESH_MECHANISM_JAMMED_ERROR

ESP_BLE_MESH_HEALTH_FAULT_ARRAY_SIZE

### Type Definitions

typedef void (*esp_ble_mesh_health_client_cb_t)(esp_ble_mesh_health_client_cb_event_t event, esp_ble_mesh_health_client_cb_param_t *param)

  Bluetooth Mesh Health Client and Server Model function.

  Health Client Model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_health_server_cb_t)(esp_ble_mesh_health_server_cb_event_t event, esp_ble_mesh_health_server_cb_param_t *param)

  Health Server Model callback function type.

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_health_client_cb_event_t

  This enum value is the event of Health Client Model

  Values:

  enumerator ESP_BLE_MESH_HEALTH_CLIENT_GET_STATE_EVT
  enumerator ESP_BLE_MESH_HEALTH_CLIENT_SET_STATE_EVT
  enumerator ESP_BLE_MESH_HEALTH_CLIENT_PUBLISH_EVT
  enumerator ESP_BLE_MESH_HEALTH_CLIENT_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_HEALTH_CLIENT_EVT_MAX

enum esp_ble_mesh_health_server_cb_event_t

  This enum value is the event of Health Server Model

  Values:

  enumerator ESP_BLE_MESH_HEALTH_SERVER_FAULT_UPDATE_COMP_EVT
  enumerator ESP_BLE_MESH_HEALTH_SERVER_FAULT_CLEAR_EVT
  enumerator ESP_BLE_MESH_HEALTH_SERVER_FAULT_TEST_EVT
  enumerator ESP_BLE_MESH_HEALTH_SERVER_ATTENTION_ON_EVT
  enumerator ESP_BLE_MESH_HEALTH_SERVER_ATTENTION_OFF_EVT
  enumerator ESP_BLE_MESH_HEALTH_SERVER_EVT_MAX

### Generic Client/Server Models

### Header File

- components/bt/esp_ble_mesh/api/models/include/esp_ble_mesh_generic_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_generic_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_generic_client_callback(esp_ble_mesh_generic_client_cb_t callback)

  Register BLE Mesh Generic Client Model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_generic_client_get_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_generic_client_get_state_t *get_state)

  Get the value of Generic Server Model states using the Generic Client Model get messages.

  备注

  If you want to find the opcodes and corresponding meanings accepted by this API, please refer to esp_ble_mesh_generic_message_opcode_t in esp_ble_mesh_defs.h

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - get_state -- [in] Pointer to generic get message value. Shall not be set to NULL.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_generic_client_set_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_generic_client_set_state_t *set_state)

  Set the value of Generic Server Model states using the Generic Client Model set messages.

  备注

  If you want to find the opcodes and corresponding meanings accepted by this API, please refer to esp_ble_mesh_generic_message_opcode_t in esp_ble_mesh_defs.h

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - set_state -- [in] Pointer to generic set message value. Shall not be set to NULL.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_generic_server_callback(esp_ble_mesh_generic_server_cb_t callback)

  Register BLE Mesh Generic Server Model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_generic_client_get_state_t
  #include <esp_ble_mesh_generic_model_api.h>

  Generic Client Model get message union.

  Public Members

  esp_ble_mesh_gen_user_property_get_t user_property_get

    For ESP_BLE_MESH_MODEL_OP_GEN_USER_PROPERTY_GET

  esp_ble_mesh_gen_admin_property_get_t admin_property_get

    For ESP_BLE_MESH_MODEL_OP_GEN_ADMIN_PROPERTY_GET

  esp_ble_mesh_gen_manufacturer_property_get_t manufacturer_property_get

    For ESP_BLE_MESH_MODEL_OP_GEN_MANUFACTURER_PROPERTY_SET

  esp_ble_mesh_gen_client_properties_get_t client_properties_get

    For ESP_BLE_MESH_MODEL_OP_GEN_CLIENT_PROPERTIES_GET

union esp_ble_mesh_generic_client_set_state_t
  #include <esp_ble_mesh_generic_model_api.h>

  Generic Client Model set message union.

  Public Members

  esp_ble_mesh_gen_onoff_set_t onoff_set

    For ESP_BLE_MESH_MODEL_OP_GEN_ONOFF_SET & ESP_BLE_MESH_MODEL_OP_GEN_ONOFF_SET_UNACK

  esp_ble_mesh_gen_level_set_t level_set

    For ESP_BLE_MESH_MODEL_OP_GEN_LEVEL_SET & ESP_BLE_MESH_MODEL_OP_GEN_LEVEL_SET_UNACK

  esp_ble_mesh_gen_delta_set_t delta_set

    For ESP_BLE_MESH_MODEL_OP_GEN_DELTA_SET & ESP_BLE_MESH_MODEL_OP_GEN_DELTA_SET_UNACK

  esp_ble_mesh_gen_move_set_t move_set

    For ESP_BLE_MESH_MODEL_OP_GEN_MOVE_SET & ESP_BLE_MESH_MODEL_OP_GEN_MOVE_SET_UNACK

  esp_ble_mesh_gen_def_trans_time_set_t def_trans_time_set

    For ESP_BLE_MESH_MODEL_OP_GEN_DEF_TRANS_TIME_SET & ESP_BLE_MESH_MODEL_OP_GEN_DEF_TRANS_TIME_SET_UNACK

  esp_ble_mesh_gen_onpowerup_set_t power_set

    For ESP_BLE_MESH_MODEL_OP_GEN_ONPOWERUP_SET & ESP_BLE_MESH_MODEL_OP_GEN_ONPOWERUP_SET_UNACK

  esp_ble_mesh_gen_power_level_set_t power_level_set

    For ESP_BLE_MESH_MODEL_OP_GEN_POWER_LEVEL_SET & ESP_BLE_MESH_MODEL_OP_GEN_POWER_LEVEL_SET_UNACK

  esp_ble_mesh_gen_power_default_set_t power_default_set

    For ESP_BLE_MESH_MODEL_OP_GEN_POWER_DEFAULT_SET & ESP_BLE_MESH_MODEL_OP_GEN_POWER_DEFAULT_SET_UNACK

  esp_ble_mesh_gen_power_range_set_t power_range_set

    For ESP_BLE_MESH_MODEL_OP_GEN_POWER_RANGE_SET & ESP_BLE_MESH_MODEL_OP_GEN_POWER_RANGE_SET_UNACK

  esp_ble_mesh_gen_loc_global_set_t loc_global_set

    For ESP_BLE_MESH_MODEL_OP_GEN_LOC_GLOBAL_SET & ESP_BLE_MESH_MODEL_OP_GEN_LOC_GLOBAL_SET_UNACK

  esp_ble_mesh_gen_loc_local_set_t loc_local_set

    For ESP_BLE_MESH_MODEL_OP_GEN_LOC_LOCAL_SET & ESP_BLE_MESH_MODEL_OP_GEN_LOC_LOCAL_SET_UNACK

  esp_ble_mesh_gen_user_property_set_t user_property_set

    For ESP_BLE_MESH_MODEL_OP_GEN_USER_PROPERTY_SET & ESP_BLE_MESH_MODEL_OP_GEN_USER_PROPERTY_SET_UNACK

  esp_ble_mesh_gen_admin_property_set_t admin_property_set

    For ESP_BLE_MESH_MODEL_OP_GEN_ADMIN_PROPERTY_SET & ESP_BLE_MESH_MODEL_OP_GEN_ADMIN_PROPERTY_SET_UNACK

  esp_ble_mesh_gen_manufacturer_property_set_t manufacturer_property_set

    For ESP_BLE_MESH_MODEL_OP_GEN_MANUFACTURER_PROPERTY_SET & ESP_BLE_MESH_MODEL_OP_GEN_MANUFACTURER_PROPERTY_SET_UNACK

union esp_ble_mesh_gen_client_status_cb_t
  #include <esp_ble_mesh_generic_model_api.h>

  Generic Client Model received message union.

  Public Members

  esp_ble_mesh_gen_onoff_status_cb_t onoff_status

    For ESP_BLE_MESH_MODEL_OP_GEN_ONOFF_STATUS

  esp_ble_mesh_gen_level_status_cb_t level_status

    For ESP_BLE_MESH_MODEL_OP_GEN_LEVEL_STATUS

  esp_ble_mesh_gen_def_trans_time_status_cb_t def_trans_time_status

    For ESP_BLE_MESH_MODEL_OP_GEN_DEF_TRANS_TIME_STATUS

  esp_ble_mesh_gen_onpowerup_status_cb_t onpowerup_status

    For ESP_BLE_MESH_MODEL_OP_GEN_ONPOWERUP_STATUS

  esp_ble_mesh_gen_power_level_status_cb_t power_level_status

    For ESP_BLE_MESH_MODEL_OP_GEN_POWER_LEVEL_STATUS

  esp_ble_mesh_gen_power_last_status_cb_t power_last_status

    For ESP_BLE_MESH_MODEL_OP_GEN_POWER_LAST_STATUS

  esp_ble_mesh_gen_power_default_status_cb_t power_default_status

    For ESP_BLE_MESH_MODEL_OP_GEN_POWER_DEFAULT_STATUS

  esp_ble_mesh_gen_power_range_status_cb_t power_range_status

    For ESP_BLE_MESH_MODEL_OP_GEN_POWER_RANGE_STATUS

  esp_ble_mesh_gen_battery_status_cb_t battery_status

    For ESP_BLE_MESH_MODEL_OP_GEN_BATTERY_STATUS

  esp_ble_mesh_gen_loc_global_status_cb_t location_global_status

    For ESP_BLE_MESH_MODEL_OP_GEN_LOC_GLOBAL_STATUS

  esp_ble_mesh_gen_loc_local_status_cb_t location_local_status

    ESP_BLE_MESH_MODEL_OP_GEN_LOC_LOCAL_STATUS

  esp_ble_mesh_gen_user_properties_status_cb_t user_properties_status

    ESP_BLE_MESH_MODEL_OP_GEN_USER_PROPERTIES_STATUS

  esp_ble_mesh_gen_user_property_status_cb_t user_property_status

    ESP_BLE_MESH_MODEL_OP_GEN_USER_PROPERTY_STATUS

  esp_ble_mesh_gen_admin_properties_status_cb_t admin_properties_status

    ESP_BLE_MESH_MODEL_OP_GEN_ADMIN_PROPERTIES_STATUS

  esp_ble_mesh_gen_admin_property_status_cb_t admin_property_status

    ESP_BLE_MESH_MODEL_OP_GEN_ADMIN_PROPERTY_STATUS

  esp_ble_mesh_gen_manufacturer_properties_status_cb_t manufacturer_properties_status

    ESP_BLE_MESH_MODEL_OP_GEN_MANUFACTURER_PROPERTIES_STATUS

  esp_ble_mesh_gen_manufacturer_property_status_cb_t manufacturer_property_status

    ESP_BLE_MESH_MODEL_OP_GEN_MANUFACTURER_PROPERTY_STATUS

  esp_ble_mesh_gen_client_properties_status_cb_t client_properties_status

    ESP_BLE_MESH_MODEL_OP_GEN_CLIENT_PROPERTIES_STATUS

union esp_ble_mesh_generic_server_state_change_t
  #include <esp_ble_mesh_generic_model_api.h>

  Generic Server Model state change value union.

  Public Members

  esp_ble_mesh_state_change_gen_onoff_set_t onoff_set

    The recv_op in ctx can be used to decide which state is changed. Generic OnOff Set

  esp_ble_mesh_state_change_gen_level_set_t level_set

    Generic Level Set

  esp_ble_mesh_state_change_gen_delta_set_t delta_set

    Generic Delta Set

  esp_ble_mesh_state_change_gen_move_set_t move_set

    Generic Move Set

  esp_ble_mesh_state_change_gen_def_trans_time_set_t def_trans_time_set

    Generic Default Transition Time Set

  esp_ble_mesh_state_change_gen_onpowerup_set_t onpowerup_set

    Generic OnPowerUp Set

  esp_ble_mesh_state_change_gen_power_level_set_t power_level_set

    Generic Power Level Set

  esp_ble_mesh_state_change_gen_power_default_set_t power_default_set

    Generic Power Default Set

  esp_ble_mesh_state_change_gen_power_range_set_t power_range_set

    Generic Power Range Set

  esp_ble_mesh_state_change_gen_loc_global_set_t loc_global_set

    Generic Location Global Set

  esp_ble_mesh_state_change_gen_loc_local_set_t loc_local_set

    Generic Location Local Set

  esp_ble_mesh_state_change_gen_user_property_set_t user_property_set

    Generic User Property Set

  esp_ble_mesh_state_change_gen_admin_property_set_t admin_property_set

    Generic Admin Property Set

  esp_ble_mesh_state_change_gen_manu_property_set_t manu_property_set

    Generic Manufacturer Property Set

union esp_ble_mesh_generic_server_recv_get_msg_t
  #include <esp_ble_mesh_generic_model_api.h>

  Generic Server Model received get message union.

  Public Members

  esp_ble_mesh_server_recv_gen_user_property_get_t user_property

    Generic User Property Get

  esp_ble_mesh_server_recv_gen_admin_property_get_t admin_property

    Generic Admin Property Get

  esp_ble_mesh_server_recv_gen_manufacturer_property_get_t manu_property

    Generic Manufacturer Property Get

  esp_ble_mesh_server_recv_gen_client_properties_get_t client_properties

    Generic Client Properties Get

union esp_ble_mesh_generic_server_recv_set_msg_t
  #include <esp_ble_mesh_generic_model_api.h>

  Generic Server Model received set message union.

  Public Members

  esp_ble_mesh_server_recv_gen_onoff_set_t onoff

    Generic OnOff Set/Generic OnOff Set Unack

  esp_ble_mesh_server_recv_gen_level_set_t level

    Generic Level Set/Generic Level Set Unack

  esp_ble_mesh_server_recv_gen_delta_set_t delta

    Generic Delta Set/Generic Delta Set Unack

  esp_ble_mesh_server_recv_gen_move_set_t move

    Generic Move Set/Generic Move Set Unack

  esp_ble_mesh_server_recv_gen_def_trans_time_set_t def_trans_time

    Generic Default Transition Time Set/Generic Default Transition Time Set Unack

  esp_ble_mesh_server_recv_gen_onpowerup_set_t onpowerup

    Generic OnPowerUp Set/Generic OnPowerUp Set Unack

  esp_ble_mesh_server_recv_gen_power_level_set_t power_level

    Generic Power Level Set/Generic Power Level Set Unack

  esp_ble_mesh_server_recv_gen_power_default_set_t power_default

    Generic Power Default Set/Generic Power Default Set Unack

  esp_ble_mesh_server_recv_gen_power_range_set_t power_range

    Generic Power Range Set/Generic Power Range Set Unack

  esp_ble_mesh_server_recv_gen_loc_global_set_t location_global

    Generic Location Global Set/Generic Location Global Set Unack

  esp_ble_mesh_server_recv_gen_loc_local_set_t location_local

    Generic Location Local Set/Generic Location Local Set Unack

  esp_ble_mesh_server_recv_gen_user_property_set_t user_property

    Generic User Property Set/Generic User Property Set Unack

  esp_ble_mesh_server_recv_gen_admin_property_set_t admin_property

    Generic Admin Property Set/Generic Admin Property Set Unack

  esp_ble_mesh_server_recv_gen_manufacturer_property_set_t manu_property

    Generic Manufacturer Property Set/Generic Manufacturer Property Set Unack

union esp_ble_mesh_generic_server_cb_value_t
  #include <esp_ble_mesh_generic_model_api.h>

  Generic Server Model callback value union.

  Public Members

  esp_ble_mesh_generic_server_state_change_t state_change

    ESP_BLE_MESH_GENERIC_SERVER_STATE_CHANGE_EVT

  esp_ble_mesh_generic_server_recv_get_msg_t get

    ESP_BLE_MESH_GENERIC_SERVER_RECV_GET_MSG_EVT

  esp_ble_mesh_generic_server_recv_set_msg_t set

    ESP_BLE_MESH_GENERIC_SERVER_RECV_SET_MSG_EVT

### Structures

struct esp_ble_mesh_gen_onoff_set_t

  Bluetooth Mesh Generic Client Model Get and Set parameters structure.

  Parameters of Generic OnOff Set.

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint8_t onoff

    Target value of Generic OnOff state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_gen_level_set_t

  Parameters of Generic Level Set.

  Public Members

  bool op_en

    Indicate if optional parameters are included

  int16_t level

    Target value of Generic Level state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_gen_delta_set_t

  Parameters of Generic Delta Set.

  Public Members

  bool op_en

    Indicate if optional parameters are included

  int32_t level

    Delta change of Generic Level state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_gen_move_set_t

  Parameters of Generic Move Set.

  Public Members

  bool op_en

    Indicate if optional parameters are included

  int16_t delta_level

    Delta Level step to calculate Move speed for Generic Level state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_gen_def_trans_time_set_t

  Parameter of Generic Default Transition Time Set.

  Public Members

  uint8_t trans_time

    The value of the Generic Default Transition Time state

struct esp_ble_mesh_gen_onpowerup_set_t

  Parameter of Generic OnPowerUp Set.

  Public Members

  uint8_t onpowerup

    The value of the Generic OnPowerUp state

struct esp_ble_mesh_gen_power_level_set_t

  Parameters of Generic Power Level Set.

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t power

    Target value of Generic Power Actual state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_gen_power_default_set_t

  Parameter of Generic Power Default Set.

  Public Members

  uint16_t power

    The value of the Generic Power Default state

struct esp_ble_mesh_gen_power_range_set_t

  Parameters of Generic Power Range Set.

  Public Members

  uint16_t range_min

    Value of Range Min field of Generic Power Range state

  uint16_t range_max

    Value of Range Max field of Generic Power Range state

struct esp_ble_mesh_gen_loc_global_set_t

  Parameters of Generic Location Global Set.

  Public Members

  int32_t global_latitude

    Global Coordinates (Latitude)

  int32_t global_longitude

    Global Coordinates (Longitude)

  int16_t global_altitude

    Global Altitude

struct esp_ble_mesh_gen_loc_local_set_t

  Parameters of Generic Location Local Set.

  Public Members

  int16_t local_north

    Local Coordinates (North)

  int16_t local_east

    Local Coordinates (East)

  int16_t local_altitude

    Local Altitude

  uint8_t floor_number

    Floor Number

  uint16_t uncertainty

    Uncertainty

struct esp_ble_mesh_gen_user_property_get_t

  Parameter of Generic User Property Get.

  Public Members

  uint16_t property_id

    Property ID identifying a Generic User Property

struct esp_ble_mesh_gen_user_property_set_t

  Parameters of Generic User Property Set.

  Public Members

  uint16_t property_id

    Property ID identifying a Generic User Property

  struct net_buf_simple *property_value

    Raw value for the User Property

struct esp_ble_mesh_gen_admin_property_get_t

  Parameter of Generic Admin Property Get.

  Public Members

  uint16_t property_id

    Property ID identifying a Generic Admin Property

struct esp_ble_mesh_gen_admin_property_set_t

  Parameters of Generic Admin Property Set.

  Public Members

  uint16_t property_id

    Property ID identifying a Generic Admin Property

  uint8_t user_access

    Enumeration indicating user access

  struct net_buf_simple *property_value

    Raw value for the Admin Property

struct esp_ble_mesh_gen_manufacturer_property_get_t

  Parameter of Generic Manufacturer Property Get.

  Public Members

  uint16_t property_id

    Property ID identifying a Generic Manufacturer Property

struct esp_ble_mesh_gen_manufacturer_property_set_t

  Parameters of Generic Manufacturer Property Set.

  Public Members

  uint16_t property_id

    Property ID identifying a Generic Manufacturer Property

  uint8_t user_access

    Enumeration indicating user access

struct esp_ble_mesh_gen_client_properties_get_t

  Parameter of Generic Client Properties Get.

  Public Members

  uint16_t property_id

    A starting Client Property ID present within an element

struct esp_ble_mesh_gen_onoff_status_cb_t

  Bluetooth Mesh Generic Client Model Get and Set callback parameters structure.

  Parameters of Generic OnOff Status.

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint8_t present_onoff

    Current value of Generic OnOff state

  uint8_t target_onoff

    Target value of Generic OnOff state (optional)

  uint8_t remain_time

    Time to complete state transition (C.1)

struct esp_ble_mesh_gen_level_status_cb_t

  Parameters of Generic Level Status.

  Public Members

  bool op_en

    Indicate if optional parameters are included

  int16_t present_level

    Current value of Generic Level state

  int16_t target_level

    Target value of the Generic Level state (optional)

  uint8_t remain_time

    Time to complete state transition (C.1)

struct esp_ble_mesh_gen_def_trans_time_status_cb_t

  Parameter of Generic Default Transition Time Status.

  Public Members

  uint8_t trans_time

    The value of the Generic Default Transition Time state

struct esp_ble_mesh_gen_onpowerup_status_cb_t

  Parameter of Generic OnPowerUp Status.

  Public Members

  uint8_t onpowerup

    The value of the Generic OnPowerUp state

struct esp_ble_mesh_gen_power_level_status_cb_t

  Parameters of Generic Power Level Status.

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t present_power

    Current value of Generic Power Actual state

  uint16_t target_power

    Target value of Generic Power Actual state (optional)

  uint8_t remain_time

    Time to complete state transition (C.1)

struct esp_ble_mesh_gen_power_last_status_cb_t

  Parameter of Generic Power Last Status.

  Public Members

  uint16_t power

    The value of the Generic Power Last state

struct esp_ble_mesh_gen_power_default_status_cb_t

  Parameter of Generic Power Default Status.

  Public Members

  uint16_t power

    The value of the Generic Default Last state

struct esp_ble_mesh_gen_power_range_status_cb_t

  Parameters of Generic Power Range Status.

  Public Members

  uint8_t status_code

    Status Code for the request message

  uint16_t range_min

    Value of Range Min field of Generic Power Range state

  uint16_t range_max

    Value of Range Max field of Generic Power Range state

struct esp_ble_mesh_gen_battery_status_cb_t

  Parameters of Generic Battery Status.

  Public Members

  uint32_t battery_level

    Value of Generic Battery Level state

  uint32_t time_to_discharge

    Value of Generic Battery Time to Discharge state

  uint32_t time_to_charge

    Value of Generic Battery Time to Charge state

  uint32_t flags

    Value of Generic Battery Flags state

struct esp_ble_mesh_gen_loc_global_status_cb_t

  Parameters of Generic Location Global Status.

  Public Members

  int32_t global_latitude

    Global Coordinates (Latitude)

  int32_t global_longitude

    Global Coordinates (Longitude)

  int16_t global_altitude

    Global Altitude

struct esp_ble_mesh_gen_loc_local_status_cb_t

  Parameters of Generic Location Local Status.

  Public Members

  int16_t local_north

    Local Coordinates (North)

  int16_t local_east

    Local Coordinates (East)

  int16_t local_altitude

    Local Altitude

  uint8_t floor_number

    Floor Number

  uint16_t uncertainty

    Uncertainty

struct esp_ble_mesh_gen_user_properties_status_cb_t

  Parameter of Generic User Properties Status.

  Public Members

  struct net_buf_simple *property_ids

    Buffer contains a sequence of N User Property IDs

struct esp_ble_mesh_gen_user_property_status_cb_t

  Parameters of Generic User Property Status.

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t property_id

    Property ID identifying a Generic User Property

  uint8_t user_access

    Enumeration indicating user access (optional)

  struct net_buf_simple *property_value

    Raw value for the User Property (C.1)

struct esp_ble_mesh_gen_admin_properties_status_cb_t

  Parameter of Generic Admin Properties Status.

  Public Members

  struct net_buf_simple *property_ids

    Buffer contains a sequence of N Admin Property IDs

struct esp_ble_mesh_gen_admin_property_status_cb_t

  Parameters of Generic Admin Property Status.

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t property_id

    Property ID identifying a Generic Admin Property

  uint8_t user_access

    Enumeration indicating user access (optional)

  struct net_buf_simple *property_value

    Raw value for the Admin Property (C.1)

struct esp_ble_mesh_gen_manufacturer_properties_status_cb_t

  Parameter of Generic Manufacturer Properties Status.

  Public Members

  struct net_buf_simple *property_ids

    Buffer contains a sequence of N Manufacturer Property IDs

struct esp_ble_mesh_gen_manufacturer_property_status_cb_t

  Parameters of Generic Manufacturer Property Status.

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t property_id

    Property ID identifying a Generic Manufacturer Property

  uint8_t user_access

    Enumeration indicating user access (optional)

  struct net_buf_simple *property_value

    Raw value for the Manufacturer Property (C.1)

struct esp_ble_mesh_gen_client_properties_status_cb_t

  Parameter of Generic Client Properties Status.

  Public Members

  struct net_buf_simple *property_ids

    Buffer contains a sequence of N Client Property IDs

struct esp_ble_mesh_generic_client_cb_param_t

  Generic Client Model callback parameters

  Public Members

  int error_code

    Appropriate error code

  esp_ble_mesh_client_common_param_t *params

    The client common parameters.

  esp_ble_mesh_gen_client_status_cb_t status_cb

    The generic status message callback values

struct esp_ble_mesh_gen_onoff_state_t

  Parameters of Generic OnOff state

  Public Members

  uint8_t onoff

    The present value of the Generic OnOff state

  uint8_t target_onoff

    The target value of the Generic OnOff state

struct esp_ble_mesh_gen_onoff_srv_t

  User data of Generic OnOff Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic OnOff Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_gen_onoff_state_t state

    Parameters of the Generic OnOff state

  esp_ble_mesh_last_msg_info_t last

    Parameters of the last received set message

  esp_ble_mesh_state_transition_t transition

    Parameters of state transition

struct esp_ble_mesh_gen_level_state_t

  Parameters of Generic Level state

  Public Members

  int16_t level

    The present value of the Generic Level state

  int16_t target_level

    The target value of the Generic Level state

  int16_t last_level

    When a new transaction starts, level should be set to last_last, and use "level + incoming delta" to calculate the target level. In another word, "last_level" is used to record "level" of the last transaction, and "last_delta" is used to record the previously received delta_level value. The last value of the Generic Level state

  int32_t last_delta

    The last delta change of the Generic Level state

  bool move_start

    Indicate if the transition of the Generic Level state has been started

  bool positive

    Indicate if the transition is positive or negative

struct esp_ble_mesh_gen_level_srv_t

  User data of Generic Level Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic Level Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_gen_level_state_t state

    Parameters of the Generic Level state

  esp_ble_mesh_last_msg_info_t last

    Parameters of the last received set message

  esp_ble_mesh_state_transition_t transition

    Parameters of state transition

  int32_t tt_delta_level

    Delta change value of level state transition

struct esp_ble_mesh_gen_def_trans_time_state_t

  Parameter of Generic Default Transition Time state

  Public Members

  uint8_t trans_time

    The value of the Generic Default Transition Time state

struct esp_ble_mesh_gen_def_trans_time_srv_t

  User data of Generic Default Transition Time Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic Default Transition Time Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_gen_def_trans_time_state_t state

    Parameters of the Generic Default Transition Time state

struct esp_ble_mesh_gen_onpowerup_state_t

  Parameter of Generic OnPowerUp state

  Public Members

  uint8_t onpowerup

    The value of the Generic OnPowerUp state

struct esp_ble_mesh_gen_power_onoff_srv_t

  User data of Generic Power OnOff Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic Power OnOff Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_gen_onpowerup_state_t *state

    Parameters of the Generic OnPowerUp state

struct esp_ble_mesh_gen_power_onoff_setup_srv_t

  User data of Generic Power OnOff Setup Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic Power OnOff Setup Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_gen_onpowerup_state_t *state

    Parameters of the Generic OnPowerUp state

struct esp_ble_mesh_gen_power_level_state_t

  Parameters of Generic Power Level state

  Public Members

  uint16_t power_actual

    The present value of the Generic Power Actual state

  uint16_t target_power_actual

    The target value of the Generic Power Actual state

  uint16_t power_last

    The value of the Generic Power Last state

  uint16_t power_default

    The value of the Generic Power Default state

  uint8_t status_code

    The status code of setting Generic Power Range state

  uint16_t power_range_min

    The minimum value of the Generic Power Range state

  uint16_t power_range_max

    The maximum value of the Generic Power Range state

struct esp_ble_mesh_gen_power_level_srv_t

  User data of Generic Power Level Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic Power Level Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_gen_power_level_state_t *state

    Parameters of the Generic Power Level state

  esp_ble_mesh_last_msg_info_t last

    Parameters of the last received set message

  esp_ble_mesh_state_transition_t transition

    Parameters of state transition

  int32_t tt_delta_level

    Delta change value of level state transition

struct esp_ble_mesh_gen_power_level_setup_srv_t

  User data of Generic Power Level Setup Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic Power Level Setup Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_gen_power_level_state_t *state

    Parameters of the Generic Power Level state

struct esp_ble_mesh_gen_battery_state_t

  Parameters of Generic Battery state

  Public Members

  uint32_t battery_level

    The value of the Generic Battery Level state

  uint32_t time_to_discharge

    The value of the Generic Battery Time to Discharge state

  uint32_t time_to_charge

    The value of the Generic Battery Time to Charge state

  uint32_t battery_flags

    The value of the Generic Battery Flags state

struct esp_ble_mesh_gen_battery_srv_t

  User data of Generic Battery Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic Battery Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_gen_battery_state_t state

    Parameters of the Generic Battery state

struct esp_ble_mesh_gen_location_state_t

  Parameters of Generic Location state

  Public Members

  int32_t global_latitude

    The value of the Global Latitude field

  int32_t global_longitude

    The value of the Global Longitude field

  int16_t global_altitude

    The value of the Global Altitude field

  int16_t local_north

    The value of the Local North field

  int16_t local_east

    The value of the Local East field

  int16_t local_altitude

    The value of the Local Altitude field

  uint8_t floor_number

    The value of the Floor Number field

  uint16_t uncertainty

    The value of the Uncertainty field

struct esp_ble_mesh_gen_location_srv_t

  User data of Generic Location Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic Location Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_gen_location_state_t *state

    Parameters of the Generic Location state

struct esp_ble_mesh_gen_location_setup_srv_t

  User data of Generic Location Setup Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic Location Setup Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_gen_location_state_t *state

    Parameters of the Generic Location state

struct esp_ble_mesh_generic_property_t

  Parameters of Generic Property states

  Public Members

  uint16_t id

    The value of User/Admin/Manufacturer Property ID

  uint8_t user_access

    The value of User Access field

  uint8_t admin_access

    The value of Admin Access field

  uint8_t manu_access

    The value of Manufacturer Access field

  struct net_buf_simple *val

    The value of User/Admin/Manufacturer Property

struct esp_ble_mesh_gen_user_prop_srv_t

  User data of Generic User Property Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic User Property Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  uint8_t property_count

    Generic User Property count

  esp_ble_mesh_generic_property_t *properties

    Parameters of the Generic User Property state

struct esp_ble_mesh_gen_admin_prop_srv_t

  User data of Generic Admin Property Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic Admin Property Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  uint8_t property_count

    Generic Admin Property count

  esp_ble_mesh_generic_property_t *properties

    Parameters of the Generic Admin Property state

struct esp_ble_mesh_gen_manu_prop_srv_t

  User data of Generic Manufacturer Property Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic Manufacturer Property Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  uint8_t property_count

    Generic Manufacturer Property count

  esp_ble_mesh_generic_property_t *properties

    Parameters of the Generic Manufacturer Property state

struct esp_ble_mesh_gen_client_prop_srv_t

  User data of Generic Client Property Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Generic Client Property Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  uint8_t id_count

    Generic Client Property ID count

  uint16_t *property_ids

    Parameters of the Generic Client Property state

struct esp_ble_mesh_state_change_gen_onoff_set_t

  Parameter of Generic OnOff Set state change event

  Public Members

  uint8_t onoff

    The value of Generic OnOff state

struct esp_ble_mesh_state_change_gen_level_set_t

  Parameter of Generic Level Set state change event

  Public Members

  int16_t level

    The value of Generic Level state

struct esp_ble_mesh_state_change_gen_delta_set_t

  Parameter of Generic Delta Set state change event

  Public Members

  int16_t level

    The value of Generic Level state

struct esp_ble_mesh_state_change_gen_move_set_t

  Parameter of Generic Move Set state change event

  Public Members

  int16_t level

    The value of Generic Level state

struct esp_ble_mesh_state_change_gen_def_trans_time_set_t

  Parameter of Generic Default Transition Time Set state change event

  Public Members

  uint8_t trans_time

    The value of Generic Default Transition Time state

struct esp_ble_mesh_state_change_gen_onpowerup_set_t

  Parameter of Generic OnPowerUp Set state change event

  Public Members

  uint8_t onpowerup

    The value of Generic OnPowerUp state

struct esp_ble_mesh_state_change_gen_power_level_set_t

  Parameter of Generic Power Level Set state change event

  Public Members

  uint16_t power

    The value of Generic Power Actual state

struct esp_ble_mesh_state_change_gen_power_default_set_t

  Parameter of Generic Power Default Set state change event

  Public Members

  uint16_t power

    The value of Generic Power Default state

struct esp_ble_mesh_state_change_gen_power_range_set_t

  Parameters of Generic Power Range Set state change event

  Public Members

  uint16_t range_min

    The minimum value of Generic Power Range state

  uint16_t range_max

    The maximum value of Generic Power Range state

struct esp_ble_mesh_state_change_gen_loc_global_set_t

  Parameters of Generic Location Global Set state change event

  Public Members

  int32_t latitude

    The Global Latitude value of Generic Location state

  int32_t longitude

    The Global Longitude value of Generic Location state

  int16_t altitude

    The Global Altitude value of Generic Location state

struct esp_ble_mesh_state_change_gen_loc_local_set_t

  Parameters of Generic Location Local Set state change event

  Public Members

  int16_t north

    The Local North value of Generic Location state

  int16_t east

    The Local East value of Generic Location state

  int16_t altitude

    The Local Altitude value of Generic Location state

  uint8_t floor_number

    The Floor Number value of Generic Location state

  uint16_t uncertainty

    The Uncertainty value of Generic Location state

struct esp_ble_mesh_state_change_gen_user_property_set_t

  Parameters of Generic User Property Set state change event

  Public Members

  uint16_t id

    The property id of Generic User Property state

  struct net_buf_simple *value

    The property value of Generic User Property state

struct esp_ble_mesh_state_change_gen_admin_property_set_t

  Parameters of Generic Admin Property Set state change event

  Public Members

  uint16_t id

    The property id of Generic Admin Property state

  uint8_t access

    The property access of Generic Admin Property state

  struct net_buf_simple *value

    The property value of Generic Admin Property state

struct esp_ble_mesh_state_change_gen_manu_property_set_t

  Parameters of Generic Manufacturer Property Set state change event

  Public Members

  uint16_t id

    The property id of Generic Manufacturer Property state

  uint8_t access

    The property value of Generic Manufacturer Property state

struct esp_ble_mesh_server_recv_gen_user_property_get_t

  Context of the received Generic User Property Get message

  Public Members

  uint16_t property_id

    Property ID identifying a Generic User Property

struct esp_ble_mesh_server_recv_gen_admin_property_get_t

  Context of the received Generic Admin Property Get message

  Public Members

  uint16_t property_id

    Property ID identifying a Generic Admin Property

struct esp_ble_mesh_server_recv_gen_manufacturer_property_get_t

  Context of the received Generic Manufacturer Property message

  Public Members

  uint16_t property_id

    Property ID identifying a Generic Manufacturer Property

struct esp_ble_mesh_server_recv_gen_client_properties_get_t

  Context of the received Generic Client Properties Get message

  Public Members

  uint16_t property_id

    A starting Client Property ID present within an element

struct esp_ble_mesh_server_recv_gen_onoff_set_t

  Context of the received Generic OnOff Set message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint8_t onoff

    Target value of Generic OnOff state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_gen_level_set_t

  Context of the received Generic Level Set message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  int16_t level

    Target value of Generic Level state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_gen_delta_set_t

  Context of the received Generic Delta Set message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  int32_t delta_level

    Delta change of Generic Level state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_gen_move_set_t

  Context of the received Generic Move Set message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  int16_t delta_level

    Delta Level step to calculate Move speed for Generic Level state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_gen_def_trans_time_set_t

  Context of the received Generic Default Transition Time Set message

  Public Members

  uint8_t trans_time

    The value of the Generic Default Transition Time state

struct esp_ble_mesh_server_recv_gen_onpowerup_set_t

  Context of the received Generic OnPowerUp Set message

  Public Members

  uint8_t onpowerup

    The value of the Generic OnPowerUp state

struct esp_ble_mesh_server_recv_gen_power_level_set_t

  Context of the received Generic Power Level Set message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t power

    Target value of Generic Power Actual state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_gen_power_default_set_t

  Context of the received Generic Power Default Set message

  Public Members

  uint16_t power

    The value of the Generic Power Default state

struct esp_ble_mesh_server_recv_gen_power_range_set_t

  Context of the received Generic Power Range Set message

  Public Members

  uint16_t range_min

    Value of Range Min field of Generic Power Range state

  uint16_t range_max

    Value of Range Max field of Generic Power Range state

struct esp_ble_mesh_server_recv_gen_loc_global_set_t

  Context of the received Generic Location Global Set message

  Public Members

  int32_t global_latitude

    Global Coordinates (Latitude)

  int32_t global_longitude

    Global Coordinates (Longitude)

  int16_t global_altitude

    Global Altitude

struct esp_ble_mesh_server_recv_gen_loc_local_set_t

  Context of the received Generic Location Local Set message

  Public Members

  int16_t local_north

    Local Coordinates (North)

  int16_t local_east

    Local Coordinates (East)

  int16_t local_altitude

    Local Altitude

  uint8_t floor_number

    Floor Number

  uint16_t uncertainty

    Uncertainty

struct esp_ble_mesh_server_recv_gen_user_property_set_t

  Context of the received Generic User Property Set message

  Public Members

  uint16_t property_id

    Property ID identifying a Generic User Property

  struct net_buf_simple *property_value

    Raw value for the User Property

struct esp_ble_mesh_server_recv_gen_admin_property_set_t

  Context of the received Generic Admin Property Set message

  Public Members

  uint16_t property_id

    Property ID identifying a Generic Admin Property

  uint8_t user_access

    Enumeration indicating user access

  struct net_buf_simple *property_value

    Raw value for the Admin Property

struct esp_ble_mesh_server_recv_gen_manufacturer_property_set_t

  Context of the received Generic Manufacturer Property Set message

  Public Members

  uint16_t property_id

    Property ID identifying a Generic Manufacturer Property

  uint8_t user_access

    Enumeration indicating user access

struct esp_ble_mesh_generic_server_cb_param_t

  Generic Server Model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to Generic Server Models

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received messages

  esp_ble_mesh_generic_server_cb_value_t value

    Value of the received Generic Messages

### Macros

ESP_BLE_MESH_MODEL_GEN_ONOFF_CLI(cli_pub, cli_data)

  Define a new Generic OnOff Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Generic OnOff Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Generic OnOff Client Model instance.

ESP_BLE_MESH_MODEL_GEN_LEVEL_CLI(cli_pub, cli_data)

  Define a new Generic Level Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Generic Level Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Generic Level Client Model instance.

ESP_BLE_MESH_MODEL_GEN_DEF_TRANS_TIME_CLI(cli_pub, cli_data)

  Define a new Generic Default Transition Time Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Generic Default Transition Time Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Generic Default Transition Time Client Model instance.

ESP_BLE_MESH_MODEL_GEN_POWER_ONOFF_CLI(cli_pub, cli_data)

  Define a new Generic Power OnOff Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Generic Power OnOff Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Generic Power OnOff Client Model instance.

ESP_BLE_MESH_MODEL_GEN_POWER_LEVEL_CLI(cli_pub, cli_data)

  Define a new Generic Power Level Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Generic Power Level Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Generic Power Level Client Model instance.

ESP_BLE_MESH_MODEL_GEN_BATTERY_CLI(cli_pub, cli_data)

  Define a new Generic Battery Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Generic Battery Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Generic Battery Client Model instance.

ESP_BLE_MESH_MODEL_GEN_LOCATION_CLI(cli_pub, cli_data)

  Define a new Generic Location Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Generic Location Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Generic Location Client Model instance.

ESP_BLE_MESH_MODEL_GEN_PROPERTY_CLI(cli_pub, cli_data)

  Define a new Generic Property Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Generic Property Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Generic Location Client Model instance.

ESP_BLE_MESH_MODEL_GEN_ONOFF_SRV(srv_pub, srv_data)

  Generic Server Models related context.

  Define a new Generic OnOff Server Model.

  备注

  1. The Generic OnOff Server Model is a root model.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_onoff_srv_t.

  返回:

    New Generic OnOff Server Model instance.

ESP_BLE_MESH_MODEL_GEN_LEVEL_SRV(srv_pub, srv_data)

  Define a new Generic Level Server Model.

  备注

  1. The Generic Level Server Model is a root model.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_level_srv_t.

  返回:

    New Generic Level Server Model instance.

ESP_BLE_MESH_MODEL_GEN_DEF_TRANS_TIME_SRV(srv_pub, srv_data)

  Define a new Generic Default Transition Time Server Model.

  备注

  1. The Generic Default Transition Time Server Model is a root model.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_def_trans_time_srv_t.

  返回:

    New Generic Default Transition Time Server Model instance.

ESP_BLE_MESH_MODEL_GEN_POWER_ONOFF_SRV(srv_pub, srv_data)

  Define a new Generic Power OnOff Server Model.

  备注

  1. The Generic Power OnOff Server model extends the Generic OnOff Server model. When this model is present on an element, the corresponding Generic Power OnOff Setup Server model shall also be present.

  1. This model may be used to represent a variety of devices that do not fit any of the model descriptions that have been defined but support the generic properties of On/Off.

  2. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_power_onoff_srv_t.

  返回:

    New Generic Power OnOff Server Model instance.

ESP_BLE_MESH_MODEL_GEN_POWER_ONOFF_SETUP_SRV(srv_pub, srv_data)

  Define a new Generic Power OnOff Setup Server Model.

  备注

  1. The Generic Power OnOff Setup Server model extends the Generic Power OnOff Server model and the Generic Default Transition Time Server model.

  1. This model shall support model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_power_onoff_setup_srv_t.

  返回:

    New Generic Power OnOff Setup Server Model instance.

ESP_BLE_MESH_MODEL_GEN_POWER_LEVEL_SRV(srv_pub, srv_data)

  Define a new Generic Power Level Server Model.

  备注

  1. The Generic Power Level Server model extends the Generic Power OnOff Server model and the Generic Level Server model. When this model is present on an Element, the corresponding Generic Power Level Setup Server model shall also be present.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_power_level_srv_t.

  返回:

    New Generic Power Level Server Model instance.

ESP_BLE_MESH_MODEL_GEN_POWER_LEVEL_SETUP_SRV(srv_pub, srv_data)

  Define a new Generic Power Level Setup Server Model.

  备注

  1. The Generic Power Level Setup Server model extends the Generic Power Level Server model and the Generic Power OnOff Setup Server model.

  1. This model shall support model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_power_level_setup_srv_t.

  返回:

    New Generic Power Level Setup Server Model instance.

ESP_BLE_MESH_MODEL_GEN_BATTERY_SRV(srv_pub, srv_data)

  Define a new Generic Battery Server Model.

  备注

  1. The Generic Battery Server Model is a root model.

  1. This model shall support model publication and model subscription.

  2. The model may be used to represent an element that is powered by a battery.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_battery_srv_t.

  返回:

    New Generic Battery Server Model instance.

ESP_BLE_MESH_MODEL_GEN_LOCATION_SRV(srv_pub, srv_data)

  Define a new Generic Location Server Model.

  备注

  1. The Generic Location Server model is a root model. When this model is present on an Element, the corresponding Generic Location Setup Server model shall also be present.

  1. This model shall support model publication and model subscription.

  2. The model may be used to represent an element that knows its location (global or local).

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_location_srv_t.

  返回:

    New Generic Location Server Model instance.

ESP_BLE_MESH_MODEL_GEN_LOCATION_SETUP_SRV(srv_pub, srv_data)

  Define a new Generic Location Setup Server Model.

  备注

  1. The Generic Location Setup Server model extends the Generic Location Server model.

  1. This model shall support model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_location_setup_srv_t.

  返回:

    New Generic Location Setup Server Model instance.

ESP_BLE_MESH_MODEL_GEN_USER_PROP_SRV(srv_pub, srv_data)

  Define a new Generic User Property Server Model.

  备注

  1. The Generic User Property Server model is a root model.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_user_prop_srv_t.

  返回:

    New Generic User Property Server Model instance.

ESP_BLE_MESH_MODEL_GEN_ADMIN_PROP_SRV(srv_pub, srv_data)

  Define a new Generic Admin Property Server Model.

  备注

  1. The Generic Admin Property Server model extends the Generic User Property Server model.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_admin_prop_srv_t.

  返回:

    New Generic Admin Property Server Model instance.

ESP_BLE_MESH_MODEL_GEN_MANUFACTURER_PROP_SRV(srv_pub, srv_data)

  Define a new Generic Manufacturer Property Server Model.

  备注

  1. The Generic Manufacturer Property Server model extends the Generic User Property Server model.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_manu_prop_srv_t.

  返回:

    New Generic Manufacturer Property Server Model instance.

ESP_BLE_MESH_MODEL_GEN_CLIENT_PROP_SRV(srv_pub, srv_data)

  Define a new Generic User Property Server Model.

  备注

  1. The Generic Client Property Server model is a root model.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_gen_client_prop_srv_t.

  返回:

    New Generic Client Property Server Model instance.

### Type Definitions

typedef void (*esp_ble_mesh_generic_client_cb_t)(esp_ble_mesh_generic_client_cb_event_t event, esp_ble_mesh_generic_client_cb_param_t *param)

  Bluetooth Mesh Generic Client Model function.

  Generic Client Model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_generic_server_cb_t)(esp_ble_mesh_generic_server_cb_event_t event, esp_ble_mesh_generic_server_cb_param_t *param)

  Bluetooth Mesh Generic Server Model function.

  Generic Server Model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_generic_client_cb_event_t

  This enum value is the event of Generic Client Model

  Values:

  enumerator ESP_BLE_MESH_GENERIC_CLIENT_GET_STATE_EVT
  enumerator ESP_BLE_MESH_GENERIC_CLIENT_SET_STATE_EVT
  enumerator ESP_BLE_MESH_GENERIC_CLIENT_PUBLISH_EVT
  enumerator ESP_BLE_MESH_GENERIC_CLIENT_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_GENERIC_CLIENT_EVT_MAX

enum esp_ble_mesh_gen_user_prop_access_t

  This enum value is the access value of Generic User Property

  Values:

  enumerator ESP_BLE_MESH_GEN_USER_ACCESS_PROHIBIT
  enumerator ESP_BLE_MESH_GEN_USER_ACCESS_READ
  enumerator ESP_BLE_MESH_GEN_USER_ACCESS_WRITE
  enumerator ESP_BLE_MESH_GEN_USER_ACCESS_READ_WRITE

enum esp_ble_mesh_gen_admin_prop_access_t

  This enum value is the access value of Generic Admin Property

  Values:

  enumerator ESP_BLE_MESH_GEN_ADMIN_NOT_USER_PROP
  enumerator ESP_BLE_MESH_GEN_ADMIN_ACCESS_READ
  enumerator ESP_BLE_MESH_GEN_ADMIN_ACCESS_WRITE
  enumerator ESP_BLE_MESH_GEN_ADMIN_ACCESS_READ_WRITE

enum esp_ble_mesh_gen_manu_prop_access_t

  This enum value is the access value of Generic Manufacturer Property

  Values:

  enumerator ESP_BLE_MESH_GEN_MANU_NOT_USER_PROP
  enumerator ESP_BLE_MESH_GEN_MANU_ACCESS_READ

enum esp_ble_mesh_generic_server_cb_event_t

  This enum value is the event of Generic Server Model

  Values:

  enumerator ESP_BLE_MESH_GENERIC_SERVER_STATE_CHANGE_EVT

    1. When get_auto_rsp is set to ESP_BLE_MESH_SERVER_AUTO_RSP, no event will be callback to the application layer when Generic Get messages are received.

    2. When set_auto_rsp is set to ESP_BLE_MESH_SERVER_AUTO_RSP, this event will be callback to the application layer when Generic Set/Set Unack messages are received.

  enumerator ESP_BLE_MESH_GENERIC_SERVER_RECV_GET_MSG_EVT

    When get_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, this event will be callback to the application layer when Generic Get messages are received.

  enumerator ESP_BLE_MESH_GENERIC_SERVER_RECV_SET_MSG_EVT

    When set_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, this event will be callback to the application layer when Generic Set/Set Unack messages are received.

  enumerator ESP_BLE_MESH_GENERIC_SERVER_EVT_MAX

### Sensor Client/Server Models

### Header File

- components/bt/esp_ble_mesh/api/models/include/esp_ble_mesh_sensor_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_sensor_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_sensor_client_callback(esp_ble_mesh_sensor_client_cb_t callback)

  Register BLE Mesh Sensor Client Model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_sensor_client_get_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_sensor_client_get_state_t *get_state)

  Get the value of Sensor Server Model states using the Sensor Client Model get messages.

  备注

  If you want to know the opcodes and corresponding meanings accepted by this API, please refer to esp_ble_mesh_sensor_message_opcode_t in esp_ble_mesh_defs.h

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - get_state -- [in] Pointer to sensor get message value. Shall not be set to NULL.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_sensor_client_set_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_sensor_client_set_state_t *set_state)

  Set the value of Sensor Server Model states using the Sensor Client Model set messages.

  备注

  If you want to know the opcodes and corresponding meanings accepted by this API, please refer to esp_ble_mesh_sensor_message_opcode_t in esp_ble_mesh_defs.h

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - set_state -- [in] Pointer to sensor set message value. Shall not be set to NULL.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_sensor_server_callback(esp_ble_mesh_sensor_server_cb_t callback)

  Register BLE Mesh Sensor Server Model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_sensor_client_get_state_t
  #include <esp_ble_mesh_sensor_model_api.h>

  Sensor Client Model get message union.

  Public Members

  esp_ble_mesh_sensor_descriptor_get_t descriptor_get

    For ESP_BLE_MESH_MODEL_OP_SENSOR_DESCRIPTOR_GET

  esp_ble_mesh_sensor_cadence_get_t cadence_get

    For ESP_BLE_MESH_MODEL_OP_SENSOR_CADENCE_GET

  esp_ble_mesh_sensor_settings_get_t settings_get

    For ESP_BLE_MESH_MODEL_OP_SENSOR_SETTINGS_GET

  esp_ble_mesh_sensor_setting_get_t setting_get

    For ESP_BLE_MESH_MODEL_OP_SENSOR_SETTING_GET

  esp_ble_mesh_sensor_get_t sensor_get

    For ESP_BLE_MESH_MODEL_OP_SENSOR_GET

  esp_ble_mesh_sensor_column_get_t column_get

    For ESP_BLE_MESH_MODEL_OP_SENSOR_COLUMN_GET

  esp_ble_mesh_sensor_series_get_t series_get

    For ESP_BLE_MESH_MODEL_OP_SENSOR_SERIES_GET

union esp_ble_mesh_sensor_client_set_state_t
  #include <esp_ble_mesh_sensor_model_api.h>

  Sensor Client Model set message union.

  Public Members

  esp_ble_mesh_sensor_cadence_set_t cadence_set

    For ESP_BLE_MESH_MODEL_OP_SENSOR_CADENCE_SET & ESP_BLE_MESH_MODEL_OP_SENSOR_CADENCE_SET_UNACK

  esp_ble_mesh_sensor_setting_set_t setting_set

    For ESP_BLE_MESH_MODEL_OP_SENSOR_SETTING_SET & ESP_BLE_MESH_MODEL_OP_SENSOR_SETTING_SET_UNACK

union esp_ble_mesh_sensor_client_status_cb_t
  #include <esp_ble_mesh_sensor_model_api.h>

  Sensor Client Model received message union.

  Public Members

  esp_ble_mesh_sensor_descriptor_status_cb_t descriptor_status

    For ESP_BLE_MESH_MODEL_OP_SENSOR_DESCRIPTOR_STATUS

  esp_ble_mesh_sensor_cadence_status_cb_t cadence_status

    For ESP_BLE_MESH_MODEL_OP_SENSOR_CADENCE_STATUS

  esp_ble_mesh_sensor_settings_status_cb_t settings_status

    For ESP_BLE_MESH_MODEL_OP_SENSOR_SETTINGS_STATUS

  esp_ble_mesh_sensor_setting_status_cb_t setting_status

    For ESP_BLE_MESH_MODEL_OP_SENSOR_SETTING_STATUS

  esp_ble_mesh_sensor_status_cb_t sensor_status

    For ESP_BLE_MESH_MODEL_OP_SENSOR_STATUS

  esp_ble_mesh_sensor_column_status_cb_t column_status

    For ESP_BLE_MESH_MODEL_OP_SENSOR_COLUMN_STATUS

  esp_ble_mesh_sensor_series_status_cb_t series_status

    For ESP_BLE_MESH_MODEL_OP_SENSOR_SERIES_STATUS

union esp_ble_mesh_sensor_server_state_change_t
  #include <esp_ble_mesh_sensor_model_api.h>

  Sensor Server Model state change value union.

  Public Members

  esp_ble_mesh_state_change_sensor_cadence_set_t sensor_cadence_set

    The recv_op in ctx can be used to decide which state is changed. Sensor Cadence Set

  esp_ble_mesh_state_change_sensor_setting_set_t sensor_setting_set

    Sensor Setting Set

union esp_ble_mesh_sensor_server_recv_get_msg_t
  #include <esp_ble_mesh_sensor_model_api.h>

  Sensor Server Model received get message union.

  Public Members

  esp_ble_mesh_server_recv_sensor_descriptor_get_t sensor_descriptor

    Sensor Descriptor Get

  esp_ble_mesh_server_recv_sensor_cadence_get_t sensor_cadence

    Sensor Cadence Get

  esp_ble_mesh_server_recv_sensor_settings_get_t sensor_settings

    Sensor Settings Get

  esp_ble_mesh_server_recv_sensor_setting_get_t sensor_setting

    Sensor Setting Get

  esp_ble_mesh_server_recv_sensor_get_t sensor_data

    Sensor Get

  esp_ble_mesh_server_recv_sensor_column_get_t sensor_column

    Sensor Column Get

  esp_ble_mesh_server_recv_sensor_series_get_t sensor_series

    Sensor Series Get

union esp_ble_mesh_sensor_server_recv_set_msg_t
  #include <esp_ble_mesh_sensor_model_api.h>

  Sensor Server Model received set message union.

  Public Members

  esp_ble_mesh_server_recv_sensor_cadence_set_t sensor_cadence

    Sensor Cadence Set

  esp_ble_mesh_server_recv_sensor_setting_set_t sensor_setting

    Sensor Setting Set

union esp_ble_mesh_sensor_server_cb_value_t
  #include <esp_ble_mesh_sensor_model_api.h>

  Sensor Server Model callback value union.

  Public Members

  esp_ble_mesh_sensor_server_state_change_t state_change

    ESP_BLE_MESH_SENSOR_SERVER_STATE_CHANGE_EVT

  esp_ble_mesh_sensor_server_recv_get_msg_t get

    ESP_BLE_MESH_SENSOR_SERVER_RECV_GET_MSG_EVT

  esp_ble_mesh_sensor_server_recv_set_msg_t set

    ESP_BLE_MESH_SENSOR_SERVER_RECV_SET_MSG_EVT

### Structures

struct esp_ble_mesh_sensor_descriptor_get_t

  Bluetooth Mesh Sensor Client Model Get and Set parameters structure.

  Parameters of Sensor Descriptor Get

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t property_id

    Property ID of a sensor (optional)

struct esp_ble_mesh_sensor_cadence_get_t

  Parameter of Sensor Cadence Get

  Public Members

  uint16_t property_id

    Property ID of a sensor

struct esp_ble_mesh_sensor_cadence_set_t

  Parameters of Sensor Cadence Set

  Public Members

  uint16_t property_id

    Property ID for the sensor

  uint8_t fast_cadence_period_divisor

    Divisor for the publish period

  uint8_t status_trigger_type

    The unit and format of the Status Trigger Delta fields

  struct net_buf_simple *status_trigger_delta_down

    Delta down value that triggers a status message

  struct net_buf_simple *status_trigger_delta_up

    Delta up value that triggers a status message

  uint8_t status_min_interval

    Minimum interval between two consecutive Status messages

  struct net_buf_simple *fast_cadence_low

    Low value for the fast cadence range

  struct net_buf_simple *fast_cadence_high

    Fast value for the fast cadence range

struct esp_ble_mesh_sensor_settings_get_t

  Parameter of Sensor Settings Get

  Public Members

  uint16_t sensor_property_id

    Property ID of a sensor

struct esp_ble_mesh_sensor_setting_get_t

  Parameters of Sensor Setting Get

  Public Members

  uint16_t sensor_property_id

    Property ID of a sensor

  uint16_t sensor_setting_property_id

    Setting ID identifying a setting within a sensor

struct esp_ble_mesh_sensor_setting_set_t

  Parameters of Sensor Setting Set

  Public Members

  uint16_t sensor_property_id

    Property ID identifying a sensor

  uint16_t sensor_setting_property_id

    Setting ID identifying a setting within a sensor

  struct net_buf_simple *sensor_setting_raw

    Raw value for the setting

struct esp_ble_mesh_sensor_get_t

  Parameters of Sensor Get

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t property_id

    Property ID for the sensor (optional)

struct esp_ble_mesh_sensor_column_get_t

  Parameters of Sensor Column Get

  Public Members

  uint16_t property_id

    Property identifying a sensor

  struct net_buf_simple *raw_value_x

    Raw value identifying a column

struct esp_ble_mesh_sensor_series_get_t

  Parameters of Sensor Series Get

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t property_id

    Property identifying a sensor

  struct net_buf_simple *raw_value_x1

    Raw value identifying a starting column (optional)

  struct net_buf_simple *raw_value_x2

    Raw value identifying an ending column (C.1)

struct esp_ble_mesh_sensor_descriptor_status_cb_t

  Bluetooth Mesh Sensor Client Model Get and Set callback parameters structure.

  Parameter of Sensor Descriptor Status

  Public Members

  struct net_buf_simple *descriptor

    Sequence of 8-octet sensor descriptors (optional)

struct esp_ble_mesh_sensor_cadence_status_cb_t

  Parameters of Sensor Cadence Status

  Public Members

  uint16_t property_id

    Property for the sensor

  struct net_buf_simple *sensor_cadence_value

    Value of sensor cadence state

struct esp_ble_mesh_sensor_settings_status_cb_t

  Parameters of Sensor Settings Status

  Public Members

  uint16_t sensor_property_id

    Property ID identifying a sensor

  struct net_buf_simple *sensor_setting_property_ids

    A sequence of N sensor setting property IDs (optional)

struct esp_ble_mesh_sensor_setting_status_cb_t

  Parameters of Sensor Setting Status

  Public Members

  bool op_en

    Indicate id optional parameters are included

  uint16_t sensor_property_id

    Property ID identifying a sensor

  uint16_t sensor_setting_property_id

    Setting ID identifying a setting within a sensor

  uint8_t sensor_setting_access

    Read/Write access rights for the setting (optional)

  struct net_buf_simple *sensor_setting_raw

    Raw value for the setting

struct esp_ble_mesh_sensor_status_cb_t

  Parameter of Sensor Status

  Public Members

  struct net_buf_simple *marshalled_sensor_data

    Value of sensor data state (optional)

struct esp_ble_mesh_sensor_column_status_cb_t

  Parameters of Sensor Column Status

  Public Members

  uint16_t property_id

    Property identifying a sensor and the Y axis

  struct net_buf_simple *sensor_column_value

    Left values of sensor column status

struct esp_ble_mesh_sensor_series_status_cb_t

  Parameters of Sensor Series Status

  Public Members

  uint16_t property_id

    Property identifying a sensor and the Y axis

  struct net_buf_simple *sensor_series_value

    Left values of sensor series status

struct esp_ble_mesh_sensor_client_cb_param_t

  Sensor Client Model callback parameters

  Public Members

  int error_code

    0: success, otherwise failure. For the error code values please refer to errno.h file. A negative sign is added to the standard error codes in errno.h.

  esp_ble_mesh_client_common_param_t *params

    The client common parameters.

  esp_ble_mesh_sensor_client_status_cb_t status_cb

    The sensor status message callback values

struct esp_ble_mesh_sensor_descriptor_t

  Parameters of Sensor Descriptor state

  Public Members

  uint32_t positive_tolerance

    The value of Sensor Positive Tolerance field

  uint32_t negative_tolerance

    The value of Sensor Negative Tolerance field

  uint32_t sampling_function

    The value of Sensor Sampling Function field

  uint8_t measure_period

    The value of Sensor Measurement Period field

  uint8_t update_interval

    The value of Sensor Update Interval field

struct esp_ble_mesh_sensor_setting_t

  Parameters of Sensor Setting state

  Public Members

  uint16_t property_id

    The value of Sensor Setting Property ID field

  uint8_t access

    The value of Sensor Setting Access field

  struct net_buf_simple *raw

    The value of Sensor Setting Raw field

struct esp_ble_mesh_sensor_cadence_t

  Parameters of Sensor Cadence state

  Public Members

  uint8_t period_divisor

    The value of Fast Cadence Period Divisor field

  uint8_t trigger_type

    The value of Status Trigger Type field

  struct net_buf_simple *trigger_delta_down

    Note: The parameter "size" in trigger_delta_down, trigger_delta_up, fast_cadence_low & fast_cadence_high indicates the exact length of these four parameters, and they are associated with the Sensor Property ID. Users need to initialize the "size" precisely. The value of Status Trigger Delta Down field

  struct net_buf_simple *trigger_delta_up

    The value of Status Trigger Delta Up field

  uint8_t min_interval

    The value of Status Min Interval field

  struct net_buf_simple *fast_cadence_low

    The value of Fast Cadence Low field

  struct net_buf_simple *fast_cadence_high

    The value of Fast Cadence High field

struct esp_ble_mesh_sensor_data_t

  Parameters of Sensor Data state

  Public Members

  uint8_t format

    Format A: The Length field is a 1-based uint4 value (valid range 0x0–0xF, representing range of 1 – 16). Format B: The Length field is a 1-based uint7 value (valid range 0x0–0x7F, representing range of 1 – 127). The value 0x7F represents a length of zero. The value of the Sensor Data format

  uint8_t length

    The value of the Sensor Data length

  struct net_buf_simple *raw_value

    The value of Sensor Data raw value

struct esp_ble_mesh_sensor_series_column_t

  Parameters of Sensor Series Column state

  Public Members

  struct net_buf_simple *raw_value_x

    The value of Sensor Raw Value X field

  struct net_buf_simple *column_width

    The value of Sensor Column Width field

  struct net_buf_simple *raw_value_y

    The value of Sensor Raw Value Y field

struct esp_ble_mesh_sensor_state_t

  Parameters of Sensor states

  Public Members

  uint16_t sensor_property_id

    The value of Sensor Property ID field

  esp_ble_mesh_sensor_descriptor_t descriptor

    Parameters of the Sensor Descriptor state

  const uint8_t setting_count

    Multiple Sensor Setting states may be present for each sensor. The Sensor Setting Property ID values shall be unique for each Sensor Property ID that identifies a sensor within an element.

  esp_ble_mesh_sensor_setting_t *settings

    Parameters of the Sensor Setting state

  esp_ble_mesh_sensor_cadence_t *cadence

    The Sensor Cadence state may be not supported by sensors based on device properties referencing "non-scalar characteristics" such as "histograms" or "composite characteristics". Parameters of the Sensor Cadence state

  esp_ble_mesh_sensor_data_t sensor_data

    Parameters of the Sensor Data state

  esp_ble_mesh_sensor_series_column_t series_column

    Parameters of the Sensor Series Column state

struct esp_ble_mesh_sensor_srv_t

  User data of Sensor Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Sensor Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  const uint8_t state_count

    Sensor state count

  esp_ble_mesh_sensor_state_t *states

    Parameters of the Sensor states

struct esp_ble_mesh_sensor_setup_srv_t

  User data of Sensor Setup Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Sensor Setup Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  const uint8_t state_count

    Sensor state count

  esp_ble_mesh_sensor_state_t *states

    Parameters of the Sensor states

struct esp_ble_mesh_state_change_sensor_cadence_set_t

  Parameters of Sensor Cadence Set state change event

  Public Members

  uint16_t property_id

    The value of Sensor Property ID state

  uint8_t period_divisor

    The value of Fast Cadence Period Divisor state

  uint8_t trigger_type

    The value of Status Trigger Type state

  struct net_buf_simple *trigger_delta_down

    The value of Status Trigger Delta Down state

  struct net_buf_simple *trigger_delta_up

    The value of Status Trigger Delta Up state

  uint8_t min_interval

    The value of Status Min Interval state

  struct net_buf_simple *fast_cadence_low

    The value of Fast Cadence Low state

  struct net_buf_simple *fast_cadence_high

    The value of Fast Cadence High state

struct esp_ble_mesh_state_change_sensor_setting_set_t

  Parameters of Sensor Setting Set state change event

  Public Members

  uint16_t property_id

    The value of Sensor Property ID state

  uint16_t setting_property_id

    The value of Sensor Setting Property ID state

  struct net_buf_simple *setting_value

    The value of Sensor Property Value state

struct esp_ble_mesh_server_recv_sensor_descriptor_get_t

  Context of the received Sensor Descriptor Get message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t property_id

    Property ID of a sensor (optional)

struct esp_ble_mesh_server_recv_sensor_cadence_get_t

  Context of the received Sensor Cadence Get message

  Public Members

  uint16_t property_id

    Property ID of a sensor

struct esp_ble_mesh_server_recv_sensor_settings_get_t

  Context of the received Sensor Settings Get message

  Public Members

  uint16_t property_id

    Property ID of a sensor

struct esp_ble_mesh_server_recv_sensor_setting_get_t

  Context of the received Sensor Setting Get message

  Public Members

  uint16_t property_id

    Property ID of a sensor

  uint16_t setting_property_id

    Setting ID identifying a setting within a sensor

struct esp_ble_mesh_server_recv_sensor_get_t

  Context of the received Sensor Get message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t property_id

    Property ID for the sensor (optional)

struct esp_ble_mesh_server_recv_sensor_column_get_t

  Context of the received Sensor Column Get message

  Public Members

  uint16_t property_id

    Property identifying a sensor

  struct net_buf_simple *raw_value_x

    Raw value identifying a column

struct esp_ble_mesh_server_recv_sensor_series_get_t

  Context of the received Sensor Series Get message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t property_id

    Property identifying a sensor

  struct net_buf_simple *raw_value

    Raw value containing X1 and X2 (optional)

struct esp_ble_mesh_server_recv_sensor_cadence_set_t

  Context of the received Sensor Cadence Set message

  Public Members

  uint16_t property_id

    Property ID for the sensor

  struct net_buf_simple *cadence

    Value of Sensor Cadence state

struct esp_ble_mesh_server_recv_sensor_setting_set_t

  Context of the received Sensor Setting Set message

  Public Members

  uint16_t property_id

    Property ID identifying a sensor

  uint16_t setting_property_id

    Setting ID identifying a setting within a sensor

  struct net_buf_simple *setting_raw

    Raw value for the setting

struct esp_ble_mesh_sensor_server_cb_param_t

  Sensor Server Model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to Sensor Server Models

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received messages

  esp_ble_mesh_sensor_server_cb_value_t value

    Value of the received Sensor Messages

### Macros

ESP_BLE_MESH_MODEL_SENSOR_CLI(cli_pub, cli_data)

  Define a new Sensor Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Sensor Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Sensor Client Model instance.

ESP_BLE_MESH_MODEL_SENSOR_SRV(srv_pub, srv_data)

  Sensor Server Models related context.

  Define a new Sensor Server Model.

  备注

  1. The Sensor Server model is a root model. When this model is present on an element, the corresponding Sensor Setup Server model shall also be present.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_sensor_srv_t.

  返回:

    New Sensor Server Model instance.

ESP_BLE_MESH_MODEL_SENSOR_SETUP_SRV(srv_pub, srv_data)

  Define a new Sensor Setup Server Model.

  备注

  1. The Sensor Setup Server model extends the Sensor Server model.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_sensor_setup_srv_t.

  返回:

    New Sensor Setup Server Model instance.

ESP_BLE_MESH_INVALID_SENSOR_PROPERTY_ID

  Invalid Sensor Property ID

ESP_BLE_MESH_SENSOR_PROPERTY_ID_LEN

  Length of Sensor Property ID

ESP_BLE_MESH_SENSOR_DESCRIPTOR_LEN

  Length of Sensor Descriptor state

ESP_BLE_MESH_SENSOR_UNSPECIFIED_POS_TOLERANCE

  Unspecified Sensor Positive Tolerance

ESP_BLE_MESH_SENSOR_UNSPECIFIED_NEG_TOLERANCE

  Unspecified Sensor Negative Tolerance

ESP_BLE_MESH_SENSOR_NOT_APPL_MEASURE_PERIOD

  Not applicable Sensor Measurement Period

ESP_BLE_MESH_SENSOR_NOT_APPL_UPDATE_INTERVAL

  Not applicable Sensor Update Interval

ESP_BLE_MESH_INVALID_SENSOR_SETTING_PROPERTY_ID

  Invalid Sensor Setting Property ID

ESP_BLE_MESH_SENSOR_SETTING_PROPERTY_ID_LEN

  Length of Sensor Setting Property ID

ESP_BLE_MESH_SENSOR_SETTING_ACCESS_LEN

  Length of Sensor Setting Access

ESP_BLE_MESH_SENSOR_SETTING_ACCESS_READ

  Sensor Setting Access - Read

ESP_BLE_MESH_SENSOR_SETTING_ACCESS_READ_WRITE

  Sensor Setting Access - Read & Write

ESP_BLE_MESH_SENSOR_DIVISOR_TRIGGER_TYPE_LEN

  Length of Sensor Divisor Trigger Type

ESP_BLE_MESH_SENSOR_STATUS_MIN_INTERVAL_LEN

  Length of Sensor Status Min Interval

ESP_BLE_MESH_SENSOR_PERIOD_DIVISOR_MAX_VALUE

  Maximum value of Sensor Period Divisor

ESP_BLE_MESH_SENSOR_STATUS_MIN_INTERVAL_MAX

  Maximum value of Sensor Status Min Interval

ESP_BLE_MESH_SENSOR_STATUS_TRIGGER_TYPE_CHAR

  Sensor Status Trigger Type - Format Type of the characteristic that the Sensor Property ID state references

ESP_BLE_MESH_SENSOR_STATUS_TRIGGER_TYPE_UINT16

  Sensor Status Trigger Type - Format Type "uint16"

ESP_BLE_MESH_SENSOR_DATA_FORMAT_A

  Sensor Data Format A

ESP_BLE_MESH_SENSOR_DATA_FORMAT_B

  Sensor Data Format B

ESP_BLE_MESH_SENSOR_DATA_FORMAT_A_MPID_LEN

  MPID length of Sensor Data Format A

ESP_BLE_MESH_SENSOR_DATA_FORMAT_B_MPID_LEN

  MPID length of Sensor Data Format B

ESP_BLE_MESH_SENSOR_DATA_ZERO_LEN

  Zero length of Sensor Data.

  Note: The Length field is a 1-based uint7 value (valid range 0x0–0x7F, representing range of 1–127). The value 0x7F represents a length of zero.

ESP_BLE_MESH_GET_SENSOR_DATA_FORMAT(_data)

  Get format of the sensor data.

  备注

  Multiple sensor data may be concatenated. Make sure the _data pointer is updated before getting the format of the corresponding sensor data.

  参数:

    - _data -- Pointer to the start of the sensor data.

  返回:

    Format of the sensor data.

ESP_BLE_MESH_GET_SENSOR_DATA_LENGTH(_data, _fmt)

  Get length of the sensor data.

  备注

  Multiple sensor data may be concatenated. Make sure the _data pointer is updated before getting the length of the corresponding sensor data.

  参数:

    - _data -- Pointer to the start of the sensor data.

    - _fmt -- Format of the sensor data.

  返回:

    Length (zero-based) of the sensor data.

ESP_BLE_MESH_GET_SENSOR_DATA_PROPERTY_ID(_data, _fmt)

  Get Sensor Property ID of the sensor data.

  备注

  Multiple sensor data may be concatenated. Make sure the _data pointer is updated before getting Sensor Property ID of the corresponding sensor data.

  参数:

    - _data -- Pointer to the start of the sensor data.

    - _fmt -- Format of the sensor data.

  返回:

    Sensor Property ID of the sensor data.

ESP_BLE_MESH_SENSOR_DATA_FORMAT_A_MPID(_len, _id)

  Generate a MPID value for sensor data with Format A.

  备注

  1. The Format field is 0b0 and indicates that Format A is used.

  1. The Length field is a 1-based uint4 value (valid range 0x0–0xF, representing range of 1–16).

  2. The Property ID is an 11-bit bit field representing 11 LSb of a Property ID.

  3. This format may be used for Property Values that are not longer than 16 octets and for Property IDs less than 0x0800.

  参数:

    - _len -- Length of Sensor Raw value.

    - _id -- Sensor Property ID.

  返回:

    2-octet MPID value for sensor data with Format A.

ESP_BLE_MESH_SENSOR_DATA_FORMAT_B_MPID(_len, _id)

  Generate a MPID value for sensor data with Format B.

  备注

  1. The Format field is 0b1 and indicates Format B is used.

  1. The Length field is a 1-based uint7 value (valid range 0x0–0x7F, representing range of 1–127). The value 0x7F represents a length of zero.

  2. The Property ID is a 16-bit bit field representing a Property ID.

  3. This format may be used for Property Values not longer than 128 octets and for any Property IDs. Property values longer than 128 octets are not supported by the Sensor Status message.

  4. Exclude the generated 1-octet value, the 2-octet Sensor Property ID

  参数:

    - _len -- Length of Sensor Raw value.

    - _id -- Sensor Property ID.

  返回:

    3-octet MPID value for sensor data with Format B.

### Type Definitions

typedef void (*esp_ble_mesh_sensor_client_cb_t)(esp_ble_mesh_sensor_client_cb_event_t event, esp_ble_mesh_sensor_client_cb_param_t *param)

  Bluetooth Mesh Sensor Client Model function.

  Sensor Client Model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_sensor_server_cb_t)(esp_ble_mesh_sensor_server_cb_event_t event, esp_ble_mesh_sensor_server_cb_param_t *param)

  Bluetooth Mesh Sensor Server Model function.

  Sensor Server Model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_sensor_client_cb_event_t

  This enum value is the event of Sensor Client Model

  Values:

  enumerator ESP_BLE_MESH_SENSOR_CLIENT_GET_STATE_EVT
  enumerator ESP_BLE_MESH_SENSOR_CLIENT_SET_STATE_EVT
  enumerator ESP_BLE_MESH_SENSOR_CLIENT_PUBLISH_EVT
  enumerator ESP_BLE_MESH_SENSOR_CLIENT_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_SENSOR_CLIENT_EVT_MAX

enum esp_ble_mesh_sensor_sample_func

  This enum value is value of Sensor Sampling Function

  Values:

  enumerator ESP_BLE_MESH_SAMPLE_FUNC_UNSPECIFIED
  enumerator ESP_BLE_MESH_SAMPLE_FUNC_INSTANTANEOUS
  enumerator ESP_BLE_MESH_SAMPLE_FUNC_ARITHMETIC_MEAN
  enumerator ESP_BLE_MESH_SAMPLE_FUNC_RMS
  enumerator ESP_BLE_MESH_SAMPLE_FUNC_MAXIMUM
  enumerator ESP_BLE_MESH_SAMPLE_FUNC_MINIMUM
  enumerator ESP_BLE_MESH_SAMPLE_FUNC_ACCUMULATED
  enumerator ESP_BLE_MESH_SAMPLE_FUNC_COUNT

enum esp_ble_mesh_sensor_server_cb_event_t

  This enum value is the event of Sensor Server Model

  Values:

  enumerator ESP_BLE_MESH_SENSOR_SERVER_STATE_CHANGE_EVT

    1. When get_auto_rsp is set to ESP_BLE_MESH_SERVER_AUTO_RSP, no event will be callback to the application layer when Sensor Get messages are received.

    2. When set_auto_rsp is set to ESP_BLE_MESH_SERVER_AUTO_RSP, this event will be callback to the application layer when Sensor Set/Set Unack messages are received.

  enumerator ESP_BLE_MESH_SENSOR_SERVER_RECV_GET_MSG_EVT

    When get_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, this event will be callback to the application layer when Sensor Get messages are received.

  enumerator ESP_BLE_MESH_SENSOR_SERVER_RECV_SET_MSG_EVT

    When set_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, this event will be callback to the application layer when Sensor Set/Set Unack messages are received.

  enumerator ESP_BLE_MESH_SENSOR_SERVER_EVT_MAX

### Time and Scenes Client/Server Models

### Header File

- components/bt/esp_ble_mesh/api/models/include/esp_ble_mesh_time_scene_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_time_scene_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_time_scene_client_callback(esp_ble_mesh_time_scene_client_cb_t callback)

  Register BLE Mesh Time Scene Client Model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_time_scene_client_get_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_time_scene_client_get_state_t *get_state)

  Get the value of Time Scene Server Model states using the Time Scene Client Model get messages.

  备注

  If you want to know the opcodes and corresponding meanings accepted by this API, please refer to esp_ble_mesh_time_scene_message_opcode_t in esp_ble_mesh_defs.h

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - get_state -- [in] Pointer to time scene get message value. Shall not be set to NULL.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_time_scene_client_set_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_time_scene_client_set_state_t *set_state)

  Set the value of Time Scene Server Model states using the Time Scene Client Model set messages.

  备注

  If you want to know the opcodes and corresponding meanings accepted by this API, please refer to esp_ble_mesh_time_scene_message_opcode_t in esp_ble_mesh_defs.h

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - set_state -- [in] Pointer to time scene set message value. Shall not be set to NULL.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_time_scene_server_callback(esp_ble_mesh_time_scene_server_cb_t callback)

  Register BLE Mesh Time and Scenes Server Model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_time_scene_client_get_state_t
  #include <esp_ble_mesh_time_scene_model_api.h>

  Time Scene Client Model get message union.

  Public Members

  esp_ble_mesh_scheduler_act_get_t scheduler_act_get

    For ESP_BLE_MESH_MODEL_OP_SCHEDULER_ACT_GET

union esp_ble_mesh_time_scene_client_set_state_t
  #include <esp_ble_mesh_time_scene_model_api.h>

  Time Scene Client Model set message union.

  Public Members

  esp_ble_mesh_time_set_t time_set

    For ESP_BLE_MESH_MODEL_OP_TIME_SET

  esp_ble_mesh_time_zone_set_t time_zone_set

    For ESP_BLE_MESH_MODEL_OP_TIME_ZONE_SET

  esp_ble_mesh_tai_utc_delta_set_t tai_utc_delta_set

    For ESP_BLE_MESH_MODEL_OP_TAI_UTC_DELTA_SET

  esp_ble_mesh_time_role_set_t time_role_set

    For ESP_BLE_MESH_MODEL_OP_TIME_ROLE_SET

  esp_ble_mesh_scene_store_t scene_store

    For ESP_BLE_MESH_MODEL_OP_SCENE_STORE & ESP_BLE_MESH_MODEL_OP_SCENE_STORE_UNACK

  esp_ble_mesh_scene_recall_t scene_recall

    For ESP_BLE_MESH_MODEL_OP_SCENE_RECALL & ESP_BLE_MESH_MODEL_OP_SCENE_RECALL_UNACK

  esp_ble_mesh_scene_delete_t scene_delete

    For ESP_BLE_MESH_MODEL_OP_SCENE_DELETE & ESP_BLE_MESH_MODEL_OP_SCENE_DELETE_UNACK

  esp_ble_mesh_scheduler_act_set_t scheduler_act_set

    For ESP_BLE_MESH_MODEL_OP_SCHEDULER_ACT_SET & ESP_BLE_MESH_MODEL_OP_SCHEDULER_ACT_SET_UNACK

union esp_ble_mesh_time_scene_client_status_cb_t
  #include <esp_ble_mesh_time_scene_model_api.h>

  Time Scene Client Model received message union.

  Public Members

  esp_ble_mesh_time_status_cb_t time_status

    For ESP_BLE_MESH_MODEL_OP_TIME_STATUS

  esp_ble_mesh_time_zone_status_cb_t time_zone_status

    For ESP_BLE_MESH_MODEL_OP_TIME_ZONE_STATUS

  esp_ble_mesh_tai_utc_delta_status_cb_t tai_utc_delta_status

    For ESP_BLE_MESH_MODEL_OP_TAI_UTC_DELTA_STATUS

  esp_ble_mesh_time_role_status_cb_t time_role_status

    For ESP_BLE_MESH_MODEL_OP_TIME_ROLE_STATUS

  esp_ble_mesh_scene_status_cb_t scene_status

    For ESP_BLE_MESH_MODEL_OP_SCENE_STATUS

  esp_ble_mesh_scene_register_status_cb_t scene_register_status

    For ESP_BLE_MESH_MODEL_OP_SCENE_REGISTER_STATUS

  esp_ble_mesh_scheduler_status_cb_t scheduler_status

    For ESP_BLE_MESH_MODEL_OP_SCHEDULER_STATUS

  esp_ble_mesh_scheduler_act_status_cb_t scheduler_act_status

    For ESP_BLE_MESH_MODEL_OP_SCHEDULER_ACT_STATUS

union esp_ble_mesh_time_scene_server_state_change_t
  #include <esp_ble_mesh_time_scene_model_api.h>

  Time Scene Server Model state change value union.

  Public Members

  esp_ble_mesh_state_change_time_set_t time_set

    The recv_op in ctx can be used to decide which state is changed. Time Set

  esp_ble_mesh_state_change_time_status_t time_status

    Time Status

  esp_ble_mesh_state_change_time_zone_set_t time_zone_set

    Time Zone Set

  esp_ble_mesh_state_change_tai_utc_delta_set_t tai_utc_delta_set

    TAI UTC Delta Set

  esp_ble_mesh_state_change_time_role_set_t time_role_set

    Time Role Set

  esp_ble_mesh_state_change_scene_store_t scene_store

    Scene Store

  esp_ble_mesh_state_change_scene_recall_t scene_recall

    Scene Recall

  esp_ble_mesh_state_change_scene_delete_t scene_delete

    Scene Delete

  esp_ble_mesh_state_change_scheduler_act_set_t scheduler_act_set

    Scheduler Action Set

union esp_ble_mesh_time_scene_server_recv_get_msg_t
  #include <esp_ble_mesh_time_scene_model_api.h>

  Time Scene Server Model received get message union.

  Public Members

  esp_ble_mesh_server_recv_scheduler_act_get_t scheduler_act

    Scheduler Action Get

union esp_ble_mesh_time_scene_server_recv_set_msg_t
  #include <esp_ble_mesh_time_scene_model_api.h>

  Time Scene Server Model received set message union.

  Public Members

  esp_ble_mesh_server_recv_time_set_t time

    Time Set

  esp_ble_mesh_server_recv_time_zone_set_t time_zone

    Time Zone Set

  esp_ble_mesh_server_recv_tai_utc_delta_set_t tai_utc_delta

    TAI-UTC Delta Set

  esp_ble_mesh_server_recv_time_role_set_t time_role

    Time Role Set

  esp_ble_mesh_server_recv_scene_store_t scene_store

    Scene Store/Scene Store Unack

  esp_ble_mesh_server_recv_scene_recall_t scene_recall

    Scene Recall/Scene Recall Unack

  esp_ble_mesh_server_recv_scene_delete_t scene_delete

    Scene Delete/Scene Delete Unack

  esp_ble_mesh_server_recv_scheduler_act_set_t scheduler_act

    Scheduler Action Set/Scheduler Action Set Unack

union esp_ble_mesh_time_scene_server_recv_status_msg_t
  #include <esp_ble_mesh_time_scene_model_api.h>

  Time Scene Server Model received status message union.

  Public Members

  esp_ble_mesh_server_recv_time_status_t time_status

    Time Status

union esp_ble_mesh_time_scene_server_cb_value_t
  #include <esp_ble_mesh_time_scene_model_api.h>

  Time Scene Server Model callback value union.

  Public Members

  esp_ble_mesh_time_scene_server_state_change_t state_change

    ESP_BLE_MESH_TIME_SCENE_SERVER_STATE_CHANGE_EVT

  esp_ble_mesh_time_scene_server_recv_get_msg_t get

    ESP_BLE_MESH_TIME_SCENE_SERVER_RECV_GET_MSG_EVT

  esp_ble_mesh_time_scene_server_recv_set_msg_t set

    ESP_BLE_MESH_TIME_SCENE_SERVER_RECV_SET_MSG_EVT

  esp_ble_mesh_time_scene_server_recv_status_msg_t status

    ESP_BLE_MESH_TIME_SCENE_SERVER_RECV_STATUS_MSG_EVT

### Structures

struct esp_ble_mesh_time_set_t

  Bluetooth Mesh Time Scene Client Model Get and Set parameters structure.

  Parameters of Time Set

  Public Members

  uint8_t tai_seconds[5]

    The current TAI time in seconds

  uint8_t sub_second

    The sub-second time in units of 1/256 second

  uint8_t uncertainty

    The estimated uncertainty in 10-millisecond steps

  uint16_t time_authority

    0 = No Time Authority, 1 = Time Authority

  uint16_t tai_utc_delta

    Current difference between TAI and UTC in seconds

  uint8_t time_zone_offset

    The local time zone offset in 15-minute increments

struct esp_ble_mesh_time_zone_set_t

  Parameters of Time Zone Set

  Public Members

  uint8_t time_zone_offset_new

    Upcoming local time zone offset

  uint8_t tai_zone_change[5]

    TAI Seconds time of the upcoming Time Zone Offset change

struct esp_ble_mesh_tai_utc_delta_set_t

  Parameters of TAI-UTC Delta Set

  Public Members

  uint16_t tai_utc_delta_new

    Upcoming difference between TAI and UTC in seconds

  uint16_t padding

    Always 0b0. Other values are Prohibited.

  uint8_t tai_delta_change[5]

    TAI Seconds time of the upcoming TAI-UTC Delta change

struct esp_ble_mesh_time_role_set_t

  Parameter of Time Role Set

  Public Members

  uint8_t time_role

    The Time Role for the element

struct esp_ble_mesh_scene_store_t

  Parameter of Scene Store

  Public Members

  uint16_t scene_number

    The number of scenes to be stored

struct esp_ble_mesh_scene_recall_t

  Parameters of Scene Recall

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t scene_number

    The number of scenes to be recalled

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_scene_delete_t

  Parameter of Scene Delete

  Public Members

  uint16_t scene_number

    The number of scenes to be deleted

struct esp_ble_mesh_scheduler_act_get_t

  Parameter of Scheduler Action Get

  Public Members

  uint8_t index

    Index of the Schedule Register entry to get

struct esp_ble_mesh_scheduler_act_set_t

  Parameters of Scheduler Action Set

  Public Members

  uint64_t index

    Index of the Schedule Register entry to set

  uint64_t year

    Scheduled year for the action

  uint64_t month

    Scheduled month for the action

  uint64_t day

    Scheduled day of the month for the action

  uint64_t hour

    Scheduled hour for the action

  uint64_t minute

    Scheduled minute for the action

  uint64_t second

    Scheduled second for the action

  uint64_t day_of_week

    Schedule days of the week for the action

  uint64_t action

    Action to be performed at the scheduled time

  uint64_t trans_time

    Transition time for this action

  uint16_t scene_number

    Transition time for this action

struct esp_ble_mesh_time_status_cb_t

  Bluetooth Mesh Time Scene Client Model Get and Set callback parameters structure.

  Parameters of Time Status

  Public Members

  uint8_t tai_seconds[5]

    The current TAI time in seconds

  uint8_t sub_second

    The sub-second time in units of 1/256 second

  uint8_t uncertainty

    The estimated uncertainty in 10-millisecond steps

  uint16_t time_authority

    0 = No Time Authority, 1 = Time Authority

  uint16_t tai_utc_delta

    Current difference between TAI and UTC in seconds

  uint8_t time_zone_offset

    The local time zone offset in 15-minute increments

struct esp_ble_mesh_time_zone_status_cb_t

  Parameters of Time Zone Status

  Public Members

  uint8_t time_zone_offset_curr

    Current local time zone offset

  uint8_t time_zone_offset_new

    Upcoming local time zone offset

  uint8_t tai_zone_change[5]

    TAI Seconds time of the upcoming Time Zone Offset change

struct esp_ble_mesh_tai_utc_delta_status_cb_t

  Parameters of TAI-UTC Delta Status

  Public Members

  uint16_t tai_utc_delta_curr

    Current difference between TAI and UTC in seconds

  uint16_t padding_1

    Always 0b0. Other values are Prohibited.

  uint16_t tai_utc_delta_new

    Upcoming difference between TAI and UTC in seconds

  uint16_t padding_2

    Always 0b0. Other values are Prohibited.

  uint8_t tai_delta_change[5]

    TAI Seconds time of the upcoming TAI-UTC Delta change

struct esp_ble_mesh_time_role_status_cb_t

  Parameter of Time Role Status

  Public Members

  uint8_t time_role

    The Time Role for the element

struct esp_ble_mesh_scene_status_cb_t

  Parameters of Scene Status

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint8_t status_code

    Status code of the last operation

  uint16_t current_scene

    Scene Number of the current scene

  uint16_t target_scene

    Scene Number of the target scene (optional)

  uint8_t remain_time

    Time to complete state transition (C.1)

struct esp_ble_mesh_scene_register_status_cb_t

  Parameters of Scene Register Status

  Public Members

  uint8_t status_code

    Status code for the previous operation

  uint16_t current_scene

    Scene Number of the current scene

  struct net_buf_simple *scenes

    A list of scenes stored within an element

struct esp_ble_mesh_scheduler_status_cb_t

  Parameter of Scheduler Status

  Public Members

  uint16_t schedules

    Bit field indicating defined Actions in the Schedule Register

struct esp_ble_mesh_scheduler_act_status_cb_t

  Parameters of Scheduler Action Status

  Public Members

  uint64_t index

    Enumerates (selects) a Schedule Register entry

  uint64_t year

    Scheduled year for the action

  uint64_t month

    Scheduled month for the action

  uint64_t day

    Scheduled day of the month for the action

  uint64_t hour

    Scheduled hour for the action

  uint64_t minute

    Scheduled minute for the action

  uint64_t second

    Scheduled second for the action

  uint64_t day_of_week

    Schedule days of the week for the action

  uint64_t action

    Action to be performed at the scheduled time

  uint64_t trans_time

    Transition time for this action

  uint16_t scene_number

    Transition time for this action

struct esp_ble_mesh_time_scene_client_cb_param_t

  Time Scene Client Model callback parameters

  Public Members

  int error_code

    Appropriate error code

  esp_ble_mesh_client_common_param_t *params

    The client common parameters.

  esp_ble_mesh_time_scene_client_status_cb_t status_cb

    The scene status message callback values

struct esp_ble_mesh_time_state_t

  Parameters of Time state

  Public Members

  uint8_t tai_seconds[5]

    The value of the TAI Seconds state

  uint8_t subsecond

    The value of the Subsecond field

  uint8_t uncertainty

    The value of the Uncertainty field

  uint8_t time_zone_offset_curr

    The value of the Time Zone Offset Current field

  uint8_t time_zone_offset_new

    The value of the Time Zone Offset New state

  uint8_t tai_zone_change[5]

    The value of the TAI of Zone Change field

  uint16_t time_authority

    The value of the Time Authority bit

  uint16_t tai_utc_delta_curr

    The value of the TAI-UTC Delta Current state

  uint16_t tai_utc_delta_new

    The value of the TAI-UTC Delta New state

  uint8_t tai_delta_change[5]

    The value of the TAI of Delta Change field

  struct esp_ble_mesh_time_state_t time

    Parameters of the Time state

  uint8_t time_role

    The value of the Time Role state

struct esp_ble_mesh_time_srv_t

  User data of Time Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Time Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_time_state_t *state

    Parameters of the Time state

struct esp_ble_mesh_time_setup_srv_t

  User data of Time Setup Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Time Setup Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_time_state_t *state

    Parameters of the Time state

struct esp_ble_mesh_scene_register_t

  1. Scene Store is an operation of storing values of a present state of an element.

  2. The structure and meaning of the stored state is determined by a model. States to be stored are specified by each model.

  3. The Scene Store operation shall persistently store all values of all states marked as Stored with Scene for all models present on all elements of a node.

  4. If a model is extending another model, the extending model shall determine the Stored with Scene behavior of that model. Parameters of Scene Register state

  Public Members

  uint16_t scene_number

    The value of the Scene Number

  uint8_t scene_type

    The value of the Scene Type

  struct net_buf_simple *scene_value

    Scene value may use a union to represent later, the union contains structures of all the model states which can be stored in a scene. The value of the Scene Value

struct esp_ble_mesh_scenes_state_t

  Parameters of Scenes state.

  Scenes serve as memory banks for storage of states (e.g., a power level or a light level/color). Values of states of an element can be stored as a scene and can be recalled later from the scene memory.

  A scene is represented by a Scene Number, which is a 16-bit non-zero, mesh-wide value. (There can be a maximum of 65535 scenes in a mesh network.) The meaning of a scene, as well as the state storage container associated with it, are determined by a model.

  The Scenes state change may start numerous parallel model transitions. In that case, each individual model handles the transition internally.

  The scene transition is defined as a group of individual model transitions started by a Scene Recall operation. The scene transition is in progress when at least one transition from the group of individual model transitions is in progress.

  Public Members

  const uint16_t scene_count

    The Scenes state's scene count

  esp_ble_mesh_scene_register_t *scenes

    Parameters of the Scenes state

  uint16_t current_scene

    The Current Scene state is a 16-bit value that contains either the Scene Number of the currently active scene or a value of 0x0000 when no scene is active.

    When a Scene Store operation or a Scene Recall operation completes with success, the Current Scene state value shall be to the Scene Number used during that operation.

    When the Current Scene Number is deleted from a Scene Register state as a result of Scene Delete operation, the Current Scene state shall be set to 0x0000.

    When any of the element's state that is marked as “Stored with Scene” has changed not as a result of a Scene Recall operation, the value of the Current Scene state shall be set to 0x0000.

    When a scene transition is in progress, the value of the Current Scene state shall be set to 0x0000. The value of the Current Scene state

  uint16_t target_scene

    The Target Scene state is a 16-bit value that contains the target Scene Number when a scene transition is in progress.

    When the scene transition is in progress and the target Scene Number is deleted from a Scene Register state as a result of Scene Delete operation, the Target Scene state shall be set to 0x0000.

    When the scene transition is in progress and a new Scene Number is stored in the Scene Register as a result of Scene Store operation, the Target Scene state shall be set to the new Scene Number.

    When the scene transition is not in progress, the value of the Target Scene state shall be set to 0x0000. The value of the Target Scene state

  uint8_t status_code

    The status code of the last scene operation

  bool in_progress

    Indicate if the scene transition is in progress

struct esp_ble_mesh_scene_srv_t

  User data of Scene Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Scene Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_scenes_state_t *state

    Parameters of the Scenes state

  esp_ble_mesh_last_msg_info_t last

    Parameters of the last received set message

  esp_ble_mesh_state_transition_t transition

    Parameters of state transition

struct esp_ble_mesh_scene_setup_srv_t

  User data of Scene Setup Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Scene Setup Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_scenes_state_t *state

    Parameters of the Scenes state

struct esp_ble_mesh_schedule_register_t

  Parameters of Scheduler Register state

  Public Members

  bool in_use

    Indicate if the registered schedule is in use

  uint64_t year

    The value of Scheduled year for the action

  uint64_t month

    The value of Scheduled month for the action

  uint64_t day

    The value of Scheduled day of the month for the action

  uint64_t hour

    The value of Scheduled hour for the action

  uint64_t minute

    The value of Scheduled minute for the action

  uint64_t second

    The value of Scheduled second for the action

  uint64_t day_of_week

    The value of Schedule days of the week for the action

  uint64_t action

    The value of Action to be performed at the scheduled time

  uint64_t trans_time

    The value of Transition time for this action

  uint16_t scene_number

    The value of Scene Number to be used for some actions

struct esp_ble_mesh_scheduler_state_t

  Parameters of Scheduler state

  Public Members

  const uint8_t schedule_count

    Scheduler count

  esp_ble_mesh_schedule_register_t *schedules

    Up to 16 scheduled entries

struct esp_ble_mesh_scheduler_srv_t

  User data of Scheduler Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Scheduler Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_scheduler_state_t *state

    Parameters of the Scheduler state

struct esp_ble_mesh_scheduler_setup_srv_t

  User data of Scheduler Setup Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Scheduler Setup Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_scheduler_state_t *state

    Parameters of the Scheduler state

struct esp_ble_mesh_state_change_time_set_t

  Parameters of Time Set state change event

  Public Members

  uint8_t tai_seconds[5]

    The current TAI time in seconds

  uint8_t subsecond

    The sub-second time in units of 1/256 second

  uint8_t uncertainty

    The estimated uncertainty in 10-millisecond steps

  uint16_t time_authority

    0 = No Time Authority, 1 = Time Authority

  uint16_t tai_utc_delta_curr

    Current difference between TAI and UTC in seconds

  uint8_t time_zone_offset_curr

    The local time zone offset in 15-minute increments

struct esp_ble_mesh_state_change_time_status_t

  Parameters of Time Status state change event

  Public Members

  uint8_t tai_seconds[5]

    The current TAI time in seconds

  uint8_t subsecond

    The sub-second time in units of 1/256 second

  uint8_t uncertainty

    The estimated uncertainty in 10-millisecond steps

  uint16_t time_authority

    0 = No Time Authority, 1 = Time Authority

  uint16_t tai_utc_delta_curr

    Current difference between TAI and UTC in seconds

  uint8_t time_zone_offset_curr

    The local time zone offset in 15-minute increments

struct esp_ble_mesh_state_change_time_zone_set_t

  Parameters of Time Zone Set state change event

  Public Members

  uint8_t time_zone_offset_new

    Upcoming local time zone offset

  uint8_t tai_zone_change[5]

    TAI Seconds time of the upcoming Time Zone Offset change

struct esp_ble_mesh_state_change_tai_utc_delta_set_t

  Parameters of TAI UTC Delta Set state change event

  Public Members

  uint16_t tai_utc_delta_new

    Upcoming difference between TAI and UTC in seconds

  uint8_t tai_delta_change[5]

    TAI Seconds time of the upcoming TAI-UTC Delta change

struct esp_ble_mesh_state_change_time_role_set_t

  Parameter of Time Role Set state change event

  Public Members

  uint8_t time_role

    The Time Role for the element

struct esp_ble_mesh_state_change_scene_store_t

  Parameter of Scene Store state change event

  Public Members

  uint16_t scene_number

    The number of scenes to be stored

struct esp_ble_mesh_state_change_scene_recall_t

  Parameter of Scene Recall state change event

  Public Members

  uint16_t scene_number

    The number of scenes to be recalled

struct esp_ble_mesh_state_change_scene_delete_t

  Parameter of Scene Delete state change event

  Public Members

  uint16_t scene_number

    The number of scenes to be deleted

struct esp_ble_mesh_state_change_scheduler_act_set_t

  Parameter of Scheduler Action Set state change event

  Public Members

  uint64_t index

    Index of the Schedule Register entry to set

  uint64_t year

    Scheduled year for the action

  uint64_t month

    Scheduled month for the action

  uint64_t day

    Scheduled day of the month for the action

  uint64_t hour

    Scheduled hour for the action

  uint64_t minute

    Scheduled minute for the action

  uint64_t second

    Scheduled second for the action

  uint64_t day_of_week

    Schedule days of the week for the action

  uint64_t action

    Action to be performed at the scheduled time

  uint64_t trans_time

    Transition time for this action

  uint16_t scene_number

    Scene number to be used for some actions

struct esp_ble_mesh_server_recv_scheduler_act_get_t

  Context of the received Scheduler Action Get message

  Public Members

  uint8_t index

    Index of the Schedule Register entry to get

struct esp_ble_mesh_server_recv_time_set_t

  Context of the received Time Set message

  Public Members

  uint8_t tai_seconds[5]

    The current TAI time in seconds

  uint8_t subsecond

    The sub-second time in units of 1/256 second

  uint8_t uncertainty

    The estimated uncertainty in 10-millisecond steps

  uint16_t time_authority

    0 = No Time Authority, 1 = Time Authority

  uint16_t tai_utc_delta

    Current difference between TAI and UTC in seconds

  uint8_t time_zone_offset

    The local time zone offset in 15-minute increments

struct esp_ble_mesh_server_recv_time_zone_set_t

  Context of the received Time Zone Set message

  Public Members

  uint8_t time_zone_offset_new

    Upcoming local time zone offset

  uint8_t tai_zone_change[5]

    TAI Seconds time of the upcoming Time Zone Offset change

struct esp_ble_mesh_server_recv_tai_utc_delta_set_t

  Context of the received TAI UTC Delta Set message

  Public Members

  uint16_t tai_utc_delta_new

    Upcoming difference between TAI and UTC in seconds

  uint16_t padding

    Always 0b0. Other values are Prohibited.

  uint8_t tai_delta_change[5]

    TAI Seconds time of the upcoming TAI-UTC Delta change

struct esp_ble_mesh_server_recv_time_role_set_t

  Context of the received Time Role Set message

  Public Members

  uint8_t time_role

    The Time Role for the element

struct esp_ble_mesh_server_recv_scene_store_t

  Context of the received Scene Store message

  Public Members

  uint16_t scene_number

    The number of scenes to be stored

struct esp_ble_mesh_server_recv_scene_recall_t

  Context of the received Scene Recall message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t scene_number

    The number of scenes to be recalled

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_scene_delete_t

  Context of the received Scene Delete message

  Public Members

  uint16_t scene_number

    The number of scenes to be deleted

struct esp_ble_mesh_server_recv_scheduler_act_set_t

  Context of the received Scheduler Action Set message

  Public Members

  uint64_t index

    Index of the Schedule Register entry to set

  uint64_t year

    Scheduled year for the action

  uint64_t month

    Scheduled month for the action

  uint64_t day

    Scheduled day of the month for the action

  uint64_t hour

    Scheduled hour for the action

  uint64_t minute

    Scheduled minute for the action

  uint64_t second

    Scheduled second for the action

  uint64_t day_of_week

    Schedule days of the week for the action

  uint64_t action

    Action to be performed at the scheduled time

  uint64_t trans_time

    Transition time for this action

  uint16_t scene_number

    Scene number to be used for some actions

struct esp_ble_mesh_server_recv_time_status_t

  Context of the received Time Status message

  Public Members

  uint8_t tai_seconds[5]

    The current TAI time in seconds

  uint8_t subsecond

    The sub-second time in units of 1/256 second

  uint8_t uncertainty

    The estimated uncertainty in 10-millisecond steps

  uint16_t time_authority

    0 = No Time Authority, 1 = Time Authority

  uint16_t tai_utc_delta

    Current difference between TAI and UTC in seconds

  uint8_t time_zone_offset

    The local time zone offset in 15-minute increments

struct esp_ble_mesh_time_scene_server_cb_param_t

  Time Scene Server Model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to Time and Scenes Server Models

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received messages

  esp_ble_mesh_time_scene_server_cb_value_t value

    Value of the received Time and Scenes Messages

### Macros

ESP_BLE_MESH_MODEL_TIME_CLI(cli_pub, cli_data)

  Define a new Time Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Time Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Time Client Model instance.

ESP_BLE_MESH_MODEL_SCENE_CLI(cli_pub, cli_data)

  Define a new Scene Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Scene Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Scene Client Model instance.

ESP_BLE_MESH_MODEL_SCHEDULER_CLI(cli_pub, cli_data)

  Define a new Scheduler Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Scheduler Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Scheduler Client Model instance.

ESP_BLE_MESH_MODEL_TIME_SRV(srv_pub, srv_data)

  Time Scene Server Models related context.

  Define a new Time Server Model.

  备注

  1. The Time Server model is a root model. When this model is present on an Element, the corresponding Time Setup Server model shall also be present.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_time_srv_t.

  返回:

    New Time Server Model instance.

ESP_BLE_MESH_MODEL_TIME_SETUP_SRV(srv_data)

  Define a new Time Setup Server Model.

  备注

  1. The Time Setup Server model extends the Time Server model. Time is sensitive information that is propagated across a mesh network.

  1. Only an authorized Time Client should be allowed to change the Time and Time Role states. A dedicated application key Bluetooth SIG Proprietary should be used on the Time Setup Server to restrict access to the server to only authorized Time Clients.

  2. This model does not support subscribing nor publishing.

  参数:

    - srv_data -- Pointer to the unique struct esp_ble_mesh_time_setup_srv_t.

  返回:

    New Time Setup Server Model instance.

ESP_BLE_MESH_MODEL_SCENE_SRV(srv_pub, srv_data)

  Define a new Scene Server Model.

  备注

  1. The Scene Server model is a root model. When this model is present on an Element, the corresponding Scene Setup Server model shall also be present.

  1. This model shall support model publication and model subscription.

  2. The model may be present only on the Primary element of a node.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_scene_srv_t.

  返回:

    New Scene Server Model instance.

ESP_BLE_MESH_MODEL_SCENE_SETUP_SRV(srv_pub, srv_data)

  Define a new Scene Setup Server Model.

  备注

  1. The Scene Setup Server model extends the Scene Server model and the Generic Default Transition Time Server model.

  1. This model shall support model subscription.

  2. The model may be present only on the Primary element of a node.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_scene_setup_srv_t.

  返回:

    New Scene Setup Server Model instance.

ESP_BLE_MESH_MODEL_SCHEDULER_SRV(srv_pub, srv_data)

  Define a new Scheduler Server Model.

  备注

  1. The Scheduler Server model extends the Scene Server model. When this model is present on an Element, the corresponding Scheduler Setup Server model shall also be present.

  1. This model shall support model publication and model subscription.

  2. The model may be present only on the Primary element of a node.

  3. The model requires the Time Server model shall be present on the element.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_scheduler_srv_t.

  返回:

    New Scheduler Server Model instance.

ESP_BLE_MESH_MODEL_SCHEDULER_SETUP_SRV(srv_pub, srv_data)

  Define a new Scheduler Setup Server Model.

  备注

  1. The Scheduler Setup Server model extends the Scheduler Server and the Scene Setup Server models.

  1. This model shall support model subscription.

  2. The model may be present only on the Primary element of a node.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_scheduler_setup_srv_t.

  返回:

    New Scheduler Setup Server Model instance.

ESP_BLE_MESH_UNKNOWN_TAI_SECONDS

  Unknown TAI Seconds

ESP_BLE_MESH_UNKNOWN_TAI_ZONE_CHANGE

  Unknown TAI of Zone Change

ESP_BLE_MESH_UNKNOWN_TAI_DELTA_CHANGE

  Unknown TAI of Delta Change

ESP_BLE_MESH_TAI_UTC_DELTA_MAX_VALUE

  Maximum TAI-UTC Delta value

ESP_BLE_MESH_TAI_SECONDS_LEN

  Length of TAI Seconds

ESP_BLE_MESH_TAI_OF_ZONE_CHANGE_LEN

  Length of TAI of Zone Change

ESP_BLE_MESH_TAI_OF_DELTA_CHANGE_LEN

  Length of TAI of Delta Change

ESP_BLE_MESH_INVALID_SCENE_NUMBER

  Invalid Scene Number

ESP_BLE_MESH_SCENE_NUMBER_LEN

  Length of the Scene Number

ESP_BLE_MESH_SCHEDULE_YEAR_ANY_YEAR

  Any year of the Scheduled year

ESP_BLE_MESH_SCHEDULE_DAY_ANY_DAY

  Any day of the Scheduled day

ESP_BLE_MESH_SCHEDULE_HOUR_ANY_HOUR

  Any hour of the Scheduled hour

ESP_BLE_MESH_SCHEDULE_HOUR_ONCE_A_DAY

  Any hour of the Scheduled Day

ESP_BLE_MESH_SCHEDULE_SEC_ANY_OF_HOUR

  Any minute of the Scheduled hour

ESP_BLE_MESH_SCHEDULE_SEC_EVERY_15_MIN

  Every 15 minutes of the Scheduled hour

ESP_BLE_MESH_SCHEDULE_SEC_EVERY_20_MIN

  Every 20 minutes of the Scheduled hour

ESP_BLE_MESH_SCHEDULE_SEC_ONCE_AN_HOUR

  Once of the Scheduled hour

ESP_BLE_MESH_SCHEDULE_SEC_ANY_OF_MIN

  Any second of the Scheduled minute

ESP_BLE_MESH_SCHEDULE_SEC_EVERY_15_SEC

  Every 15 seconds of the Scheduled minute

ESP_BLE_MESH_SCHEDULE_SEC_EVERY_20_SEC

  Every 20 seconds of the Scheduled minute

ESP_BLE_MESH_SCHEDULE_SEC_ONCE_AN_MIN

  Once of the Scheduled minute

ESP_BLE_MESH_SCHEDULE_ACT_TURN_OFF

  Scheduled Action - Turn Off

ESP_BLE_MESH_SCHEDULE_ACT_TURN_ON

  Scheduled Action - Turn On

ESP_BLE_MESH_SCHEDULE_ACT_SCENE_RECALL

  Scheduled Action - Scene Recall

ESP_BLE_MESH_SCHEDULE_ACT_NO_ACTION

  Scheduled Action - No Action

ESP_BLE_MESH_SCHEDULE_SCENE_NO_SCENE

  Scheduled Scene - No Scene

ESP_BLE_MESH_SCHEDULE_ENTRY_MAX_INDEX

  Maximum number of Scheduled entries

ESP_BLE_MESH_TIME_NONE

  Time Role - None

ESP_BLE_MESH_TIME_AUTHORITY

  Time Role - Mesh Time Authority

ESP_BLE_MESH_TIME_RELAY

  Time Role - Mesh Time Relay

ESP_BLE_MESH_TIME_CLIENT

  Time Role - Mesh Time Client

ESP_BLE_MESH_SCENE_SUCCESS

  Scene operation - Success

ESP_BLE_MESH_SCENE_REG_FULL

  Scene operation - Scene Register Full

ESP_BLE_MESH_SCENE_NOT_FOUND

  Scene operation - Scene Not Found

### Type Definitions

typedef void (*esp_ble_mesh_time_scene_client_cb_t)(esp_ble_mesh_time_scene_client_cb_event_t event, esp_ble_mesh_time_scene_client_cb_param_t *param)

  Bluetooth Mesh Time Scene Client Model function.

  Time Scene Client Model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_time_scene_server_cb_t)(esp_ble_mesh_time_scene_server_cb_event_t event, esp_ble_mesh_time_scene_server_cb_param_t *param)

  Bluetooth Mesh Time and Scenes Server Model function.

  Time Scene Server Model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_time_scene_client_cb_event_t

  This enum value is the event of Time Scene Client Model

  Values:

  enumerator ESP_BLE_MESH_TIME_SCENE_CLIENT_GET_STATE_EVT
  enumerator ESP_BLE_MESH_TIME_SCENE_CLIENT_SET_STATE_EVT
  enumerator ESP_BLE_MESH_TIME_SCENE_CLIENT_PUBLISH_EVT
  enumerator ESP_BLE_MESH_TIME_SCENE_CLIENT_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_TIME_SCENE_CLIENT_EVT_MAX

enum esp_ble_mesh_time_scene_server_cb_event_t

  This enum value is the event of Time Scene Server Model

  Values:

  enumerator ESP_BLE_MESH_TIME_SCENE_SERVER_STATE_CHANGE_EVT

    1. When get_auto_rsp is set to ESP_BLE_MESH_SERVER_AUTO_RSP, no event will be callback to the application layer when Time Scene Get messages are received.

    2. When set_auto_rsp is set to ESP_BLE_MESH_SERVER_AUTO_RSP, this event will be callback to the application layer when Time Scene Set/Set Unack messages are received.

  enumerator ESP_BLE_MESH_TIME_SCENE_SERVER_RECV_GET_MSG_EVT

    When get_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, this event will be callback to the application layer when Time Scene Get messages are received.

  enumerator ESP_BLE_MESH_TIME_SCENE_SERVER_RECV_SET_MSG_EVT

    When set_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, this event will be callback to the application layer when Time Scene Set/Set Unack messages are received.

  enumerator ESP_BLE_MESH_TIME_SCENE_SERVER_RECV_STATUS_MSG_EVT

    When status_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, this event will be callback to the application layer when TIme Status message is received.

  enumerator ESP_BLE_MESH_TIME_SCENE_SERVER_EVT_MAX

### Lighting Client/Server Models

### Header File

- components/bt/esp_ble_mesh/api/models/include/esp_ble_mesh_lighting_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_lighting_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_light_client_callback(esp_ble_mesh_light_client_cb_t callback)

  Register BLE Mesh Light Client Model callback.

  参数:

    callback -- [in] pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_light_client_get_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_light_client_get_state_t *get_state)

  Get the value of Light Server Model states using the Light Client Model get messages.

  备注

  If you want to know the opcodes and corresponding meanings accepted by this API, please refer to esp_ble_mesh_light_message_opcode_t in esp_ble_mesh_defs.h

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - get_state -- [in] Pointer of light get message value. Shall not be set to NULL.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_light_client_set_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_light_client_set_state_t *set_state)

  Set the value of Light Server Model states using the Light Client Model set messages.

  备注

  If you want to know the opcodes and corresponding meanings accepted by this API, please refer to esp_ble_mesh_light_message_opcode_t in esp_ble_mesh_defs.h

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - set_state -- [in] Pointer of light set message value. Shall not be set to NULL.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_lighting_server_callback(esp_ble_mesh_lighting_server_cb_t callback)

  Register BLE Mesh Lighting Server Model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_light_client_get_state_t
  #include <esp_ble_mesh_lighting_model_api.h>

  Lighting Client Model get message union.

  Public Members

  esp_ble_mesh_light_lc_property_get_t lc_property_get

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LC_PROPERTY_GET

union esp_ble_mesh_light_client_set_state_t
  #include <esp_ble_mesh_lighting_model_api.h>

  Lighting Client Model set message union.

  Public Members

  esp_ble_mesh_light_lightness_set_t lightness_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_SET_UNACK

  esp_ble_mesh_light_lightness_linear_set_t lightness_linear_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_LINEAR_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_LINEAR_SET_UNACK

  esp_ble_mesh_light_lightness_default_set_t lightness_default_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_DEFAULT_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_DEFAULT_SET_UNACK

  esp_ble_mesh_light_lightness_range_set_t lightness_range_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_RANGE_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_RANGE_SET_UNACK

  esp_ble_mesh_light_ctl_set_t ctl_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_SET_UNACK

  esp_ble_mesh_light_ctl_temperature_set_t ctl_temperature_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_SET_UNACK

  esp_ble_mesh_light_ctl_temperature_range_set_t ctl_temperature_range_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_RANGE_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_RANGE_SET_UNACK

  esp_ble_mesh_light_ctl_default_set_t ctl_default_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_DEFAULT_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_DEFAULT_SET_UNACK

  esp_ble_mesh_light_hsl_set_t hsl_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_SET_UNACK

  esp_ble_mesh_light_hsl_hue_set_t hsl_hue_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_HUE_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_HUE_SET_UNACK

  esp_ble_mesh_light_hsl_saturation_set_t hsl_saturation_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_SATURATION_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_SATURATION_SET_UNACK

  esp_ble_mesh_light_hsl_default_set_t hsl_default_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_DEFAULT_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_DEFAULT_SET_UNACK

  esp_ble_mesh_light_hsl_range_set_t hsl_range_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_RANGE_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_RANGE_SET_UNACK

  esp_ble_mesh_light_xyl_set_t xyl_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_SET_UNACK

  esp_ble_mesh_light_xyl_default_set_t xyl_default_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_DEFAULT_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_DEFAULT_SET_UNACK

  esp_ble_mesh_light_xyl_range_set_t xyl_range_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_RANGE_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_RANGE_SET_UNACK

  esp_ble_mesh_light_lc_mode_set_t lc_mode_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LC_MODE_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_LC_MODE_SET_UNACK

  esp_ble_mesh_light_lc_om_set_t lc_om_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LC_OM_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_LC_OM_SET_UNACK

  esp_ble_mesh_light_lc_light_onoff_set_t lc_light_onoff_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LC_LIGHT_ONOFF_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_LC_LIGHT_ONOFF_SET_UNACK

  esp_ble_mesh_light_lc_property_set_t lc_property_set

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LC_PROPERTY_SET & ESP_BLE_MESH_MODEL_OP_LIGHT_LC_PROPERTY_SET_UNACK

union esp_ble_mesh_light_client_status_cb_t
  #include <esp_ble_mesh_lighting_model_api.h>

  Lighting Client Model received message union.

  Public Members

  esp_ble_mesh_light_lightness_status_cb_t lightness_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_STATUS

  esp_ble_mesh_light_lightness_linear_status_cb_t lightness_linear_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_LINEAR_STATUS

  esp_ble_mesh_light_lightness_last_status_cb_t lightness_last_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_LAST_STATUS

  esp_ble_mesh_light_lightness_default_status_cb_t lightness_default_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_DEFAULT_STATUS

  esp_ble_mesh_light_lightness_range_status_cb_t lightness_range_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LIGHTNESS_RANGE_STATUS

  esp_ble_mesh_light_ctl_status_cb_t ctl_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_STATUS

  esp_ble_mesh_light_ctl_temperature_status_cb_t ctl_temperature_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_STATUS

  esp_ble_mesh_light_ctl_temperature_range_status_cb_t ctl_temperature_range_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_TEMPERATURE_RANGE_STATUS

  esp_ble_mesh_light_ctl_default_status_cb_t ctl_default_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_CTL_DEFAULT_STATUS

  esp_ble_mesh_light_hsl_status_cb_t hsl_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_STATUS

  esp_ble_mesh_light_hsl_target_status_cb_t hsl_target_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_TARGET_STATUS

  esp_ble_mesh_light_hsl_hue_status_cb_t hsl_hue_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_HUE_STATUS

  esp_ble_mesh_light_hsl_saturation_status_cb_t hsl_saturation_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_SATURATION_STATUS

  esp_ble_mesh_light_hsl_default_status_cb_t hsl_default_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_DEFAULT_STATUS

  esp_ble_mesh_light_hsl_range_status_cb_t hsl_range_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_HSL_RANGE_STATUS

  esp_ble_mesh_light_xyl_status_cb_t xyl_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_STATUS

  esp_ble_mesh_light_xyl_target_status_cb_t xyl_target_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_TARGET_STATUS

  esp_ble_mesh_light_xyl_default_status_cb_t xyl_default_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_DEFAULT_STATUS

  esp_ble_mesh_light_xyl_range_status_cb_t xyl_range_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_XYL_RANGE_STATUS

  esp_ble_mesh_light_lc_mode_status_cb_t lc_mode_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LC_MODE_STATUS

  esp_ble_mesh_light_lc_om_status_cb_t lc_om_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LC_OM_STATUS

  esp_ble_mesh_light_lc_light_onoff_status_cb_t lc_light_onoff_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LC_LIGHT_ONOFF_STATUS

  esp_ble_mesh_light_lc_property_status_cb_t lc_property_status

    For ESP_BLE_MESH_MODEL_OP_LIGHT_LC_PROPERTY_STATUS

union esp_ble_mesh_lighting_server_state_change_t
  #include <esp_ble_mesh_lighting_model_api.h>

  Lighting Server Model state change value union.

  Public Members

  esp_ble_mesh_state_change_light_lightness_set_t lightness_set

    The recv_op in ctx can be used to decide which state is changed. Light Lightness Set

  esp_ble_mesh_state_change_light_lightness_linear_set_t lightness_linear_set

    Light Lightness Linear Set

  esp_ble_mesh_state_change_light_lightness_default_set_t lightness_default_set

    Light Lightness Default Set

  esp_ble_mesh_state_change_light_lightness_range_set_t lightness_range_set

    Light Lightness Range Set

  esp_ble_mesh_state_change_light_ctl_set_t ctl_set

    Light CTL Set

  esp_ble_mesh_state_change_light_ctl_temperature_set_t ctl_temp_set

    Light CTL Temperature Set

  esp_ble_mesh_state_change_light_ctl_temperature_range_set_t ctl_temp_range_set

    Light CTL Temperature Range Set

  esp_ble_mesh_state_change_light_ctl_default_set_t ctl_default_set

    Light CTL Default Set

  esp_ble_mesh_state_change_light_hsl_set_t hsl_set

    Light HSL Set

  esp_ble_mesh_state_change_light_hsl_hue_set_t hsl_hue_set

    Light HSL Hue Set

  esp_ble_mesh_state_change_light_hsl_saturation_set_t hsl_saturation_set

    Light HSL Saturation Set

  esp_ble_mesh_state_change_light_hsl_default_set_t hsl_default_set

    Light HSL Default Set

  esp_ble_mesh_state_change_light_hsl_range_set_t hsl_range_set

    Light HSL Range Set

  esp_ble_mesh_state_change_light_xyl_set_t xyl_set

    Light xyL Set

  esp_ble_mesh_state_change_light_xyl_default_set_t xyl_default_set

    Light xyL Default Set

  esp_ble_mesh_state_change_light_xyl_range_set_t xyl_range_set

    Light xyL Range Set

  esp_ble_mesh_state_change_light_lc_mode_set_t lc_mode_set

    Light LC Mode Set

  esp_ble_mesh_state_change_light_lc_om_set_t lc_om_set

    Light LC Occupancy Mode Set

  esp_ble_mesh_state_change_light_lc_light_onoff_set_t lc_light_onoff_set

    Light LC Light OnOff Set

  esp_ble_mesh_state_change_light_lc_property_set_t lc_property_set

    Light LC Property Set

  esp_ble_mesh_state_change_sensor_status_t sensor_status

    Sensor Status

union esp_ble_mesh_lighting_server_recv_get_msg_t
  #include <esp_ble_mesh_lighting_model_api.h>

  Lighting Server Model received get message union.

  Public Members

  esp_ble_mesh_server_recv_light_lc_property_get_t lc_property

    Light LC Property Get

union esp_ble_mesh_lighting_server_recv_set_msg_t
  #include <esp_ble_mesh_lighting_model_api.h>

  Lighting Server Model received set message union.

  Public Members

  esp_ble_mesh_server_recv_light_lightness_set_t lightness

    Light Lightness Set/Light Lightness Set Unack

  esp_ble_mesh_server_recv_light_lightness_linear_set_t lightness_linear

    Light Lightness Linear Set/Light Lightness Linear Set Unack

  esp_ble_mesh_server_recv_light_lightness_default_set_t lightness_default

    Light Lightness Default Set/Light Lightness Default Set Unack

  esp_ble_mesh_server_recv_light_lightness_range_set_t lightness_range

    Light Lightness Range Set/Light Lightness Range Set Unack

  esp_ble_mesh_server_recv_light_ctl_set_t ctl

    Light CTL Set/Light CTL Set Unack

  esp_ble_mesh_server_recv_light_ctl_temperature_set_t ctl_temp

    Light CTL Temperature Set/Light CTL Temperature Set Unack

  esp_ble_mesh_server_recv_light_ctl_temperature_range_set_t ctl_temp_range

    Light CTL Temperature Range Set/Light CTL Temperature Range Set Unack

  esp_ble_mesh_server_recv_light_ctl_default_set_t ctl_default

    Light CTL Default Set/Light CTL Default Set Unack

  esp_ble_mesh_server_recv_light_hsl_set_t hsl

    Light HSL Set/Light HSL Set Unack

  esp_ble_mesh_server_recv_light_hsl_hue_set_t hsl_hue

    Light HSL Hue Set/Light HSL Hue Set Unack

  esp_ble_mesh_server_recv_light_hsl_saturation_set_t hsl_saturation

    Light HSL Saturation Set/Light HSL Saturation Set Unack

  esp_ble_mesh_server_recv_light_hsl_default_set_t hsl_default

    Light HSL Default Set/Light HSL Default Set Unack

  esp_ble_mesh_server_recv_light_hsl_range_set_t hsl_range

    Light HSL Range Set/Light HSL Range Set Unack

  esp_ble_mesh_server_recv_light_xyl_set_t xyl

    Light xyL Set/Light xyL Set Unack

  esp_ble_mesh_server_recv_light_xyl_default_set_t xyl_default

    Light xyL Default Set/Light xyL Default Set Unack

  esp_ble_mesh_server_recv_light_xyl_range_set_t xyl_range

    Light xyL Range Set/Light xyL Range Set Unack

  esp_ble_mesh_server_recv_light_lc_mode_set_t lc_mode

    Light LC Mode Set/Light LC Mode Set Unack

  esp_ble_mesh_server_recv_light_lc_om_set_t lc_om

    Light LC OM Set/Light LC OM Set Unack

  esp_ble_mesh_server_recv_light_lc_light_onoff_set_t lc_light_onoff

    Light LC Light OnOff Set/Light LC Light OnOff Set Unack

  esp_ble_mesh_server_recv_light_lc_property_set_t lc_property

    Light LC Property Set/Light LC Property Set Unack

union esp_ble_mesh_lighting_server_recv_status_msg_t
  #include <esp_ble_mesh_lighting_model_api.h>

  Lighting Server Model received status message union.

  Public Members

  esp_ble_mesh_server_recv_sensor_status_t sensor_status

    Sensor Status

union esp_ble_mesh_lighting_server_cb_value_t
  #include <esp_ble_mesh_lighting_model_api.h>

  Lighting Server Model callback value union.

  Public Members

  esp_ble_mesh_lighting_server_state_change_t state_change

    ESP_BLE_MESH_LIGHTING_SERVER_STATE_CHANGE_EVT

  esp_ble_mesh_lighting_server_recv_get_msg_t get

    ESP_BLE_MESH_LIGHTING_SERVER_RECV_GET_MSG_EVT

  esp_ble_mesh_lighting_server_recv_set_msg_t set

    ESP_BLE_MESH_LIGHTING_SERVER_RECV_SET_MSG_EVT

  esp_ble_mesh_lighting_server_recv_status_msg_t status

    ESP_BLE_MESH_LIGHTING_SERVER_RECV_STATUS_MSG_EVT

### Structures

struct esp_ble_mesh_light_lightness_set_t

  Bluetooth Mesh Light Lightness Client Model Get and Set parameters structure.

  Parameters of Light Lightness Set

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t lightness

    Target value of light lightness actual state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_light_lightness_linear_set_t

  Parameters of Light Lightness Linear Set

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t lightness

    Target value of light lightness linear state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_light_lightness_default_set_t

  Parameter of Light Lightness Default Set

  Public Members

  uint16_t lightness

    The value of the Light Lightness Default state

struct esp_ble_mesh_light_lightness_range_set_t

  Parameters of Light Lightness Range Set

  Public Members

  uint16_t range_min

    Value of range min field of light lightness range state

  uint16_t range_max

    Value of range max field of light lightness range state

struct esp_ble_mesh_light_ctl_set_t

  Parameters of Light CTL Set

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t ctl_lightness

    Target value of light ctl lightness state

  uint16_t ctl_temperature

    Target value of light ctl temperature state

  int16_t ctl_delta_uv

    Target value of light ctl delta UV state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_light_ctl_temperature_set_t

  Parameters of Light CTL Temperature Set

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t ctl_temperature

    Target value of light ctl temperature state

  int16_t ctl_delta_uv

    Target value of light ctl delta UV state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_light_ctl_temperature_range_set_t

  Parameters of Light CTL Temperature Range Set

  Public Members

  uint16_t range_min

    Value of temperature range min field of light ctl temperature range state

  uint16_t range_max

    Value of temperature range max field of light ctl temperature range state

struct esp_ble_mesh_light_ctl_default_set_t

  Parameters of Light CTL Default Set

  Public Members

  uint16_t lightness

    Value of light lightness default state

  uint16_t temperature

    Value of light temperature default state

  int16_t delta_uv

    Value of light delta UV default state

struct esp_ble_mesh_light_hsl_set_t

  Parameters of Light HSL Set

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t hsl_lightness

    Target value of light hsl lightness state

  uint16_t hsl_hue

    Target value of light hsl hue state

  uint16_t hsl_saturation

    Target value of light hsl saturation state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_light_hsl_hue_set_t

  Parameters of Light HSL Hue Set

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t hue

    Target value of light hsl hue state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_light_hsl_saturation_set_t

  Parameters of Light HSL Saturation Set

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t saturation

    Target value of light hsl hue state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_light_hsl_default_set_t

  Parameters of Light HSL Default Set

  Public Members

  uint16_t lightness

    Value of light lightness default state

  uint16_t hue

    Value of light hue default state

  uint16_t saturation

    Value of light saturation default state

struct esp_ble_mesh_light_hsl_range_set_t

  Parameters of Light HSL Range Set

  Public Members

  uint16_t hue_range_min

    Value of hue range min field of light hsl hue range state

  uint16_t hue_range_max

    Value of hue range max field of light hsl hue range state

  uint16_t saturation_range_min

    Value of saturation range min field of light hsl saturation range state

  uint16_t saturation_range_max

    Value of saturation range max field of light hsl saturation range state

struct esp_ble_mesh_light_xyl_set_t

  Parameters of Light xyL Set

  Public Members

  bool op_en

    Indicate whether optional parameters included

  uint16_t xyl_lightness

    The target value of the Light xyL Lightness state

  uint16_t xyl_x

    The target value of the Light xyL x state

  uint16_t xyl_y

    The target value of the Light xyL y state

  uint8_t tid

    Transaction Identifier

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_light_xyl_default_set_t

  Parameters of Light xyL Default Set

  Public Members

  uint16_t lightness

    The value of the Light Lightness Default state

  uint16_t xyl_x

    The value of the Light xyL x Default state

  uint16_t xyl_y

    The value of the Light xyL y Default state

struct esp_ble_mesh_light_xyl_range_set_t

  Parameters of Light xyL Range Set

  Public Members

  uint16_t xyl_x_range_min

    The value of the xyL x Range Min field of the Light xyL x Range state

  uint16_t xyl_x_range_max

    The value of the xyL x Range Max field of the Light xyL x Range state

  uint16_t xyl_y_range_min

    The value of the xyL y Range Min field of the Light xyL y Range state

  uint16_t xyl_y_range_max

    The value of the xyL y Range Max field of the Light xyL y Range state

struct esp_ble_mesh_light_lc_mode_set_t

  Parameter of Light LC Mode Set

  Public Members

  uint8_t mode

    The target value of the Light LC Mode state

struct esp_ble_mesh_light_lc_om_set_t

  Parameter of Light LC OM Set

  Public Members

  uint8_t mode

    The target value of the Light LC Occupancy Mode state

struct esp_ble_mesh_light_lc_light_onoff_set_t

  Parameters of Light LC Light OnOff Set

  Public Members

  bool op_en

    Indicate whether optional parameters included

  uint8_t light_onoff

    The target value of the Light LC Light OnOff state

  uint8_t tid

    Transaction Identifier

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_light_lc_property_get_t

  Parameter of Light LC Property Get

  Public Members

  uint16_t property_id

    Property ID identifying a Light LC Property

struct esp_ble_mesh_light_lc_property_set_t

  Parameters of Light LC Property Set

  Public Members

  uint16_t property_id

    Property ID identifying a Light LC Property

  struct net_buf_simple *property_value

    Raw value for the Light LC Property

struct esp_ble_mesh_light_lightness_status_cb_t

  Bluetooth Mesh Light Lightness Client Model Get and Set callback parameters structure.

  Parameters of Light Lightness Status

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t present_lightness

    Current value of light lightness actual state

  uint16_t target_lightness

    Target value of light lightness actual state (optional)

  uint8_t remain_time

    Time to complete state transition (C.1)

struct esp_ble_mesh_light_lightness_linear_status_cb_t

  Parameters of Light Lightness Linear Status

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t present_lightness

    Current value of light lightness linear state

  uint16_t target_lightness

    Target value of light lightness linear state (optional)

  uint8_t remain_time

    Time to complete state transition (C.1)

struct esp_ble_mesh_light_lightness_last_status_cb_t

  Parameter of Light Lightness Last Status

  Public Members

  uint16_t lightness

    The value of the Light Lightness Last state

struct esp_ble_mesh_light_lightness_default_status_cb_t

  Parameter of Light Lightness Default Status

  Public Members

  uint16_t lightness

    The value of the Light Lightness default State

struct esp_ble_mesh_light_lightness_range_status_cb_t

  Parameters of Light Lightness Range Status

  Public Members

  uint8_t status_code

    Status Code for the request message

  uint16_t range_min

    Value of range min field of light lightness range state

  uint16_t range_max

    Value of range max field of light lightness range state

struct esp_ble_mesh_light_ctl_status_cb_t

  Parameters of Light CTL Status

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t present_ctl_lightness

    Current value of light ctl lightness state

  uint16_t present_ctl_temperature

    Current value of light ctl temperature state

  uint16_t target_ctl_lightness

    Target value of light ctl lightness state (optional)

  uint16_t target_ctl_temperature

    Target value of light ctl temperature state (C.1)

  uint8_t remain_time

    Time to complete state transition (C.1)

struct esp_ble_mesh_light_ctl_temperature_status_cb_t

  Parameters of Light CTL Temperature Status

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t present_ctl_temperature

    Current value of light ctl temperature state

  uint16_t present_ctl_delta_uv

    Current value of light ctl delta UV state

  uint16_t target_ctl_temperature

    Target value of light ctl temperature state (optional)

  uint16_t target_ctl_delta_uv

    Target value of light ctl delta UV state (C.1)

  uint8_t remain_time

    Time to complete state transition (C.1)

struct esp_ble_mesh_light_ctl_temperature_range_status_cb_t

  Parameters of Light CTL Temperature Range Status

  Public Members

  uint8_t status_code

    Status code for the request message

  uint16_t range_min

    Value of temperature range min field of light ctl temperature range state

  uint16_t range_max

    Value of temperature range max field of light ctl temperature range state

struct esp_ble_mesh_light_ctl_default_status_cb_t

  Parameters of Light CTL Default Status

  Public Members

  uint16_t lightness

    Value of light lightness default state

  uint16_t temperature

    Value of light temperature default state

  int16_t delta_uv

    Value of light delta UV default state

struct esp_ble_mesh_light_hsl_status_cb_t

  Parameters of Light HSL Status

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t hsl_lightness

    Current value of light hsl lightness state

  uint16_t hsl_hue

    Current value of light hsl hue state

  uint16_t hsl_saturation

    Current value of light hsl saturation state

  uint8_t remain_time

    Time to complete state transition (optional)

struct esp_ble_mesh_light_hsl_target_status_cb_t

  Parameters of Light HSL Target Status

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t hsl_lightness_target

    Target value of light hsl lightness state

  uint16_t hsl_hue_target

    Target value of light hsl hue state

  uint16_t hsl_saturation_target

    Target value of light hsl saturation state

  uint8_t remain_time

    Time to complete state transition (optional)

struct esp_ble_mesh_light_hsl_hue_status_cb_t

  Parameters of Light HSL Hue Status

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t present_hue

    Current value of light hsl hue state

  uint16_t target_hue

    Target value of light hsl hue state (optional)

  uint8_t remain_time

    Time to complete state transition (C.1)

struct esp_ble_mesh_light_hsl_saturation_status_cb_t

  Parameters of Light HSL Saturation Status

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t present_saturation

    Current value of light hsl saturation state

  uint16_t target_saturation

    Target value of light hsl saturation state (optional)

  uint8_t remain_time

    Time to complete state transition (C.1)

struct esp_ble_mesh_light_hsl_default_status_cb_t

  Parameters of Light HSL Default Status

  Public Members

  uint16_t lightness

    Value of light lightness default state

  uint16_t hue

    Value of light hue default state

  uint16_t saturation

    Value of light saturation default state

struct esp_ble_mesh_light_hsl_range_status_cb_t

  Parameters of Light HSL Range Status

  Public Members

  uint8_t status_code

    Status code for the request message

  uint16_t hue_range_min

    Value of hue range min field of light hsl hue range state

  uint16_t hue_range_max

    Value of hue range max field of light hsl hue range state

  uint16_t saturation_range_min

    Value of saturation range min field of light hsl saturation range state

  uint16_t saturation_range_max

    Value of saturation range max field of light hsl saturation range state

struct esp_ble_mesh_light_xyl_status_cb_t

  Parameters of Light xyL Status

  Public Members

  bool op_en

    Indicate whether optional parameters included

  uint16_t xyl_lightness

    The present value of the Light xyL Lightness state

  uint16_t xyl_x

    The present value of the Light xyL x state

  uint16_t xyl_y

    The present value of the Light xyL y state

  uint8_t remain_time

    Time to complete state transition (optional)

struct esp_ble_mesh_light_xyl_target_status_cb_t

  Parameters of Light xyL Target Status

  Public Members

  bool op_en

    Indicate whether optional parameters included

  uint16_t target_xyl_lightness

    The target value of the Light xyL Lightness state

  uint16_t target_xyl_x

    The target value of the Light xyL x state

  uint16_t target_xyl_y

    The target value of the Light xyL y state

  uint8_t remain_time

    Time to complete state transition (optional)

struct esp_ble_mesh_light_xyl_default_status_cb_t

  Parameters of Light xyL Default Status

  Public Members

  uint16_t lightness

    The value of the Light Lightness Default state

  uint16_t xyl_x

    The value of the Light xyL x Default state

  uint16_t xyl_y

    The value of the Light xyL y Default state

struct esp_ble_mesh_light_xyl_range_status_cb_t

  Parameters of Light xyL Range Status

  Public Members

  uint8_t status_code

    Status Code for the requesting message

  uint16_t xyl_x_range_min

    The value of the xyL x Range Min field of the Light xyL x Range state

  uint16_t xyl_x_range_max

    The value of the xyL x Range Max field of the Light xyL x Range state

  uint16_t xyl_y_range_min

    The value of the xyL y Range Min field of the Light xyL y Range state

  uint16_t xyl_y_range_max

    The value of the xyL y Range Max field of the Light xyL y Range state

struct esp_ble_mesh_light_lc_mode_status_cb_t

  Parameter of Light LC Mode Status

  Public Members

  uint8_t mode

    The present value of the Light LC Mode state

struct esp_ble_mesh_light_lc_om_status_cb_t

  Parameter of Light LC OM Status

  Public Members

  uint8_t mode

    The present value of the Light LC Occupancy Mode state

struct esp_ble_mesh_light_lc_light_onoff_status_cb_t

  Parameters of Light LC Light OnOff Status

  Public Members

  bool op_en

    Indicate whether optional parameters included

  uint8_t present_light_onoff

    The present value of the Light LC Light OnOff state

  uint8_t target_light_onoff

    The target value of the Light LC Light OnOff state (Optional)

  uint8_t remain_time

    Time to complete state transition (C.1)

struct esp_ble_mesh_light_lc_property_status_cb_t

  Parameters of Light LC Property Status

  Public Members

  uint16_t property_id

    Property ID identifying a Light LC Property

  struct net_buf_simple *property_value

    Raw value for the Light LC Property

struct esp_ble_mesh_light_client_cb_param_t

  Lighting Client Model callback parameters

  Public Members

  int error_code

    Appropriate error code

  esp_ble_mesh_client_common_param_t *params

    The client common parameters.

  esp_ble_mesh_light_client_status_cb_t status_cb

    The light status message callback values

struct esp_ble_mesh_light_lightness_state_t

  Parameters of Light Lightness state

  Public Members

  uint16_t lightness_linear

    The present value of Light Lightness Linear state

  uint16_t target_lightness_linear

    The target value of Light Lightness Linear state

  uint16_t lightness_actual

    The present value of Light Lightness Actual state

  uint16_t target_lightness_actual

    The target value of Light Lightness Actual state

  uint16_t lightness_last

    The value of Light Lightness Last state

  uint16_t lightness_default

    The value of Light Lightness Default state

  uint8_t status_code

    The status code of setting Light Lightness Range state

  uint16_t lightness_range_min

    The minimum value of Light Lightness Range state

  uint16_t lightness_range_max

    The maximum value of Light Lightness Range state

struct esp_ble_mesh_light_lightness_srv_t

  User data of Light Lightness Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting Lightness Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_lightness_state_t *state

    Parameters of the Light Lightness state

  esp_ble_mesh_last_msg_info_t last

    Parameters of the last received set message

  esp_ble_mesh_state_transition_t actual_transition

    Parameters of state transition

  esp_ble_mesh_state_transition_t linear_transition

    Parameters of state transition

  int32_t tt_delta_lightness_actual

    Delta change value of lightness actual state transition

  int32_t tt_delta_lightness_linear

    Delta change value of lightness linear state transition

struct esp_ble_mesh_light_lightness_setup_srv_t

  User data of Light Lightness Setup Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting Lightness Setup Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_lightness_state_t *state

    Parameters of the Light Lightness state

struct esp_ble_mesh_light_ctl_state_t

  Parameters of Light CTL state

  Public Members

  uint16_t lightness

    The present value of Light CTL Lightness state

  uint16_t target_lightness

    The target value of Light CTL Lightness state

  uint16_t temperature

    The present value of Light CTL Temperature state

  uint16_t target_temperature

    The target value of Light CTL Temperature state

  int16_t delta_uv

    The present value of Light CTL Delta UV state

  int16_t target_delta_uv

    The target value of Light CTL Delta UV state

  uint8_t status_code

    The statue code of setting Light CTL Temperature Range state

  uint16_t temperature_range_min

    The minimum value of Light CTL Temperature Range state

  uint16_t temperature_range_max

    The maximum value of Light CTL Temperature Range state

  uint16_t lightness_default

    The value of Light Lightness Default state

  uint16_t temperature_default

    The value of Light CTL Temperature Default state

  int16_t delta_uv_default

    The value of Light CTL Delta UV Default state

struct esp_ble_mesh_light_ctl_srv_t

  User data of Light CTL Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting CTL Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_ctl_state_t *state

    Parameters of the Light CTL state

  esp_ble_mesh_last_msg_info_t last

    Parameters of the last received set message

  esp_ble_mesh_state_transition_t transition

    Parameters of state transition

  int32_t tt_delta_lightness

    Delta change value of lightness state transition

  int32_t tt_delta_temperature

    Delta change value of temperature state transition

  int32_t tt_delta_delta_uv

    Delta change value of delta uv state transition

struct esp_ble_mesh_light_ctl_setup_srv_t

  User data of Light CTL Setup Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting CTL Setup Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_ctl_state_t *state

    Parameters of the Light CTL state

struct esp_ble_mesh_light_ctl_temp_srv_t

  User data of Light CTL Temperature Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting CTL Temperature Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_ctl_state_t *state

    Parameters of the Light CTL state

  esp_ble_mesh_last_msg_info_t last

    Parameters of the last received set message

  esp_ble_mesh_state_transition_t transition

    Parameters of state transition

  int32_t tt_delta_temperature

    Delta change value of temperature state transition

  int32_t tt_delta_delta_uv

    Delta change value of delta uv state transition

struct esp_ble_mesh_light_hsl_state_t

  Parameters of Light HSL state

  Public Members

  uint16_t lightness

    The present value of Light HSL Lightness state

  uint16_t target_lightness

    The target value of Light HSL Lightness state

  uint16_t hue

    The present value of Light HSL Hue state

  uint16_t target_hue

    The target value of Light HSL Hue state

  uint16_t saturation

    The present value of Light HSL Saturation state

  uint16_t target_saturation

    The target value of Light HSL Saturation state

  uint16_t lightness_default

    The value of Light Lightness Default state

  uint16_t hue_default

    The value of Light HSL Hue Default state

  uint16_t saturation_default

    The value of Light HSL Saturation Default state

  uint8_t status_code

    The status code of setting Light HSL Hue & Saturation Range state

  uint16_t hue_range_min

    The minimum value of Light HSL Hue Range state

  uint16_t hue_range_max

    The maximum value of Light HSL Hue Range state

  uint16_t saturation_range_min

    The minimum value of Light HSL Saturation state

  uint16_t saturation_range_max

    The maximum value of Light HSL Saturation state

struct esp_ble_mesh_light_hsl_srv_t

  User data of Light HSL Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting HSL Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_hsl_state_t *state

    Parameters of the Light HSL state

  esp_ble_mesh_last_msg_info_t last

    Parameters of the last received set message

  esp_ble_mesh_state_transition_t transition

    Parameters of state transition

  int32_t tt_delta_lightness

    Delta change value of lightness state transition

  int32_t tt_delta_hue

    Delta change value of hue state transition

  int32_t tt_delta_saturation

    Delta change value of saturation state transition

struct esp_ble_mesh_light_hsl_setup_srv_t

  User data of Light HSL Setup Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting HSL Setup Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_hsl_state_t *state

    Parameters of the Light HSL state

struct esp_ble_mesh_light_hsl_hue_srv_t

  User data of Light HSL Hue Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting HSL Hue Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_hsl_state_t *state

    Parameters of the Light HSL state

  esp_ble_mesh_last_msg_info_t last

    Parameters of the last received set message

  esp_ble_mesh_state_transition_t transition

    Parameters of state transition

  int32_t tt_delta_hue

    Delta change value of hue state transition

struct esp_ble_mesh_light_hsl_sat_srv_t

  User data of Light HSL Saturation Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting HSL Saturation Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_hsl_state_t *state

    Parameters of the Light HSL state

  esp_ble_mesh_last_msg_info_t last

    Parameters of the last received set message

  esp_ble_mesh_state_transition_t transition

    Parameters of state transition

  int32_t tt_delta_saturation

    Delta change value of saturation state transition

struct esp_ble_mesh_light_xyl_state_t

  Parameters of Light xyL state

  Public Members

  uint16_t lightness

    The present value of Light xyL Lightness state

  uint16_t target_lightness

    The target value of Light xyL Lightness state

  uint16_t x

    The present value of Light xyL x state

  uint16_t target_x

    The target value of Light xyL x state

  uint16_t y

    The present value of Light xyL y state

  uint16_t target_y

    The target value of Light xyL y state

  uint16_t lightness_default

    The value of Light Lightness Default state

  uint16_t x_default

    The value of Light xyL x Default state

  uint16_t y_default

    The value of Light xyL y Default state

  uint8_t status_code

    The status code of setting Light xyL x & y Range state

  uint16_t x_range_min

    The minimum value of Light xyL x Range state

  uint16_t x_range_max

    The maximum value of Light xyL x Range state

  uint16_t y_range_min

    The minimum value of Light xyL y Range state

  uint16_t y_range_max

    The maximum value of Light xyL y Range state

struct esp_ble_mesh_light_xyl_srv_t

  User data of Light xyL Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting xyL Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_xyl_state_t *state

    Parameters of the Light xyL state

  esp_ble_mesh_last_msg_info_t last

    Parameters of the last received set message

  esp_ble_mesh_state_transition_t transition

    Parameters of state transition

  int32_t tt_delta_lightness

    Delta change value of lightness state transition

  int32_t tt_delta_x

    Delta change value of x state transition

  int32_t tt_delta_y

    Delta change value of y state transition

struct esp_ble_mesh_light_xyl_setup_srv_t

  User data of Light xyL Setup Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting xyL Setup Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_xyl_state_t *state

    Parameters of the Light xyL state

struct esp_ble_mesh_light_lc_state_t

  Parameters of Light LC states

  Public Members

  uint32_t mode

    0b0 The controller is turned off.

    - The binding with the Light Lightness state is disabled. 0b1 The controller is turned on.

    - The binding with the Light Lightness state is enabled. The value of Light LC Mode state

  uint32_t occupancy_mode

    The value of Light LC Occupancy Mode state

  uint32_t light_onoff

    The present value of Light LC Light OnOff state

  uint32_t target_light_onoff

    The target value of Light LC Light OnOff state

  uint32_t occupancy

    The value of Light LC Occupancy state

  uint32_t ambient_luxlevel

    The value of Light LC Ambient LuxLevel state

  uint16_t linear_output

    1. Light LC Linear Output = max((Lightness Out)^2/65535, Regulator Output)

    2. If the Light LC Mode state is set to 0b1, the binding is enabled and upon a change of the Light LC Linear Output state, the following operation shall be performed: Light Lightness Linear = Light LC Linear Output

    3. If the Light LC Mode state is set to 0b0, the binding is disabled (i.e., upon a change of the Light LC Linear Output state, no operation on the Light Lightness Linear state is performed). The value of Light LC Linear Output state

struct esp_ble_mesh_light_lc_property_state_t

  Parameters of Light Property states. The Light LC Property states are read / write states that determine the configuration of a Light Lightness Controller. Each state is represented by a device property and is controlled by Light LC Property messages.

  Public Members

  uint32_t time_occupancy_delay

    A timing state that determines the delay for changing the Light LC Occupancy state upon receiving a Sensor Status message from an occupancy sensor. The value of Light LC Time Occupancy Delay state

  uint32_t time_fade_on

    A timing state that determines the time the controlled lights fade to the level determined by the Light LC Lightness On state. The value of Light LC Time Fade On state

  uint32_t time_run_on

    A timing state that determines the time the controlled lights stay at the level determined by the Light LC Lightness On state. The value of Light LC Time Run On state

  uint32_t time_fade

    A timing state that determines the time the controlled lights fade from the level determined by the Light LC Lightness On state to the level determined by the Light Lightness Prolong state. The value of Light LC Time Fade state

  uint32_t time_prolong

    A timing state that determines the time the controlled lights stay at the level determined by the Light LC Lightness Prolong state. The value of Light LC Time Prolong state

  uint32_t time_fade_standby_auto

    A timing state that determines the time the controlled lights fade from the level determined by the Light LC Lightness Prolong state to the level determined by the Light LC Lightness Standby state when the transition is automatic. The value of Light LC Time Fade Standby Auto state

  uint32_t time_fade_standby_manual

    A timing state that determines the time the controlled lights fade from the level determined by the Light LC Lightness Prolong state to the level determined by the Light LC Lightness Standby state when the transition is triggered by a change in the Light LC Light OnOff state. The value of Light LC Time Fade Standby Manual state

  uint16_t lightness_on

    A lightness state that determines the perceptive light lightness at the Occupancy and Run internal controller states. The value of Light LC Lightness On state

  uint16_t lightness_prolong

    A lightness state that determines the light lightness at the Prolong internal controller state. The value of Light LC Lightness Prolong state

  uint16_t lightness_standby

    A lightness state that determines the light lightness at the Standby internal controller state. The value of Light LC Lightness Standby state

  uint16_t ambient_luxlevel_on

    A uint16 state representing the Ambient LuxLevel level that determines if the controller transitions from the Light Control Standby state. The value of Light LC Ambient LuxLevel On state

  uint16_t ambient_luxlevel_prolong

    A uint16 state representing the required Ambient LuxLevel level in the Prolong state. The value of Light LC Ambient LuxLevel Prolong state

  uint16_t ambient_luxlevel_standby

    A uint16 state representing the required Ambient LuxLevel level in the Standby state. The value of Light LC Ambient LuxLevel Standby state

  float regulator_kiu

    A float32 state representing the integral coefficient that determines the integral part of the equation defining the output of the Light LC PI Feedback Regulator, when Light LC Ambient LuxLevel is less than LuxLevel Out. Valid range: 0.0 ~ 1000.0. The default value is 250.0. The value of Light LC Regulator Kiu state

  float regulator_kid

    A float32 state representing the integral coefficient that determines the integral part of the equation defining the output of the Light LC PI Feedback Regulator, when Light LC Ambient LuxLevel is greater than or equal to the value of the LuxLevel Out state. Valid range: 0.0 ~ 1000.0. The default value is 25.0. The value of Light LC Regulator Kid state

  float regulator_kpu

    A float32 state representing the proportional coefficient that determines the proportional part of the equation defining the output of the Light LC PI Feedback Regulator, when Light LC Ambient LuxLevel is less than the value of the LuxLevel Out state. Valid range: 0.0 ~ 1000.0. The default value is 80.0. The value of Light LC Regulator Kpu state

  float regulator_kpd

    A float32 state representing the proportional coefficient that determines the proportional part of the equation defining the output of the Light LC PI Feedback Regulator, when Light LC Ambient LuxLevel is greater than or equal to the value of the LuxLevel Out state. Valid range: 0.0 ~ 1000.0. The default value is 80.0. The value of Light LC Regulator Kpd state

  int8_t regulator_accuracy

    A int8 state representing the percentage accuracy of the Light LC PI Feedback Regulator. Valid range: 0.0 ~ 100.0. The default value is 2.0. The value of Light LC Regulator Accuracy state

  uint32_t set_occupancy_to_1_delay

    If the message Raw field contains a Raw Value for the Time Since Motion Sensed device property, which represents a value less than or equal to the value of the Light LC Occupancy Delay state, it shall delay setting the Light LC Occupancy state to 0b1 by the difference between the value of the Light LC Occupancy Delay state and the received Time Since Motion value. The value of the difference between value of the Light LC Occupancy Delay state and the received Time Since Motion value

struct esp_ble_mesh_light_lc_state_machine_t

  Parameters of Light LC state machine

  Public Members

  uint8_t fade_on

    The value of transition time of Light LC Time Fade On

  uint8_t fade

    The value of transition time of Light LC Time Fade

  uint8_t fade_standby_auto

    The value of transition time of Light LC Time Fade Standby Auto

  uint8_t fade_standby_manual

    The value of transition time of Light LC Time Fade Standby Manual

  struct esp_ble_mesh_light_lc_state_machine_t trans_time

    The Fade On, Fade, Fade Standby Auto, and Fade Standby Manual states are transition states that define the transition of the Lightness Out and LuxLevel Out states. This transition can be started as a result of the Light LC State Machine change or as a result of receiving the Light LC Light OnOff Set or Light LC Light Set Unacknowledged message. The value of transition time

  esp_ble_mesh_lc_state_t state

    The value of Light LC state machine state

  struct k_delayed_work timer

    Timer of Light LC state machine

struct esp_ble_mesh_light_control_t

  Parameters of Light Lightness controller

  Public Members

  esp_ble_mesh_light_lc_state_t state

    Parameters of Light LC state

  esp_ble_mesh_light_lc_property_state_t prop_state

    Parameters of Light LC Property state

  esp_ble_mesh_light_lc_state_machine_t state_machine

    Parameters of Light LC state machine

struct esp_ble_mesh_light_lc_srv_t

  User data of Light LC Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting LC Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_control_t *lc

    Parameters of the Light controller

  esp_ble_mesh_last_msg_info_t last

    Parameters of the last received set message

  esp_ble_mesh_state_transition_t transition

    Parameters of state transition

struct esp_ble_mesh_light_lc_setup_srv_t

  User data of Light LC Setup Server Model

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the Lighting LC Setup Server Model. Initialized internally.

  esp_ble_mesh_server_rsp_ctrl_t rsp_ctrl

    Response control of the server model received messages

  esp_ble_mesh_light_control_t *lc

    Parameters of the Light controller

struct esp_ble_mesh_state_change_light_lightness_set_t

  Parameter of Light Lightness Actual state change event

  Public Members

  uint16_t lightness

    The value of Light Lightness Actual state

struct esp_ble_mesh_state_change_light_lightness_linear_set_t

  Parameter of Light Lightness Linear state change event

  Public Members

  uint16_t lightness

    The value of Light Lightness Linear state

struct esp_ble_mesh_state_change_light_lightness_default_set_t

  Parameter of Light Lightness Default state change event

  Public Members

  uint16_t lightness

    The value of Light Lightness Default state

struct esp_ble_mesh_state_change_light_lightness_range_set_t

  Parameters of Light Lightness Range state change event

  Public Members

  uint16_t range_min

    The minimum value of Light Lightness Range state

  uint16_t range_max

    The maximum value of Light Lightness Range state

struct esp_ble_mesh_state_change_light_ctl_set_t

  Parameters of Light CTL state change event

  Public Members

  uint16_t lightness

    The value of Light CTL Lightness state

  uint16_t temperature

    The value of Light CTL Temperature state

  int16_t delta_uv

    The value of Light CTL Delta UV state

struct esp_ble_mesh_state_change_light_ctl_temperature_set_t

  Parameters of Light CTL Temperature state change event

  Public Members

  uint16_t temperature

    The value of Light CTL Temperature state

  int16_t delta_uv

    The value of Light CTL Delta UV state

struct esp_ble_mesh_state_change_light_ctl_temperature_range_set_t

  Parameters of Light CTL Temperature Range state change event

  Public Members

  uint16_t range_min

    The minimum value of Light CTL Temperature Range state

  uint16_t range_max

    The maximum value of Light CTL Temperature Range state

struct esp_ble_mesh_state_change_light_ctl_default_set_t

  Parameters of Light CTL Default state change event

  Public Members

  uint16_t lightness

    The value of Light Lightness Default state

  uint16_t temperature

    The value of Light CTL Temperature Default state

  int16_t delta_uv

    The value of Light CTL Delta UV Default state

struct esp_ble_mesh_state_change_light_hsl_set_t

  Parameters of Light HSL state change event

  Public Members

  uint16_t lightness

    The value of Light HSL Lightness state

  uint16_t hue

    The value of Light HSL Hue state

  uint16_t saturation

    The value of Light HSL Saturation state

struct esp_ble_mesh_state_change_light_hsl_hue_set_t

  Parameter of Light HSL Hue state change event

  Public Members

  uint16_t hue

    The value of Light HSL Hue state

struct esp_ble_mesh_state_change_light_hsl_saturation_set_t

  Parameter of Light HSL Saturation state change event

  Public Members

  uint16_t saturation

    The value of Light HSL Saturation state

struct esp_ble_mesh_state_change_light_hsl_default_set_t

  Parameters of Light HSL Default state change event

  Public Members

  uint16_t lightness

    The value of Light HSL Lightness Default state

  uint16_t hue

    The value of Light HSL Hue Default state

  uint16_t saturation

    The value of Light HSL Saturation Default state

struct esp_ble_mesh_state_change_light_hsl_range_set_t

  Parameters of Light HSL Range state change event

  Public Members

  uint16_t hue_range_min

    The minimum hue value of Light HSL Range state

  uint16_t hue_range_max

    The maximum hue value of Light HSL Range state

  uint16_t saturation_range_min

    The minimum saturation value of Light HSL Range state

  uint16_t saturation_range_max

    The maximum saturation value of Light HSL Range state

struct esp_ble_mesh_state_change_light_xyl_set_t

  Parameters of Light xyL state change event

  Public Members

  uint16_t lightness

    The value of Light xyL Lightness state

  uint16_t x

    The value of Light xyL x state

  uint16_t y

    The value of Light xyL y state

struct esp_ble_mesh_state_change_light_xyl_default_set_t

  Parameters of Light xyL Default state change event

  Public Members

  uint16_t lightness

    The value of Light Lightness Default state

  uint16_t x

    The value of Light xyL x Default state

  uint16_t y

    The value of Light xyL y Default state

struct esp_ble_mesh_state_change_light_xyl_range_set_t

  Parameters of Light xyL Range state change event

  Public Members

  uint16_t x_range_min

    The minimum value of Light xyL x Range state

  uint16_t x_range_max

    The maximum value of Light xyL x Range state

  uint16_t y_range_min

    The minimum value of Light xyL y Range state

  uint16_t y_range_max

    The maximum value of Light xyL y Range state

struct esp_ble_mesh_state_change_light_lc_mode_set_t

  Parameter of Light LC Mode state change event

  Public Members

  uint8_t mode

    The value of Light LC Mode state

struct esp_ble_mesh_state_change_light_lc_om_set_t

  Parameter of Light LC Occupancy Mode state change event

  Public Members

  uint8_t mode

    The value of Light LC Occupancy Mode state

struct esp_ble_mesh_state_change_light_lc_light_onoff_set_t

  Parameter of Light LC Light OnOff state change event

  Public Members

  uint8_t onoff

    The value of Light LC Light OnOff state

struct esp_ble_mesh_state_change_light_lc_property_set_t

  Parameters of Light LC Property state change event

  Public Members

  uint16_t property_id

    The property id of Light LC Property state

  struct net_buf_simple *property_value

    The property value of Light LC Property state

struct esp_ble_mesh_state_change_sensor_status_t

  Parameters of Sensor Status state change event

  Public Members

  uint16_t property_id

    The value of Sensor Property ID

  uint8_t occupancy

    The value of Light LC Occupancy state

  uint32_t set_occupancy_to_1_delay

    The value of Light LC Set Occupancy to 1 Delay state

  uint32_t ambient_luxlevel

    The value of Light LC Ambient Luxlevel state

  union esp_ble_mesh_state_change_sensor_status_t state

    Parameters of Sensor Status related state

struct esp_ble_mesh_server_recv_light_lc_property_get_t

  Context of the received Light LC Property Get message

  Public Members

  uint16_t property_id

    Property ID identifying a Light LC Property

struct esp_ble_mesh_server_recv_light_lightness_set_t

  Context of the received Light Lightness Set message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t lightness

    Target value of light lightness actual state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_light_lightness_linear_set_t

  Context of the received Light Lightness Linear Set message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t lightness

    Target value of light lightness linear state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_light_lightness_default_set_t

  Context of the received Light Lightness Default Set message

  Public Members

  uint16_t lightness

    The value of the Light Lightness Default state

struct esp_ble_mesh_server_recv_light_lightness_range_set_t

  Context of the received Light Lightness Range Set message

  Public Members

  uint16_t range_min

    Value of range min field of light lightness range state

  uint16_t range_max

    Value of range max field of light lightness range state

struct esp_ble_mesh_server_recv_light_ctl_set_t

  Context of the received Light CTL Set message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t lightness

    Target value of light ctl lightness state

  uint16_t temperature

    Target value of light ctl temperature state

  int16_t delta_uv

    Target value of light ctl delta UV state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_light_ctl_temperature_set_t

  Context of the received Light CTL Temperature Set message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t temperature

    Target value of light ctl temperature state

  int16_t delta_uv

    Target value of light ctl delta UV state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_light_ctl_temperature_range_set_t

  Context of the received Light CTL Temperature Range Set message

  Public Members

  uint16_t range_min

    Value of temperature range min field of light ctl temperature range state

  uint16_t range_max

    Value of temperature range max field of light ctl temperature range state

struct esp_ble_mesh_server_recv_light_ctl_default_set_t

  Context of the received Light CTL Default Set message

  Public Members

  uint16_t lightness

    Value of light lightness default state

  uint16_t temperature

    Value of light temperature default state

  int16_t delta_uv

    Value of light delta UV default state

struct esp_ble_mesh_server_recv_light_hsl_set_t

  Context of the received Light HSL Set message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t lightness

    Target value of light hsl lightness state

  uint16_t hue

    Target value of light hsl hue state

  uint16_t saturation

    Target value of light hsl saturation state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_light_hsl_hue_set_t

  Context of the received Light HSL Hue Set message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t hue

    Target value of light hsl hue state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_light_hsl_saturation_set_t

  Context of the received Light HSL Saturation Set message

  Public Members

  bool op_en

    Indicate if optional parameters are included

  uint16_t saturation

    Target value of light hsl hue state

  uint8_t tid

    Transaction ID

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_light_hsl_default_set_t

  Context of the received Light HSL Default Set message

  Public Members

  uint16_t lightness

    Value of light lightness default state

  uint16_t hue

    Value of light hue default state

  uint16_t saturation

    Value of light saturation default state

struct esp_ble_mesh_server_recv_light_hsl_range_set_t

  Context of the received Light HSL Range Set message

  Public Members

  uint16_t hue_range_min

    Value of hue range min field of light hsl hue range state

  uint16_t hue_range_max

    Value of hue range max field of light hsl hue range state

  uint16_t saturation_range_min

    Value of saturation range min field of light hsl saturation range state

  uint16_t saturation_range_max

    Value of saturation range max field of light hsl saturation range state

struct esp_ble_mesh_server_recv_light_xyl_set_t

  Context of the received Light xyL Set message

  Public Members

  bool op_en

    Indicate whether optional parameters included

  uint16_t lightness

    The target value of the Light xyL Lightness state

  uint16_t x

    The target value of the Light xyL x state

  uint16_t y

    The target value of the Light xyL y state

  uint8_t tid

    Transaction Identifier

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_light_xyl_default_set_t

  Context of the received Light xyL Default Set message

  Public Members

  uint16_t lightness

    The value of the Light Lightness Default state

  uint16_t x

    The value of the Light xyL x Default state

  uint16_t y

    The value of the Light xyL y Default state

struct esp_ble_mesh_server_recv_light_xyl_range_set_t

  Context of the received Light xyl Range Set message

  Public Members

  uint16_t x_range_min

    The value of the xyL x Range Min field of the Light xyL x Range state

  uint16_t x_range_max

    The value of the xyL x Range Max field of the Light xyL x Range state

  uint16_t y_range_min

    The value of the xyL y Range Min field of the Light xyL y Range state

  uint16_t y_range_max

    The value of the xyL y Range Max field of the Light xyL y Range state

struct esp_ble_mesh_server_recv_light_lc_mode_set_t

  Context of the received Light LC Mode Set message

  Public Members

  uint8_t mode

    The target value of the Light LC Mode state

struct esp_ble_mesh_server_recv_light_lc_om_set_t

  Context of the received Light OM Set message

  Public Members

  uint8_t mode

    The target value of the Light LC Occupancy Mode state

struct esp_ble_mesh_server_recv_light_lc_light_onoff_set_t

  Context of the received Light LC Light OnOff Set message

  Public Members

  bool op_en

    Indicate whether optional parameters included

  uint8_t light_onoff

    The target value of the Light LC Light OnOff state

  uint8_t tid

    Transaction Identifier

  uint8_t trans_time

    Time to complete state transition (optional)

  uint8_t delay

    Indicate message execution delay (C.1)

struct esp_ble_mesh_server_recv_light_lc_property_set_t

  Context of the received Light LC Property Set message

  Public Members

  uint16_t property_id

    Property ID identifying a Light LC Property

  struct net_buf_simple *property_value

    Raw value for the Light LC Property

struct esp_ble_mesh_server_recv_sensor_status_t

  Context of the received Sensor Status message

  Public Members

  struct net_buf_simple *data

    Value of sensor data state (optional)

struct esp_ble_mesh_lighting_server_cb_param_t

  Lighting Server Model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to Lighting Server Models

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received messages

  esp_ble_mesh_lighting_server_cb_value_t value

    Value of the received Lighting Messages

### Macros

ESP_BLE_MESH_MODEL_LIGHT_LIGHTNESS_CLI(cli_pub, cli_data)

  Define a new Light Lightness Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Light Lightness Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Light Lightness Client Model instance.

ESP_BLE_MESH_MODEL_LIGHT_CTL_CLI(cli_pub, cli_data)

  Define a new Light CTL Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Light CTL Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Light CTL Client Model instance.

ESP_BLE_MESH_MODEL_LIGHT_HSL_CLI(cli_pub, cli_data)

  Define a new Light HSL Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Light HSL Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Light HSL Client Model instance.

ESP_BLE_MESH_MODEL_LIGHT_XYL_CLI(cli_pub, cli_data)

  Define a new Light xyL Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Light xyL Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Light xyL Client Model instance.

ESP_BLE_MESH_MODEL_LIGHT_LC_CLI(cli_pub, cli_data)

  Define a new Light LC Client Model.

  备注

  This API needs to be called for each element on which the application needs to have a Light LC Client Model.

  参数:

    - cli_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - cli_data -- Pointer to the unique struct esp_ble_mesh_client_t.

  返回:

    New Light LC Client Model instance.

ESP_BLE_MESH_MODEL_LIGHT_LIGHTNESS_SRV(srv_pub, srv_data)

  Lighting Server Models related context.

  Define a new Light Lightness Server Model.

  备注

  1. The Light Lightness Server model extends the Generic Power OnOff Server model and the Generic Level Server model. When this model is present on an Element, the corresponding Light Lightness Setup Server model shall also be present.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_lightness_srv_t.

  返回:

    New Light Lightness Server Model instance.

ESP_BLE_MESH_MODEL_LIGHT_LIGHTNESS_SETUP_SRV(srv_pub, srv_data)

  Define a new Light Lightness Setup Server Model.

  备注

  1. The Light Lightness Setup Server model extends the Light Lightness Server model and the Generic Power OnOff Setup Server model.

  1. This model shall support model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_lightness_setup_srv_t.

  返回:

    New Light Lightness Setup Server Model instance.

ESP_BLE_MESH_MODEL_LIGHT_CTL_SRV(srv_pub, srv_data)

  Define a new Light CTL Server Model.

  备注

  1. The Light CTL Server model extends the Light Lightness Server model. When this model is present on an Element, the corresponding Light CTL Temperature Server model and the corresponding Light CTL Setup Server model shall also be present.

  1. This model shall support model publication and model subscription.

  2. The model requires two elements: the main element and the Temperature element. The Temperature element contains the corresponding Light CTL Temperature Server model and an instance of a Generic Level state bound to the Light CTL Temperature state on the Temperature element. The Light CTL Temperature state on the Temperature element is bound to the Light CTL state on the main element.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_ctl_srv_t.

  返回:

    New Light CTL Server Model instance.

ESP_BLE_MESH_MODEL_LIGHT_CTL_SETUP_SRV(srv_pub, srv_data)

  Define a new Light CTL Setup Server Model.

  备注

  1. The Light CTL Setup Server model extends the Light CTL Server and the Light Lightness Setup Server.

  1. This model shall support model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_ctl_setup_srv_t.

  返回:

    New Light CTL Setup Server Model instance.

ESP_BLE_MESH_MODEL_LIGHT_CTL_TEMP_SRV(srv_pub, srv_data)

  Define a new Light CTL Temperature Server Model.

  备注

  1. The Light CTL Temperature Server model extends the Generic Level Server model.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_ctl_temp_srv_t.

  返回:

    New Light CTL Temperature Server Model instance.

ESP_BLE_MESH_MODEL_LIGHT_HSL_SRV(srv_pub, srv_data)

  Define a new Light HSL Server Model.

  备注

  1. The Light HSL Server model extends the Light Lightness Server model. When this model is present on an Element, the corresponding Light HSL Hue Server model and the corresponding Light HSL Saturation Server model and the corresponding Light HSL Setup Server model shall also be present.

  1. This model shall support model publication and model subscription.

  2. The model requires three elements: the main element and the Hue element and the Saturation element. The Hue element contains the corresponding Light HSL Hue Server model and an instance of a Generic Level state bound to the Light HSL Hue state on the Hue element. The Saturation element contains the corresponding Light HSL Saturation Server model and an instance of a Generic Level state bound to the Light HSL Saturation state on the Saturation element. The Light HSL Hue state on the Hue element is bound to the Light HSL state on the main element and the Light HSL Saturation state on the Saturation element is bound to the Light HSL state on the main element.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_hsl_srv_t.

  返回:

    New Light HSL Server Model instance.

ESP_BLE_MESH_MODEL_LIGHT_HSL_SETUP_SRV(srv_pub, srv_data)

  Define a new Light HSL Setup Server Model.

  备注

  1. The Light HSL Setup Server model extends the Light HSL Server and the Light Lightness Setup Server.

  1. This model shall support model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_hsl_setup_srv_t.

  返回:

    New Light HSL Setup Server Model instance.

ESP_BLE_MESH_MODEL_LIGHT_HSL_HUE_SRV(srv_pub, srv_data)

  Define a new Light HSL Hue Server Model.

  备注

  1. The Light HSL Hue Server model extends the Generic Level Server model. This model is associated with the Light HSL Server model.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_hsl_hue_srv_t.

  返回:

    New Light HSL Hue Server Model instance.

ESP_BLE_MESH_MODEL_LIGHT_HSL_SAT_SRV(srv_pub, srv_data)

  Define a new Light HSL Saturation Server Model.

  备注

  1. The Light HSL Saturation Server model extends the Generic Level Server model. This model is associated with the Light HSL Server model.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_hsl_sat_srv_t.

  返回:

    New Light HSL Saturation Server Model instance.

ESP_BLE_MESH_MODEL_LIGHT_XYL_SRV(srv_pub, srv_data)

  Define a new Light xyL Server Model.

  备注

  1. The Light xyL Server model extends the Light Lightness Server model. When this model is present on an Element, the corresponding Light xyL Setup Server model shall also be present.

  1. This model shall support model publication and model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_xyl_srv_t.

  返回:

    New Light xyL Server Model instance.

ESP_BLE_MESH_MODEL_LIGHT_XYL_SETUP_SRV(srv_pub, srv_data)

  Define a new Light xyL Setup Server Model.

  备注

  1. The Light xyL Setup Server model extends the Light xyL Server and the Light Lightness Setup Server.

  1. This model shall support model subscription.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_xyl_setup_srv_t.

  返回:

    New Light xyL Setup Server Model instance.

ESP_BLE_MESH_MODEL_LIGHT_LC_SRV(srv_pub, srv_data)

  Define a new Light LC Server Model.

  备注

  1. The Light LC (Lightness Control) Server model extends the Light Lightness Server model and the Generic OnOff Server model. When this model is present on an Element, the corresponding Light LC Setup Server model shall also be present.

  1. This model shall support model publication and model subscription.

  2. This model may be used to represent an element that is a client to a Sensor Server model and controls the Light Lightness Actual state via defined state bindings.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_lc_srv_t.

  返回:

    New Light LC Server Model instance.

ESP_BLE_MESH_MODEL_LIGHT_LC_SETUP_SRV(srv_pub, srv_data)

  Define a new Light LC Setup Server Model.

  备注

  1. The Light LC (Lightness Control) Setup model extends the Light LC Server model.

  1. This model shall support model publication and model subscription.

  2. This model may be used to configure setup parameters for the Light LC Server model.

  参数:

    - srv_pub -- Pointer to the unique struct esp_ble_mesh_model_pub_t.

    - srv_data -- Pointer to the unique struct esp_ble_mesh_light_lc_setup_srv_t.

  返回:

    New Light LC Setup Server Model instance.

### Type Definitions

typedef void (*esp_ble_mesh_light_client_cb_t)(esp_ble_mesh_light_client_cb_event_t event, esp_ble_mesh_light_client_cb_param_t *param)

  Bluetooth Mesh Light Client Model function.

  Lighting Client Model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_lighting_server_cb_t)(esp_ble_mesh_lighting_server_cb_event_t event, esp_ble_mesh_lighting_server_cb_param_t *param)

  Bluetooth Mesh Lighting Server Model function.

  Lighting Server Model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_light_client_cb_event_t

  This enum value is the event of Lighting Client Model

  Values:

  enumerator ESP_BLE_MESH_LIGHT_CLIENT_GET_STATE_EVT
  enumerator ESP_BLE_MESH_LIGHT_CLIENT_SET_STATE_EVT
  enumerator ESP_BLE_MESH_LIGHT_CLIENT_PUBLISH_EVT
  enumerator ESP_BLE_MESH_LIGHT_CLIENT_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_LIGHT_CLIENT_EVT_MAX

enum esp_ble_mesh_lc_state_t

  This enum value is the Light LC State Machine states

  Values:

  enumerator ESP_BLE_MESH_LC_OFF
  enumerator ESP_BLE_MESH_LC_STANDBY
  enumerator ESP_BLE_MESH_LC_FADE_ON
  enumerator ESP_BLE_MESH_LC_RUN
  enumerator ESP_BLE_MESH_LC_FADE
  enumerator ESP_BLE_MESH_LC_PROLONG
  enumerator ESP_BLE_MESH_LC_FADE_STANDBY_AUTO
  enumerator ESP_BLE_MESH_LC_FADE_STANDBY_MANUAL

enum esp_ble_mesh_lighting_server_cb_event_t

  This enum value is the event of Lighting Server Model

  Values:

  enumerator ESP_BLE_MESH_LIGHTING_SERVER_STATE_CHANGE_EVT

    1. When get_auto_rsp is set to ESP_BLE_MESH_SERVER_AUTO_RSP, no event will be callback to the application layer when Lighting Get messages are received.

    2. When set_auto_rsp is set to ESP_BLE_MESH_SERVER_AUTO_RSP, this event will be callback to the application layer when Lighting Set/Set Unack messages are received.

  enumerator ESP_BLE_MESH_LIGHTING_SERVER_RECV_GET_MSG_EVT

    When get_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, this event will be callback to the application layer when Lighting Get messages are received.

  enumerator ESP_BLE_MESH_LIGHTING_SERVER_RECV_SET_MSG_EVT

    When set_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, this event will be callback to the application layer when Lighting Set/Set Unack messages are received.

  enumerator ESP_BLE_MESH_LIGHTING_SERVER_RECV_STATUS_MSG_EVT

    When status_auto_rsp is set to ESP_BLE_MESH_SERVER_RSP_BY_APP, this event will be callback to the application layer when Sensor Status message is received.

  enumerator ESP_BLE_MESH_LIGHTING_SERVER_EVT_MAX

## ESP-BLE-MESH (v1.1) Core API Reference

备注

This section is a preview version, so the related structures, macros, and APIs may be changed.

This section contains ESP-BLE-MESH v1.1 Core related APIs, event types, event parameters, etc.

This API reference covers 10 components:

- Remote Provisioning

- Directed Forwarding

- Subnet Bridge Configuration

- Mesh Private Beacon

- On-Demand Private Proxy

- SAR Configuration

- Solicitation PDU RPL Configuration

- Opcodes Aggregator

- Large Composition Data

- Composition and Metadata

### Remote Provisioning

### Header File

- components/bt/esp_ble_mesh/v1.1/api/core/include/esp_ble_mesh_rpr_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_rpr_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_rpr_client_callback(esp_ble_mesh_rpr_client_cb_t callback)

  Register BLE Mesh Remote Provisioning Client model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_rpr_client_send(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_rpr_client_msg_t *msg)

  Get the value of Remote Provisioning Server model state with the corresponding get message.

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - msg -- [in] Pointer to Remote Provisioning Client message.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_rpr_client_action(esp_ble_mesh_rpr_client_act_type_t type, esp_ble_mesh_rpr_client_act_param_t *param)

  Remote Provisioning Client model perform related actions, e.g. start remote provisioning.

  参数:

    - type -- [in] Type of the action to be performed.

    - param -- [in] Parameters of the action to be performed.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_rpr_server_callback(esp_ble_mesh_rpr_server_cb_t callback)

  Register BLE Mesh Remote Provisioning Server model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_rpr_server_set_uuid_match(const uint8_t *match_val, uint8_t match_len, uint8_t offset)

  This function is called by Remote Provisioning Server to set the part of the device UUID to be compared before starting to remote provision.

  参数:

    - match_val -- [in] Value to be compared with the part of the device UUID.

    - match_len -- [in] Length of the compared match value.

    - offset -- [in] Offset of the device UUID to be compared (based on zero).

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_rpr_client_msg_t
  #include <esp_ble_mesh_rpr_model_api.h>

  Remote Provisioning Client model message union.

  Public Members

  esp_ble_mesh_rpr_scan_start_t scan_start

    For ESP_BLE_MESH_MODEL_OP_RPR_SCAN_START

  esp_ble_mesh_rpr_ext_scan_start_t ext_scan_start

    For ESP_BLE_MESH_MODEL_OP_RPR_EXT_SCAN_START

  esp_ble_mesh_rpr_link_open_t link_open

    For ESP_BLE_MESH_MODEL_OP_RPR_LINK_OPEN

  esp_ble_mesh_rpr_link_close_t link_close

    For ESP_BLE_MESH_MODEL_OP_RPR_LINK_CLOSE

union esp_ble_mesh_rpr_client_act_param_t
  #include <esp_ble_mesh_rpr_model_api.h>

  Remote Provisioning Client model action union.

  Public Members

  esp_ble_mesh_rpr_client_start_rpr_t start_rpr

    Start remote provisioning

union esp_ble_mesh_rpr_client_recv_cb_t
  #include <esp_ble_mesh_rpr_model_api.h>

  Remote Provisioning Client model received message union.

  Public Members

  esp_ble_mesh_rpr_scan_caps_status_t scan_caps_status

    For ESP_BLE_MESH_MODEL_OP_RPR_SCAN_CAPS_STATUS

  esp_ble_mesh_rpr_scan_status_t scan_status

    For ESP_BLE_MESH_MODEL_OP_RPR_SCAN_STATUS

  esp_ble_mesh_rpr_scan_report_t scan_report

    For ESP_BLE_MESH_MODEL_OP_RPR_SCAN_REPORT

  esp_ble_mesh_rpr_ext_scan_report_t ext_scan_report

    For ESP_BLE_MESH_MODEL_OP_RPR_EXT_SCAN_REPORT

  esp_ble_mesh_rpr_link_status_t link_status

    For ESP_BLE_MESH_MODEL_OP_RPR_LINK_STATUS

  esp_ble_mesh_rpr_link_report_t link_report

    For ESP_BLE_MESH_MODEL_OP_RPR_LINK_REPORT

union esp_ble_mesh_rpr_client_cb_param_t
  #include <esp_ble_mesh_rpr_model_api.h>

  Remote Provisioning Client model callback parameters

  Public Members

  int err_code

    Result of sending a message

    Result of starting remote provisioning

  esp_ble_mesh_client_common_param_t *params

    Client common parameters

  struct esp_ble_mesh_rpr_client_cb_param_t send

    Event parameters of sending messages Event parameters of sending messages

  esp_ble_mesh_rpr_client_recv_cb_t val

    Parameters of received status message

  struct esp_ble_mesh_rpr_client_cb_param_t recv

    Event parameters of receiving messages Event parameters of receiving messages

  esp_ble_mesh_rpr_client_act_evt_t sub_evt

    Event type of the performed action

  esp_ble_mesh_model_t *model

    Pointer of Remote Provisioning Client

  uint16_t rpr_srv_addr

    Unicast address of Remote Provisioning Server

  struct esp_ble_mesh_rpr_client_cb_param_t start_rpr_comp

    ESP_BLE_MESH_START_RPR_COMP_SUB_EVT.

    Event parameter of ESP_BLE_MESH_START_RPR_COMP_SUB_EVT

  struct esp_ble_mesh_rpr_client_cb_param_t act

    Event parameters of performed actions Event parameters of performed actions

  struct esp_ble_mesh_rpr_client_cb_param_t link_open

    ESP_BLE_MESH_RPR_CLIENT_LINK_OPEN_EVT.

    Event parameters of ESP_BLE_MESH_RPR_CLIENT_LINK_OPEN_EVT

  uint8_t reason

    Reason of closing provisioning link

  struct esp_ble_mesh_rpr_client_cb_param_t link_close

    ESP_BLE_MESH_RPR_CLIENT_LINK_CLOSE_EVT.

    Event parameters of ESP_BLE_MESH_RPR_CLIENT_LINK_CLOSE_EVT

  uint8_t nppi

    NPPI Procedure

  uint16_t index

    Index of the provisioned node

  uint8_t uuid[16]

    Device UUID

  uint16_t unicast_addr

    Primary element address

  uint8_t element_num

    Element number

  uint16_t net_idx

    NetKey Index

  struct esp_ble_mesh_rpr_client_cb_param_t prov

    ESP_BLE_MESH_RPR_CLIENT_PROV_COMP_EVT.

    Event parameters of ESP_BLE_MESH_RPR_CLIENT_PROV_COMP_EVT

union esp_ble_mesh_rpr_server_cb_param_t
  #include <esp_ble_mesh_rpr_model_api.h>

  Remote Provisioning Server model related context.

  Remote Provisioning Server model callback value union

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the server model structure

  uint8_t scan_items_limit

    Maximum number of scanned items to be reported

  uint8_t timeout

    Time limit for a scan (in seconds)

    Time limit for extended scan (in seconds)

    Time limit for opening a link (in seconds)

  uint8_t uuid[16]

    Device UUID (All ZERO if not present)

    Device UUID (ZERO if not present)

  uint16_t net_idx

    NetKey Index used by Remote Provisioning Client

  uint16_t rpr_cli_addr

    Unicast address of Remote Provisioning Client

  struct esp_ble_mesh_rpr_server_cb_param_t scan_start

    ESP_BLE_MESH_RPR_SERVER_SCAN_START_EVT.

  struct esp_ble_mesh_rpr_server_cb_param_t scan_stop

    ESP_BLE_MESH_RPR_SERVER_SCAN_STOP_EVT.

  uint8_t ad_type_filter_count

    Number of AD Types in the ADTypeFilter field

  uint8_t *ad_type_filter

    List of AD Types to be reported

  uint8_t index

    Index of the extended scan instance

  struct esp_ble_mesh_rpr_server_cb_param_t ext_scan_start

    ESP_BLE_MESH_RPR_SERVER_EXT_SCAN_START_EVT.

  struct esp_ble_mesh_rpr_server_cb_param_t ext_scan_stop

    ESP_BLE_MESH_RPR_SERVER_EXT_SCAN_STOP_EVT.

  uint8_t status

    Status of Link Open procedure

  uint8_t nppi

    Node Provisioning Protocol Interface

    Provisioning bearer link close reason code

  struct esp_ble_mesh_rpr_server_cb_param_t link_open

    ESP_BLE_MESH_RPR_SERVER_LINK_OPEN_EVT.

  bool close_by_device

    Indicate if the link is closed by the Unprovisioned Device

  uint8_t reason

    Provisioning bearer link close reason code

  struct esp_ble_mesh_rpr_server_cb_param_t link_close

    ESP_BLE_MESH_RPR_SERVER_LINK_CLOSE_EVT.

  struct esp_ble_mesh_rpr_server_cb_param_t prov_comp

    ESP_BLE_MESH_RPR_SERVER_PROV_COMP_EVT. TODO: Duplicate with Link Close event?

  int err_code

    Indicate the result of setting Device UUID match value by the Remote Provisioning Server

  struct esp_ble_mesh_rpr_server_cb_param_t set_uuid_match_comp

    ESP_BLE_MESH_RPR_SERVER_SET_UUID_MATCH_COMP_EVT.

### Structures

struct esp_ble_mesh_rpr_scan_start_t

  Remote Provisioning Server model context Parameters of Remote Provisioning Scan Start

  Public Members

  uint8_t scan_items_limit

    Maximum number of scanned items to be reported

  uint8_t timeout

    Time limit for a scan (in seconds)

  bool uuid_en

    Indicate if Device UUID is present

  uint8_t uuid[16]

    Device UUID (Optional)

struct esp_ble_mesh_rpr_ext_scan_start_t

  Parameters of Remote Provisioning Extended Scan Start

  Public Members

  uint8_t ad_type_filter_count

    Number of AD Types in the ADTypeFilter field

  uint8_t ad_type_filter[16]

    List of AD Types to be reported. Minimum is 1, maximum is 16

  bool uuid_en

    Indicate if Device UUID is present

  uint8_t uuid[16]

    Device UUID (Optional)

  uint8_t timeout

    Time limit for a scan (in seconds) (C.1)

struct esp_ble_mesh_rpr_link_open_t

  Parameters of Remote Provisioning Link Open

  Public Members

  bool uuid_en

    Indicate if Device UUID is present

  uint8_t uuid[16]

    Device UUID (Optional)

  bool timeout_en

    Indicate if Link open timeout is present

  uint8_t timeout

    Link open timeout in seconds (C.1)

  uint8_t nppi

    Node Provisioning Protocol Interface (C.2)

struct esp_ble_mesh_rpr_link_close_t

  Parameters of Remote Provisioning Link Close

  Public Members

  uint8_t reason

    Provisioning bearer link close reason code

struct esp_ble_mesh_rpr_client_start_rpr_t

  Parameters of starting remote provisioning

  Public Members

  esp_ble_mesh_model_t *model

    Pointer of Remote Provisioning Client

  uint16_t rpr_srv_addr

    Unicast address of Remote Provisioning Server

struct esp_ble_mesh_rpr_scan_caps_status_t

  Parameters of Remote Provisioning Scan Capabilities Status

  Public Members

  uint8_t max_scan_items

    The maximum number of UUIDs that can be reported during scanning

  uint8_t active_scan

    Indication if active scan is supported

struct esp_ble_mesh_rpr_scan_status_t

  Parameters of Remote Provisioning Scan Status

  Public Members

  uint8_t status

    Status for the requesting message

  uint8_t rpr_scanning

    The Remote Provisioning Scan state value

  uint8_t scan_items_limit

    Maximum number of scanned items to be reported

  uint8_t timeout

    Time limit for a scan (in seconds)

struct esp_ble_mesh_rpr_scan_report_t

  Parameters of Remote Provisioning Scan Report

  Public Members

  int8_t rssi

    An indication of received signal strength measured in dBm

  uint8_t uuid[16]

    Device UUID

  uint16_t oob_info

    OOB information

  uint32_t uri_hash

    URI Hash (Optional)

struct esp_ble_mesh_rpr_ext_scan_report_t

  Parameters of Remote Provisioning Extended Scan Report

  Public Members

  uint8_t status

    Status for the requesting message

  uint8_t uuid[16]

    Device UUID

  bool oob_info_en

    Indicate if OOB Information is present

  uint16_t oob_info

    OOB Information (Optional)

  struct net_buf_simple *adv_structures

    Concatenated list of AD Structures (C.1)

struct esp_ble_mesh_rpr_link_status_t

  Parameters of Remote Provisioning Link Status

  Public Members

  uint8_t status

    Status for the requesting message

  uint8_t rpr_state

    Remote Provisioning Link state

struct esp_ble_mesh_rpr_link_report_t

  Parameters of Remote Provisioning Link Report

  Public Members

  uint8_t status

    Status of the provisioning bearer or the NPPI

  uint8_t rpr_state

    Remote Provisioning Link state

  bool reason_en

    Indicate if Link close Reason code is present

  uint8_t reason

    Link close Reason code (Optional)

### Macros

ESP_BLE_MESH_MODEL_OP_RPR_SCAN_CAPS_GET

ESP_BLE_MESH_MODEL_OP_RPR_SCAN_CAPS_STATUS

ESP_BLE_MESH_MODEL_OP_RPR_SCAN_GET

ESP_BLE_MESH_MODEL_OP_RPR_SCAN_START

ESP_BLE_MESH_MODEL_OP_RPR_SCAN_STOP

ESP_BLE_MESH_MODEL_OP_RPR_SCAN_STATUS

ESP_BLE_MESH_MODEL_OP_RPR_SCAN_REPORT

ESP_BLE_MESH_MODEL_OP_RPR_EXT_SCAN_START

ESP_BLE_MESH_MODEL_OP_RPR_EXT_SCAN_REPORT

ESP_BLE_MESH_MODEL_OP_RPR_LINK_GET

ESP_BLE_MESH_MODEL_OP_RPR_LINK_OPEN

ESP_BLE_MESH_MODEL_OP_RPR_LINK_CLOSE

ESP_BLE_MESH_MODEL_OP_RPR_LINK_STATUS

ESP_BLE_MESH_MODEL_OP_RPR_LINK_REPORT

ESP_BLE_MESH_MODEL_OP_RPR_PDU_SEND

ESP_BLE_MESH_MODEL_OP_RPR_PDU_OUTBOUND_REPORT

ESP_BLE_MESH_MODEL_OP_RPR_PDU_REPORT

ESP_BLE_MESH_RPR_SRV_MAX_SCANNED_ITEMS_MIN

ESP_BLE_MESH_RPR_NOT_SUPPORT_ACTIVE_SCAN

ESP_BLE_MESH_RPR_SUPPORT_ACTIVE_SCAN

ESP_BLE_MESH_RPR_SCAN_IDLE

ESP_BLE_MESH_RPR_SCAN_MULTIPLE_DEVICE

ESP_BLE_MESH_RPR_SCAN_SINGLE_DEVICE

ESP_BLE_MESH_RPR_SCAN_NOT_IN_PROGRESS

ESP_BLE_MESH_RPR_PROHIBIT_SCAN_TIMEOUT

ESP_BLE_MESH_RPR_EXT_SCAN_TIMEOUT_MIN

ESP_BLE_MESH_RPR_EXT_SCAN_TIMEOUT_MAX

ESP_BLE_MESH_RPR_AD_TYPE_FILTER_CNT_MIN

ESP_BLE_MESH_RPR_AD_TYPE_FILTER_CNT_MAX

ESP_BLE_MESH_RPR_LINK_OPEN_TIMEOUT_MIN

ESP_BLE_MESH_RPR_LINK_OPEN_TIMEOUT_MAX

ESP_BLE_MESH_RPR_LINK_TIMEOUT_DEFAULT

ESP_BLE_MESH_RPR_REASON_SUCCESS

ESP_BLE_MESH_RPR_REASON_FAIL

ESP_BLE_MESH_RPR_LINK_IDLE

ESP_BLE_MESH_RPR_LINK_OPENING

ESP_BLE_MESH_RPR_LINK_ACTIVE

ESP_BLE_MESH_RPR_OUTBOUND_PACKET_TRANSFER

ESP_BLE_MESH_RPR_LINK_CLOSING

ESP_BLE_MESH_RPR_STATUS_SUCCESS

ESP_BLE_MESH_RPR_STATUS_SCANNING_CANNOT_START

ESP_BLE_MESH_RPR_STATUS_INVALID_STATE

ESP_BLE_MESH_RPR_STATUS_LIMITED_RESOURCES

ESP_BLE_MESH_RPR_STATUS_LINK_CANNOT_OPEN

ESP_BLE_MESH_RPR_STATUS_LINK_OPEN_FAILED

ESP_BLE_MESH_RPR_STATUS_LINK_CLOSED_BY_DEVICE

ESP_BLE_MESH_RPR_STATUS_LINK_CLOSED_BY_SERVER

ESP_BLE_MESH_RPR_STATUS_LINK_CLOSED_BY_CLIENT

ESP_BLE_MESH_RPR_STATUS_LINK_CLOSED_AS_CANNOT_RECEIVE_PDU

ESP_BLE_MESH_RPR_STATUS_LINK_CLOSED_AS_CANNOT_SEND_PDU

ESP_BLE_MESH_RPR_STATUS_LINK_CLOSED_AS_CANNOT_DELIVER_PDU_REPORT

ESP_BLE_MESH_MODEL_RPR_SRV(srv_data)

  Define a new Remote Provisioning Server model.

  备注

  If supported, the model shall be supported by a primary element and may be supported by any secondary element.

  参数:

    - srv_data -- Pointer to a unique Remote Provisioning Server model user_data.

  返回:

    New Remote Provisioning Server model instance.

ESP_BLE_MESH_MODEL_RPR_CLI(cli_data)

  Define a new Remote Provisioning Client model.

  备注

  If supported, the model shall be supported by a primary element and may be supported by any secondary element.

  参数:

    - cli_data -- Pointer to a unique Remote Provisioning Client model user_data.

  返回:

    New Remote Provisioning Client model instance.

### Type Definitions

typedef void (*esp_ble_mesh_rpr_client_cb_t)(esp_ble_mesh_rpr_client_cb_event_t event, esp_ble_mesh_rpr_client_cb_param_t *param)

  Remote Provisioning client and server model functions.

  Remote Provisioning Client model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_rpr_server_cb_t)(esp_ble_mesh_rpr_server_cb_event_t event, esp_ble_mesh_rpr_server_cb_param_t *param)

  Remote Provisioning Server model callback function type.

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_rpr_client_act_type_t

  This enum value is the action of Remote Provisioning Client model

  Values:

  enumerator ESP_BLE_MESH_RPR_CLIENT_ACT_START_RPR
  enumerator ESP_BLE_MESH_RPR_CLIENT_ACT_MAX

enum esp_ble_mesh_rpr_client_act_evt_t

  This enum value is the event type of the performed action

  Values:

  enumerator ESP_BLE_MESH_START_RPR_COMP_SUB_EVT

enum esp_ble_mesh_rpr_client_cb_event_t

  This enum value is the event of Remote Provisioning Client model

  Values:

  enumerator ESP_BLE_MESH_RPR_CLIENT_SEND_COMP_EVT
  enumerator ESP_BLE_MESH_RPR_CLIENT_SEND_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_RPR_CLIENT_RECV_RSP_EVT
  enumerator ESP_BLE_MESH_RPR_CLIENT_RECV_PUB_EVT
  enumerator ESP_BLE_MESH_RPR_CLIENT_ACT_COMP_EVT
  enumerator ESP_BLE_MESH_RPR_CLIENT_LINK_OPEN_EVT
  enumerator ESP_BLE_MESH_RPR_CLIENT_LINK_CLOSE_EVT
  enumerator ESP_BLE_MESH_RPR_CLIENT_PROV_COMP_EVT
  enumerator ESP_BLE_MESH_RPR_CLIENT_EVT_MAX

enum esp_ble_mesh_rpr_server_cb_event_t

  This enum value is the event of Remote Provisioning Server model

  Values:

  enumerator ESP_BLE_MESH_RPR_SERVER_SCAN_START_EVT
  enumerator ESP_BLE_MESH_RPR_SERVER_SCAN_STOP_EVT
  enumerator ESP_BLE_MESH_RPR_SERVER_EXT_SCAN_START_EVT
  enumerator ESP_BLE_MESH_RPR_SERVER_EXT_SCAN_STOP_EVT
  enumerator ESP_BLE_MESH_RPR_SERVER_LINK_OPEN_EVT
  enumerator ESP_BLE_MESH_RPR_SERVER_LINK_CLOSE_EVT
  enumerator ESP_BLE_MESH_RPR_SERVER_PROV_COMP_EVT
  enumerator ESP_BLE_MESH_RPR_SERVER_SET_UUID_MATCH_COMP_EVT
  enumerator ESP_BLE_MESH_RPR_SERVER_EVT_MAX

### Directed Forwarding

### Header File

- components/bt/esp_ble_mesh/v1.1/api/core/include/esp_ble_mesh_df_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_df_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_df_client_callback(esp_ble_mesh_df_client_cb_t callback)

  Register BLE Mesh Directed Forwarding Configuration Client model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_df_server_callback(esp_ble_mesh_df_server_cb_t callback)

  Register BLE Mesh Directed Forwarding Configuration Server model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_df_client_get_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_df_client_get_t *get)

  Get the value of Directed Forwarding Configuration Server model state with the corresponding get message.

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - get -- [in] Pointer to a union, each kind of opcode corresponds to one structure inside.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_df_client_set_state(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_df_client_set_t *set)

  Set the value of Directed Forwarding Configuration Server model state with the corresponding set message.

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - set -- [in] Pointer to a union, each kind of opcode corresponds to one structure inside.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_df_client_get_t
  #include <esp_ble_mesh_df_model_api.h>

  Directed Forwarding Configuration Client model get message union.

  Public Members

  esp_ble_mesh_directed_control_get_t directed_control_get

    For ESP_BLE_MESH_MODEL_OP_DIRECTED_CONTROL_GET

  esp_ble_mesh_path_metric_get_t path_metric_get

    For ESP_BLE_MESH_MODEL_OP_PATH_METRIC_GET

  esp_ble_mesh_discovery_table_caps_get_t disc_table_caps_get

    For ESP_BLE_MESH_MODEL_OP_DISCOVERY_TABLE_CAPS_GET

  esp_ble_mesh_forwarding_table_entries_cnt_get_t forwarding_table_entries_cnt_get

    For ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_ENTRIES_CNT_GET

  esp_ble_mesh_forwarding_table_entries_get_t forwarding_table_entries_get

    For ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_ENTRIES_GET

  esp_ble_mesh_forwarding_table_deps_get_t forwarding_table_deps_get

    For ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_DEPS_GET

  esp_ble_mesh_wanted_lanes_get_t wanted_lanes_get

    For ESP_BLE_MESH_MODEL_OP_WANTED_LANES_GET

  esp_ble_mesh_two_way_path_get_t two_way_path_get

    For ESP_BLE_MESH_MODEL_OP_TWO_WAY_PATH_GET

  esp_ble_mesh_path_echo_interval_get_t path_echo_interval_get

    For ESP_BLE_MESH_MODEL_OP_PATH_ECHO_INTERVAL_GET

  esp_ble_mesh_directed_publish_policy_get_t directed_pub_policy_get

    For ESP_BLE_MESH_MODEL_OP_DIRECTED_PUB_POLICY_GET

union esp_ble_mesh_df_client_set_t
  #include <esp_ble_mesh_df_model_api.h>

  Directed Forwarding Configuration Client model set message union.

  Public Members

  esp_ble_mesh_directed_control_set_t directed_control_set

    For ESP_BLE_MESH_MODEL_OP_DIRECTED_CONTROL_SET

  esp_ble_mesh_path_metric_set_t path_metric_set

    For ESP_BLE_MESH_MODEL_OP_PATH_METRIC_SET

  esp_ble_mesh_discovery_table_caps_set_t disc_table_caps_set

    For ESP_BLE_MESH_MODEL_OP_DISCOVERY_TABLE_CAPS_SET

  esp_ble_mesh_forwarding_table_add_t forwarding_table_add

    For ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_ADD

  esp_ble_mesh_forwarding_table_delete_t forwarding_table_del

    For ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_DEL

  esp_ble_mesh_forwarding_table_deps_add_t forwarding_table_deps_add

    For ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_DEPS_ADD

  esp_ble_mesh_forwarding_table_deps_delete_t forwarding_table_deps_del

    For ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_DEPS_DEL

  esp_ble_mesh_wanted_lanes_set_t wanted_lanes_set

    For ESP_BLE_MESH_MODEL_OP_WANTED_LANES_SET

  esp_ble_mesh_two_way_path_set_t two_way_path_set

    For ESP_BLE_MESH_MODEL_OP_TWO_WAY_PATH_SET

  esp_ble_mesh_path_echo_interval_set_t path_echo_interval_set

    For ESP_BLE_MESH_MODEL_OP_PATH_ECHO_INTERVAL_SET

  esp_ble_mesh_directed_net_transmit_set_t directed_net_transmit_set

    For ESP_BLE_MESH_MODEL_OP_DIRECTED_NET_TRANSMIT_SET

  esp_ble_mesh_directed_relay_retransmit_set_t directed_relay_retransmit_set

    For ESP_BLE_MESH_MODEL_OP_DIRECTED_RELAY_RETRANSMIT_SET

  esp_ble_mesh_rssi_threshold_set_t rssi_threshold_set

    For ESP_BLE_MESH_MODEL_OP_RSSI_THRESHOLD_SET

  esp_ble_mesh_directed_publish_policy_set_t directed_pub_policy_set

    For ESP_BLE_MESH_MODEL_OP_DIRECTED_PUB_POLICY_SET

  esp_ble_mesh_path_discovery_timing_ctl_set_t path_disc_timing_ctl_set

    For ESP_BLE_MESH_MODEL_OP_PATH_DISCOVERY_TIMING_CTL_SET

  esp_ble_mesh_directed_ctl_net_transmit_set_t directed_ctl_net_transmit_set

    For ESP_BLE_MESH_MODEL_OP_DIRECTED_CTL_NET_TRANSMIT_SET

  esp_ble_mesh_directed_ctl_relay_retransmit_set_t directed_ctl_relay_retransmit_set

    For ESP_BLE_MESH_MODEL_OP_DIRECTED_CTL_RELAY_RETRANSMIT_SET

union esp_ble_mesh_df_client_recv_cb_t
  #include <esp_ble_mesh_df_model_api.h>

  Directed Forwarding Configuration Client model received message union.

  Public Members

  esp_ble_mesh_directed_control_status_t directed_control_status

    ESP_BLE_MESH_MODEL_OP_DIRECTED_CONTROL_STATUS

  esp_ble_mesh_path_metric_status_t path_metric_status

    ESP_BLE_MESH_MODEL_OP_PATH_METRIC_STATUS

  esp_ble_mesh_discovery_table_caps_status_t disc_table_caps_status

    ESP_BLE_MESH_MODEL_OP_DISCOVERY_TABLE_CAPS_STATUS

  esp_ble_mesh_forwarding_table_status_t forwarding_table_status

    ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_STATUS

  esp_ble_mesh_forwarding_table_deps_status_t forwarding_table_deps_status

    ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_DEPS_STATUS

  esp_ble_mesh_forwarding_table_entries_cnt_status_t forwarding_table_entries_cnt_status

    ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_ENTRIES_CNT_STATUS

  esp_ble_mesh_forwarding_table_entries_status_t forwarding_table_entries_status

    ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_ENTRIES_STATUS

  esp_ble_mesh_forwarding_table_deps_get_status_t forwarding_table_deps_get_status

    ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_DEPS_GET_STATUS

  esp_ble_mesh_wanted_lanes_status_t wanted_lanes_status

    ESP_BLE_MESH_MODEL_OP_WANTED_LANES_STATUS

  esp_ble_mesh_two_way_path_status_t two_way_path_status

    ESP_BLE_MESH_MODEL_OP_TWO_WAY_PATH_STATUS

  esp_ble_mesh_path_echo_interval_status_t path_echo_interval_status

    ESP_BLE_MESH_MODEL_OP_PATH_ECHO_INTERVAL_STATUS

  esp_ble_mesh_directed_net_transmit_status_t directed_net_transmit_status

    ESP_BLE_MESH_MODEL_OP_DIRECTED_NET_TRANSMIT_STATUS

  esp_ble_mesh_directed_relay_retransmit_status_t directed_relay_retransmit_status

    ESP_BLE_MESH_MODEL_OP_DIRECTED_RELAY_RETRANSMIT_STATUS

  esp_ble_mesh_rssi_threshold_status_t rssi_threshold_status

    ESP_BLE_MESH_MODEL_OP_RSSI_THRESHOLD_STATUS

  esp_ble_mesh_directed_paths_status_t directed_paths_status

    ESP_BLE_MESH_MODEL_OP_DIRECTED_PATHS_STATUS

  esp_ble_mesh_directed_pub_policy_status_t directed_pub_policy_status

    ESP_BLE_MESH_MODEL_OP_DIRECTED_PUB_POLICY_STATUS

  esp_ble_mesh_path_disc_timing_ctl_status_cb_t path_disc_timing_ctl_status

    ESP_BLE_MESH_MODEL_OP_PATH_DISCOVERY_TIMING_CTL_STATUS

  esp_ble_mesh_directed_ctl_net_transmit_status_t directed_ctl_net_transmit_status

    ESP_BLE_MESH_MODEL_OP_DIRECTED_CTL_NET_TRANSMIT_STATUS

  esp_ble_mesh_directed_ctl_relay_retransmit_status_t directed_ctl_relay_retransmit_status

    ESP_BLE_MESH_MODEL_OP_DIRECTED_CTL_RELAY_RETRANSMIT_STATUS

union esp_ble_mesh_df_server_state_change_t
  #include <esp_ble_mesh_df_model_api.h>

  Directed Forwarding Configuration Server model related context.

  Directed Forwarding Configuration Server model state change value union

  Public Members

  uint8_t dummy

    Event not used currently

union esp_ble_mesh_df_server_cb_value_t
  #include <esp_ble_mesh_df_model_api.h>

  Directed Forwarding Configuration Server model callback value union.

  Public Members

  esp_ble_mesh_df_server_state_change_t state_change

    For ESP_BLE_MESH_DF_SERVER_STATE_CHANGE_EVT

  esp_ble_mesh_df_server_table_change_t table_change

    For ESP_BLE_MESH_DF_SERVER_TABLE_CHANGE_EVT

### Structures

struct esp_ble_mesh_df_srv_t

  Directed Forwarding Configuration Server model context

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to Directed Forwarding Configuration Server model

  uint8_t directed_net_transmit

    Directed Network Transmit state

  uint8_t directed_relay_retransmit

    Directed Relay Retransmit state

  int8_t default_rssi_threshold

    Default RSSI Threshold state

  uint8_t rssi_margin

    RSSI Margin state

  uint16_t directed_node_paths

    Directed Node Paths state

  uint16_t directed_relay_paths

    Directed Relay Paths state

  uint16_t directed_proxy_paths

    Directed Proxy Paths state

  uint16_t directed_friend_paths

    Directed Friend Paths state

  uint16_t path_monitor_interval

    Path Monitoring Interval state

  uint16_t path_disc_retry_interval

    Path Discovery Retry Interval state

  uint8_t path_disc_interval

    Path Discovery Interval state

  uint8_t lane_disc_guard_interval

    Lane Discovery Guard Interval state

  uint8_t directed_ctl_net_transmit

    Directed Control Network Transmit state

  uint8_t directed_ctl_relay_retransmit

    Directed Control Relay Retransmit state

struct esp_ble_mesh_directed_control_get_t

  Parameters of Directed Control Get.

  Public Members

  uint16_t net_idx

    NetKey Index

struct esp_ble_mesh_directed_control_set_t

  Parameters of Directed Control Set.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint8_t directed_forwarding

    New Directed Forwarding state

  uint8_t directed_relay

    New Directed Relay state

  uint8_t directed_proxy

    New Directed Proxy state

  uint8_t directed_proxy_use_default

    New Directed Proxy Use Directed Default state or value to ignore

  uint8_t directed_friend

    New Directed Friend state or value to ignore

struct esp_ble_mesh_path_metric_get_t

  Parameters of Path Metric Get.

  Public Members

  uint16_t net_idx

    NetKey Index

struct esp_ble_mesh_path_metric_set_t

  Parameters of Path Metric Set.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint8_t path_metric_type

    New Path Metric Type state

  uint8_t path_lifetime

    New Path Lifetime state

struct esp_ble_mesh_discovery_table_caps_get_t

  Parameters of Discovery Table Capabilities Get.

  Public Members

  uint16_t net_idx

    NetKey Index

struct esp_ble_mesh_discovery_table_caps_set_t

  Parameters of Discovery Table Capabilities Set.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint8_t max_concurr_init

    New Max Concurrent Init state

struct esp_ble_mesh_forwarding_table_add_t

  Parameters of Forwarding Table Add.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint16_t unicast_dst

    Indicates whether or not the destination of the path is a unicast address

  uint16_t bw_path_validated

    Indicates whether or not the backward path has been validated

  esp_ble_mesh_uar_t path_origin

    Unicast address range of the Path Origin

  esp_ble_mesh_uar_t path_target

    Unicast address range of the Path Target

  uint16_t multicast_dst

    Multicast destination address

  union esp_ble_mesh_forwarding_table_add_t

    Path target address

  uint16_t bearer_twd_path_origin

    Index of the bearer toward the Path Origin

  uint16_t bearer_twd_path_target

    Index of the bearer toward the Path Target

struct esp_ble_mesh_forwarding_table_delete_t

  Parameters of Forwarding Table Delete.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint16_t path_origin

    Primary element address of the Path Origin

  uint16_t dst

    Destination address

struct esp_ble_mesh_forwarding_table_deps_add_t

  Parameters of Forwarding Table Dependents Add.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint16_t path_origin

    Primary element address of the Path Origin

  uint16_t dst

    Destination address

  uint8_t dep_origin_uar_list_size

    Number of entries in the Dependent_Origin_Unicast_Addr_Range_List field

  uint8_t dep_target_uar_list_size

    Number of entries in the Dependent_Target_Unicast_Addr_Range_List field

  esp_ble_mesh_uar_t *dep_origin_uar_list

    List of the unicast address ranges of the dependent nodes of the Path Origin

  esp_ble_mesh_uar_t *dep_target_uar_list

    List of the unicast address ranges of the dependent nodes of the Path Target

struct esp_ble_mesh_forwarding_table_deps_delete_t

  Parameters of Forwarding Table Dependents Delete.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint16_t path_origin

    Primary element address of the Path Origin

  uint16_t dst

    Destination address

  uint8_t dep_origin_list_size

    Number of entries in the Dependent_Origin_List field

  uint8_t dep_target_list_size

    Number of entries in the Dependent_Target_List field

  uint16_t *dep_origin_list

    List of the primary element addresses of the dependent nodes of the Path Origin

  uint16_t *dep_target_list

    List of the primary element addresses of the dependent nodes of the Path Target

struct esp_ble_mesh_forwarding_table_entries_cnt_get_t

  Parameters of Forwarding Table Entries Count Get.

  Public Members

  uint16_t net_idx

    NetKey Index

struct esp_ble_mesh_forwarding_table_entries_get_t

  Parameters of Forwarding Table Entries Get.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint16_t filter_mask

    Filter to be applied to the Forwarding Table entries

  uint16_t start_index

    Start offset to read in units of Forwarding Table entries

  uint16_t path_origin

    Primary element address of the Path Origin

  uint16_t dst

    Destination address

  bool include_id

    Indicate whether or not the Forwarding Table Update Identifier is present

  uint16_t update_id

    Last saved Forwarding Table Update Identifier (Optional)

struct esp_ble_mesh_forwarding_table_deps_get_t

  Parameters of Forwarding Table Dependents Get.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint16_t dep_list_mask

    Filter applied to the lists of unicast address ranges for dependent nodes

  uint16_t fixed_path_flag

    Indicate whether or not to return the unicast address ranges of dependent nodes in a fixed path entry

  uint16_t start_index

    Start offset in units of unicast address ranges

  uint16_t path_origin

    Primary element address of the Path Origin

  uint16_t dst

    Destination address

  bool include_id

    Indicate whether or not the Forwarding Table Update Identifier is present

  uint16_t update_id

    Last saved Forwarding Table Update Identifier (Optional)

struct esp_ble_mesh_wanted_lanes_get_t

  Parameters of Wanted Lanes Get.

  Public Members

  uint16_t net_idx

    NetKey Index

struct esp_ble_mesh_wanted_lanes_set_t

  Parameters of Wanted Lanes Set.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint8_t wanted_lanes

    New Wanted Lanes state

struct esp_ble_mesh_two_way_path_get_t

  Parameters of Two Way Path Get.

  Public Members

  uint16_t net_idx

    NetKey Index

struct esp_ble_mesh_two_way_path_set_t

  Parameters of Two Way Path Set.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint8_t two_way_path

    Two way path flag

struct esp_ble_mesh_path_echo_interval_get_t

  Parameters of Path Echo Interval Get.

  Public Members

  uint16_t net_idx

    NetKey Index

struct esp_ble_mesh_path_echo_interval_set_t

  Parameters of Path Echo Interval Set.

  Public Members

  uint16_t net_idx

    NetKey Index

  uint8_t unicast_echo_interval

    New Unicast Echo Interval state or indication of no state change

  uint8_t multicast_echo_interval

    New Multicast Echo Interval state or indication of no state change

struct esp_ble_mesh_directed_net_transmit_set_t

  Parameters of Directed Network Transmit Set.

  Public Members

  uint8_t net_transmit

    New Directed Network Transmit state

struct esp_ble_mesh_directed_relay_retransmit_set_t

  Parameters of Directed Relay Retransmit Set.

  Public Members

  uint8_t relay_retransmit

    New Directed Relay Retransmit state

struct esp_ble_mesh_rssi_threshold_set_t

  Parameters of RSSI Threshold Set.

  Public Members

  uint8_t rssi_margin

    New RSSI Margin state

struct esp_ble_mesh_directed_publish_policy_get_t

  Parameters of Directed Publish Policy Get.

  Public Members

  uint16_t element_addr

    Address of the element

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

struct esp_ble_mesh_directed_publish_policy_set_t

  Parameters of Directed Publish Policy Set.

  Public Members

  uint8_t direct_pub_policy

    New Directed Publish Policy state

  uint16_t element_addr

    Address of the element

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

struct esp_ble_mesh_path_discovery_timing_ctl_set_t

  Parameters of Path Discovery Timing Control Set.

  Public Members

  uint16_t path_monitor_interval

    New Path Monitoring Interval state

  uint16_t path_disc_retry_interval

    New Path Discovery Retry Interval state

  uint8_t path_disc_interval

    New Path Discovery Interval state

  uint8_t lane_disc_guard_interval

    New Lane Discovery Guard Interval state

struct esp_ble_mesh_directed_ctl_net_transmit_set_t

  Parameters of Directed Control Network Transmit Set.

  Public Members

  uint8_t net_transmit

    New Directed Control Network Transmit Count state

struct esp_ble_mesh_directed_ctl_relay_retransmit_set_t

  Parameters of Directed Control Relay Retransmit Set.

  Public Members

  uint8_t relay_retransmit

    New Directed Control Relay Retransmit Count state

struct esp_ble_mesh_directed_control_status_t

  Parameters of Directed Control Status.

  Public Members

  uint8_t status

    Status code for the requesting message

  uint16_t net_idx

    NetKey Index

  uint8_t directed_forwarding

    Current Directed Forwarding state

  uint8_t directed_relay

    Current Directed Relay state

  uint8_t directed_proxy

    Current Directed Proxy state

  uint8_t directed_proxy_use_default

    Current Directed Proxy Use Directed Default state or 0xFF

  uint8_t directed_friend

    Current Directed Friend state

struct esp_ble_mesh_path_metric_status_t

  Parameters of Path Metric Status.

  Public Members

  uint8_t status

    Status code for the requesting message

  uint16_t net_idx

    NetKey Index

  uint8_t path_metric_type

    Current Path Metric Type state

  uint8_t path_lifetime

    Current Path Lifetime state

struct esp_ble_mesh_discovery_table_caps_status_t

  Parameters of Discovery Table Capabilities Status.

  Public Members

  uint8_t status

    Status code for the requesting message

  uint16_t net_idx

    NetKey Index

  uint8_t max_concurr_init

    Current Max Concurrent Init state

  uint8_t max_disc_entries

    Max Discovery Table Entries Count state

struct esp_ble_mesh_forwarding_table_status_t

  Parameters of Forwarding Table Status.

  Public Members

  uint8_t status

    Status code for the requesting message

  uint16_t net_idx

    NetKey Index

  uint16_t path_origin

    Primary element address of the Path Origin

  uint16_t dst

    Destination address

struct esp_ble_mesh_forwarding_table_deps_status_t

  Parameters of Forwarding Table Dependent Status.

  Public Members

  uint8_t status

    Status code for the requesting message

  uint16_t net_idx

    NetKey Index

  uint16_t path_origin

    Primary element address of the Path Origin

  uint16_t dst

    Destination address

struct esp_ble_mesh_forwarding_table_entries_cnt_status_t

  Parameters of Forwarding Table Entries Count Status.

  Public Members

  uint8_t status

    Status code for the requesting message

  uint16_t net_idx

    NetKey Index

  uint16_t update_id

    Current Forwarding Table Update Identifier state

  uint16_t fixed_entry_cnt

    Number of fixed path entries in the Forwarding Table

  uint16_t non_fixed_entry_cnt

    Number of non-fixed path entries in the Forwarding Table

struct esp_ble_mesh_forwarding_table_entry_t

  Parameters of Forwarding Table Entry.

  Public Members

  uint16_t fixed_path_flag

    Indicates whether the table entry is a fixed path entry or a non-fixed path entry

  uint16_t unicast_dst_flag

    Indicates whether or not the destination of the path is a unicast address

  uint16_t bw_path_validated_flag

    Indicates whether or not the backward path has been validated

  uint16_t bearer_twd_path_origin_ind

    Indicates the presence or absence of the Bearer_Toward_Path_Origin field

  uint16_t bearer_twd_path_target_ind

    Indicates the presence or absence of the Bearer_Toward_Path_Target field

  uint16_t dep_origin_list_size_ind

    Indicates the size of the Dependent_Origin_List field

  uint16_t dep_target_list_size_ind

    Indicates the size of the Dependent_Target_List field

  uint8_t lane_counter

    Number of lanes in the path

  uint16_t path_remaining_time

    Path lifetime remaining

  uint8_t path_origin_forward_number

    Forwarding number of the Path Origin

  esp_ble_mesh_uar_t path_origin

    Path Origin unicast address range

  uint16_t dep_origin_list_size

    Current number of entries in the list of dependent nodes of the Path Origin

  uint16_t bearer_twd_path_origin

    Index of the bearer toward the Path Origin

  esp_ble_mesh_uar_t path_target

    Path Target unicast address range

  uint16_t multicast_dst

    Multicast destination address

  uint16_t dep_target_list_size

    Current number of entries in the list of dependent nodes of the Path Target

  uint16_t bearer_twd_path_target

    Index of the bearer toward the Path Target

struct esp_ble_mesh_forwarding_table_entries_status_t

  Parameters of Forwarding Table Entries Status.

  Public Members

  uint8_t status

    Status code for the requesting message

  uint16_t net_idx

    NetKey Index

  uint16_t filter_mask

    Filter applied to the Forwarding Table entries

  uint16_t start_index

    Start offset in units of Forwarding Table entries

  uint16_t path_origin

    Primary element address of the Path Origin

  uint16_t dst

    Destination address

  bool include_id

    Indicate whether or not the Forwarding Table Update Identifier is present

  uint16_t update_id

    Current Forwarding Table Update Identifier state

  uint8_t entry_list_size

    Current number of entries in the list of Forwarding Table entries

  esp_ble_mesh_forwarding_table_entry_t *entry_list

    List of Forwarding Table entries

struct esp_ble_mesh_forwarding_table_deps_get_status_t

  Parameters of Forwarding Table Dependents Get Status.

  Public Members

  uint8_t status

    Status code for the requesting message

  uint16_t net_idx

    NetKey Index

  uint16_t dep_list_mask

    Filter applied to the lists of unicast address ranges for dependent nodes

  uint16_t fixed_path_flag

    Flag indicating whether or not to return the unicast address ranges of dependent nodes in a fixed path entry

  uint16_t start_index

    Start offset in units of unicast address ranges

  uint16_t path_origin

    Primary element address of the Path Origin

  uint16_t dst

    Destination address

  bool include_id

    Indicate whether or not the Forwarding Table Update Identifier is present

  uint16_t update_id

    Current Forwarding Table Update Identifier state

  uint8_t dep_origin_uar_list_size

    Number of unicast address ranges in the Dependent_Origin_Unicast_Addr_Range_List field

  uint8_t dep_target_uar_list_size

    Number of unicast address ranges in the Dependent_Target_Unicast_Addr_Range_List field

  esp_ble_mesh_uar_t *dep_origin_uar_list

    List of unicast address ranges of dependent nodes of the Path Origin

  esp_ble_mesh_uar_t *dep_target_uar_list

    List of unicast address ranges of dependent nodes of the Path Target

struct esp_ble_mesh_wanted_lanes_status_t

  Parameters of Wanted Lanes Status.

  Public Members

  uint8_t status

    Status code for the requesting message

  uint16_t net_idx

    NetKey Index

  uint8_t wanted_lanes

    Current Wanted Lanes state

struct esp_ble_mesh_two_way_path_status_t

  Parameters of Two Way Path Status.

  Public Members

  uint8_t status

    Status code for the requesting message

  uint16_t net_idx

    NetKey Index

  uint8_t two_way_path

    Current Two Way Path state

struct esp_ble_mesh_path_echo_interval_status_t

  Parameters of Path Echo Interval Status.

  Public Members

  uint8_t status

    Status code for the requesting message

  uint16_t net_idx

    NetKey Index

  uint8_t unicast_echo_interval

    Current Unicast Echo Interval state

  uint8_t multicast_echo_interval

    Current Multicast Echo Interval state

struct esp_ble_mesh_directed_net_transmit_status_t

  Parameters of Directed Network Transmit Status.

  Public Members

  uint8_t net_transmit

    Current Directed Network Transmit state

struct esp_ble_mesh_directed_relay_retransmit_status_t

  Parameters of Directed Relay Retransmit Status.

  Public Members

  uint8_t relay_retransmit

    Current Directed Relay Retransmit state

struct esp_ble_mesh_rssi_threshold_status_t

  Parameters of RSSI Threshold Status.

  Public Members

  uint8_t default_rssi_threshold

    Default RSSI Threshold state

  uint8_t rssi_margin

    Current RSSI Margin state

struct esp_ble_mesh_directed_paths_status_t

  Parameters of Directed Paths Status.

  Public Members

  uint16_t directed_node_paths

    Directed Node Paths state

  uint16_t directed_relay_paths

    Directed Relay Paths state

  uint16_t directed_proxy_paths

    Directed Proxy Paths state

  uint16_t directed_friend_paths

    Directed Friend Paths state

struct esp_ble_mesh_directed_pub_policy_status_t

  Parameters of Directed Publish Policy Status.

  Public Members

  uint8_t status

    Status code for the requesting message

  uint8_t directed_pub_policy

    Current Directed Publish Policy state

  uint16_t element_addr

    Address of the element

  uint16_t company_id

    Company ID

  uint16_t model_id

    Model ID

struct esp_ble_mesh_path_disc_timing_ctl_status_cb_t

  Parameters of Path Discovery Timing Control Status.

  Public Members

  uint16_t path_monitor_interval

    Current Path Monitoring Interval state

  uint16_t path_disc_retry_interval

    Current Path Discovery Retry Interval state

  uint8_t path_disc_interval

    Current Path Discovery Interval state

  uint8_t lane_disc_guard_interval

    Current Lane Discovery Guard Interval state

struct esp_ble_mesh_directed_ctl_net_transmit_status_t

  Parameters of Directed Control Network Transmit Status.

  Public Members

  uint8_t net_transmit

    Current Directed Control Network Transmit state

struct esp_ble_mesh_directed_ctl_relay_retransmit_status_t

  Parameters of Directed Control Relay Retransmit Status.

  Public Members

  uint8_t relay_retransmit

    Current Directed Control Relay Retransmit state

struct esp_ble_mesh_df_client_send_cb_t

  Result of sending Directed Forwarding Configuration Client messages

  Public Members

  int err_code

    Result of sending a message

struct esp_ble_mesh_df_client_cb_param_t

  Directed Forwarding Configuration Client model callback parameters

  Public Members

  esp_ble_mesh_client_common_param_t *params

    Client common parameters, used by all events.

  esp_ble_mesh_df_client_send_cb_t send

    Result of sending a message

  esp_ble_mesh_df_client_recv_cb_t recv

    Parameters of received status message

  union esp_ble_mesh_df_client_cb_param_t

    Union of DF Client callback

struct esp_ble_mesh_df_server_table_change_t

  Parameters of directed forwarding table entry change

  Public Members

  esp_ble_mesh_df_table_action_t action

    Action of directed forwarding table

  esp_ble_mesh_uar_t path_origin

    Primary element address of the Path Origin

  esp_ble_mesh_uar_t path_target

    Primary element address of the Path Target

  esp_ble_mesh_uar_t *dep_origin_data

    List of the primary element addresses of the dependent nodes of the Path Origin

  uint32_t dep_origin_num

    Number of entries in the Dependent_Origin_List field of the message

  esp_ble_mesh_uar_t *dep_target_data

    List of the primary element addresses of the dependent nodes of the Path Target

  uint32_t dep_target_num

    Number of entries in the Dependent_Target_List field of the message

  uint8_t fixed_path

    Indicates whether the table entry is a fixed path entry or a non-fixed path entry

  uint8_t bw_path_validate

    Indicates whether or not the backward path has been validated

  uint8_t path_not_ready

    Flag indicating whether or not the path is ready for use

  uint8_t forward_number

    Forwarding number of the Path Origin; If the entry is associated with a fixed path, the value is 0

  uint8_t lane_counter

    Number of lanes discovered; if the entry is associated with a fixed path, the value is 1.

  struct esp_ble_mesh_df_server_table_change_t df_table_entry_add_remove

    Structure of directed forwarding table add and remove Structure of directed forwarding table add and remove

  uint8_t dummy

    Event not used currently

  struct esp_ble_mesh_df_server_table_change_t df_table_entry_change

    Structure of directed forwarding table entry change Directed forwarding table entry change

  union esp_ble_mesh_df_server_table_change_t df_table_info

    Union of directed forwarding table information Directed forwarding table information

struct esp_ble_mesh_df_server_cb_param_t

  Directed Forwarding Configuration Server model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the server model structure

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received message

  esp_ble_mesh_df_server_cb_value_t value

    Value of the received configuration messages

### Macros

ESP_BLE_MESH_MODEL_OP_DIRECTED_CONTROL_GET

ESP_BLE_MESH_MODEL_OP_DIRECTED_CONTROL_SET

ESP_BLE_MESH_MODEL_OP_DIRECTED_CONTROL_STATUS

ESP_BLE_MESH_MODEL_OP_PATH_METRIC_GET

ESP_BLE_MESH_MODEL_OP_PATH_METRIC_SET

ESP_BLE_MESH_MODEL_OP_PATH_METRIC_STATUS

ESP_BLE_MESH_MODEL_OP_DISCOVERY_TABLE_CAPS_GET

ESP_BLE_MESH_MODEL_OP_DISCOVERY_TABLE_CAPS_SET

ESP_BLE_MESH_MODEL_OP_DISCOVERY_TABLE_CAPS_STATUS

ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_ADD

ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_DEL

ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_STATUS

ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_DEPS_ADD

ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_DEPS_DEL

ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_DEPS_STATUS

ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_DEPS_GET

ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_DEPS_GET_STATUS

ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_ENTRIES_CNT_GET

ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_ENTRIES_CNT_STATUS

ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_ENTRIES_GET

ESP_BLE_MESH_MODEL_OP_FORWARDING_TABLE_ENTRIES_STATUS

ESP_BLE_MESH_MODEL_OP_WANTED_LANES_GET

ESP_BLE_MESH_MODEL_OP_WANTED_LANES_SET

ESP_BLE_MESH_MODEL_OP_WANTED_LANES_STATUS

ESP_BLE_MESH_MODEL_OP_TWO_WAY_PATH_GET

ESP_BLE_MESH_MODEL_OP_TWO_WAY_PATH_SET

ESP_BLE_MESH_MODEL_OP_TWO_WAY_PATH_STATUS

ESP_BLE_MESH_MODEL_OP_PATH_ECHO_INTERVAL_GET

ESP_BLE_MESH_MODEL_OP_PATH_ECHO_INTERVAL_SET

ESP_BLE_MESH_MODEL_OP_PATH_ECHO_INTERVAL_STATUS

ESP_BLE_MESH_MODEL_OP_DIRECTED_NET_TRANSMIT_GET

ESP_BLE_MESH_MODEL_OP_DIRECTED_NET_TRANSMIT_SET

ESP_BLE_MESH_MODEL_OP_DIRECTED_NET_TRANSMIT_STATUS

ESP_BLE_MESH_MODEL_OP_DIRECTED_RELAY_RETRANSMIT_GET

ESP_BLE_MESH_MODEL_OP_DIRECTED_RELAY_RETRANSMIT_SET

ESP_BLE_MESH_MODEL_OP_DIRECTED_RELAY_RETRANSMIT_STATUS

ESP_BLE_MESH_MODEL_OP_RSSI_THRESHOLD_GET

ESP_BLE_MESH_MODEL_OP_RSSI_THRESHOLD_SET

ESP_BLE_MESH_MODEL_OP_RSSI_THRESHOLD_STATUS

ESP_BLE_MESH_MODEL_OP_DIRECTED_PATHS_GET

ESP_BLE_MESH_MODEL_OP_DIRECTED_PATHS_STATUS

ESP_BLE_MESH_MODEL_OP_DIRECTED_PUB_POLICY_GET

ESP_BLE_MESH_MODEL_OP_DIRECTED_PUB_POLICY_SET

ESP_BLE_MESH_MODEL_OP_DIRECTED_PUB_POLICY_STATUS

ESP_BLE_MESH_MODEL_OP_PATH_DISCOVERY_TIMING_CTL_GET

ESP_BLE_MESH_MODEL_OP_PATH_DISCOVERY_TIMING_CTL_SET

ESP_BLE_MESH_MODEL_OP_PATH_DISCOVERY_TIMING_CTL_STATUS

ESP_BLE_MESH_MODEL_OP_DIRECTED_CTL_NET_TRANSMIT_GET

ESP_BLE_MESH_MODEL_OP_DIRECTED_CTL_NET_TRANSMIT_SET

ESP_BLE_MESH_MODEL_OP_DIRECTED_CTL_NET_TRANSMIT_STATUS

ESP_BLE_MESH_MODEL_OP_DIRECTED_CTL_RELAY_RETRANSMIT_GET

ESP_BLE_MESH_MODEL_OP_DIRECTED_CTL_RELAY_RETRANSMIT_SET

ESP_BLE_MESH_MODEL_OP_DIRECTED_CTL_RELAY_RETRANSMIT_STATUS

ESP_BLE_MESH_PATH_DISC_INTERVAL_5_SEC

ESP_BLE_MESH_PATH_DISC_INTERVAL_30_SEC

ESP_BLE_MESH_LANE_DISC_GUARD_INTERVAL_2_SEC

ESP_BLE_MESH_LANE_DISC_GUARD_INTERVAL_10_SEC

ESP_BLE_MESH_DIRECTED_PUB_POLICY_MANAGED_FLOODING

ESP_BLE_MESH_DIRECTED_PUB_POLICY_DIRECTED_FORWARDING

ESP_BLE_MESH_GET_FILTER_MASK(fp, nfp, pom, dm)

ESP_BLE_MESH_MODEL_DF_SRV(srv_data)

  Define a new Directed Forwarding Configuration Server model.

  备注

  If supported, the model shall be supported by a primary element and shall not be supported by any secondary elements.

  参数:

    - srv_data -- Pointer to a unique Directed Forwarding Configuration Server model user_data.

  返回:

    New Directed Forwarding Configuration Server model instance.

ESP_BLE_MESH_MODEL_DF_CLI(cli_data)

  Define a new Directed Forwarding Configuration Client model.

  备注

  If supported, the model shall be supported by a primary element and shall not be supported by any secondary elements.

  参数:

    - cli_data -- Pointer to a unique Directed Forwarding Configuration Client model user_data.

  返回:

    New Directed Forwarding Configuration Client model instance.

### Type Definitions

typedef void (*esp_ble_mesh_df_client_cb_t)(esp_ble_mesh_df_client_cb_event_t event, esp_ble_mesh_df_client_cb_param_t *param)

  Bluetooth Mesh Directed Forwarding Configuration client and server model functions.

  Directed Forwarding Configuration Client model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_df_server_cb_t)(esp_ble_mesh_df_server_cb_event_t event, esp_ble_mesh_df_server_cb_param_t *param)

  Directed Forwarding Configuration Server model callback function type.

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_df_client_cb_event_t

  This enum value is the event of Directed Forwarding Configuration Client model

  Values:

  enumerator ESP_BLE_MESH_DF_CLIENT_SEND_COMP_EVT
  enumerator ESP_BLE_MESH_DF_CLIENT_SEND_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_DF_CLIENT_RECV_GET_RSP_EVT
  enumerator ESP_BLE_MESH_DF_CLIENT_RECV_SET_RSP_EVT
  enumerator ESP_BLE_MESH_DF_CLIENT_RECV_PUB_EVT
  enumerator ESP_BLE_MESH_DF_CLIENT_EVT_MAX

enum esp_ble_mesh_df_table_action_t

  Values:

  enumerator ESP_BLE_MESH_DF_TABLE_ACT_EMPTY
  enumerator ESP_BLE_MESH_DF_TABLE_ADD
  enumerator ESP_BLE_MESH_DF_TABLE_REMOVE
  enumerator ESP_BLE_MESH_DF_TABLE_ENTRY_CHANGE
  enumerator ESP_BLE_MESH_DF_TABLE_ACT_MAX_LIMIT

enum esp_ble_mesh_df_server_cb_event_t

  This enum value is the event of Directed Forwarding Configuration Server model

  Values:

  enumerator ESP_BLE_MESH_DF_SERVER_STATE_CHANGE_EVT
  enumerator ESP_BLE_MESH_DF_SERVER_TABLE_CHANGE_EVT
  enumerator ESP_BLE_MESH_DF_SERVER_EVT_MAX

### Subnet Bridge Configuration

### Header File

- components/bt/esp_ble_mesh/v1.1/api/core/include/esp_ble_mesh_brc_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_brc_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_brc_client_callback(esp_ble_mesh_brc_client_cb_t callback)

  Register BLE Mesh Bridge Configuration Client model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_brc_server_callback(esp_ble_mesh_brc_server_cb_t callback)

  Register BLE Mesh Bridge Configuration Server model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_brc_client_send(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_brc_client_msg_t *msg)

  Get/Set the value of Bridge Configuration Server model state with the corresponding message.

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - msg -- [in] Pointer to Bridge Configuration Client message.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_brc_client_msg_t
  #include <esp_ble_mesh_brc_model_api.h>

  Bridge Configuration Client model message union.

  Public Members

  esp_ble_mesh_bridged_subnets_get_t bridged_subnets_get

    For ESP_BLE_MESH_MODEL_OP_BRIDGED_SUBNETS_GET

  esp_ble_mesh_bridging_table_get_t bridging_table_get

    For ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_GET

  esp_ble_mesh_subnet_bridge_set_t subnet_bridge_set

    For ESP_BLE_MESH_MODEL_OP_SUBNET_BRIDGE_SET

  esp_ble_mesh_bridging_table_add_t bridging_table_add

    For ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_ADD

  esp_ble_mesh_bridging_table_remove_t bridging_table_remove

    For ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_REMOVE

union esp_ble_mesh_brc_client_recv_cb_t
  #include <esp_ble_mesh_brc_model_api.h>

  Bridge Configuration Client model received message union.

  Public Members

  esp_ble_mesh_subnet_bridge_status_t subnet_bridge_status

    ESP_BLE_MESH_MODEL_OP_SUBNET_BRIDGE_STATUS

  esp_ble_mesh_bridging_table_status_t bridging_table_status

    ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_STATUS

  esp_ble_mesh_bridged_subnets_list_t bridged_subnets_list

    ESP_BLE_MESH_MODEL_OP_BRIDGED_SUBNETS_LIST

  esp_ble_mesh_bridging_table_list_t bridging_table_list

    ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_LIST

  esp_ble_mesh_bridging_table_size_status_t bridging_table_size_status

    ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_SIZE_STATUS

union esp_ble_mesh_brc_server_state_change_t
  #include <esp_ble_mesh_brc_model_api.h>

  Bridge Configuration Server model state change value union.

  Public Members

  esp_ble_mesh_state_change_bridging_table_add_t bridging_table_add

    The recv_op in ctx can be used to decide which state is changed. Bridging Table Add

  esp_ble_mesh_state_change_bridging_table_remove_t bridging_table_remove

    Bridging Table Remove

union esp_ble_mesh_brc_server_cb_value_t
  #include <esp_ble_mesh_brc_model_api.h>

  Bridge Configuration Server model callback value union.

  Public Members

  esp_ble_mesh_brc_server_state_change_t state_change

    For ESP_BLE_MESH_BRC_SERVER_STATE_CHANGE_EVT

### Structures

struct esp_ble_mesh_subnet_bridge_table_t

  Parameters of subnet bridge table

  Public Members

  uint8_t bridge_direction

    Allowed directions for the bridged traffic

  uint8_t bridge_net_idx[3]

    Two NetKey Indexes are packed into three octets

  uint16_t bridge_addr_1

    Address of the node in the first subnet

  uint16_t bridge_addr_2

    Address of the node in the second subnet

struct esp_ble_mesh_subnet_bridge_set_t

  Parameters of Subnet Bridge Set

  Public Members

  uint8_t subnet_bridge

    New Subnet Bridge state

struct esp_ble_mesh_bridging_table_add_t

  Parameters of Bridging Table Add

  Public Members

  uint8_t bridge_direction

    Allowed directions for the bridged traffic

  uint16_t bridge_net_idx_1

    NetKey Index of the first subnet

  uint16_t bridge_net_idx_2

    NetKey Index of the second subnet

  uint16_t bridge_addr_1

    Address of the node in the first subnet

  uint16_t bridge_addr_2

    Address of the node in the second subnet

struct esp_ble_mesh_bridging_table_remove_t

  Parameters of Bridging Table Remove

  Public Members

  uint16_t bridge_net_idx_1

    NetKey Index of the first subnet

  uint16_t bridge_net_idx_2

    NetKey Index of the second subnet

  uint16_t bridge_addr_1

    Address of the node in the first subnet

  uint16_t bridge_addr_2

    Address of the node in the second subnet

struct esp_ble_mesh_bridged_subnets_get_t

  Parameters of Bridged Subnets Get

  Public Members

  uint16_t bridge_filter

    Filter to be applied when reporting the set of pairs of NetKey Indexes

  uint16_t bridge_net_idx

    NetKey Index of any of the subnets

  uint8_t bridge_start_idx

    Start offset in units of Bridging Table state entries

struct esp_ble_mesh_bridging_table_get_t

  Parameters of Bridging Table Get

  Public Members

  uint16_t bridge_net_idx_1

    NetKey Index of first subnet

  uint16_t bridge_net_idx_2

    NetKey Index of the second subnet

  uint16_t bridge_start_idx

    Start offset in units of Bridging Table state entries

struct esp_ble_mesh_subnet_bridge_status_t

  Parameters of Subnet Bridge Status

  Public Members

  uint8_t subnet_bridge

    Current Subnet Bridge state

struct esp_ble_mesh_bridging_table_status_t

  Parameters of Bridging Table Status

  Public Members

  uint8_t status

    Status Code for the requesting message

  uint8_t bridge_direction

    Allowed directions for the bridged traffic

  uint16_t bridge_net_idx_1

    NetKey Index of the first subnet

  uint16_t bridge_net_idx_2

    NetKey Index of the second subnet

  uint16_t bridge_addr_1

    Address of the node in the first subnet

  uint16_t bridge_addr_2

    Address of the node in the second subnet

struct esp_ble_mesh_bridge_net_idx_pair_entry_t

  Bridged_Subnets_List entry format

  Public Members

  uint16_t bridge_net_idx_1

    NetKey Index of the first subnet

  uint16_t bridge_net_idx_2

    NetKey Index of the second subnet

struct esp_ble_mesh_bridged_subnets_list_t

  Parameters of Bridged Subnets List

  Public Members

  uint16_t bridge_filter

    Filter applied to the set of pairs of NetKey Indexes

  uint16_t bridge_net_idx

    NetKey Index used for filtering or ignored

  uint8_t bridge_start_idx

    Start offset in units of bridges

  uint8_t bridged_entry_list_size

    Num of pairs of NetKey Indexes

  esp_ble_mesh_bridge_net_idx_pair_entry_t *net_idx_pair

    Filtered set of N pairs of NetKey Indexes

struct esp_ble_mesh_bridged_addr_list_entry_t

  Bridged_Addresses_List entry format

  Public Members

  uint8_t bridge_direction

    Allowed directions for bridged traffic

  uint16_t bridge_addr_1

    Address of the node in the first subnet

  uint16_t bridge_addr_2

    Address of the node in the second subnet

struct esp_ble_mesh_bridging_table_list_t

  Parameters of Bridging Table List

  Public Members

  uint8_t status

    Status Code for the requesting message

  uint16_t bridge_net_idx_1

    NetKey Index of the first subnet

  uint16_t bridge_net_idx_2

    NetKey Index of the second subnet

  uint16_t bridge_start_idx

    Start offset in units of Bridging Table state entries

  uint16_t bridged_addr_list_size

    Num of pairs of entry

  esp_ble_mesh_bridged_addr_list_entry_t *bridged_addr_list

    List of bridged addresses and allowed traffic directions

struct esp_ble_mesh_bridging_table_size_status_t

  Parameters of Bridging Table Size Status

  Public Members

  uint16_t bridging_table_size

    Bridging Table Size state

struct esp_ble_mesh_brc_client_send_cb_t

  Result of sending Bridge Configuration Client messages

  Public Members

  int err_code

    Result of sending a message

struct esp_ble_mesh_brc_client_cb_param_t

  Bridge Configuration Client model callback parameters

  Public Members

  esp_ble_mesh_client_common_param_t *params

    Client common parameters, used by all events.

  esp_ble_mesh_brc_client_send_cb_t send

    Result of sending a message

  esp_ble_mesh_brc_client_recv_cb_t recv

    Parameters of received status message

  union esp_ble_mesh_brc_client_cb_param_t

    Union of Bridge Configuration Client callback

struct esp_ble_mesh_state_change_bridging_table_add_t

  Bridge Configuration Server model related context.

  Parameters of Bridging Table Add

  Public Members

  uint8_t bridge_direction

    Allowed directions for the bridged traffic

  uint16_t bridge_net_idx_1

    NetKey Index of the first subnet

  uint16_t bridge_net_idx_2

    NetKey Index of the second subnet

  uint16_t bridge_addr_1

    Address of the node in the first subnet

  uint16_t bridge_addr_2

    Address of the node in the second subnet

struct esp_ble_mesh_state_change_bridging_table_remove_t

  Parameters of Bridging Table Remove

  Public Members

  uint16_t bridge_net_idx_1

    NetKey Index of the first subnet

  uint16_t bridge_net_idx_2

    NetKey Index of the second subnet

  uint16_t bridge_addr_1

    Address of the node in the first subnet

  uint16_t bridge_addr_2

    Address of the node in the second subnet

struct esp_ble_mesh_brc_server_cb_param_t

  Bridge Configuration Server model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the server model structure

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received message

  esp_ble_mesh_brc_server_cb_value_t value

    Value of the received configuration messages

### Macros

ESP_BLE_MESH_MODEL_OP_SUBNET_BRIDGE_GET

ESP_BLE_MESH_MODEL_OP_SUBNET_BRIDGE_SET

ESP_BLE_MESH_MODEL_OP_SUBNET_BRIDGE_STATUS

ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_ADD

ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_REMOVE

ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_STATUS

ESP_BLE_MESH_MODEL_OP_BRIDGED_SUBNETS_GET

ESP_BLE_MESH_MODEL_OP_BRIDGED_SUBNETS_LIST

ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_GET

ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_LIST

ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_SIZE_GET

ESP_BLE_MESH_MODEL_OP_BRIDGING_TABLE_SIZE_STATUS

ESP_BLE_MESH_MODEL_BRC_SRV(srv_data)

  Define a new Bridge Configuration Server model.

  备注

  If supported, the model shall be supported by a primary element and shall not be supported by any secondary elements.

  参数:

    - srv_data -- Pointer to a unique Bridge Configuration Server model user_data.

  返回:

    New Bridge Configuration Server model instance.

ESP_BLE_MESH_MODEL_BRC_CLI(cli_data)

  Define a new Bridge Configuration Client model.

  备注

  If supported, the model shall be supported by a primary element and shall not be supported by any secondary elements.

  参数:

    - cli_data -- Pointer to a unique Bridge Configuration Client model user_data.

  返回:

    New Bridge Configuration Client model instance.

### Type Definitions

typedef void (*esp_ble_mesh_brc_client_cb_t)(esp_ble_mesh_brc_client_cb_event_t event, esp_ble_mesh_brc_client_cb_param_t *param)

  Bluetooth Mesh Bridge Configuration client and server model functions.

  Bridge Configuration Client model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_brc_server_cb_t)(esp_ble_mesh_brc_server_cb_event_t event, esp_ble_mesh_brc_server_cb_param_t *param)

  Bridge Configuration Server model callback function type.

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_brc_client_cb_event_t

  This enum value is the event of Bridge Configuration Client model

  Values:

  enumerator ESP_BLE_MESH_BRC_CLIENT_SEND_COMP_EVT
  enumerator ESP_BLE_MESH_BRC_CLIENT_SEND_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_BRC_CLIENT_RECV_RSP_EVT
  enumerator ESP_BLE_MESH_BRC_CLIENT_RECV_PUB_EVT
  enumerator ESP_BLE_MESH_BRC_CLIENT_EVT_MAX

enum esp_ble_mesh_brc_server_cb_event_t

  This enum value is the event of Bridge Configuration Server model

  Values:

  enumerator ESP_BLE_MESH_BRC_SERVER_STATE_CHANGE_EVT
  enumerator ESP_BLE_MESH_BRC_SERVER_EVT_MAX

### Mesh Private Beacon

### Header File

- components/bt/esp_ble_mesh/v1.1/api/core/include/esp_ble_mesh_prb_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_prb_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_prb_client_callback(esp_ble_mesh_prb_client_cb_t callback)

  Register BLE Mesh Private Beacon Client Model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_prb_server_callback(esp_ble_mesh_prb_server_cb_t callback)

  Register BLE Mesh Private Beacon Server Model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_prb_client_send(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_prb_client_msg_t *msg)

  Get/Set the value of Private Beacon Server Model states using the corresponding messages of Private Beacon Client Model.

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - msg -- [in] Pointer to Mesh Private Beacon Client message.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_prb_client_msg_t
  #include <esp_ble_mesh_prb_model_api.h>

  Mesh Private Beacon Client model message union.

  Public Members

  esp_ble_mesh_priv_beacon_set_t priv_beacon_set

    ESP_BLE_MESH_MODEL_OP_PRIV_BEACON_SET.

  esp_ble_mesh_priv_gatt_proxy_set_t priv_gatt_proxy_set

    ESP_BLE_MESH_MODEL_OP_PRIV_GATT_PROXY_SET.

  esp_ble_mesh_priv_node_id_get_t priv_node_id_get

    ESP_BLE_MESH_MODEL_OP_PRIV_NODE_IDENTITY_GET.

  esp_ble_mesh_priv_node_id_set_t priv_node_id_set

    ESP_BLE_MESH_MODEL_OP_PRIV_NODE_IDENTITY_SET.

union esp_ble_mesh_prb_client_recv_cb_t
  #include <esp_ble_mesh_prb_model_api.h>

  Private Beacon Client Model received message union.

  Public Members

  esp_ble_mesh_priv_beacon_status_cb_t priv_beacon_status

    The private beacon status value

  esp_ble_mesh_priv_gatt_proxy_status_cb_t priv_gatt_proxy_status

    The private gatt proxy status value

  esp_ble_mesh_priv_node_identity_status_cb_t priv_node_id_status

    The private node identity status value

union esp_ble_mesh_prb_server_state_change_t
  #include <esp_ble_mesh_prb_model_api.h>

  Mesh Private Beacon Server model state change value union.

  Public Members

  esp_ble_mesh_state_change_priv_beacon_set_t priv_beacon_set

    The recv_op in ctx can be used to decide which state is changed. Private Beacon Set

  esp_ble_mesh_state_change_priv_gatt_proxy_set_t priv_gatt_proxy_set

    Private GATT Proxy Set

  esp_ble_mesh_state_change_priv_node_id_set_t priv_node_id_set

    Private Node Identity Set

union esp_ble_mesh_prb_server_cb_value_t
  #include <esp_ble_mesh_prb_model_api.h>

  Private Beacon Server model callback value union.

  Public Members

  esp_ble_mesh_prb_server_state_change_t state_change

    ESP_BLE_MESH_PRB_SERVER_STATE_CHANGE_EVT

### Structures

struct esp_ble_mesh_prb_srv_t

  Private Beacon Server Model context

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to Private Beacon Server Model

  uint8_t private_beacon

    Value of Private Beacon state

  uint8_t random_update_interval

    Value of Random Update Interval Steps state

  uint8_t private_gatt_proxy

    Value of Private GATT Proxy state

  struct k_delayed_work update_timer

    Timer for update the random field of private beacon

struct esp_ble_mesh_priv_beacon_set_t

  Parameter of private Beacon Set

  Public Members

  uint8_t private_beacon

    New Private Beacon state

  bool is_effect

    Decide if update_interval exists

  uint8_t update_interval

    New Random Update Interval Steps state

struct esp_ble_mesh_priv_gatt_proxy_set_t

  Parameter of Private GATT Proxy Set

  Public Members

  uint8_t private_gatt_proxy

    New Private GATT Proxy state

struct esp_ble_mesh_priv_node_id_get_t

  Parameter of Private node identity Get

  Public Members

  uint16_t net_idx

    Index of the NetKey

struct esp_ble_mesh_priv_node_id_set_t

  Parameter of Private node identity Set

  Public Members

  uint16_t net_idx

    Index of the NetKey

  uint8_t private_node_id

    New Private Node Identity state

struct esp_ble_mesh_priv_beacon_status_cb_t

  Parameter of Private Beacon Status

  Public Members

  uint8_t private_beacon

    Current value of the Private Beacon state

  uint8_t update_interval

    Current value of the Random Update Interval Steps state

struct esp_ble_mesh_priv_gatt_proxy_status_cb_t

  Parameter of Private GATT Proxy Status

  Public Members

  uint8_t private_gatt_proxy

    Private GATT Proxy state

struct esp_ble_mesh_priv_node_identity_status_cb_t

  Parameters of Private Node Identity Status

  Public Members

  uint8_t status

    Status Code for the requesting message

  uint16_t net_idx

    Index of the NetKey

  uint8_t private_node_id

    Private Node Identity state

struct esp_ble_mesh_prb_client_send_cb_t

  Result of sending Bridge Configuration Client messages

  Public Members

  int err_code

    Result of sending a message

struct esp_ble_mesh_prb_client_cb_param_t

  Mesh Private Beacon Client Model callback parameters

  Public Members

  esp_ble_mesh_client_common_param_t *params

    The client common parameters.

  esp_ble_mesh_prb_client_send_cb_t send

    Result of sending a message

  esp_ble_mesh_prb_client_recv_cb_t recv

    The private beacon message status callback values

  union esp_ble_mesh_prb_client_cb_param_t

    Union of Private Beacon Client callback

struct esp_ble_mesh_state_change_priv_beacon_set_t

  Mesh Private Beacon Server model related context.

  Parameters of Private Beacon Set.

  Public Members

  uint8_t private_beacon

    Private Beacon state

  bool is_effect

    Decide whether update_interval effect

  uint8_t update_interval

    Random Update Interval Steps state

struct esp_ble_mesh_state_change_priv_gatt_proxy_set_t

  Parameters of Private GATT Proxy Set.

  Public Members

  uint8_t private_gatt_proxy

    Private GATT Proxy state

struct esp_ble_mesh_state_change_priv_node_id_set_t

  Parameters of Private Node Identity Set.

  Public Members

  uint16_t net_idx

    Index of the NetKey

  uint8_t private_node_id

    Private Node Identity state

struct esp_ble_mesh_prb_server_cb_param_t

  Private Beacon Server model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the server model structure

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received message

  esp_ble_mesh_prb_server_cb_value_t value

    Value of the received private beacon messages

### Macros

ESP_BLE_MESH_MODEL_OP_PRIV_BEACON_GET

ESP_BLE_MESH_MODEL_OP_PRIV_BEACON_SET

ESP_BLE_MESH_MODEL_OP_PRIV_BEACON_STATUS

ESP_BLE_MESH_MODEL_OP_PRIV_GATT_PROXY_GET

ESP_BLE_MESH_MODEL_OP_PRIV_GATT_PROXY_SET

ESP_BLE_MESH_MODEL_OP_PRIV_GATT_PROXY_STATUS

ESP_BLE_MESH_MODEL_OP_PRIV_NODE_IDENTITY_GET

ESP_BLE_MESH_MODEL_OP_PRIV_NODE_IDENTITY_SET

ESP_BLE_MESH_MODEL_OP_PRIV_NODE_IDENTITY_STATUS

ESP_BLE_MESH_MODEL_PRB_SRV(srv_data)

  Define a new Private Beacon Server Model.

  备注

  The Private Beacon Server Model can only be included by a Primary Element.

  参数:

    - srv_data -- Pointer to a unique Private Beacon Server Model user_data.

  返回:

    New Private Beacon Server Model instance.

ESP_BLE_MESH_MODEL_PRB_CLI(cli_data)

  Define a new Private Beacon Client Model.

  备注

  The Private Beacon Client Model can only be included by a Primary Element.

  参数:

    - cli_data -- Pointer to a unique struct esp_ble_mesh_client_t.

  返回:

    New Private Beacon Client Model instance.

### Type Definitions

typedef void (*esp_ble_mesh_prb_client_cb_t)(esp_ble_mesh_prb_client_cb_event_t event, esp_ble_mesh_prb_client_cb_param_t *param)

  Bluetooth Mesh Private Beacon Client and Server Model functions.

  Private Beacon Client Model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_prb_server_cb_t)(esp_ble_mesh_prb_server_cb_event_t event, esp_ble_mesh_prb_server_cb_param_t *param)

  Private Beacon Server Model callback function type.

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_prb_client_cb_event_t

  This enum value is the event of Private Beacon Client Model

  Values:

  enumerator ESP_BLE_MESH_PRB_CLIENT_SEND_COMP_EVT
  enumerator ESP_BLE_MESH_PRB_CLIENT_SEND_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_PRB_CLIENT_RECV_RSP_EVT
  enumerator ESP_BLE_MESH_PRB_CLIENT_RECV_PUB_EVT
  enumerator ESP_BLE_MESH_PRB_CLIENT_EVT_MAX

enum esp_ble_mesh_prb_server_cb_event_t

  This enum value is the event of Private Beacon Server model

  Values:

  enumerator ESP_BLE_MESH_PRB_SERVER_STATE_CHANGE_EVT
  enumerator ESP_BLE_MESH_PRB_SERVER_EVT_MAX

### On-Demand Private Proxy

### Header File

- components/bt/esp_ble_mesh/v1.1/api/core/include/esp_ble_mesh_odp_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_odp_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_odp_client_callback(esp_ble_mesh_odp_client_cb_t callback)

  Register BLE Mesh On-Demand Private Proxy Config Client model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_odp_client_send(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_odp_client_msg_t *msg)

  Get the value of On-Demand Private Proxy Config Server model state with the corresponding get message.

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - msg -- [in] Pointer to On-Demand Private Proxy Config Client message.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_odp_server_callback(esp_ble_mesh_odp_server_cb_t callback)

  Register BLE Mesh On-Demand Private Proxy Config Server model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_odp_client_msg_t
  #include <esp_ble_mesh_odp_model_api.h>

  On-Demand Private Proxy Client model message union.

  Public Members

  esp_ble_mesh_od_priv_proxy_set_t od_priv_proxy_set

    For ESP_BLE_MESH_MODEL_OP_OD_PRIV_PROXY_SET

union esp_ble_mesh_odp_client_recv_cb_t
  #include <esp_ble_mesh_odp_model_api.h>

  On-Demand Private Proxy Client model received message union.

  Public Members

  esp_ble_mesh_od_priv_proxy_status_t od_priv_proxy_status

    For ESP_BLE_MESH_MODEL_OP_OD_PRIV_PROXY_STATUS

union esp_ble_mesh_odp_server_state_change_t
  #include <esp_ble_mesh_odp_model_api.h>

  On-Demand Private Proxy Config Server model related context.

  On-Demand Private Proxy Config Server model state change value union

  Public Members

  uint8_t dummy

    Event not used currently

union esp_ble_mesh_odp_server_cb_value_t
  #include <esp_ble_mesh_odp_model_api.h>

  On-Demand Private Proxy Config Server model callback value union.

  Public Members

  esp_ble_mesh_odp_server_state_change_t state_change

    For ESP_BLE_MESH_ODP_SERVER_STATE_CHANGE_EVT

### Structures

struct esp_ble_mesh_odp_srv_t

  On-Demand Private Proxy Config Server model context

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to On-Demand Private Proxy Config Server model

  uint8_t on_demand_private_gatt_proxy

    Duration in seconds of the interval during which advertising with Private Network Identity type is enabled after receiving a Solicitation PDU or after a client disconnect. Note: Binding with the Private GATT Proxy state.

struct esp_ble_mesh_od_priv_proxy_set_t

  Parameter of On-Demand Private Proxy Set

  Public Members

  uint8_t gatt_proxy

    On-Demand Private GATT Proxy

struct esp_ble_mesh_od_priv_proxy_status_t

  Parameter of On-Demand Private Proxy Status

  Public Members

  uint8_t gatt_proxy

    On-Demand Private GATT Proxy

struct esp_ble_mesh_odp_client_send_cb_t

  Result of sending On-Demand Private Proxy Client messages

  Public Members

  int err_code

    Result of sending a message

struct esp_ble_mesh_odp_client_cb_param_t

  On-Demand Private Proxy Config Client model callback parameters

  Public Members

  esp_ble_mesh_client_common_param_t *params

    Client common parameters, used by all events

  esp_ble_mesh_odp_client_send_cb_t send

    Result of sending a message

  esp_ble_mesh_odp_client_recv_cb_t recv

    Parameters of received status message

  union esp_ble_mesh_odp_client_cb_param_t

    Union of ODP Client callback

struct esp_ble_mesh_odp_server_cb_param_t

  On-Demand Private Proxy Config Server model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the server model structure

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received message

  esp_ble_mesh_odp_server_cb_value_t value

    Value of the received configuration messages

### Macros

ESP_BLE_MESH_MODEL_OP_OD_PRIV_PROXY_GET

ESP_BLE_MESH_MODEL_OP_OD_PRIV_PROXY_SET

ESP_BLE_MESH_MODEL_OP_OD_PRIV_PROXY_STATUS

ESP_BLE_MESH_MODEL_ODP_SRV(srv_data)

  Define a new On-Demand Private Proxy Config Server model.

  备注

  The On-Demand Private Proxy Server model is used to represent the ability to enable advertising with Private Network Identity type of a node. This model extends the Mesh Private Beacon Server model. When this model is present on an element, the corresponding Solicitation PDU RPL Configuration Server model shall also be present. The model shall be supported by a primary element and shall not be supported by any secondary elements.

  参数:

    - srv_data -- Pointer to a unique On-Demand Private Proxy Config Server model user_data.

  返回:

    New On-Demand Private Proxy Config Server model instance.

ESP_BLE_MESH_MODEL_ODP_CLI(cli_data)

  Define a new On-Demand Private Proxy Config Client model.

  备注

  The model shall be supported by a primary element and shall not be supported by any secondary elements.

  参数:

    - cli_data -- Pointer to a unique On-Demand Private Proxy Config Client model user_data.

  返回:

    New On-Demand Private Proxy Config Client model instance.

### Type Definitions

typedef void (*esp_ble_mesh_odp_client_cb_t)(esp_ble_mesh_odp_client_cb_event_t event, esp_ble_mesh_odp_client_cb_param_t *param)

  Bluetooth Mesh On-Demand Private Proxy Config client and server model functions.

  On-Demand Private Proxy Config Client model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_odp_server_cb_t)(esp_ble_mesh_odp_server_cb_event_t event, esp_ble_mesh_odp_server_cb_param_t *param)

  On-Demand Private Proxy Config Server model callback function type.

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_odp_client_cb_event_t

  This enum value is the event of On-Demand Private Proxy Config Client model

  Values:

  enumerator ESP_BLE_MESH_ODP_CLIENT_SEND_COMP_EVT
  enumerator ESP_BLE_MESH_ODP_CLIENT_SEND_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_ODP_CLIENT_RECV_RSP_EVT
  enumerator ESP_BLE_MESH_ODP_CLIENT_RECV_PUB_EVT
  enumerator ESP_BLE_MESH_ODP_CLIENT_EVT_MAX

enum esp_ble_mesh_odp_server_cb_event_t

  This enum value is the event of On-Demand Private Proxy Config Server model

  Values:

  enumerator ESP_BLE_MESH_ODP_SERVER_STATE_CHANGE_EVT
  enumerator ESP_BLE_MESH_ODP_SERVER_EVT_MAX

### SAR Configuration

### Header File

- components/bt/esp_ble_mesh/v1.1/api/core/include/esp_ble_mesh_sar_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_sar_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_sar_client_callback(esp_ble_mesh_sar_client_cb_t callback)

  Register BLE Mesh SAR Configuration Client model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_sar_client_send(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_sar_client_msg_t *msg)

  Get the value of SAR Configuration Server model state with the corresponding get message.

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - msg -- [in] Pointer to SAR Configuration Client message.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_sar_server_callback(esp_ble_mesh_sar_server_cb_t callback)

  Register BLE Mesh SAR Configuration Server model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_sar_client_msg_t
  #include <esp_ble_mesh_sar_model_api.h>

  SAR Configuration Client model message union.

  Public Members

  esp_ble_mesh_sar_transmitter_set_t sar_transmitter_set

    For ESP_BLE_MESH_MODEL_OP_SAR_TRANSMITTER_SET

  esp_ble_mesh_sar_receiver_set_t sar_receiver_set

    For ESP_BLE_MESH_MODEL_OP_SAR_RECEIVER_SET

union esp_ble_mesh_sar_client_recv_cb_t
  #include <esp_ble_mesh_sar_model_api.h>

  SAR Configuration Client model received message union.

  Public Members

  esp_ble_mesh_sar_transmitter_status_t sar_transmitter_status

    For ESP_BLE_MESH_MODEL_OP_SAR_TRANSMITTER_STATUS

  esp_ble_mesh_sar_receiver_status_t sar_receiver_status

    For ESP_BLE_MESH_MODEL_OP_SAR_RECEIVE_STATUS

union esp_ble_mesh_sar_server_state_change_t
  #include <esp_ble_mesh_sar_model_api.h>

  SAR Configuration Server model related context.

  SAR Configuration Server model state change value union

  Public Members

  uint8_t dummy

    Event not used currently

union esp_ble_mesh_sar_server_cb_value_t
  #include <esp_ble_mesh_sar_model_api.h>

  SAR Configuration Server model callback value union.

  Public Members

  esp_ble_mesh_sar_server_state_change_t state_change

    For ESP_BLE_MESH_SAR_SERVER_STATE_CHANGE_EVT

### Structures

struct esp_ble_mesh_sar_srv_t

  SAR Configuration Server model context

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to SAR Configuration Server model

struct esp_ble_mesh_sar_transmitter_set_t

  Parameters of SAR Transmitter Set

  Public Members

  uint8_t sar_segment_interval_step

    SAR Segment Interval Step state value

  uint8_t sar_unicast_retrans_count

    SAR Unicast Retransmissions Count state

  uint8_t sar_unicast_retrans_without_progress_count

    SAR Unicast Retransmissions Without Progress Count state

  uint8_t sar_unicast_retrans_interval_step

    SAR Unicast Retransmissions Interval Step state

  uint8_t sar_unicast_retrans_interval_increment

    SAR Unicast Retransmissions Interval Increment state

  uint8_t sar_multicast_retrans_count

    SAR Multicast Retransmissions Count state

  uint8_t sar_multicast_retrans_interval_step

    SAR Multicast Retransmissions Interval state

struct esp_ble_mesh_sar_receiver_set_t

  Parameters of SAR Receiver Set

  Public Members

  uint8_t sar_segments_threshold

    SAR Segments Threshold state

  uint8_t sar_ack_delay_increment

    SAR Acknowledgment Delay Increment state

  uint8_t sar_discard_timeout

    SAR Discard Timeout state

  uint8_t sar_receiver_segment_interval_step

    SAR Receiver Segment Interval Step state

  uint8_t sar_ack_retrans_count

    SAR Acknowledgment Retransmissions Count state

struct esp_ble_mesh_sar_transmitter_status_t

  Parameters of SAR Transmitter Status

  Public Members

  uint8_t sar_segment_interval_step

    SAR Segment Interval Step state value

  uint8_t sar_unicast_retrans_count

    SAR Unicast Retransmissions Count state

  uint8_t sar_unicast_retrans_without_progress_count

    SAR Unicast Retransmissions Without Progress Count state

  uint8_t sar_unicast_retrans_interval_step

    SAR Unicast Retransmissions Interval Step state

  uint8_t sar_unicast_retrans_interval_increment

    SAR Unicast Retransmissions Interval Increment state

  uint8_t sar_multicast_retrans_count

    SAR Multicast Retransmissions Count state

  uint8_t sar_multicast_retrans_interval_step

    SAR Multicast Retransmissions Interval state

struct esp_ble_mesh_sar_receiver_status_t

  Parameters of SAR Receiver Status

  Public Members

  uint8_t sar_segments_threshold

    SAR Segments Threshold state

  uint8_t sar_ack_delay_increment

    SAR Acknowledgment Delay Increment state

  uint8_t sar_discard_timeout

    SAR Discard Timeout state

  uint8_t sar_receiver_segment_interval_step

    SAR Receiver Segment Interval Step state

  uint8_t sar_ack_retrans_count

    SAR Acknowledgment Retransmissions Count state

struct esp_ble_mesh_sar_client_send_cb_t

  Result of sending SAR Configuration Client messages

  Public Members

  int err_code

    Result of sending a message

struct esp_ble_mesh_sar_client_cb_param_t

  SAR Configuration Client model callback parameters

  Public Members

  esp_ble_mesh_client_common_param_t *params

    Client common parameters, used by all events.

  esp_ble_mesh_sar_client_send_cb_t send

    Result of sending a message

  esp_ble_mesh_sar_client_recv_cb_t recv

    Parameters of received status message

  union esp_ble_mesh_sar_client_cb_param_t

    Union of SAR Client callback

struct esp_ble_mesh_sar_server_cb_param_t

  SAR Configuration Server model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the server model structure

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received message

  esp_ble_mesh_sar_server_cb_value_t value

    Value of the received configuration messages

### Macros

ESP_BLE_MESH_MODEL_OP_SAR_TRANSMITTER_GET

ESP_BLE_MESH_MODEL_OP_SAR_TRANSMITTER_SET

ESP_BLE_MESH_MODEL_OP_SAR_TRANSMITTER_STATUS

ESP_BLE_MESH_MODEL_OP_SAR_RECEIVER_GET

ESP_BLE_MESH_MODEL_OP_SAR_RECEIVER_SET

ESP_BLE_MESH_MODEL_OP_SAR_RECEIVER_STATUS

ESP_BLE_MESH_MODEL_SAR_SRV(srv_data)

  Define a new SAR Configuration Server model.

  备注

  If supported, the model shall be supported by a primary element and shall not be supported by any secondary elements.

  参数:

    - srv_data -- Pointer to a unique SAR Configuration Server model user_data.

  返回:

    New SAR Configuration Server model instance.

ESP_BLE_MESH_MODEL_SAR_CLI(cli_data)

  Define a new SAR Configuration Client model.

  备注

  If supported, the model shall be supported by the primary element and shall not be supported by any secondary elements.

  参数:

    - cli_data -- Pointer to a unique SAR Configuration Client model user_data.

  返回:

    New SAR Configuration Client model instance.

### Type Definitions

typedef void (*esp_ble_mesh_sar_client_cb_t)(esp_ble_mesh_sar_client_cb_event_t event, esp_ble_mesh_sar_client_cb_param_t *param)

  Bluetooth Mesh SAR Configuration client and server model functions.

  SAR Configuration Client model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_sar_server_cb_t)(esp_ble_mesh_sar_server_cb_event_t event, esp_ble_mesh_sar_server_cb_param_t *param)

  SAR Configuration Server model callback function type.

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_sar_client_cb_event_t

  This enum value is the event of SAR Configuration Client model

  Values:

  enumerator ESP_BLE_MESH_SAR_CLIENT_SEND_COMP_EVT
  enumerator ESP_BLE_MESH_SAR_CLIENT_SEND_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_SAR_CLIENT_RECV_RSP_EVT
  enumerator ESP_BLE_MESH_SAR_CLIENT_RECV_PUB_EVT
  enumerator ESP_BLE_MESH_SAR_CLIENT_EVT_MAX

enum esp_ble_mesh_sar_server_cb_event_t

  This enum value is the event of SAR Configuration Server model

  Values:

  enumerator ESP_BLE_MESH_SAR_SERVER_STATE_CHANGE_EVT
  enumerator ESP_BLE_MESH_SAR_SERVER_EVT_MAX

### Solicitation PDU RPL Configuration

### Header File

- components/bt/esp_ble_mesh/v1.1/api/core/include/esp_ble_mesh_srpl_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_srpl_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_srpl_client_callback(esp_ble_mesh_srpl_client_cb_t callback)

  Register BLE Mesh Solicitation PDU RPL Configuration Client model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_srpl_client_send(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_srpl_client_msg_t *msg)

  Set the value of Solicitation PDU RPL Configuration Server model state with the corresponding set message.

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - msg -- [in] Pointer to Solicitation PDU RPL Configuration Client message.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_srpl_server_callback(esp_ble_mesh_srpl_server_cb_t callback)

  Register BLE Mesh Solicitation PDU RPL Configuration Server model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_srpl_client_msg_t
  #include <esp_ble_mesh_srpl_model_api.h>

  Solicitation PDU RPL Configuration Client model message union.

  Public Members

  esp_ble_mesh_srpl_items_clear_t srpl_items_clear

    For ESP_BLE_MESH_MODEL_OP_SRPL_ITEMS_CLEAR

union esp_ble_mesh_srpl_client_recv_cb_t
  #include <esp_ble_mesh_srpl_model_api.h>

  Solicitation PDU RPL Configuration Client model received message union.

  Public Members

  esp_ble_mesh_srpl_items_status_t srpl_items_status

    For ESP_BLE_MESH_MODEL_OP_SRPL_ITEMS_STATUS

union esp_ble_mesh_srpl_server_state_change_t
  #include <esp_ble_mesh_srpl_model_api.h>

  Solicitation PDU RPL Configuration Server model related context.

  Solicitation PDU RPL Configuration Server model state change value union

  Public Members

  uint8_t dummy

    Currently this event is not used.

union esp_ble_mesh_srpl_server_cb_value_t
  #include <esp_ble_mesh_srpl_model_api.h>

  Solicitation PDU RPL Configuration Server model callback value union.

  Public Members

  esp_ble_mesh_srpl_server_state_change_t state_change

    ESP_BLE_MESH_SRPL_SERVER_STATE_CHANGE_EVT

### Structures

struct esp_ble_mesh_srpl_srv_t

  Solicitation PDU RPL Configuration Server model context

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to Solicitation PDU RPL Configuration Server model

struct esp_ble_mesh_srpl_items_clear_t

  Parameter of Solicitation PDU RPL Items Clear

  Public Members

  esp_ble_mesh_uar_t addr_range

    Unicast address range

struct esp_ble_mesh_srpl_items_status_t

  Parameter of Solicitation PDU RPL Items Clear Status

  Public Members

  esp_ble_mesh_uar_t addr_range

    Unicast address range

struct esp_ble_mesh_srpl_client_send_cb_t

  Result of sending Solicitation PDU RPL Configuration Client messages

  Public Members

  int err_code

    Result of sending a message

struct esp_ble_mesh_srpl_client_cb_param_t

  Solicitation PDU RPL Configuration Client model callback parameters

  Public Members

  esp_ble_mesh_client_common_param_t *params

    Client common parameters, used by all events.

  esp_ble_mesh_srpl_client_send_cb_t send

    Result of sending a message

  esp_ble_mesh_srpl_client_recv_cb_t recv

    Parameters of received status message

  union esp_ble_mesh_srpl_client_cb_param_t

    Union of SRPL Client callback

struct esp_ble_mesh_srpl_server_cb_param_t

  Solicitation PDU RPL Configuration Server model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the server model structure

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received message

  esp_ble_mesh_srpl_server_cb_value_t value

    Value of the received configuration messages

### Macros

ESP_BLE_MESH_MODEL_OP_SRPL_ITEMS_CLEAR

ESP_BLE_MESH_MODEL_OP_SRPL_ITEMS_CLEAR_UNACK

ESP_BLE_MESH_MODEL_OP_SRPL_ITEMS_STATUS

ESP_BLE_MESH_MODEL_SRPL_SRV(srv_data)

  Define a new Solicitation PDU RPL Configuration Server model.

  备注

  The Solicitation PDU RPL Configuration Server model extends the On-Demand Private Proxy Server model. If the model is supported, the model shall be supported by a primary element and shall not be supported by any secondary elements.

  参数:

    - srv_data -- Pointer to a unique Solicitation PDU RPL Configuration Server model user_data.

  返回:

    New Solicitation PDU RPL Configuration Server model instance.

ESP_BLE_MESH_MODEL_SRPL_CLI(cli_data)

  Define a new Solicitation PDU RPL Configuration Client model.

  备注

  If supported, the model shall be supported by the primary element and shall not be supported by any secondary elements.

  参数:

    - cli_data -- Pointer to a unique Solicitation PDU RPL Configuration Client model user_data.

  返回:

    New Solicitation PDU RPL Configuration Client model instance.

### Type Definitions

typedef void (*esp_ble_mesh_srpl_client_cb_t)(esp_ble_mesh_srpl_client_cb_event_t event, esp_ble_mesh_srpl_client_cb_param_t *param)

  Bluetooth Mesh Solicitation PDU RPL Configuration client and server model functions.

  Solicitation PDU RPL Configuration Client model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_srpl_server_cb_t)(esp_ble_mesh_srpl_server_cb_event_t event, esp_ble_mesh_srpl_server_cb_param_t *param)

  Solicitation PDU RPL Configuration Server model callback function type.

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_srpl_client_cb_event_t

  This enum value is the event of Solicitation PDU RPL Configuration Client model

  Values:

  enumerator ESP_BLE_MESH_SRPL_CLIENT_SEND_COMP_EVT
  enumerator ESP_BLE_MESH_SRPL_CLIENT_SEND_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_SRPL_CLIENT_RECV_RSP_EVT
  enumerator ESP_BLE_MESH_SRPL_CLIENT_RECV_PUB_EVT
  enumerator ESP_BLE_MESH_SRPL_CLIENT_EVT_MAX

enum esp_ble_mesh_srpl_server_cb_event_t

  This enum value is the event of Solicitation PDU RPL Configuration Server model

  Values:

  enumerator ESP_BLE_MESH_SRPL_SERVER_STATE_CHANGE_EVT
  enumerator ESP_BLE_MESH_SRPL_SERVER_EVT_MAX

### Opcodes Aggregator

### Header File

- components/bt/esp_ble_mesh/v1.1/api/core/include/esp_ble_mesh_agg_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_agg_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_agg_client_callback(esp_ble_mesh_agg_client_cb_t callback)

  Register BLE Mesh Opcodes Aggregator Client model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_agg_client_send(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_agg_client_msg_t *msg)

  Set the value of Opcodes Aggregator Server model state with the corresponding set message.

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - msg -- [in] Pointer to Opcodes Aggregator Client message.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_agg_server_callback(esp_ble_mesh_agg_server_cb_t callback)

  Register BLE Mesh Opcodes Aggregator Server model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_agg_client_msg_t
  #include <esp_ble_mesh_agg_model_api.h>

  Opcodes Aggregator Client model message union.

  Public Members

  esp_ble_mesh_agg_sequence_t agg_sequence

    For ESP_BLE_MESH_MODEL_OP_AGG_SEQUENCE

union esp_ble_mesh_agg_client_recv_cb_t
  #include <esp_ble_mesh_agg_model_api.h>

  Opcodes Aggregator Client model received message union.

  Public Members

  esp_ble_mesh_agg_status_t agg_status

    For ESP_BLE_MESH_MODEL_OP_AGG_STATUS

union esp_ble_mesh_agg_server_recv_msg_t
  #include <esp_ble_mesh_agg_model_api.h>

  Opcodes Aggregator Server model related context.

  Opcodes Aggregator Server model received message union

  Public Members

  esp_ble_mesh_agg_sequence_t agg_sequence

    For ESP_BLE_MESH_MODEL_OP_AGG_SEQUENCE

### Structures

struct esp_ble_mesh_agg_srv_t

  Opcodes Aggregator Server model context

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to Opcodes Aggregator Server model

struct esp_ble_mesh_agg_item_t

  Parameters of Aggregator Item

  Public Members

  uint16_t length_format

    0: Length_Short; 1: Length_Long

  uint16_t length

    Size of Opcode_And_Parameters field

  const uint8_t *data

    Opcode and parameters

struct esp_ble_mesh_agg_sequence_t

  Parameters of Opcodes Aggregator Sequence

  Public Members

  uint16_t element_addr

    Element address

  struct net_buf_simple *items

    List of items with each item represented as an Aggregator Item

struct esp_ble_mesh_agg_status_t

  Parameters of Opcodes Aggregator Status

  Public Members

  uint8_t status

    Status of the most recent operation

  uint16_t element_addr

    Element Address

  struct net_buf_simple *items

    List of status items with each status item containing an unacknowledged access layer message or empty item (Optional)

struct esp_ble_mesh_agg_client_send_cb_t

  Result of sending Opcodes Aggregator Client messages

  Public Members

  int err_code

    Result of sending a message

struct esp_ble_mesh_agg_client_cb_param_t

  Opcodes Aggregator Client model callback parameters

  Public Members

  esp_ble_mesh_client_common_param_t *params

    Client common parameters, used by all events

  esp_ble_mesh_agg_client_send_cb_t send

    Result of sending a message

  esp_ble_mesh_agg_client_recv_cb_t recv

    Parameters of received status message

  union esp_ble_mesh_agg_client_cb_param_t

    Union of AGG Client callback

struct esp_ble_mesh_agg_server_cb_param_t

  Opcodes Aggregator Server model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the server model structure

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received message

  esp_ble_mesh_agg_server_recv_msg_t recv

    Received message callback values

  union esp_ble_mesh_agg_server_cb_param_t

    Union of AGG Server callback

### Macros

ESP_BLE_MESH_MODEL_OP_AGG_SEQUENCE

  Defines the Opcodes Aggregator message opcode.

ESP_BLE_MESH_MODEL_OP_AGG_STATUS

ESP_BLE_MESH_AGG_STATUS_SUCCESS

  Defines the status codes for Opcodes Aggregator messages.

ESP_BLE_MESH_AGG_STATUS_INVALID_ADDRESS

ESP_BLE_MESH_AGG_STATUS_INVALID_MODEL

ESP_BLE_MESH_AGG_STATUS_WRONG_ACCESS_KEY

ESP_BLE_MESH_AGG_STATUS_WRONG_OPCODE

ESP_BLE_MESH_AGG_STATUS_MSG_NOT_UNDERSTOOD

ESP_BLE_MESH_AGG_ITEM_LENGTH_FORMAT_SHORT

  Values of the Length_Format

ESP_BLE_MESH_AGG_ITEM_LENGTH_FORMAT_LONG

ESP_BLE_MESH_MODEL_AGG_SRV(srv_data)

  Define a new Opcodes Aggregator Server model.

  备注

  If supported, the Opcodes Aggregator Server model shall be supported by a primary element.

  参数:

    - srv_data -- Pointer to a unique Opcodes Aggregator Server model user_data.

  返回:

    New Opcodes Aggregator Server model instance.

ESP_BLE_MESH_MODEL_AGG_CLI(cli_data)

  Define a new Opcodes Aggregator Client model.

  备注

  If supported, the model shall be supported by the primary element and shall not be supported by any secondary elements.

  参数:

    - cli_data -- Pointer to a unique Opcodes Aggregator Client model user_data.

  返回:

    New Opcodes Aggregator Client model instance.

### Type Definitions

typedef void (*esp_ble_mesh_agg_client_cb_t)(esp_ble_mesh_agg_client_cb_event_t event, esp_ble_mesh_agg_client_cb_param_t *param)

  Bluetooth Mesh Opcodes Aggregator client and server model functions.

  Opcodes Aggregator Client model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_agg_server_cb_t)(esp_ble_mesh_agg_server_cb_event_t event, esp_ble_mesh_agg_server_cb_param_t *param)

  Opcodes Aggregator Server model callback function type.

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_agg_client_cb_event_t

  This enum value is the event of Opcodes Aggregator Client model

  Values:

  enumerator ESP_BLE_MESH_AGG_CLIENT_SEND_COMP_EVT
  enumerator ESP_BLE_MESH_AGG_CLIENT_SEND_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_AGG_CLIENT_RECV_RSP_EVT
  enumerator ESP_BLE_MESH_AGG_CLIENT_RECV_PUB_EVT
  enumerator ESP_BLE_MESH_AGG_CLIENT_EVT_MAX

enum esp_ble_mesh_agg_server_cb_event_t

  This enum value is the event of Opcodes Aggregator Server model

  Values:

  enumerator ESP_BLE_MESH_AGG_SERVER_RECV_MSG_EVT
  enumerator ESP_BLE_MESH_AGG_SERVER_EVT_MAX

### Large Composition Data

### Header File

- components/bt/esp_ble_mesh/v1.1/api/core/include/esp_ble_mesh_lcd_model_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_lcd_model_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_register_lcd_client_callback(esp_ble_mesh_lcd_client_cb_t callback)

  Register BLE Mesh Large Composition Data Client model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_lcd_client_send(esp_ble_mesh_client_common_param_t *params, esp_ble_mesh_lcd_client_msg_t *msg)

  Get the value of Large Composition Data Server model state with the corresponding get message.

  参数:

    - params -- [in] Pointer to BLE Mesh common client parameters.

    - msg -- [in] Pointer to Large Composition Data Client message.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_register_lcd_server_callback(esp_ble_mesh_lcd_server_cb_t callback)

  Register BLE Mesh Large Composition Data Server model callback.

  参数:

    callback -- [in] Pointer to the callback function.

  返回:

    ESP_OK on success or error code otherwise.

### Unions

union esp_ble_mesh_lcd_client_msg_t
  #include <esp_ble_mesh_lcd_model_api.h>

  Large Composition Data Client model message union.

  Public Members

  esp_ble_mesh_large_comp_data_get_t large_comp_data_get

    For ESP_BLE_MESH_MODEL_OP_LARGE_COMP_DATA_GET

  esp_ble_mesh_models_metadata_get_t models_metadata_get

    For ESP_BLE_MESH_MODEL_OP_MODELS_METADATA_GET

union esp_ble_mesh_lcd_client_recv_cb_t
  #include <esp_ble_mesh_lcd_model_api.h>

  Large Composition Data Client model received message union.

  Public Members

  esp_ble_mesh_large_comp_data_status_t large_comp_data_status

    For ESP_BLE_MESH_MODEL_OP_LARGE_COMP_DATA_STATUS

  esp_ble_mesh_models_metadata_status_t models_metadata_status

    For ESP_BLE_MESH_MODEL_OP_MODELS_METADATA_STATUS

union esp_ble_mesh_lcd_server_state_change_t
  #include <esp_ble_mesh_lcd_model_api.h>

  Large Composition Data Server model related context.

  Large Composition Data Server model state change value union

  Public Members

  uint8_t dummy

    Event not used currently

union esp_ble_mesh_lcd_server_cb_value_t
  #include <esp_ble_mesh_lcd_model_api.h>

  Large Composition Data Server model callback value union.

  Public Members

  esp_ble_mesh_lcd_server_state_change_t state_change

    For ESP_BLE_MESH_LCD_SERVER_STATE_CHANGE_EVT

### Structures

struct esp_ble_mesh_lcd_srv_t

  Large Composition Data Server model context

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to Large Composition Data Server model

struct esp_ble_mesh_large_comp_data_get_t

  Parameters of Large Composition Data Get

  Public Members

  uint8_t page

    Page number of the Composition Data

  uint16_t offset

    Offset within the page

struct esp_ble_mesh_models_metadata_get_t

  Parameters of Models Metadata Get

  Public Members

  uint8_t metadata_page

    Page number of the Models Metadata

  uint16_t offset

    Offset within the page

struct esp_ble_mesh_large_comp_data_status_t

  Parameters of Large Composition Data Status

  Public Members

  uint8_t page

    Page number of the Composition Data

  uint16_t offset

    Offset within the page

  uint16_t total_size

    Total size of the page

  struct net_buf_simple *data

    Composition Data for the identified portion of the page

struct esp_ble_mesh_models_metadata_status_t

  Parameters of Models Metadata Data Status

  Public Members

  uint8_t metadata_page

    Page number of the Models Metadata

  uint16_t offset

    Offset within the page

  uint16_t total_size

    Total size of the page

  struct net_buf_simple *data

    Models Metadata for the identified portion of the page

struct esp_ble_mesh_lcd_client_send_cb_t

  Result of sending Large Composition Data Client messages

  Public Members

  int err_code

    Result of sending a message

struct esp_ble_mesh_lcd_client_cb_param_t

  Large Composition Data Client model callback parameters

  Public Members

  esp_ble_mesh_client_common_param_t *params

    Client common parameters, used by all events.

  esp_ble_mesh_lcd_client_send_cb_t send

    Result of sending a message

  esp_ble_mesh_lcd_client_recv_cb_t recv

    Parameters of received status message

  union esp_ble_mesh_lcd_client_cb_param_t

    Union of LCD Client callback

struct esp_ble_mesh_lcd_server_cb_param_t

  Large Composition Data Server model callback parameters

  Public Members

  esp_ble_mesh_model_t *model

    Pointer to the server model structure

  esp_ble_mesh_msg_ctx_t ctx

    Context of the received message

  esp_ble_mesh_lcd_server_cb_value_t value

    Value of the received configuration messages

### Macros

ESP_BLE_MESH_MODEL_OP_LARGE_COMP_DATA_GET

ESP_BLE_MESH_MODEL_OP_LARGE_COMP_DATA_STATUS

ESP_BLE_MESH_MODEL_OP_MODELS_METADATA_GET

ESP_BLE_MESH_MODEL_OP_MODELS_METADATA_STATUS

ESP_BLE_MESH_MODEL_LCD_SRV(srv_data)

  Define a new Large Composition Data Server model.

  备注

  If supported, the model shall be supported by a primary element and shall not be supported by any secondary elements.

  参数:

    - srv_data -- Pointer to a unique Large Composition Data Server model user_data.

  返回:

    New Large Composition Data Server model instance.

ESP_BLE_MESH_MODEL_LCD_CLI(cli_data)

  Define a new Large Composition Data Client model.

  备注

  If supported, the model shall be supported by the primary element and shall not be supported by any secondary elements.

  参数:

    - cli_data -- Pointer to a unique Large Composition Data Client model user_data.

  返回:

    New Large Composition Data Client model instance.

### Type Definitions

typedef void (*esp_ble_mesh_lcd_client_cb_t)(esp_ble_mesh_lcd_client_cb_event_t event, esp_ble_mesh_lcd_client_cb_param_t *param)

  Large Composition Data client and server model functions.

  Large Composition Data Client model callback function type

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

typedef void (*esp_ble_mesh_lcd_server_cb_t)(esp_ble_mesh_lcd_server_cb_event_t event, esp_ble_mesh_lcd_server_cb_param_t *param)

  Large Composition Data Server model callback function type.

  Param event:

    Event type

  Param param:

    Pointer to callback parameter

### Enumerations

enum esp_ble_mesh_lcd_client_cb_event_t

  This enum value is the event of Large Composition Data Client model

  Values:

  enumerator ESP_BLE_MESH_LCD_CLIENT_SEND_COMP_EVT
  enumerator ESP_BLE_MESH_LCD_CLIENT_SEND_TIMEOUT_EVT
  enumerator ESP_BLE_MESH_LCD_CLIENT_RECV_RSP_EVT
  enumerator ESP_BLE_MESH_LCD_CLIENT_RECV_PUB_EVT
  enumerator ESP_BLE_MESH_LCD_CLIENT_EVT_MAX

enum esp_ble_mesh_lcd_server_cb_event_t

  This enum value is the event of Large Composition Data Server model

  Values:

  enumerator ESP_BLE_MESH_LCD_SERVER_STATE_CHANGE_EVT
  enumerator ESP_BLE_MESH_LCD_SERVER_EVT_MAX

### Composition and Metadata

### Header File

- components/bt/esp_ble_mesh/v1.1/api/core/include/esp_ble_mesh_cm_data_api.h

- This header file can be included with:

  >     #include "esp_ble_mesh_cm_data_api.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_ble_mesh_comp_1_register(const esp_ble_mesh_comp_1_t *comp)

  Register Composition Data Page 1.

  参数:

    comp -- [in] Pointer to Composition Data Page 1.

  返回:

    ESP_OK on success or error code otherwise.

esp_err_t esp_ble_mesh_models_metadata_register(const esp_ble_mesh_models_metadata_t *metadata, uint8_t metadata_page)

  Register Models Metadata Page 0 or 128.

  参数:

    - metadata -- [in] Pointer to Models Metadata Page 0 or 128.

    - metadata_page -- [in] Models Metadata Page number, i.e. 0 or 128.

  返回:

    ESP_OK on success or error code otherwise.

### Structures

struct esp_ble_mesh_extended_model_item_t

  Format of Extended Model Item

  Public Members

  uint8_t element_offset

    Element address modifier, in the range -4 to 3. See above.

  uint8_t model_item_idx

    Model Index, in the range 0 to 31

    Model index, in the range 0 to 255

  int8_t element_offset

    Element address modifier, in the range -128 to 127

  struct esp_ble_mesh_extended_model_item_t long_fmt

    Extended Model Item long format Extended Model Item long format

  union esp_ble_mesh_extended_model_item_t

    Union of Extended Model Item

struct esp_ble_mesh_model_item_t

  Format of Model Item

  Public Members

  uint8_t corresponding_present

    Corresponding_Group_ID field indicator

  uint8_t format

    Format of Extended_Model_Items indicator

  uint8_t extended_items_count

    Number of Extended Model Items in the Extended_Model_Items field

  uint8_t corresponding_group_id

    Corresponding group identifier

  esp_ble_mesh_extended_model_item_t *const extended_model_items

    List of Extended Model Items

struct esp_ble_mesh_comp_1_elem_t

  Format of element of Composition Data Page 1

  Public Members

  const uint8_t num_s

    A count of SIG Models Items in this element

  const uint8_t num_v

    A count of Vendor Models Items in this element

  esp_ble_mesh_model_item_t *const model_items_s

    A sequence of "num_s" SIG Model Items

  esp_ble_mesh_model_item_t *const model_items_v

    A sequence of "num_v" Vendor Model Items

struct esp_ble_mesh_comp_1_t

  Format of Composition Data Page 1

  Public Members

  size_t element_count

    Element count

  esp_ble_mesh_comp_1_elem_t *elements

    A sequence of element descriptions

struct esp_ble_mesh_metadata_entry_t

  Format of Metadata entry

  Public Members

  uint16_t metadata_len

    Size of the Metadata field

  uint16_t metadata_id

    Bluetooth assigned number for the Metadata Identifier

  const uint8_t *metadata

    Model’s metadata

struct esp_ble_mesh_metadata_item_t

  Format of Metadata item

  Public Members

  uint16_t model_id

    Model ID

  uint16_t company_id

    Company ID

  struct esp_ble_mesh_metadata_item_t vnd

    Vendor model identifier Vendor model identifier

  union esp_ble_mesh_metadata_item_t

    Union of model ID

  uint8_t metadata_entries_num

    Number of metadata entries

  esp_ble_mesh_metadata_entry_t *const metadata_entries

    List of model’s metadata

struct esp_ble_mesh_metadata_elem_t

  Format of Metadata element of Models Metadata Page 0/128

  Public Members

  const uint8_t items_num_s

    Number of metadata items for SIG models in the element

  const uint8_t items_num_v

    Number of metadata items for Vendor models in the element

  esp_ble_mesh_metadata_item_t *const metadata_items_s

    List of metadata items for SIG models in the element

  esp_ble_mesh_metadata_item_t *const metadata_items_v

    List of metadata items for Vendor models in the element

struct esp_ble_mesh_models_metadata_t

  Format of the Models Metadata Page 0/128

  Public Members

  size_t element_count

    Element count

  esp_ble_mesh_metadata_elem_t *elements

    List of metadata for models for each element

### Macros

ESP_BLE_MESH_MODEL_ITEM_SHORT

  < Definitions of the format of Extended_Model_Items indicator

ESP_BLE_MESH_MODEL_ITEM_LONG

此文档对您有帮助吗？

- 反馈已收到，谢谢！
- 如果您有其他意见，欢迎填写乐鑫文档反馈表。

- 我们重视您的反馈。
- 您可以填写乐鑫文档反馈表告诉我们如何改进该文档。