# Bluetooth® Device APIs

## Overview

Bluetooth device reference APIs.

## Application Examples

- bluetooth/bluedroid/classic_bt/bt_spp_vfs_acceptor demonstrates how to use Serial Port Protocol (SPP) APIs to create an SPP acceptor that acts as a server and registers into the VFS. It also shows how to implement Secure Simple Pairing (SSP) in your own applications.

## API Reference

### Header File

- components/bt/host/bluedroid/api/include/api/esp_bt_device.h

- This header file can be included with:

  >     #include "esp_bt_device.h"

- This header file is a part of the API provided by the `bt` component. To declare that your component depends on `bt`, add the following to your CMakeLists.txt:

  >     REQUIRES bt

  > or

  >     PRIV_REQUIRES bt

### Functions

esp_err_t esp_bt_dev_register_callback(esp_bt_dev_cb_t callback)

  register callback function. This function should be called after esp_bluedroid_enable() completes successfully

  返回:

    - ESP_OK : Succeed

    - ESP_FAIL: others

const uint8_t *esp_bt_dev_get_address(void)

  Get bluetooth device address. Must use after "esp_bluedroid_enable".

  返回:

    bluetooth device address (six bytes), or NULL if bluetooth stack is not enabled

esp_err_t esp_bt_dev_set_device_name(const char *name)

  Set bluetooth device name. This function should be called after esp_bluedroid_enable() completes successfully.

  A BR/EDR/LE device type shall have a single Bluetooth device name which shall be identical irrespective of the physical channel used to perform the name discovery procedure.

  参数:

    name -- [in] : device name to be set

  返回:

    - ESP_OK : Succeed

    - ESP_ERR_INVALID_ARG : if name is NULL pointer or empty, or string length out of limit

    - ESP_ERR_INVALID_STATE : if bluetooth stack is not yet enabled

    - ESP_FAIL : others

esp_err_t esp_bt_dev_get_device_name(void)

  Get bluetooth device name. This function should be called after esp_bluedroid_enable() completes successfully.

  A BR/EDR/LE device type shall have a single Bluetooth device name which shall be identical irrespective of the physical channel used to perform the name discovery procedure.

  返回:

    - ESP_OK : Succeed

    - ESP_ERR_INVALID_STATE : if bluetooth stack is not yet enabled

    - ESP_FAIL : others

esp_err_t esp_bt_dev_coex_status_config(esp_bt_dev_coex_type_t type, esp_bt_dev_coex_op_t op, uint8_t status)

  Config bluetooth device coexis status. This function should be called after esp_bluedroid_enable() completes successfully.

  参数:

    - type -- [in] : coexist type to operate on

    - op -- [in] : clear or set coexist status

    - status -- [in] : coexist status to be configured

  返回:

    - ESP_OK : Succeed

    - ESP_ERR_INVALID_ARG : if name is NULL pointer or empty, or string length out of limit

    - ESP_ERR_INVALID_STATE : if bluetooth stack is not yet enabled

    - ESP_FAIL : others

esp_err_t esp_bt_config_file_path_get(char *file_path)

  This function is used to get the path name of the Bluetooth bond keys saved in the NVS module.

  参数:

    file_path -- [out] buffer to store the config file path, max length NVS_KEY_NAME_MAX_SIZE

  返回:

    - ESP_OK: success

esp_err_t esp_bt_config_file_path_update(const char *file_path)

  This function is used to update the path name of bluetooth bond keys saved in the NVS module and need to be called before esp_bluedroid_init().

  参数:

    file_path -- [in] the name of config file path, the length of file_path should be less than NVS_NS_NAME_MAX_SIZE

  返回:

    - ESP_OK: success

    - other: failed

### Unions

union esp_bt_dev_cb_param_t
  #include <esp_bt_device.h>

  BT device callback parameters.

  Public Members

  struct esp_bt_dev_cb_param_t::name_res_param name_res

    discovery result parameter struct

  struct name_res_param
    #include <esp_bt_device.h>

    ESP_BT_DEV_NAME_RES_EVT.

    Public Members

    esp_bt_status_t status

      Status of getting device name

    char *name

      Name of Bluetooth device

### Macros

ESP_BT_DEV_COEX_BLE_ST_MESH_CONFIG

ESP_BT_DEV_COEX_BLE_ST_MESH_TRAFFIC

ESP_BT_DEV_COEX_BLE_ST_MESH_STANDBY

ESP_BT_DEV_COEX_BT_ST_A2DP_STREAMING

ESP_BT_DEV_COEX_BT_ST_A2DP_PAUSED

ESP_BT_DEV_COEX_OP_CLEAR

ESP_BT_DEV_COEX_OP_SET

### Type Definitions

typedef uint8_t esp_bt_dev_coex_op_t

typedef void (*esp_bt_dev_cb_t)(esp_bt_dev_cb_event_t event, esp_bt_dev_cb_param_t *param)

  bluetooth device callback function type

  Param event:

    : Event type

  Param param:

    : Pointer to callback parameter

### Enumerations

enum esp_bt_dev_coex_type_t

  Bluetooth device coex type.

  Values:

  enumerator ESP_BT_DEV_COEX_TYPE_BLE
  enumerator ESP_BT_DEV_COEX_TYPE_BT

enum esp_bt_dev_cb_event_t

  BT device callback events.

  Values:

  enumerator ESP_BT_DEV_NAME_RES_EVT

    Device name result event

  enumerator ESP_BT_DEV_EVT_MAX

此文档对您有帮助吗？

- 反馈已收到，谢谢！
- 如果您有其他意见，欢迎填写乐鑫文档反馈表。

- 我们重视您的反馈。
- 您可以填写乐鑫文档反馈表告诉我们如何改进该文档。