# 非易失性存储库

[English]

## 简介

非易失性存储 (NVS) 库主要用于在 flash 中存储键值格式的数据。本文档将详细介绍 NVS 常用的一些概念。

### 底层存储

NVS 库通过调用 esp_partition API 使用主 flash 的部分空间，即类型为 `data` 且子类型为 `nvs` 的所有分区。应用程序可调用 `nvs_open()` API 选择使用带有 `nvs` 标签的分区，也可以通过调用 `nvs_open_from_partition()` API 选择使用指定名称的任意分区。

NVS 库后续版本可能会增加其他存储器后端，来将数据保存至其他 flash 芯片（SPI 或 I2C 接口）、RTC 或 FRAM 中。

备注

如果 NVS 分区被截断（例如，更改分区表布局时），则应擦除分区内容。可以使用 ESP-IDF 构建系统中的 `idf.py erase-flash` 命令擦除 flash 上的所有内容。

备注

NVS 最适合存储一些较小的数据，而非字符串或二进制大对象 (BLOB) 等较大的数据。如需存储较大的 BLOB 或者字符串，请考虑使用基于磨损均衡库的 FAT 文件系统。

备注

NVS 组件在设计上支持磨损均衡。进行设置操作时，新数据会添加至现存条目之后。即便要使旧值失效，也无需立即执行 flash 擦除操作。通过将数据存储在页面和条目中，该 NVS 空间组织方式大幅降低了 flash 擦除和写入的频率，实现了 126 倍的效率提升。

### 在 NVS 中存储大量数据

NVS 支持至多存储数万个键，且 NVS 分区的大小也可以达到几兆字节（但并不推荐按此上限进行存储）。

备注

NVS 组件会在堆上占用一定的 RAM 空间，具体占用量取决于 flash 上 NVS 分区的大小以及使用的键的数量。可以参考以下近似数值，估算 RAM 的使用情况：每 1 MB 的 NVS flash 分区会占用 22 KB 的 RAM，每 1000 个键会占用 5.5 KB 的 RAM。

备注

使用 `nvs_flash_init()` 初始化 NVS 的时间与已有键的数量成正比。每有 1000 个键，NVS 的初始化时间则增加约 0.5 秒。

默认情况下，内部 NVS 会在设备的内部 RAM 中分配堆。当 NVS 分区较大或键的数量较多时，可能会因为使用内部 NVS 所需的内存开销过大，设备的内部 RAM 堆耗尽，导致应用程序遇到内存不足的问题。 如果应用程序使用了带有 SPI 连接的 PSRAM 模块，则可以通过启用 Kconfig 选项 CONFIG_NVS_ALLOCATE_CACHE_IN_SPIRAM 来克服此限制。启用该选项后，RAM 分配会重定向至带有 SPI 连接的 PSRAM 上。 启用 SPIRAM 且将 CONFIG_SPIRAM_USE 设为 `CONFIG_SPIRAM_USE_CAPS_ALLOC` 后，即可在 menuconfig 菜单的 nvs_flash 组件中启用 CONFIG_NVS_ALLOCATE_CACHE_IN_SPIRAM 选项。 .. note:: 使用带有 SPI 连接的 PSRAM 会导致 NVS API 的整数操作速度减慢约 2.5 倍。

## 在引导加载程序代码中使用 NVS

运行中的应用程序可使用本指南中描述的标准 NVS API。也可以在自定义引导加载程序代码中从 NVS 读取数据。更多信息请参阅 在引导程序中使用 NVS 指南。

### 键值对

NVS 的操作对象为键值对，其中键是 ASCII 字符串，当前支持的最大键长为 15 个字符。值可以为以下几种类型：

- 整数型：`uint8_t`、`int8_t`、`uint16_t`、`int16_t`、`uint32_t`、`int32_t`、`uint64_t` 和 `int64_t`；

- 以 0 结尾的字符串；

- 可变长度的二进制数据 (BLOB)

备注

字符串值当前上限为 4000 字节，其中包括空终止符。BLOB 值上限为 508,000 字节或分区大小的 97.6% 减去 4000 字节，以较低值为准。

备注

在设置新的或更新现有的键值对之前，需要确保 NVS 页面具备可用的空闲条目。对于整数类型，确保至少有一个可用的空闲条目。对于字符串值，确保至少有一个 NVS 页面，页面中有足够的连续空闲条目，以便能够完整地存储整个字符串。对于 Blob 值，确保在 NVS 中有足够的空闲条目，以容纳新数据的大小。

后续可能会增加对 `float` 和 `double` 等其他类型数据的支持。

键必须唯一。为现有的键写入新值时，会将旧的值及数据类型更新为写入操作指定的值和数据类型。

读取值时会执行数据类型检查。如果读取操作预期的数据类型与对应键的数据类型不匹配，则返回错误。

### 命名空间

为了减少不同组件之间键名的潜在冲突，NVS 将每个键值对分配给一个命名空间。命名空间的命名规则遵循键名的命名规则，例如，最多可占 15 个字符。此外，单个 NVS 分区最多只能容纳 254 个不同的命名空间。命名空间的名称在调用 `nvs_open()` 或 `nvs_open_from_partition` 中指定，调用后将返回一个不透明句柄，用于后续调用 `nvs_get_*`、`nvs_set_*` 和 `nvs_commit` 函数。这样，一个句柄关联一个命名空间，键名便不会与其他命名空间中相同键名冲突。请注意，不同 NVS 分区中具有相同名称的命名空间将被视为不同的命名空间。

### NVS 迭代器

迭代器允许根据指定的分区名称、命名空间和数据类型轮询 NVS 中存储的键值对。

使用以下函数，可执行相关操作：

- `nvs_entry_find`：创建一个不透明句柄，用于后续调用 `nvs_entry_next` 和 `nvs_entry_info` 函数；

- `nvs_entry_next`：让迭代器指向下一个键值对；

- `nvs_entry_info`：返回每个键值对的信息。

总的来说，所有通过 `nvs_entry_find()` 获得的迭代器（包括 `NULL` 迭代器）都必须使用 `nvs_release_iterator()` 释放。

一般情况下，`nvs_entry_find()` 和 `nvs_entry_next()` 会将给定的迭代器设置为 `NULL` 或为一个有效的迭代器。但如果出现参数错误（如返回 `ESP_ERR_NVS_NOT_FOUND`），给定的迭代器不会被修改。因此，在调用 `nvs_entry_find()` 之前最好将迭代器初始化为 `NULL`，这样可以避免在释放迭代器之前进行复杂的错误检查。

### 安全性、篡改性及鲁棒性

NVS 与 ESP32-S3 flash 加密系统不直接兼容。然而，如果 NVS 加密与 ESP32-S3 flash 加密或 HMAC 外设一起使用，数据仍可以加密形式存储。详情请参考 NVS 加密。

如果未启用 NVS 加密，任何对 flash 芯片有物理访问权限的用户都可以修改、擦除或添加键值对。NVS 加密启用后，如果不知道相应的 NVS 加密密钥，则无法修改或添加键值对并将其识别为有效键值对。但是，针对擦除操作没有相应的防篡改功能。

当 flash 处于不一致状态时，NVS 库会尝试恢复。在任何时间点关闭设备电源，然后重新打开电源，不会导致数据丢失；但如果关闭设备电源时正在写入新的键值对，这一键值对可能会丢失。该库还应该能够在 flash 中存在任何随机数据的情况下正常初始化。

## NVS 加密

详情请参考 NVS 加密。

## NVS 分区生成程序

NVS 分区生成程序帮助生成 NVS 分区二进制文件，可使用烧录程序将二进制文件单独烧录至特定分区。烧录至分区上的键值对由 CSV 文件提供，详情请参考 NVS 分区生成程序。

可以直接使用函数 `nvs_create_partition_image` 通过 CMake 创建分区二进制文件，无需手动调用 `nvs_partition_gen.py` 工具:

    nvs_create_partition_image(<partition> <csv> [FLASH_IN_PROJECT] [DEPENDS  dep dep dep ...])

位置参数:

参数 | 描述
--- | ---
`partition` | NVS 分区名
`csv` | 解析的 CSV 文件路径

可选参数:

参数 | 描述
--- | ---
`FLASH_IN_PROJECT` | NVS 分区名
`DEPENDS` | 指定命令依赖的文件

在没有指定 `FLASH_IN_PROJECT` 的情况下，也支持生成分区镜像，不过此时需要使用 `idf.py <partition>-flash` 手动进行烧录。举个例子，如果分区名为 `nvs`，则需使用的命令为 `idf.py nvs-flash`。

目前，仅支持从组件中的 `CMakeLists.txt` 文件调用 `nvs_create_partition_image`，且此选项仅适用于非加密分区。

## 应用示例

ESP-IDF storage/nvs 目录下提供了数个代码示例：

storage/nvs/nvs_rw_value

> 演示如何读取及写入 NVS 单个整数值。

> 此示例中的值表示 ESP32-S3 模组重启次数。NVS 中数据不会因为模组重启而丢失，因此只有将这一值存储于 NVS 中，才能起到重启次数计数器的作用。

> 该示例也演示了如何检测读取/写入操作是否成功，以及某个特定值是否在 NVS 中尚未初始化。诊断程序以纯文本形式提供，有助于追踪程序流程，及时发现问题。

storage/nvs/nvs_rw_blob

> 演示如何读取及写入 NVS 单个整数值和 BLOB（二进制大对象），并在 NVS 中存储这一数值，即便 ESP32-S3 模组重启也不会消失。

> > - value - 记录 ESP32-S3 模组软重启次数和硬重启次数。

> > - blob - 内含记录模组运行次数的表格。此表格将被从 NVS 读取至动态分配的 RAM 上。每次手动软重启后，表格内运行次数即增加一次，新加的运行次数被写入 NVS。下拉 GPIO0 即可手动软重启。

> 该示例也演示了如何执行诊断程序以检测读取/写入操作是否成功。

storage/nvs/nvs_rw_value_cxx

> 这个例子与 storage/nvs/nvs_rw_value 完全一样，只是使用了 C++ 的 NVS 句柄类。

storage/nvs/nvs_statistics

> 该示例演示了如何获取并解读 NVS 使用情况统计信息：包括指定 NVS 分区中的空闲、已用、可用、总条目数、以及命名空间数量。

> 默认的 NVS 分区会在运行本示例前被擦除，以确保干净的运行环境。随后，会写入模拟的字符串类型数据。

> 在写入数据前后分别获取使用情况统计信息，并将两者的差异与新占用条目的预期值进行比较。

storage/nvs/nvs_iteration

> 该示例演示了如何遍历特定（或任意）NVS 数据类型的条目，以及如何获取这些条目的相关信息。

> 默认的 NVS 分区会在运行本示例前被擦除，以确保干净的运行环境。随后，会写入包含不同 NVS 整型数据类型的模拟数据。

> 之后，本示例会遍历各个数据类型以及通用的 `NVS_TYPE_ANY` 类型，并记录在每次遍历过程中获取到的信息。

## 内部实现

### 键值对日志

NVS 按顺序存储键值对，新的键值对添加在最后。因此，如需更新某一键值对，实际是在日志最后增加一对新的键值对，同时将旧的键值对标记为已擦除。

### 页面和条目

NVS 库在其操作中主要使用两个实体：页面和条目。页面是一个逻辑结构，用于存储部分的整体日志。逻辑页面对应 flash 的一个物理扇区，正在使用中的页面具有与之相关联的 序列号。序列号赋予了页面顺序，较高的序列号对应较晚创建的页面。页面有以下几种状态：

空或未初始化

  页面对应的 flash 扇区为空白状态（所有字节均为 `0xff`）。此时，页面未存储任何数据且没有关联的序列号。

活跃状态

  此时 flash 已完成初始化，页头部写入 flash，页面已具备有效序列号。页面中存在一些空条目，可写入数据。任意时刻，至多有一个页面处于活跃状态。

写满状态

  flash 已写满键值对，状态不再改变。 用户无法向写满状态下的页面写入新键值对，但仍可将一些键值对标记为已擦除。

擦除状态

  未擦除的键值对将移至其他页面，以便擦除当前页面。这一状态仅为暂时性状态，即 API 调用返回时，页面应脱离这一状态。如果设备突然断电，下次开机时，设备将继续把未擦除的键值对移至其他页面，并继续擦除当前页面。

损坏状态

  页头部包含无效数据，无法进一步解析该页面中的数据，因此之前写入该页面的所有条目均无法访问。相应的 flash 扇区并不会被立即擦除，而是与其他处于未初始化状态的扇区一起等待后续使用。这一状态可能对调试有用。

flash 扇区映射至逻辑页面并没有特定的顺序，NVS 库会检查存储在 flash 扇区的页面序列号，并根据序列号组织页面。

    +--------+     +--------+     +--------+     +--------+
    | Page 1 |     | Page 2 |     | Page 3 |     | Page 4 |
    | Full   +---> | Full   +---> | Active |     | Empty  |   <- 状态
    | #11    |     | #12    |     | #14    |     |        |   <- 序列号
    +---+----+     +----+---+     +----+---+     +---+----+
        |               |              |             |
        |               |              |             |
        |               |              |             |
    +---v------+  +-----v----+  +------v---+  +------v---+
    | Sector 3 |  | Sector 0 |  | Sector 2 |  | Sector 1 |    <- 物理扇区
    +----------+  +----------+  +----------+  +----------+

### 页面结构

当前，我们假设 flash 扇区大小为 4096 字节，并且 ESP32-S3 flash 加密硬件在 32 字节块上运行。未来有可能引入一些编译时可配置项（可通过 menuconfig 进行配置），以适配具有不同扇区大小的 flash 芯片。但目前尚不清楚 SPI flash 驱动和 SPI flash cache 之类的系统组件是否支持其他扇区大小。

页面由头部、条目状态位图和条目三部分组成。为了实现与 ESP32-S3 flash 加密功能兼容，条目大小设置为 32 字节。如果键值为整数型，条目则保存一个键值对；如果键值为字符串或 BLOB 类型，则条目仅保存一个键值对的部分内容（更多信息详见条目结构描述）。

页面结构如下图所示，括号内数字表示该部分的大小（以字节为单位）。

    +-----------+--------------+-------------+-------------------------+
    | State (4) | Seq. no. (4) | version (1) | Unused (19) | CRC32 (4) |   页头部 (32)
    +-----------+--------------+-------------+-------------------------+
    |                Entry state bitmap (32)                           |
    +------------------------------------------------------------------+
    |                       Entry 0 (32)                               |
    +------------------------------------------------------------------+
    |                       Entry 1 (32)                               |
    +------------------------------------------------------------------+
    /                                                                  /
    /                                                                  /
    +------------------------------------------------------------------+
    |                       Entry 125 (32)                             |
    +------------------------------------------------------------------+

头部和条目状态位图写入 flash 时不加密。如果启用了 ESP32-S3 flash 加密功能，则条目写入 flash 时将会加密。

通过将 0 写入某些位可以定义页面状态值，表示状态改变。因此，如果需要变更页面状态，并不一定要擦除页面，除非要将其变更为 擦除 状态。

头部中的 `version` 字段反映了所用的 NVS 格式版本。为实现向后兼容，版本升级从 0xff 开始依次递减（例如，version-1 为 0xff，version-2 为 0xfe，以此类推）。

头部中 CRC32 值是由不包含状态值的条目计算所得（4 到 28 字节）。当前未使用的条目用 `0xff` 字节填充。

条目结构和条目状态位图的详细信息见下文描述。

### 条目和条目状态位图

每个条目可处于以下三种状态之一，每个状态在条目状态位图中用两位表示。位图中的最后四位 (256 - 2 * 126) 未使用。

空 (2'b11)

  条目还未写入任何内容，处于未初始化状态（全部字节为 `0xff`）。

写入（2'b10）

  一个键值对（或跨多个条目的键值对的部分内容）已写入条目中。

擦除（2'b00）

  条目中的键值对已丢弃，条目内容不再解析。

### 条目结构

如果键值类型为基础类型，即 1 - 8 个字节长度的整数型，条目将保存一个键值对；如果键值类型为字符串或 BLOB 类型，条目将保存整个键值对的部分内容。另外，如果键值为字符串类型且跨多个条目，则键值所跨的所有条目均保存在同一页面。BLOB 则可以切分为多个块，实现跨多个页面。BLOB 索引是一个附加的固定长度元数据条目，用于追踪 BLOB 块。目前条目仍支持早期 BLOB 格式（可读取可修改），但这些 BLOB 一经修改，即以新格式储存至条目。

    +--------+----------+----------+----------------+-----------+---------------+----------+
    | NS (1) | Type (1) | Span (1) | ChunkIndex (1) | CRC32 (4) |    Key (16)   | Data (8) |
    +--------+----------+----------+----------------+-----------+---------------+----------+

                                             Primitive  +--------------------------------+
                                            +-------->  |     Data (8)                   |
                                            | Types     +--------------------------------+
                       +-> Fixed length --
                       |                    |           +---------+--------------+---------------+-------+
                       |                    +-------->  | Size(4) | ChunkCount(1)| ChunkStart(1) | Rsv(2)|
        Data format ---+                    BLOB Index  +---------+--------------+---------------+-------+
                       |
                       |                             +----------+---------+-----------+
                       +->   Variable length   -->   | Size (2) | Rsv (2) | CRC32 (4) |
                            (Strings, BLOB Data)     +----------+---------+-----------+

条目结构中各个字段含义如下：

命名空间 (NS, NameSpace)

  该条目的命名空间索引，详细信息参见命名空间实现章节。

类型 (Type)

  一个字节表示的值的数据类型，nvs_flash/include/nvs_handle.hpp 下的 `ItemType` 枚举了可能的类型。

跨度 (Span)

  该键值对所用的条目数量。如果键值为整数型，条目数量即为 1。如果键值为字符串或 BLOB，则条目数量取决于值的长度。

块索引 (ChunkIndex)

  用于存储 BLOB 类型数据块的索引。如果键值为其他数据类型，则此处索引应写入 `0xff`。

CRC32

  对条目下所有字节进行校验后，所得的校验和（CRC32 字段不计算在内）。

键 (Key)

  即以零结尾的 ASCII 字符串，字符串最长为 15 字节，不包含最后一个字节的零终止符。

数据 (Data)

  如果键值类型为整数型，则数据字段仅包含键值。如果键值小于八个字节，使用 `0xff` 填充未使用的部分（右侧）。

  如果键值类型为 BLOB 索引条目，则该字段的八个字节将保存以下数据块信息：

  - 块大小

      整个 BLOB 数据的大小（以字节为单位）。该字段仅用于 BLOB 索引类型条目。

  - ChunkCount

      存储过程中 BLOB 分成的数据块总量。该字段仅用于 BLOB 索引类型条目。

  - ChunkStart

      BLOB 第一个数据块的块索引，后续数据块索引依次递增，步长为 1。该字段仅用于 BLOB 索引类型条目。

  如果键值类型为字符串或 BLOB 数据块，数据字段的这八个字节将保存该键值的一些附加信息，如下所示：

  - 数据大小

      实际数据的大小（以字节为单位）。如果键值类型为字符串，此字段也应将零终止符包含在内。此字段仅用于字符串和 BLOB 类型条目。

  - CRC32

      数据所有字节的校验和，该字段仅用于字符串和 BLOB 类型条目。

可变长度值（字符串和 BLOB）写入后续条目，每个条目 32 字节。第一个条目的 `Span` 字段将指明使用了多少条目。

### 命名空间

如上所述，每个键值对属于一个命名空间。命名空间标识符（字符串）也作为键值对的键，存储在索引为 0 的命名空间中。与这些键对应的值就是这些命名空间的索引。

    +-------------------------------------------+
    | NS=0 Type=uint8_t Key="wifi" Value=1      |   Entry describing namespace "wifi"
    +-------------------------------------------+
    | NS=1 Type=uint32_t Key="channel" Value=6  |   Key "channel" in namespace "wifi"
    +-------------------------------------------+
    | NS=0 Type=uint8_t Key="pwm" Value=2       |   Entry describing namespace "pwm"
    +-------------------------------------------+
    | NS=2 Type=uint16_t Key="channel" Value=20 |   Key "channel" in namespace "pwm"
    +-------------------------------------------+

### 条目哈希列表

为了减少对 flash 执行的读操作次数，Page 类对象均设有一个列表，包含一对数据：条目索引和条目哈希值。该列表可大大提高检索速度，而无需迭代所有条目并逐个从 flash 中读取。`Page::findItem` 首先从哈希列表中检索条目哈希值，如果条目存在，则在页面内给出条目索引。由于哈希冲突，在哈希列表中检索条目哈希值可能会得到不同的条目，对 flash 中条目再次迭代可解决这一冲突。

哈希列表中每个节点均包含一个 24 位哈希值和 8 位条目索引。哈希值根据条目命名空间、键名和块索引由 CRC32 计算所得，计算结果保留 24 位。为减少将 32 位条目存储在链表中的开销，链表采用了数组的双向链表。每个数组占用 128 个字节，包含 29 个条目、两个链表指针和一个 32 位计数字段。因此，每页额外需要的 RAM 最少为 128 字节，最多为 640 字节。

### 只读 NVS

NVS 正常运行所需的最小大小默认为 12kiB (`0x3000`)，这意味着至少需要 3 个页面，其中一个页面必须处于 Empty 状态。但是，如果 NVS 分区在分区表 CSV 中标记为 `readonly` 并以只读 (read-only) 模式打开，则该分区大小最少只需 4kiB（`0x1000`），此时仅需一个 Active 状态的页面，无需 Empty 页面。因为在这种情况下，库无需向分区写入任何数据。此类型分区适用于存储不会更改的数据，如校准数据或出厂设置。大小为 0x1000 和 0x2000 的分区始终为只读分区。大小为 0x3000 及以上的分区始终支持读写 (read-write)，但仍可以在代码中以只读模式打开。

## API 参考

### Header File

- components/nvs_flash/include/nvs_flash.h

- This header file can be included with:

  >     #include "nvs_flash.h"

- This header file is a part of the API provided by the `nvs_flash` component. To declare that your component depends on `nvs_flash`, add the following to your CMakeLists.txt:

  >     REQUIRES nvs_flash

  > or

  >     PRIV_REQUIRES nvs_flash

### Functions

esp_err_t nvs_flash_init(void)

  Initialize the default NVS partition.

  This API initialises the default NVS partition. The default NVS partition is the one that is labeled "nvs" in the partition table.

  When "NVS_ENCRYPTION" is enabled in the menuconfig, this API enables the NVS encryption for the default NVS partition as follows

  1. Read security configurations from the first NVS key partition listed in the partition table. (NVS key partition is any "data" type partition which has the subtype value set to "nvs_keys")

  2. If the NVS key partition obtained in the previous step is empty, generate and store new keys in that NVS key partition.

  3. Internally call "nvs_flash_secure_init()" with the security configurations obtained/generated in the previous steps.

  Post initialization NVS read/write APIs remain the same irrespective of NVS encryption.

  返回:

    - ESP_OK if storage was successfully initialized.

    - ESP_ERR_NVS_NO_FREE_PAGES if the NVS storage contains no empty pages (which may happen if NVS partition was truncated)

    - ESP_ERR_NOT_FOUND if no partition with label "nvs" is found in the partition table

    - ESP_ERR_NO_MEM in case memory could not be allocated for the internal structures

    - one of the error codes from the underlying flash storage driver

    - error codes from nvs_flash_read_security_cfg API (when "NVS_ENCRYPTION" is enabled).

    - error codes from nvs_flash_generate_keys API (when "NVS_ENCRYPTION" is enabled).

    - error codes from nvs_flash_secure_init_partition API (when "NVS_ENCRYPTION" is enabled) .

esp_err_t nvs_flash_init_partition(const char *partition_label)

  Initialize NVS flash storage for the specified partition.

  参数:

    partition_label -- [in] Label of the partition. Must be no longer than 16 characters.

  返回:

    - ESP_OK if storage was successfully initialized.

    - ESP_ERR_NVS_NO_FREE_PAGES if the NVS storage contains no empty pages (which may happen if NVS partition was truncated)

    - ESP_ERR_NOT_FOUND if specified partition is not found in the partition table

    - ESP_ERR_NO_MEM in case memory could not be allocated for the internal structures

    - one of the error codes from the underlying flash storage driver

esp_err_t nvs_flash_init_partition_ptr(const esp_partition_t *partition)

  Initialize NVS flash storage for the partition specified by partition pointer.

  参数:

    partition -- [in] pointer to a partition obtained by the ESP partition API.

  返回:

    - ESP_OK if storage was successfully initialized

    - ESP_ERR_NVS_NO_FREE_PAGES if the NVS storage contains no empty pages (which may happen if NVS partition was truncated)

    - ESP_ERR_INVALID_ARG in case partition is NULL

    - ESP_ERR_NO_MEM in case memory could not be allocated for the internal structures

    - one of the error codes from the underlying flash storage driver

esp_err_t nvs_flash_deinit(void)

  Deinitialize NVS storage for the default NVS partition.

  Default NVS partition is the partition with "nvs" label in the partition table.

  返回:

    - ESP_OK on success (storage was deinitialized)

    - ESP_ERR_NVS_NOT_INITIALIZED if the storage was not initialized prior to this call

esp_err_t nvs_flash_deinit_partition(const char *partition_label)

  Deinitialize NVS storage for the given NVS partition.

  参数:

    partition_label -- [in] Label of the partition

  返回:

    - ESP_OK on success

    - ESP_ERR_NVS_NOT_INITIALIZED if the storage for given partition was not initialized prior to this call

esp_err_t nvs_flash_erase(void)

  Erase the default NVS partition.

  Erases all contents of the default NVS partition (one with label "nvs").

  备注

  If the partition is initialized, this function first de-initializes it. Afterwards, the partition has to be initialized again to be used.

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_FOUND if there is no NVS partition labeled "nvs" in the partition table

    - different error in case de-initialization fails (shouldn't happen)

esp_err_t nvs_flash_erase_partition(const char *part_name)

  Erase specified NVS partition.

  Erase all content of a specified NVS partition

  备注

  If the partition is initialized, this function first de-initializes it. Afterwards, the partition has to be initialized again to be used.

  参数:

    part_name -- [in] Name (label) of the partition which should be erased

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_FOUND if there is no NVS partition with the specified name in the partition table

    - different error in case de-initialization fails (shouldn't happen)

esp_err_t nvs_flash_erase_partition_ptr(const esp_partition_t *partition)

  Erase custom partition.

  Erase all content of specified custom partition.

  备注

  If the partition is initialized, this function first de-initializes it. Afterwards, the partition has to be initialized again to be used.

  参数:

    partition -- [in] pointer to a partition obtained by the ESP partition API.

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_FOUND if there is no partition with the specified parameters in the partition table

    - ESP_ERR_INVALID_ARG in case partition is NULL

    - one of the error codes from the underlying flash storage driver

esp_err_t nvs_flash_secure_init(nvs_sec_cfg_t *cfg)

  Initialize the default NVS partition.

  This API initialises the default NVS partition. The default NVS partition is the one that is labeled "nvs" in the partition table.

  参数:

    cfg -- [in] Security configuration (keys) to be used for NVS encryption/decryption. If cfg is NULL, no encryption is used.

  返回:

    - ESP_OK if storage has been initialized successfully.

    - ESP_ERR_NVS_NO_FREE_PAGES if the NVS storage contains no empty pages (which may happen if NVS partition was truncated)

    - ESP_ERR_NOT_FOUND if no partition with label "nvs" is found in the partition table

    - ESP_ERR_NO_MEM in case memory could not be allocated for the internal structures

    - one of the error codes from the underlying flash storage driver

esp_err_t nvs_flash_secure_init_partition(const char *partition_label, nvs_sec_cfg_t *cfg)

  Initialize NVS flash storage for the specified partition.

  参数:

    - partition_label -- [in] Label of the partition. Note that internally, a reference to passed value is kept and it should be accessible for future operations

    - cfg -- [in] Security configuration (keys) to be used for NVS encryption/decryption. If cfg is null, no encryption/decryption is used.

  返回:

    - ESP_OK if storage has been initialized successfully.

    - ESP_ERR_NVS_NO_FREE_PAGES if the NVS storage contains no empty pages (which may happen if NVS partition was truncated)

    - ESP_ERR_NOT_FOUND if specified partition is not found in the partition table

    - ESP_ERR_NO_MEM in case memory could not be allocated for the internal structures

    - one of the error codes from the underlying flash storage driver

esp_err_t nvs_flash_generate_keys(const esp_partition_t *partition, nvs_sec_cfg_t *cfg)

  Generate and store NVS keys in the provided esp partition.

  参数:

    - partition -- [in] Pointer to partition structure obtained using esp_partition_find_first or esp_partition_get. Must be non-NULL.

    - cfg -- [out] Pointer to nvs security configuration structure. Pointer must be non-NULL. Generated keys will be populated in this structure.

  返回:

    - ESP_OK, if cfg was read successfully;

    - ESP_ERR_INVALID_ARG, if partition or cfg is NULL;

    - or error codes from esp_partition_write/erase APIs.

esp_err_t nvs_flash_read_security_cfg(const esp_partition_t *partition, nvs_sec_cfg_t *cfg)

  Read NVS security configuration from a partition.

  备注

  Provided partition is assumed to be marked 'encrypted'.

  参数:

    - partition -- [in] Pointer to partition structure obtained using esp_partition_find_first or esp_partition_get. Must be non-NULL.

    - cfg -- [out] Pointer to nvs security configuration structure. Pointer must be non-NULL.

  返回:

    - ESP_OK, if cfg was read successfully;

    - ESP_ERR_INVALID_ARG, if partition or cfg is NULL

    - ESP_ERR_NVS_KEYS_NOT_INITIALIZED, if the partition is not yet written with keys.

    - ESP_ERR_NVS_CORRUPT_KEY_PART, if the partition containing keys is found to be corrupt

    - or error codes from esp_partition_read API.

esp_err_t nvs_flash_register_security_scheme(nvs_sec_scheme_t *scheme_cfg)

  Registers the given security scheme for NVS encryption The scheme registered with sec_scheme_id by this API be used as the default security scheme for the "nvs" partition. Users will have to call this API explicitly in their application.

  参数:

    scheme_cfg -- [in] Pointer to the security scheme configuration structure that the user (or the nvs_key_provider) wants to register.

  返回:

    - ESP_OK, if security scheme registration succeeds;

    - ESP_ERR_INVALID_ARG, if scheme_cfg is NULL;

    - ESP_FAIL, if security scheme registration fails

nvs_sec_scheme_t *nvs_flash_get_default_security_scheme(void)

  Fetch the configuration structure for the default active security scheme for NVS encryption.

  返回:

    Pointer to the default active security scheme configuration (NULL if no scheme is registered yet i.e. active)

esp_err_t nvs_flash_generate_keys_v2(nvs_sec_scheme_t *scheme_cfg, nvs_sec_cfg_t *cfg)

  Generate (and store) the NVS keys using the specified key-protection scheme.

  参数:

    - scheme_cfg -- [in] Security scheme specific configuration

    - cfg -- [out] Security configuration (encryption keys)

  返回:

    - ESP_OK, if cfg was populated successfully with generated encryption keys;

    - ESP_ERR_INVALID_ARG, if scheme_cfg or cfg is NULL;

    - ESP_FAIL, if the key generation process fails

esp_err_t nvs_flash_read_security_cfg_v2(nvs_sec_scheme_t *scheme_cfg, nvs_sec_cfg_t *cfg)

  Read NVS security configuration set by the specified security scheme.

  参数:

    - scheme_cfg -- [in] Security scheme specific configuration

    - cfg -- [out] Security configuration (encryption keys)

  返回:

    - ESP_OK, if cfg was read successfully;

    - ESP_ERR_INVALID_ARG, if scheme_cfg or cfg is NULL;

    - ESP_FAIL, if the key reading process fails

### Structures

struct nvs_sec_cfg_t

  Key for encryption and decryption.

  Public Members

  uint8_t eky[NVS_KEY_SIZE]

    XTS encryption and decryption key

  uint8_t tky[NVS_KEY_SIZE]

    XTS tweak key

struct nvs_sec_scheme_t

  NVS encryption: Security scheme configuration structure.

  Public Members

  int scheme_id

    Security Scheme ID (E.g. HMAC)

  void *scheme_data

    Scheme-specific data (E.g. eFuse block for HMAC-based key generation)

  nvs_flash_generate_keys_t nvs_flash_key_gen

    Callback for the nvs_flash_key_gen implementation

  nvs_flash_read_cfg_t nvs_flash_read_cfg

    Callback for the nvs_flash_read_keys implementation

### Macros

NVS_KEY_SIZE

### Type Definitions

typedef esp_err_t (*nvs_flash_generate_keys_t)(const void *scheme_data, nvs_sec_cfg_t *cfg)

  Callback function prototype for generating the NVS encryption keys.

typedef esp_err_t (*nvs_flash_read_cfg_t)(const void *scheme_data, nvs_sec_cfg_t *cfg)

  Callback function prototype for reading the NVS encryption keys.

### Header File

- components/nvs_flash/include/nvs.h

- This header file can be included with:

  >     #include "nvs.h"

- This header file is a part of the API provided by the `nvs_flash` component. To declare that your component depends on `nvs_flash`, add the following to your CMakeLists.txt:

  >     REQUIRES nvs_flash

  > or

  >     PRIV_REQUIRES nvs_flash

### Functions

esp_err_t nvs_set_i8(nvs_handle_t handle, const char *key, int8_t value)

  set int8_t value for given key

  Set value for the key, given its name. Note that the actual storage will not be updated until `nvs_commit` is called. Regardless whether key-value pair is created or updated, function always requires at least one nvs available entry. See `nvs_get_stats` . After create type of operation, the number of available entries is decreased by one. After update type of operation, the number of available entries remains the same.

  参数:

    - handle -- [in] Handle obtained from nvs_open function. Handles that were opened read only cannot be used.

    - key -- [in] Key name. Maximum length is (NVS_KEY_NAME_MAX_SIZE-1) characters. Shouldn't be empty.

    - value -- [in] The value to set.

  返回:

    - ESP_OK if value was set successfully

    - ESP_FAIL if there is an internal error; most likely due to corrupted NVS partition (only if NVS assertion checks are disabled)

    - ESP_ERR_NVS_INVALID_HANDLE if handle has been closed or is NULL

    - ESP_ERR_NVS_READ_ONLY if storage handle was opened as read only

    - ESP_ERR_NVS_INVALID_NAME if key name doesn't satisfy constraints

    - ESP_ERR_NVS_NOT_ENOUGH_SPACE if there is not enough space in the underlying storage to save the value

    - ESP_ERR_NVS_REMOVE_FAILED if the value wasn't updated because flash write operation has failed. The value was written however, and update will be finished after re-initialization of nvs, provided that flash operation doesn't fail again.

esp_err_t nvs_set_u8(nvs_handle_t handle, const char *key, uint8_t value)

  set uint8_t value for given key

  This function is the same as `nvs_set_i8` except for the data type.

esp_err_t nvs_set_i16(nvs_handle_t handle, const char *key, int16_t value)

  set int16_t value for given key

  This function is the same as `nvs_set_i8` except for the data type.

esp_err_t nvs_set_u16(nvs_handle_t handle, const char *key, uint16_t value)

  set uint16_t value for given key

  This function is the same as `nvs_set_i8` except for the data type.

esp_err_t nvs_set_i32(nvs_handle_t handle, const char *key, int32_t value)

  set int32_t value for given key

  This function is the same as `nvs_set_i8` except for the data type.

esp_err_t nvs_set_u32(nvs_handle_t handle, const char *key, uint32_t value)

  set uint32_t value for given key

  This function is the same as `nvs_set_i8` except for the data type.

esp_err_t nvs_set_i64(nvs_handle_t handle, const char *key, int64_t value)

  set int64_t value for given key

  This function is the same as `nvs_set_i8` except for the data type.

esp_err_t nvs_set_u64(nvs_handle_t handle, const char *key, uint64_t value)

  set uint64_t value for given key

  This function is the same as `nvs_set_i8` except for the data type.

esp_err_t nvs_set_str(nvs_handle_t handle, const char *key, const char *value)

  set string for given key

  Sets string value for the key. Function requires whole space for new data to be available as contiguous entries in same nvs page. Operation consumes 1 overhead entry and 1 entry per each 32 characters of new string including zero character to be set. In case of value update for existing key, entries occupied by the previous value and overhead entry are returned to the pool of available entries. Note that storage of long string values can fail due to fragmentation of nvs pages even if `available_entries` returned by `nvs_get_stats` suggests enough overall space available. Note that the underlying storage will not be updated until `nvs_commit` is called.

  参数:

    - handle -- [in] Handle obtained from nvs_open function. Handles that were opened read only cannot be used.

    - key -- [in] Key name. Maximum length is (NVS_KEY_NAME_MAX_SIZE-1) characters. Shouldn't be empty.

    - value -- [in] The value to set. For strings, the maximum length (including null character) is 4000 bytes, if there is one complete page free for writing. This decreases, however, if the free space is fragmented.

  返回:

    - ESP_OK if value was set successfully

    - ESP_ERR_NVS_INVALID_HANDLE if handle has been closed or is NULL

    - ESP_ERR_NVS_READ_ONLY if storage handle was opened as read only

    - ESP_ERR_NVS_INVALID_NAME if key name doesn't satisfy constraints

    - ESP_ERR_NVS_NOT_ENOUGH_SPACE if there is not enough space in the underlying storage to save the value

    - ESP_ERR_NVS_REMOVE_FAILED if the value wasn't updated because flash write operation has failed. The value was written however, and update will be finished after re-initialization of nvs, provided that flash operation doesn't fail again.

    - ESP_ERR_NVS_VALUE_TOO_LONG if the string value is too long

esp_err_t nvs_get_i8(nvs_handle_t handle, const char *key, int8_t *out_value)

  get int8_t value for given key

  These functions retrieve value for the key, given its name. If `key` does not exist, or the requested variable type doesn't match the type which was used when setting a value, an error is returned.

  In case of any error, out_value is not modified.

  `out_value` has to be a pointer to an already allocated variable of the given type.

      // Example of using nvs_get_i32:
      int32_t max_buffer_size = 4096; // default value
      esp_err_t err = nvs_get_i32(my_handle, "max_buffer_size", &max_buffer_size);
      assert(err == ESP_OK || err == ESP_ERR_NVS_NOT_FOUND);
      // if ESP_ERR_NVS_NOT_FOUND was returned, max_buffer_size will still
      // have its default value.

  参数:

    - handle -- [in] Handle obtained from nvs_open function.

    - key -- [in] Key name. Maximum length is (NVS_KEY_NAME_MAX_SIZE-1) characters. Shouldn't be empty.

    - out_value -- Pointer to the output value. May be NULL for nvs_get_str and nvs_get_blob, in this case required length will be returned in length argument.

  返回:

    - ESP_OK if the value was retrieved successfully

    - ESP_FAIL if there is an internal error; most likely due to corrupted NVS partition (only if NVS assertion checks are disabled)

    - ESP_ERR_NVS_NOT_FOUND if the requested key doesn't exist

    - ESP_ERR_NVS_INVALID_HANDLE if handle has been closed or is NULL

    - ESP_ERR_NVS_INVALID_NAME if key name doesn't satisfy constraints

    - ESP_ERR_NVS_INVALID_LENGTH if length is not sufficient to store data

esp_err_t nvs_get_u8(nvs_handle_t handle, const char *key, uint8_t *out_value)

  get uint8_t value for given key

  This function is the same as `nvs_get_i8` except for the data type.

esp_err_t nvs_get_i16(nvs_handle_t handle, const char *key, int16_t *out_value)

  get int16_t value for given key

  This function is the same as `nvs_get_i8` except for the data type.

esp_err_t nvs_get_u16(nvs_handle_t handle, const char *key, uint16_t *out_value)

  get uint16_t value for given key

  This function is the same as `nvs_get_i8` except for the data type.

esp_err_t nvs_get_i32(nvs_handle_t handle, const char *key, int32_t *out_value)

  get int32_t value for given key

  This function is the same as `nvs_get_i8` except for the data type.

esp_err_t nvs_get_u32(nvs_handle_t handle, const char *key, uint32_t *out_value)

  get uint32_t value for given key

  This function is the same as `nvs_get_i8` except for the data type.

esp_err_t nvs_get_i64(nvs_handle_t handle, const char *key, int64_t *out_value)

  get int64_t value for given key

  This function is the same as `nvs_get_i8` except for the data type.

esp_err_t nvs_get_u64(nvs_handle_t handle, const char *key, uint64_t *out_value)

  get uint64_t value for given key

  This function is the same as `nvs_get_i8` except for the data type.

esp_err_t nvs_get_str(nvs_handle_t handle, const char *key, char *out_value, size_t *length)

  get string value for given key

  These functions retrieve the data of an entry, given its key. If key does not exist, or the requested variable type doesn't match the type which was used when setting a value, an error is returned.

  In case of any error, out_value is not modified.

  All functions expect out_value to be a pointer to an already allocated variable of the given type.

  nvs_get_str and nvs_get_blob functions support WinAPI-style length queries. To get the size necessary to store the value, call nvs_get_str or nvs_get_blob with zero out_value and non-zero pointer to length. Variable pointed to by length argument will be set to the required length. For nvs_get_str, this length includes the zero terminator. When calling nvs_get_str and nvs_get_blob with non-zero out_value, length has to be non-zero and has to point to the length available in out_value. It is suggested that nvs_get/set_str is used for zero-terminated C strings, and nvs_get/set_blob used for arbitrary data structures.

      // Example (without error checking) of using nvs_get_str to get a string into dynamic array:
      size_t required_size;
      nvs_get_str(my_handle, "server_name", NULL, &required_size);
      char* server_name = malloc(required_size);
      nvs_get_str(my_handle, "server_name", server_name, &required_size);

      // Example (without error checking) of using nvs_get_blob to get a binary data
      into a static array:
      uint8_t mac_addr[6];
      size_t size = sizeof(mac_addr);
      nvs_get_blob(my_handle, "dst_mac_addr", mac_addr, &size);

  参数:

    - handle -- [in] Handle obtained from nvs_open function.

    - key -- [in] Key name. Maximum length is (NVS_KEY_NAME_MAX_SIZE-1) characters. Shouldn't be empty.

    - out_value -- [out] Pointer to the output value. May be NULL for nvs_get_str and nvs_get_blob, in this case required length will be returned in length argument.

    - length -- [inout] A non-zero pointer to the variable holding the length of out_value. In case out_value a zero, will be set to the length required to hold the value. In case out_value is not zero, will be set to the actual length of the value written. For nvs_get_str this includes zero terminator.

  返回:

    - ESP_OK if the value was retrieved successfully

    - ESP_FAIL if there is an internal error; most likely due to corrupted NVS partition (only if NVS assertion checks are disabled)

    - ESP_ERR_NVS_NOT_FOUND if the requested key doesn't exist

    - ESP_ERR_NVS_INVALID_HANDLE if handle has been closed or is NULL

    - ESP_ERR_NVS_INVALID_NAME if key name doesn't satisfy constraints

    - ESP_ERR_NVS_INVALID_LENGTH if `length` is not sufficient to store data

esp_err_t nvs_get_blob(nvs_handle_t handle, const char *key, void *out_value, size_t *length)

  get blob value for given key

  This function behaves the same as `nvs_get_str`, except for the data type.

esp_err_t nvs_open(const char *namespace_name, nvs_open_mode_t open_mode, nvs_handle_t *out_handle)

  Open non-volatile storage with a given namespace from the default NVS partition.

  Multiple internal ESP-IDF and third party application modules can store their key-value pairs in the NVS module. In order to reduce possible conflicts on key names, each module can use its own namespace. The default NVS partition is the one that is labelled "nvs" in the partition table.

  参数:

    - namespace_name -- [in] Namespace name. Maximum length is (NVS_KEY_NAME_MAX_SIZE-1) characters. Shouldn't be empty.

    - open_mode -- [in] NVS_READWRITE or NVS_READONLY. If NVS_READONLY, will open a handle for reading only. All write requests will be rejected for this handle.

    - out_handle -- [out] If successful (return code is zero), handle will be returned in this argument.

  返回:

    - ESP_OK if storage handle was opened successfully

    - ESP_FAIL if there is an internal error; most likely due to corrupted NVS partition (only if NVS assertion checks are disabled)

    - ESP_ERR_NVS_NOT_INITIALIZED if the storage driver is not initialized

    - ESP_ERR_NVS_PART_NOT_FOUND if the partition with label "nvs" is not found

    - ESP_ERR_NVS_NOT_FOUND id namespace doesn't exist yet and mode is NVS_READONLY

    - ESP_ERR_NVS_INVALID_NAME if namespace name doesn't satisfy constraints

    - ESP_ERR_NO_MEM in case memory could not be allocated for the internal structures

    - ESP_ERR_NVS_NOT_ENOUGH_SPACE if there is no space for a new entry or there are too many different namespaces (maximum allowed different namespaces: 254)

    - ESP_ERR_NOT_ALLOWED if the NVS partition is read-only and mode is NVS_READWRITE

    - ESP_ERR_INVALID_ARG if out_handle is equal to NULL

    - other error codes from the underlying storage driver

esp_err_t nvs_open_from_partition(const char *part_name, const char *namespace_name, nvs_open_mode_t open_mode, nvs_handle_t *out_handle)

  Open non-volatile storage with a given namespace from specified partition.

  The behaviour is same as nvs_open() API. However this API can operate on a specified NVS partition instead of default NVS partition. Note that the specified partition must be registered with NVS using nvs_flash_init_partition() API.

  参数:

    - part_name -- [in] Label (name) of the partition of interest for object read/write/erase

    - namespace_name -- [in] Namespace name. Maximum length is (NVS_KEY_NAME_MAX_SIZE-1) characters. Shouldn't be empty.

    - open_mode -- [in] NVS_READWRITE or NVS_READONLY. If NVS_READONLY, will open a handle for reading only. All write requests will be rejected for this handle.

    - out_handle -- [out] If successful (return code is zero), handle will be returned in this argument.

  返回:

    - ESP_OK if storage handle was opened successfully

    - ESP_FAIL if there is an internal error; most likely due to corrupted NVS partition (only if NVS assertion checks are disabled)

    - ESP_ERR_NVS_NOT_INITIALIZED if the storage driver is not initialized

    - ESP_ERR_NVS_PART_NOT_FOUND if the partition with specified name is not found

    - ESP_ERR_NVS_NOT_FOUND id namespace doesn't exist yet and mode is NVS_READONLY

    - ESP_ERR_NVS_INVALID_NAME if namespace name doesn't satisfy constraints

    - ESP_ERR_NO_MEM in case memory could not be allocated for the internal structures

    - ESP_ERR_NVS_NOT_ENOUGH_SPACE if there is no space for a new entry or there are too many different namespaces (maximum allowed different namespaces: 254)

    - ESP_ERR_NOT_ALLOWED if the NVS partition is read-only and mode is NVS_READWRITE

    - ESP_ERR_INVALID_ARG if out_handle is equal to NULL

    - other error codes from the underlying storage driver

esp_err_t nvs_set_blob(nvs_handle_t handle, const char *key, const void *value, size_t length)

  set variable length binary value for given key

  Sets variable length binary value for the key. Function uses 2 overhead and 1 entry per each 32 bytes of new data from the pool of available entries. See `nvs_get_stats` . In case of value update for existing key, space occupied by the existing value and 2 overhead entries are returned to the pool of available entries. Note that the underlying storage will not be updated until `nvs_commit` is called.

  参数:

    - handle -- [in] Handle obtained from nvs_open function. Handles that were opened read only cannot be used.

    - key -- [in] Key name. Maximum length is (NVS_KEY_NAME_MAX_SIZE-1) characters. Shouldn't be empty.

    - value -- [in] The value to set.

    - length -- [in] length of binary value to set, in bytes; Maximum length is 508000 bytes or (97.6% of the partition size - 4000) bytes whichever is lower.

  返回:

    - ESP_OK if value was set successfully

    - ESP_FAIL if there is an internal error; most likely due to corrupted NVS partition (only if NVS assertion checks are disabled)

    - ESP_ERR_NVS_INVALID_HANDLE if handle has been closed or is NULL

    - ESP_ERR_NVS_READ_ONLY if storage handle was opened as read only

    - ESP_ERR_NVS_INVALID_NAME if key name doesn't satisfy constraints

    - ESP_ERR_NVS_NOT_ENOUGH_SPACE if there is not enough space in the underlying storage to save the value

    - ESP_ERR_NVS_REMOVE_FAILED if the value wasn't updated because flash write operation has failed. The value was written however, and update will be finished after re-initialization of nvs, provided that flash operation doesn't fail again.

    - ESP_ERR_NVS_VALUE_TOO_LONG if the value is too long

esp_err_t nvs_find_key(nvs_handle_t handle, const char *key, nvs_type_t *out_type)

  Lookup key-value pair with given key name.

  Note that function may indicate both existence of the key as well as the data type of NVS entry if it is found.

  参数:

    - handle -- [in] Storage handle obtained with nvs_open.

    - key -- [in] Key name. Maximum length is (NVS_KEY_NAME_MAX_SIZE-1) characters. Shouldn't be empty.

    - out_type -- [out] Pointer to the output variable populated with data type of NVS entry in case key was found. May be NULL, respective data type is then not provided.

  返回:

    - ESP_OK if NVS entry for key provided was found

    - ESP_ERR_NVS_NOT_FOUND if the requested key doesn't exist

    - ESP_ERR_NVS_INVALID_HANDLE if handle has been closed or is NULL

    - ESP_FAIL if there is an internal error; most likely due to corrupted NVS partition (only if NVS assertion checks are disabled)

    - other error codes from the underlying storage driver

esp_err_t nvs_erase_key(nvs_handle_t handle, const char *key)

  Erase key-value pair with given key name.

  Note that actual storage may not be updated until nvs_commit function is called.

  参数:

    - handle -- [in] Storage handle obtained with nvs_open. Handles that were opened read only cannot be used.

    - key -- [in] Key name. Maximum length is (NVS_KEY_NAME_MAX_SIZE-1) characters. Shouldn't be empty.

  返回:

    - ESP_OK if erase operation was successful

    - ESP_FAIL if there is an internal error; most likely due to corrupted NVS partition (only if NVS assertion checks are disabled)

    - ESP_ERR_NVS_INVALID_HANDLE if handle has been closed or is NULL

    - ESP_ERR_NVS_READ_ONLY if handle was opened as read only

    - ESP_ERR_NVS_NOT_FOUND if the requested key doesn't exist

    - other error codes from the underlying storage driver

esp_err_t nvs_erase_all(nvs_handle_t handle)

  Erase all key-value pairs in a namespace.

  Note that actual storage may not be updated until nvs_commit function is called.

  参数:

    handle -- [in] Storage handle obtained with nvs_open. Handles that were opened read only cannot be used.

  返回:

    - ESP_OK if erase operation was successful

    - ESP_FAIL if there is an internal error; most likely due to corrupted NVS partition (only if NVS assertion checks are disabled)

    - ESP_ERR_NVS_INVALID_HANDLE if handle has been closed or is NULL

    - ESP_ERR_NVS_READ_ONLY if handle was opened as read only

    - other error codes from the underlying storage driver

esp_err_t nvs_commit(nvs_handle_t handle)

  Write any pending changes to non-volatile storage.

  After setting any values, nvs_commit() must be called to ensure changes are written to non-volatile storage. Individual implementations may write to storage at other times, but this is not guaranteed.

  参数:

    handle -- [in] Storage handle obtained with nvs_open. Handles that were opened read only cannot be used.

  返回:

    - ESP_OK if the changes have been written successfully

    - ESP_ERR_NVS_INVALID_HANDLE if handle has been closed or is NULL

    - other error codes from the underlying storage driver

void nvs_close(nvs_handle_t handle)

  Close the storage handle and free any allocated resources.

  This function should be called for each handle opened with nvs_open once the handle is not in use any more. Closing the handle may not automatically write the changes to nonvolatile storage. This has to be done explicitly using nvs_commit function. Once this function is called on a handle, the handle should no longer be used.

  参数:

    handle -- [in] Storage handle to close

esp_err_t nvs_get_stats(const char *part_name, nvs_stats_t *nvs_stats)

  Fill structure nvs_stats_t. It provides info about memory used by NVS.

  This function calculates the number of used entries, free entries, available entries, total entries and number of namespaces in partition.

      // Example of nvs_get_stats() to get overview of actual statistics of data entries :
      nvs_stats_t nvs_stats;
      nvs_get_stats(NULL, &nvs_stats);
      printf("Count: UsedEntries = (%lu), FreeEntries = (%lu), AvailableEntries = (%lu), AllEntries = (%lu)\n",
             nvs_stats.used_entries, nvs_stats.free_entries, nvs_stats.available_entries, nvs_stats.total_entries);

  参数:

    - part_name -- [in] Partition name NVS in the partition table. If pass a NULL than will use NVS_DEFAULT_PART_NAME ("nvs").

    - nvs_stats -- [out] Returns filled structure nvs_states_t. It provides info about used memory the partition.

  返回:

    - ESP_OK if the changes have been written successfully. Return param nvs_stats will be filled.

    - ESP_ERR_NVS_PART_NOT_FOUND if the partition with label "name" is not found. Return param nvs_stats will be filled 0.

    - ESP_ERR_NVS_NOT_INITIALIZED if the storage driver is not initialized. Return param nvs_stats will be filled 0.

    - ESP_ERR_INVALID_ARG if nvs_stats is equal to NULL.

    - ESP_ERR_INVALID_STATE if there is page with the status of INVALID. Return param nvs_stats will be filled not with correct values because not all pages will be counted. Counting will be interrupted at the first INVALID page.

esp_err_t nvs_get_used_entry_count(nvs_handle_t handle, size_t *used_entries)

  Calculate all entries in a namespace.

  An entry represents the smallest storage unit in NVS. Strings and blobs may occupy more than one entry. Note that to find out the total number of entries occupied by the namespace, add one to the returned value used_entries (if err is equal to ESP_OK). Because the name space entry takes one entry.

      // Example of nvs_get_used_entry_count() to get amount of all key-value pairs in one namespace:
      nvs_handle_t handle;
      nvs_open("namespace1", NVS_READWRITE, &handle);
      ...
      size_t used_entries;
      size_t total_entries_namespace;
      if(nvs_get_used_entry_count(handle, &used_entries) == ESP_OK){
      // the total number of entries occupied by the namespace
          total_entries_namespace = used_entries + 1;
      }

  参数:

    - handle -- [in] Handle obtained from nvs_open function.

    - used_entries -- [out] Returns amount of used entries from a namespace.

  返回:

    - ESP_OK if the changes have been written successfully. Return param used_entries will be filled valid value.

    - ESP_ERR_NVS_NOT_INITIALIZED if the storage driver is not initialized. Return param used_entries will be filled 0.

    - ESP_ERR_NVS_INVALID_HANDLE if handle has been closed or is NULL. Return param used_entries will be filled 0.

    - ESP_ERR_INVALID_ARG if used_entries is equal to NULL.

    - Other error codes from the underlying storage driver. Return param used_entries will be filled 0.

esp_err_t nvs_entry_find(const char *part_name, const char *namespace_name, nvs_type_t type, nvs_iterator_t *output_iterator)

  Create an iterator to enumerate NVS entries based on one or more parameters.

      // Example of listing all the key-value pairs of any type under specified partition and namespace
       nvs_iterator_t it = NULL;
       esp_err_t res = nvs_entry_find(<nvs_partition_name>, <namespace>, NVS_TYPE_ANY, &it);
       while(res == ESP_OK) {
      nvs_entry_info_t info;
           nvs_entry_info(it, &info); // Can omit error check if parameters are guaranteed to be non-NULL
           printf("key '%s', type '%d' \n", info.key, info.type);
           res = nvs_entry_next(&it);
       }
       nvs_release_iterator(it);

  参数:

    - part_name -- [in] Partition name

    - namespace_name -- [in] Set this value if looking for entries with a specific namespace. Pass NULL otherwise.

    - type -- [in] One of nvs_type_t values.

    - output_iterator -- [out] Set to a valid iterator to enumerate all the entries found. Set to NULL if no entry for specified criteria was found. If any other error except ESP_ERR_INVALID_ARG occurs, `output_iterator` is NULL, too. If ESP_ERR_INVALID_ARG occurs, `output_iterator` is not changed. If a valid iterator is obtained through this function, it has to be released using `nvs_release_iterator` when not used any more, unless ESP_ERR_INVALID_ARG is returned.

  返回:

    - ESP_OK if no internal error or programming error occurred.

    - ESP_ERR_NVS_NOT_FOUND if no element of specified criteria has been found.

    - ESP_ERR_NO_MEM if memory has been exhausted during allocation of internal structures.

    - ESP_ERR_INVALID_ARG if any of the parameters is NULL. Note: don't release `output_iterator` in case ESP_ERR_INVALID_ARG has been returned

esp_err_t nvs_entry_find_in_handle(nvs_handle_t handle, nvs_type_t type, nvs_iterator_t *output_iterator)

  Create an iterator to enumerate NVS entries based on a handle and type.

      // Example of listing all the key-value pairs of any type under specified handle (which defines a partition and namespace)
       nvs_iterator_t it = NULL;
       esp_err_t res = nvs_entry_find_in_handle(<nvs_handle>, NVS_TYPE_ANY, &it);
       while(res == ESP_OK) {
      nvs_entry_info_t info;
           nvs_entry_info(it, &info); // Can omit error check if parameters are guaranteed to be non-NULL
           printf("key '%s', type '%d' \n", info.key, info.type);
           res = nvs_entry_next(&it);
       }
       nvs_release_iterator(it);

  参数:

    - handle -- [in] Handle obtained from nvs_open function.

    - type -- [in] One of nvs_type_t values.

    - output_iterator -- [out] Set to a valid iterator to enumerate all the entries found. Set to NULL if no entry for specified criteria was found. If any other error except ESP_ERR_INVALID_ARG occurs, `output_iterator` is NULL, too. If ESP_ERR_INVALID_ARG occurs, `output_iterator` is not changed. If a valid iterator is obtained through this function, it has to be released using `nvs_release_iterator` when not used any more, unless ESP_ERR_INVALID_ARG is returned.

  返回:

    - ESP_OK if no internal error or programming error occurred.

    - ESP_ERR_NVS_NOT_FOUND if no element of specified criteria has been found.

    - ESP_ERR_NO_MEM if memory has been exhausted during allocation of internal structures.

    - ESP_ERR_NVS_INVALID_HANDLE if unknown handle was specified.

    - ESP_ERR_INVALID_ARG if output_iterator parameter is NULL. Note: don't release `output_iterator` in case ESP_ERR_INVALID_ARG has been returned

esp_err_t nvs_entry_next(nvs_iterator_t *iterator)

  Advances the iterator to next item matching the iterator criteria.

  Note that any copies of the iterator will be invalid after this call.

  参数:

    iterator -- [inout] Iterator obtained from nvs_entry_find or nvs_entry_find_in_handle function. Must be non-NULL. If any error except ESP_ERR_INVALID_ARG occurs, `iterator` is set to NULL. If ESP_ERR_INVALID_ARG occurs, `iterator` is not changed.

  返回:

    - ESP_OK if no internal error or programming error occurred.

    - ESP_ERR_NVS_NOT_FOUND if no next element matching the iterator criteria.

    - ESP_ERR_INVALID_ARG if `iterator` is NULL.

    - Possibly other errors in the future for internal programming or flash errors.

esp_err_t nvs_entry_info(const nvs_iterator_t iterator, nvs_entry_info_t *out_info)

  Fills nvs_entry_info_t structure with information about entry pointed to by the iterator.

  参数:

    - iterator -- [in] Iterator obtained from nvs_entry_find or nvs_entry_find_in_handle function. Must be non-NULL.

    - out_info -- [out] Structure to which entry information is copied.

  返回:

    - ESP_OK if all parameters are valid; current iterator data has been written to out_info

    - ESP_ERR_INVALID_ARG if one of the parameters is NULL.

void nvs_release_iterator(nvs_iterator_t iterator)

  Release iterator.

  参数:

    iterator -- [in] Release iterator obtained from nvs_entry_find or nvs_entry_find_in_handle or nvs_entry_next function. NULL argument is allowed.

### Structures

struct nvs_entry_info_t

  information about entry obtained from nvs_entry_info function

  Public Members

  char namespace_name[NVS_NS_NAME_MAX_SIZE]

    Namespace to which key-value belong

  char key[NVS_KEY_NAME_MAX_SIZE]

    Key of stored key-value pair

  nvs_type_t type

    Type of stored key-value pair

struct nvs_stats_t

  备注

  Info about storage space NVS.

  Public Members

  size_t used_entries

    Number of used entries.

  size_t free_entries

    Number of free entries. It includes also reserved entries.

  size_t available_entries

    Number of entries available for data storage.

  size_t total_entries

    Number of all entries.

  size_t namespace_count

    Number of namespaces.

### Macros

ESP_ERR_NVS_BASE

  Starting number of error codes

ESP_ERR_NVS_NOT_INITIALIZED

  The storage driver is not initialized

ESP_ERR_NVS_NOT_FOUND

  A requested entry couldn't be found or namespace doesn’t exist yet and mode is NVS_READONLY

ESP_ERR_NVS_TYPE_MISMATCH

  The type of set or get operation doesn't match the type of value stored in NVS

ESP_ERR_NVS_READ_ONLY

  Storage handle was opened as read only

ESP_ERR_NVS_NOT_ENOUGH_SPACE

  There is not enough space in the underlying storage to save the value

ESP_ERR_NVS_INVALID_NAME

  Namespace name doesn’t satisfy constraints

ESP_ERR_NVS_INVALID_HANDLE

  Handle has been closed or is NULL

ESP_ERR_NVS_REMOVE_FAILED

  The value wasn’t updated because flash write operation has failed. The value was written however, and update will be finished after re-initialization of nvs, provided that flash operation doesn’t fail again.

ESP_ERR_NVS_KEY_TOO_LONG

  Key name is too long

ESP_ERR_NVS_PAGE_FULL

  Internal error; never returned by nvs API functions

ESP_ERR_NVS_INVALID_STATE

  NVS is in an inconsistent state due to a previous error. Call nvs_flash_init and nvs_open again, then retry.

ESP_ERR_NVS_INVALID_LENGTH

  String or blob length is not sufficient to store data

ESP_ERR_NVS_NO_FREE_PAGES

  NVS partition doesn't contain any empty pages. This may happen if NVS partition was truncated. Erase the whole partition and call nvs_flash_init again.

ESP_ERR_NVS_VALUE_TOO_LONG

  Value doesn't fit into the entry or string or blob length is longer than supported by the implementation

ESP_ERR_NVS_PART_NOT_FOUND

  Partition with specified name is not found in the partition table

ESP_ERR_NVS_NEW_VERSION_FOUND

  NVS partition contains data in new format and cannot be recognized by this version of code

ESP_ERR_NVS_XTS_ENCR_FAILED

  XTS encryption failed while writing NVS entry

ESP_ERR_NVS_XTS_DECR_FAILED

  XTS decryption failed while reading NVS entry

ESP_ERR_NVS_XTS_CFG_FAILED

  XTS configuration setting failed

ESP_ERR_NVS_XTS_CFG_NOT_FOUND

  XTS configuration not found

ESP_ERR_NVS_ENCR_NOT_SUPPORTED

  NVS encryption is not supported in this version

ESP_ERR_NVS_KEYS_NOT_INITIALIZED

  NVS key partition is uninitialized

ESP_ERR_NVS_CORRUPT_KEY_PART

  NVS key partition is corrupt

ESP_ERR_NVS_WRONG_ENCRYPTION

  NVS partition is marked as encrypted with generic flash encryption. This is forbidden since the NVS encryption works differently.

ESP_ERR_NVS_CONTENT_DIFFERS

  Internal error; never returned by nvs API functions. NVS key is different in comparison

NVS_DEFAULT_PART_NAME

  Default partition name of the NVS partition in the partition table

NVS_PART_NAME_MAX_SIZE

  maximum length of partition name (excluding null terminator)

NVS_KEY_NAME_MAX_SIZE

  Maximum length of NVS key name (including null terminator)

NVS_NS_NAME_MAX_SIZE

  Maximum length of NVS namespace name (including null terminator)

NVS_GUARD_SYSVIEW_MACRO_EXPANSION_PUSH()

NVS_GUARD_SYSVIEW_MACRO_EXPANSION_POP()

### Type Definitions

typedef uint32_t nvs_handle_t

  Opaque pointer type representing non-volatile storage handle

typedef nvs_handle_t nvs_handle

typedef nvs_open_mode_t nvs_open_mode

typedef struct nvs_opaque_iterator_t *nvs_iterator_t

  Opaque pointer type representing iterator to nvs entries

### Enumerations

enum nvs_open_mode_t

  Mode of opening the non-volatile storage.

  Values:

  enumerator NVS_READONLY

    Read only

  enumerator NVS_READWRITE

    Read and write

enum nvs_type_t

  Types of variables.

  Values:

  enumerator NVS_TYPE_U8

    Type uint8_t

  enumerator NVS_TYPE_I8

    Type int8_t

  enumerator NVS_TYPE_U16

    Type uint16_t

  enumerator NVS_TYPE_I16

    Type int16_t

  enumerator NVS_TYPE_U32

    Type uint32_t

  enumerator NVS_TYPE_I32

    Type int32_t

  enumerator NVS_TYPE_U64

    Type uint64_t

  enumerator NVS_TYPE_I64

    Type int64_t

  enumerator NVS_TYPE_STR

    Type string

  enumerator NVS_TYPE_BLOB

    Type blob

  enumerator NVS_TYPE_ANY

    Must be last

此文档对您有帮助吗？

- 反馈已收到，谢谢！
- 如果您有其他意见，欢迎填写乐鑫文档反馈表。

- 我们重视您的反馈。
- 您可以填写乐鑫文档反馈表告诉我们如何改进该文档。