# 使用 C 语言宏编程 ULP FSM 协处理器（遗留）

[English]

想要为 ULP FSM 协处理器生成程序，除了用 ESP32-S2 ULP 协处理器目前的 binutils 端口外，还可以将类似汇编的宏嵌入到 ESP32-S2 应用程序中。以下是一个示例:

    const ulp_insn_t program[] = {
        I_MOVI(R3, 16),         // R3 <- 16
        I_LD(R0, R3, 0),        // R0 <- RTC_SLOW_MEM[R3 + 0]
        I_LD(R1, R3, 1),        // R1 <- RTC_SLOW_MEM[R3 + 1]
        I_ADDR(R2, R0, R1),     // R2 <- R0 + R1
        I_ST(R2, R3, 2),        // R2 -> RTC_SLOW_MEM[R2 + 2]
        I_HALT()
    };
    size_t load_addr = 0;
    size_t size = sizeof(program)/sizeof(ulp_insn_t);
    ulp_process_macros_and_load(load_addr, program, &size);
    ulp_run(load_addr);

`program` 数组是一个 `ulp_insn_t` 数组，即 ULP 协处理器指令。每个 `I_XXX` 预处理宏都会转换为单个 32 位指令。这些预处理宏的参数可以是寄存器号 (`R0 — R3`) 和字面常量。有关指令及其参数的详细信息，请参阅本指南末尾的 API 参考部分。

备注

由于一些宏指令会展开为内联函数调用，将这样的数组定义为全局数组会导致编译器报错："initializer element is not constant"。要修复此错误，请定义指令数组为局部数组。

备注

加载指令 (LD)、存储指令 (ST) 和移动指令 (MOV) 均使用 32 位字地址。地址 0 对应 `RTC_SLOW_MEM` 的第一个字。 这与汇编代码中相同指令的地址参数处理方式不同。详情请参阅 寻址注意事项。

要生成分支指令，使用特殊的 `M_` 预处理宏定义。 `M_LABEL` 宏定义可用于定义分支目标。标签标识符是一个 16 位整数。 `M_Bxxx` 宏定义可用于生成目标设置为特定标签的分支指令。

实现注意事项：这些 `M_` 预处理宏将被转换为两个 ulp_insn_t 值：一个是包含标签号的令牌值，另一个是实际指令。 `ulp_process_macros_and_load` 函数将标签号解析为地址，修改分支指令以使用正确的地址，并移除包含标签号的额外 `ulp_insn_t` 令牌。

以下是使用标签和分支的示例:

    const ulp_insn_t program[] = {
        I_MOVI(R0, 34),         // R0 <- 34
        M_LABEL(1),             // label_1
        I_MOVI(R1, 32),         // R1 <- 32
        I_LD(R1, R1, 0),        // R1 <- RTC_SLOW_MEM[R1]
        I_MOVI(R2, 33),         // R2 <- 33
        I_LD(R2, R2, 0),        // R2 <- RTC_SLOW_MEM[R2]
        I_SUBR(R3, R1, R2),     // R3 <- R1 - R2
        I_ST(R3, R0, 0),        // R3 -> RTC_SLOW_MEM[R0 + 0]
        I_ADDI(R0, R0, 1),      // R0++
        M_BL(1, 64),            // if (R0 < 64) goto label_1
        I_HALT(),
    };
    RTC_SLOW_MEM[32] = 42;
    RTC_SLOW_MEM[33] = 18;
    size_t load_addr = 0;
    size_t size = sizeof(program)/sizeof(ulp_insn_t);
    ulp_process_macros_and_load(load_addr, program, &size);
    ulp_run(load_addr);

## API 参考

### Header File

- components/ulp/ulp_fsm/include/esp32s2/ulp.h

- This header file can be included with:

  >     #include "ulp.h"

- This header file is a part of the API provided by the `ulp` component. To declare that your component depends on `ulp`, add the following to your CMakeLists.txt:

  >     REQUIRES ulp

  > or

  >     PRIV_REQUIRES ulp

### Functions

static inline uint32_t SOC_REG_TO_ULP_PERIPH_SEL(uint32_t reg)

  Map SoC peripheral register to periph_sel field of RD_REG and WR_REG instructions.

  参数:

    reg -- peripheral register in RTC_CNTL_, RTC_IO_, SENS_, RTC_I2C peripherals.

  返回:

    periph_sel value for the peripheral to which this register belongs.

### Unions

union ulp_insn
  #include <ulp.h>

  Instruction format structure.

  All ULP instructions are 32 bit long. This union contains field layouts used by all of the supported instructions. This union also includes a special "macro" instruction layout. This is not a real instruction which can be executed by the CPU. It acts as a token which is removed from the program by the ulp_process_macros_and_load function.

  These structures are not intended to be used directly. Preprocessor definitions provided below fill the fields of these structure with the right arguments.

  Public Members

  uint32_t cycles

    Number of cycles to sleep

    TBD, cycles used for measurement

  uint32_t unused

    Unused

  uint32_t opcode

    Opcode (OPCODE_DELAY)

    Opcode (OPCODE_ST)

    Opcode (OPCODE_LD)

    Opcode (OPCODE_HALT)

    Opcode (OPCODE_BRANCH)

    Opcode (OPCODE_ALU)

    Opcode (OPCODE_WR_REG)

    Opcode (OPCODE_RD_REG)

    Opcode (OPCODE_ADC)

    Opcode (OPCODE_TSENS)

    Opcode (OPCODE_I2C)

    Opcode (OPCODE_END)

    Opcode (OPCODE_MACRO)

  struct ulp_insn delay

    Format of DELAY instruction

  uint32_t dreg

    Register which contains data to store

    Register where the data should be loaded to

    Register which contains target PC, expressed in words (used if .reg == 1)

    Destination register

    Register where to store ADC result

    Register where to store temperature measurement result

  uint32_t sreg

    Register which contains address in RTC memory (expressed in words)

    Register with operand A

  uint32_t label

    Data label, 2-bit user defined unsigned value

    Label number

  uint32_t upper

    0: write the low half-word; 1: write the high half-word

  uint32_t wr_way

    0: write the full-word; 1: with the label; 3: without the label

  uint32_t unused1

    Unused

  uint32_t offset

    Offset to add to sreg

    Absolute value of target PC offset w.r.t. current PC, expressed in words

  uint32_t unused2

    Unused

  uint32_t sub_opcode

    Sub opcode (SUB_OPCODE_ST)

    Sub opcode (SUB_OPCODE_BX)

    Sub opcode (SUB_OPCODE_B)

    Sub opcode (SUB_OPCODE_ALU_REG)

    Sub opcode (SUB_OPCODE_ALU_IMM)

    Sub opcode (SUB_OPCODE_ALU_CNT)

    Sub opcode (SUB_OPCODE_WAKEUP)

    SUB_OPCODE_MACRO_LABEL or SUB_OPCODE_MACRO_BRANCH

  struct ulp_insn st

    Format of ST instruction

  uint32_t rd_upper

    0: read the high half-word; 1: read the low half-word

  struct ulp_insn ld

    Format of LD instruction

  struct ulp_insn halt

    Format of HALT instruction

  uint32_t addr

    Target PC, expressed in words (used if .reg == 0)

    Address within either RTC_CNTL, RTC_IO, or SARADC

  uint32_t reg

    Target PC in register (1) or immediate (0)

  uint32_t type

    Jump condition (BX_JUMP_TYPE_xxx)

  struct ulp_insn bx

    Format of BRANCH instruction (absolute address)

  uint32_t imm

    Immediate value to compare against

    Immediate value of operand B

    Immediate value

  uint32_t cmp

    Comparison to perform: B_CMP_L or B_CMP_GE

  uint32_t sign

    Sign of target PC offset: 0: positive, 1: negative

  struct ulp_insn b

    Format of BRANCH instruction (relative address)

  uint32_t treg

    Register with operand B

  uint32_t sel

    Operation to perform, one of ALU_SEL_xxx

  struct ulp_insn alu_reg

    Format of ALU instruction (both sources are registers)

  struct ulp_insn alu_imm

    Format of ALU instruction (one source is an immediate)

  uint32_t unused3

    Unused

  struct ulp_insn alu_cnt

    Format of ALU instruction with stage count register and an immediate

  uint32_t periph_sel

    Select peripheral: RTC_CNTL (0), RTC_IO(1), SARADC(2)

  uint32_t data

    8 bits of data to write

    Data to read or write

  uint32_t low

    Low bit

  uint32_t high

    High bit

  struct ulp_insn wr_reg

    Format of WR_REG instruction

  struct ulp_insn rd_reg

    Format of RD_REG instruction

  uint32_t mux

    Select SARADC pad (mux + 1)

  uint32_t sar_sel

    Select SARADC0 (0) or SARADC1 (1)

  struct ulp_insn adc

    Format of ADC instruction

  uint32_t wait_delay

    Cycles to wait after measurement is done

  uint32_t reserved

    Reserved, set to 0

  struct ulp_insn tsens

    Format of TSENS instruction

  uint32_t i2c_addr

    I2C slave address

  uint32_t low_bits

    TBD

  uint32_t high_bits

    TBD

  uint32_t i2c_sel

    TBD, select reg_i2c_slave_address[7:0]

  uint32_t rw

    Write (1) or read (0)

  struct ulp_insn i2c

    Format of I2C instruction

  uint32_t wakeup

    Set to 1 to wake up chip

  struct ulp_insn end

    Format of END instruction with wakeup

  struct ulp_insn macro

    Format of tokens used by LABEL and BRANCH macros

### Macros

I_DELAY(cycles_)

  Delay (nop) for a given number of cycles

I_HALT()

  Halt the coprocessor.

  This instruction halts the coprocessor, but keeps ULP timer active. As such, ULP program will be restarted again by timer. To stop the program and prevent the timer from restarting the program, use I_END(0) instruction.

I_WR_REG(reg, low_bit, high_bit, val)

  Write literal value to a peripheral register

  reg[high_bit : low_bit] = val This instruction can access RTC_CNTL_, RTC_IO_, SENS_, and RTC_I2C peripheral registers.

I_RD_REG(reg, low_bit, high_bit)

  Read from peripheral register into R0

  R0 = reg[high_bit : low_bit] This instruction can access RTC_CNTL_, RTC_IO_, SENS_, and RTC_I2C peripheral registers.

I_WR_REG_BIT(reg, shift, val)

  Set or clear a bit in the peripheral register.

  Sets bit (1 << shift) of register reg to value val. This instruction can access RTC_CNTL_, RTC_IO_, SENS_, and RTC_I2C peripheral registers.

I_WAKE()

  Wake the SoC from deep sleep.

  This instruction initiates wake up from deep sleep. Use esp_deep_sleep_enable_ulp_wakeup to enable deep sleep wakeup triggered by the ULP before going into deep sleep. Note that ULP program will still keep running until the I_HALT instruction, and it will still be restarted by timer at regular intervals, even when the SoC is woken up.

  To stop the ULP program, use I_HALT instruction.

  To disable the timer which start ULP program, use I_END() instruction. I_END instruction clears the RTC_CNTL_ULP_CP_SLP_TIMER_EN_S bit of RTC_CNTL_ULP_CP_TIMER_REG register, which controls the ULP timer.

I_END()

  Stop ULP program timer.

  This is a convenience macro which disables the ULP program timer. Once this instruction is used, ULP program will not be restarted anymore until ulp_run function is called.

  ULP program will continue running after this instruction. To stop the currently running program, use I_HALT().

I_TSENS(reg_dest, delay)

  Perform temperature sensor measurement and store it into reg_dest.

  Delay can be set between 1 and ((1 << 14) - 1). Higher values give higher measurement resolution.

I_ADC(reg_dest, adc_idx, pad_idx)

  Perform ADC measurement and store result in reg_dest.

  adc_idx selects ADC (0 or 1). pad_idx selects ADC pad (0 - 7).

I_ST_MANUAL(reg_val, reg_addr, offset_, label_, upper_, wr_way_)

  Store lower half-word, upper half-word or full-word data from register reg_val into RTC memory address.

  This instruction can be used to write data to discontinuous addresses in the RTC_SLOW_MEM. The value is written to an offset calculated by adding the value of reg_addr register and offset_ field (this offset is expressed in 32-bit words). The storage method is dictated by the wr_way and upper field settings as summarized in the following table:

      * |--------|-------|----------------------------------------------------------------------------------------|----------------------------|
      * | wr_way | upper |                                        data                                            |          operation         |
      * |--------|-------|----------------------------------------------------------------------------------------|----------------------------|
      * |        |       |                                                                                        | Write full-word, including |
      * |   0    |   X   | RTC_SLOW_MEM[addr + offset_]{31:0} = {insn_PC[10:0], 3’b0, label_[1:0], reg_val[15:0]} | the PC and the data        |
      * |--------|-------|----------------------------------------------------------------------------------------|----------------------------|
      * |        |       |                                                                                        | Store the data with label  |
      * |   1    |   0   | RTC_SLOW_MEM[addr + offset_]{15:0} = {label_[1:0], reg_val[13:0]}                      | in the low half-word       |
      * |--------|-------|----------------------------------------------------------------------------------------|----------------------------|
      * |        |       |                                                                                        | Store the data with label  |
      * |   1    |   1   | RTC_SLOW_MEM[addr + offset_]{31:16} = {label_[1:0], reg_val[13:0]}                     | in the high half-word      |
      * |--------|-------|----------------------------------------------------------------------------------------|----------------------------|
      * |        |       |                                                                                        | Store the data without     |
      * |   3    |   0   | RTC_SLOW_MEM[addr + offset_]{15:0} = reg_val[15:0]                                     | label in the low half-word |
      * |--------|-------|----------------------------------------------------------------------------------------|----------------------------|
      * |        |       |                                                                                        | Store the data without     |
      * |   3    |   1   | RTC_SLOW_MEM[addr + offset_]{31:16} = reg_val[15:0]                                    | label in the high half-word|
      * |--------|-------|----------------------------------------------------------------------------------------|----------------------------|
      *

  SUB_OPCODE_ST = manual_en:1, offset_set:0, wr_auto:0

I_ST(reg_val, reg_addr, offset_)

  Store value from register reg_val into RTC memory.

  I_ST() instruction provides backward compatibility for code written for esp32 to be run on esp32s2. This instruction is equivalent to calling I_ST_MANUAL() instruction with label = 0, upper = 0 and wr_way = 3.

I_STL(reg_val, reg_addr, offset_)

  Store value from register reg_val to lower 16 bits of the RTC memory address.

  This instruction is equivalent to calling I_ST_MANUAL() instruction with label = 0, upper = 0 and wr_way = 3.

I_STH(reg_val, reg_addr, offset_)

  Store value from register reg_val to upper 16 bits of the RTC memory address.

  This instruction is equivalent to calling I_ST_MANUAL() instruction with label = 0, upper = 1 and wr_way = 3.

I_ST32(reg_val, reg_addr, offset_, label_)

  Store value from register reg_val to full 32 bit word of the RTC memory address.

  This instruction is equivalent to calling I_ST_MANUAL() instruction with wr_way = 0.

I_STL_LABEL(reg_val, reg_addr, offset_, label_)

  Store value from register reg_val with label to lower 16 bits of RTC memory address.

  This instruction is equivalent to calling I_ST_MANUAL() instruction with label = label_, upper = 0 and wr_way = 1.

I_STH_LABEL(reg_val, reg_addr, offset_, label_)

  Store value from register reg_val with label to upper 16 bits of RTC memory address.

  This instruction is equivalent to calling I_ST_MANUAL() instruction with label = label_, upper = 1 and wr_way = 1.

I_ST_AUTO(reg_val, reg_addr, label_, wr_way_)

  Store lower half-word, upper half-word or full-word data from register reg_val into RTC memory address with auto-increment of the offset value.

  This instruction can be used to write data to continuous addresses in the RTC_SLOW_MEM. The initial address must be set using the SUB_OPCODE_ST_OFFSET instruction before the auto store instruction is called. The data written to the RTC memory address could be written to the full 32 bit word or to the lower half-word or the upper half-word. The storage method is dictated by the wr_way field and the number of times the SUB_OPCODE_ST_AUTO instruction is called. write_cnt indicates the later. The following table summarizes the storage method:

      * |--------|-----------|----------------------------------------------------------------------------------------|----------------------------|
      * | wr_way | write_cnt |                                        data                                            |          operation         |
      * |--------|-----------|----------------------------------------------------------------------------------------|----------------------------|
      * |        |           |                                                                                        | Write full-word, including |
      * |   0    |     X     | RTC_SLOW_MEM[addr + offset_]{31:0} = {insn_PC[10:0], 3’b0, label_[1:0], reg_val[15:0]} | the PC and the data        |
      * |--------|-----------|----------------------------------------------------------------------------------------|----------------------------|
      * |        |           |                                                                                        | Store the data with label  |
      * |   1    |    odd    | RTC_SLOW_MEM[addr + offset_]{15:0} = {label_[1:0], reg_val[13:0]}                      | in the low half-word       |
      * |--------|-----------|----------------------------------------------------------------------------------------|----------------------------|
      * |        |           |                                                                                        | Store the data with label  |
      * |   1    |    even   | RTC_SLOW_MEM[addr + offset_]{31:16} = {label_[1:0], reg_val[13:0]}                     | in the high half-word      |
      * |--------|-----------|----------------------------------------------------------------------------------------|----------------------------|
      * |        |           |                                                                                        | Store the data without     |
      * |   3    |    odd    | RTC_SLOW_MEM[addr + offset_]{15:0} = reg_val[15:0]                                     | label in the low half-word |
      * |--------|-----------|----------------------------------------------------------------------------------------|----------------------------|
      * |        |           |                                                                                        | Store the data without     |
      * |   3    |    even   | RTC_SLOW_MEM[addr + offset_]{31:16} = reg_val[15:0]                                    | label in the high half-word|
      * |--------|-----------|----------------------------------------------------------------------------------------|----------------------------|
      *

  The initial address offset is incremented after each store operation as follows:

  - When a full-word is written, the offset is automatically incremented by 1 after each SUB_OPCODE_ST_AUTO operation.

  - When a half-word is written (lower half-word first), the offset is automatically incremented by 1 after two SUB_OPCODE_ST_AUTO operations.

    SUB_OPCODE_ST_AUTO = manual_en:0, offset_set:0, wr_auto:1

I_STO(offset_)

  Set the initial address offset for auto-store operation

  This instruction sets the initial address of the RTC_SLOW_MEM to be used by the auto-store operation. The offset is incremented automatically. Refer I_ST_AUTO() for detailed explaination.

  SUB_OPCODE_ST_OFFSET = manual_en:0, offset_set:1, wr_auto:1

I_STI(reg_val, reg_addr)

  Store value from register reg_val to 32 bit word of the RTC memory address.

  This instruction is equivalent to calling I_ST_AUTO() instruction with label = 0 and wr_way = 3. The data in reg_val will be either written to the lower half-word or the upper half-word of the RTC memory address depending on the count of the number of times the I_STI() instruction is called. The initial offset is automatically incremented with I_STI() is called twice. Refer I_ST_AUTO() for detailed explaination.

I_STI_LABEL(reg_val, reg_addr, label_)

  Store value from register reg_val with label to 32 bit word of the RTC memory address.

  This instruction is equivalent to calling I_ST_AUTO() instruction with label = label_ and wr_way = 1. The data in reg_val will be either written to the lower half-word or the upper half-word of the RTC memory address depending on the count of the number of times the I_STI_LABEL() instruction is called. The initial offset is automatically incremented with I_STI_LABEL() is called twice. Refer I_ST_AUTO() for detailed explaination.

I_STI32(reg_val, reg_addr, label_)

  Store value from register reg_val to full 32 bit word of the RTC memory address.

  This instruction is equivalent to calling I_ST_AUTO() instruction with label = label_ and wr_way = 0. The data in reg_val will be written to the RTC memory address along with the label and the PC. The initial offset is automatically incremented each time the I_STI32() instruction is called. Refer I_ST_AUTO() for detailed explaination.

I_LD_MANUAL(reg_dest, reg_addr, offset_, rd_upper_)

  Load lower half-word, upper half-word or full-word data from RTC memory address into the register reg_dest.

  This instruction reads the lower half-word or upper half-word of the RTC memory address depending on the value of rd_upper_. The following table summarizes the loading method:

      * |----------|------------------------------------------------------|-------------------------|
      * | rd_upper |                       data                           |        operation        |
      * |----------|------------------------------------------------------|-------------------------|
      * |          |                                                      | Read lower half-word of |
      * |    0     | reg_dest{15:0} = RTC_SLOW_MEM[addr + offset_]{31:16} | the memory              |
      * |----------|------------------------------------------------------|-------------------------|
      * |          |                                                      | Read upper half-word of |
      * |    1     | reg_dest{15:0} = RTC_SLOW_MEM[addr + offset_]{15:0}  | the memory              |
      * |----------|------------------------------------------------------|-------------------------|
      *

I_LD(reg_dest, reg_addr, offset_)

  Load lower 16 bits value from RTC memory into reg_dest register.

  Loads 16 LSBs (rd_upper = 1) from RTC memory word given by the sum of value in reg_addr and value of offset_. I_LD() instruction provides backward compatibility for code written for esp32 to be run on esp32s2.

I_LDL(reg_dest, reg_addr, offset_)

  Load lower 16 bits value from RTC memory into reg_dest register.

  I_LDL() instruction and I_LD() instruction can be used interchangably.

I_LDH(reg_dest, reg_addr, offset_)

  Load upper 16 bits value from RTC memory into reg_dest register.

  Loads 16 MSBs (rd_upper = 0) from RTC memory word given by the sum of value in reg_addr and value of offset_.

I_BL(pc_offset, imm_value)

  Branch relative if R0 register less than the immediate value.

  pc_offset is expressed in words, and can be from -127 to 127 imm_value is a 16-bit value to compare R0 against

I_BG(pc_offset, imm_value)

  Branch relative if R0 register greater than the immediate value.

  pc_offset is expressed in words, and can be from -127 to 127 imm_value is a 16-bit value to compare R0 against

I_BE(pc_offset, imm_value)

  Branch relative if R0 register is equal to the immediate value.

  pc_offset is expressed in words, and can be from -127 to 127 imm_value is a 16-bit value to compare R0 against

I_BXR(reg_pc)

  Unconditional branch to absolute PC, address in register.

  reg_pc is the register which contains address to jump to. Address is expressed in 32-bit words.

I_BXI(imm_pc)

  Unconditional branch to absolute PC, immediate address.

  Address imm_pc is expressed in 32-bit words.

I_BXZR(reg_pc)

  Branch to absolute PC if ALU result is zero, address in register.

  reg_pc is the register which contains address to jump to. Address is expressed in 32-bit words.

I_BXZI(imm_pc)

  Branch to absolute PC if ALU result is zero, immediate address.

  Address imm_pc is expressed in 32-bit words.

I_BXFR(reg_pc)

  Branch to absolute PC if ALU overflow, address in register

  reg_pc is the register which contains address to jump to. Address is expressed in 32-bit words.

I_BXFI(imm_pc)

  Branch to absolute PC if ALU overflow, immediate address

  Address imm_pc is expressed in 32-bit words.

I_BSLE(pc_offset, imm_value)

  Branch relative if stage_cnt is less than or equal to the immediate value.

  pc_offset is expressed in words, and can be from -127 to 127 imm_value is a 16-bit value to compare R0 against

I_BSGE(pc_offset, imm_value)

  Branch relative if stage_cnt register is greater than or equal to the immediate value.

  pc_offset is expressed in words, and can be from -127 to 127 imm_value is a 16-bit value to compare R0 against

I_BSL(pc_offset, imm_value)

  Branch relative if stage_cnt register is less than the immediate value.

  pc_offset is expressed in words, and can be from -127 to 127 imm_value is a 16-bit value to compare R0 against

I_ADDR(reg_dest, reg_src1, reg_src2)

  Addition: dest = src1 + src2

I_SUBR(reg_dest, reg_src1, reg_src2)

  Subtraction: dest = src1 - src2

I_ANDR(reg_dest, reg_src1, reg_src2)

  Logical AND: dest = src1 & src2

I_ORR(reg_dest, reg_src1, reg_src2)

  Logical OR: dest = src1 | src2

I_MOVR(reg_dest, reg_src)

  Copy: dest = src

I_LSHR(reg_dest, reg_src, reg_shift)

  Logical shift left: dest = src << shift

I_RSHR(reg_dest, reg_src, reg_shift)

  Logical shift right: dest = src >> shift

I_ADDI(reg_dest, reg_src, imm_)

  Add register and an immediate value: dest = src1 + imm

I_SUBI(reg_dest, reg_src, imm_)

  Subtract register and an immediate value: dest = src - imm

I_ANDI(reg_dest, reg_src, imm_)

  Logical AND register and an immediate value: dest = src & imm

I_ORI(reg_dest, reg_src, imm_)

  Logical OR register and an immediate value: dest = src | imm

I_MOVI(reg_dest, imm_)

  Copy an immediate value into register: dest = imm

I_LSHI(reg_dest, reg_src, imm_)

  Logical shift left register value by an immediate: dest = src << imm

I_RSHI(reg_dest, reg_src, imm_)

  Logical shift right register value by an immediate: dest = val >> imm

I_STAGE_INC(reg_dest, reg_src, imm_)

  Increment stage_cnt register by an immediate: stage_cnt = stage_cnt + imm

I_STAGE_DEC(reg_dest, reg_src, imm_)

  Decrement stage_cnt register by an immediate: stage_cnt = stage_cnt - imm

I_STAGE_RST(reg_dest, reg_src, imm_)

  Reset stage_cnt register by an immediate: stage_cnt = 0

M_LABEL(label_num)

  Define a label with number label_num.

  This is a macro which doesn't generate a real instruction. The token generated by this macro is removed by ulp_process_macros_and_load function. Label defined using this macro can be used in branch macros defined below.

M_BRANCH(label_num)

  Token macro used by M_B and M_BX macros. Not to be used directly.

M_BL(label_num, imm_value)

  Macro: branch to label label_num if R0 is less than immediate value.

  This macro generates two ulp_insn_t values separated by a comma, and should be used when defining contents of ulp_insn_t arrays. First value is not a real instruction; it is a token which is removed by ulp_process_macros_and_load function.

M_BG(label_num, imm_value)

  Macro: branch to label label_num if R0 is greater than immediate value

  This macro generates two ulp_insn_t values separated by a comma, and should be used when defining contents of ulp_insn_t arrays. First value is not a real instruction; it is a token which is removed by ulp_process_macros_and_load function.

M_BE(label_num, imm_value)

  Macro: branch to label label_num if R0 equal to the immediate value

  This macro generates two ulp_insn_t values separated by a comma, and should be used when defining contents of ulp_insn_t arrays. First value is not a real instruction; it is a token which is removed by ulp_process_macros_and_load function.

M_BX(label_num)

  Macro: unconditional branch to label

  This macro generates two ulp_insn_t values separated by a comma, and should be used when defining contents of ulp_insn_t arrays. First value is not a real instruction; it is a token which is removed by ulp_process_macros_and_load function.

M_BXZ(label_num)

  Macro: branch to label if ALU result is zero

  This macro generates two ulp_insn_t values separated by a comma, and should be used when defining contents of ulp_insn_t arrays. First value is not a real instruction; it is a token which is removed by ulp_process_macros_and_load function.

M_BXF(label_num)

  Macro: branch to label if ALU overflow

  This macro generates two ulp_insn_t values separated by a comma, and should be used when defining contents of ulp_insn_t arrays. First value is not a real instruction; it is a token which is removed by ulp_process_macros_and_load function.

此文档对您有帮助吗？

- 反馈已收到，谢谢！
- 如果您有其他意见，欢迎填写乐鑫文档反馈表。

- 我们重视您的反馈。
- 您可以填写乐鑫文档反馈表告诉我们如何改进该文档。