警告

This document is not updated for ESP32C61 yet, so some of the content may not be correct.

This warning was automatically inserted due to the source file being in the add_warnings_pages list.

# Wi-Fi Easy ConnectTM (DPP)

[English]

Wi-Fi Easy ConnectTM 是 Wi-Fi Alliance 认证的配网协议，也称为设备配网协议 (DPP) 或 Easy Connect，是一种安全和标准化的 Wi-Fi 设备配网协议。使用 Easy Connect 将新设备添加入网就像扫描二维码一样简单，特别是对于没有 UI 的智能家居和物联网产品而言，大大降低了联网复杂性，加强了的用户体验。与旧的协议如 Wi-Fi Protected Setup (WPS) 等旧协议相比，Wi-Fi Easy Connect 的公钥加密技术额外确保了添加新设备时的网络安全。

Easy Connect 从以下几个方面改善了用户体验：

> - 操作简单直观，设置新设备时无需阅读冗长的指南

> - 无需记住需配网设备的密码或输入密码

> - 支持电子/打印的二维码以及其他人类可读的字符串

> - 同时支持 WPA2 和 WPA3 网络

如需了解更多信息，请参考 Wi-Fi Alliance 的官方介绍：Easy Connect。

ESP32-C61 支持 Easy Connect 的二维码配网模式，用户需要使用显示器显示二维码，随后使用兼容的设备扫描此二维码，并将 ESP32-C61 添加到自己的 Wi-Fi 网络中。此兼容设备需连接到无需支持 Wi-Fi Easy ConnectTM 的 AP 上。

Easy Connect 协议仍在不断发展。目前已知支持二维码的平台为部分运行 Android 10 及更高系统版本的 Android 智能手机等。使用 Easy Connect 时，无需在智能手机上安装额外的应用程序。

## 应用示例

- wifi/wifi_easy_connect/dpp-enrollee 演示如何使用 DPP 将 ESP32-C61 配置为注册设备，通过二维码和 Android 10 及以上的设备安全地将 ESP 设备接入网络。

## API 参考

### Header File

- components/wpa_supplicant/esp_supplicant/include/esp_dpp.h

- This header file can be included with:

  >     #include "esp_dpp.h"

- This header file is a part of the API provided by the `wpa_supplicant` component. To declare that your component depends on `wpa_supplicant`, add the following to your CMakeLists.txt:

  >     REQUIRES wpa_supplicant

  > or

  >     PRIV_REQUIRES wpa_supplicant

### Functions

esp_err_t esp_supp_dpp_init(void)

  Initialize DPP Supplicant.

         Starts DPP Supplicant and initializes related Data Structures.

  return

  - ESP_OK: Success

  - ESP_FAIL: Failure

esp_err_t esp_supp_dpp_deinit(void)

  De-initialize DPP Supplicant.

         Frees memory from DPP Supplicant Data Structures.

  返回:

    - ESP_OK: Success

esp_err_t esp_supp_dpp_bootstrap_gen(const char *chan_list, esp_supp_dpp_bootstrap_t type, const char *key, const char *info)

  Generates Bootstrap Information as an Enrollee.

         Generates Out Of Band Bootstrap information as an Enrollee which can be
         used by a DPP Configurator to provision the Enrollee.

  参数:

    - chan_list -- Comma-separated list of channels for listening (must not be NULL). A single channel (e.g., "6") is recommended for reliable discovery. If using multiple, prefer non-overlapping channels (e.g., "1,6,11").

    - type -- Bootstrap method type, only QR Code method is supported for now.

    - key -- (Optional) 32 byte Raw Private Key for generating a Bootstrapping Public Key

    - info -- (Optional) Ancillary Device Information like Serial Number

  返回:

    - ESP_OK: Success

    - ESP_ERR_DPP_INVALID_LIST: Channel list not valid

    - ESP_FAIL: Failure

esp_err_t esp_supp_dpp_start_listen(void)

  Start listening on Channels provided during esp_supp_dpp_bootstrap_gen.

         Listens on every Channel from Channel List for a pre-defined wait time.

  返回:

    - ESP_OK: Success

    - ESP_FAIL: Generic Failure

    - ESP_ERR_INVALID_STATE: ROC attempted before WiFi is started

    - ESP_ERR_NO_MEM: Memory allocation failed while posting ROC request

esp_err_t esp_supp_dpp_stop_listen(void)

  Stop listening on Channels.

         Stops listening on Channels and cancels ongoing listen operation.

  返回:

    - ESP_OK: Success

    - ESP_FAIL: Failure

### Macros

ESP_DPP_MAX_CHAN_COUNT

ESP_ERR_DPP_FAILURE

  Generic failure during DPP Operation

ESP_ERR_DPP_TX_FAILURE

  DPP Frame Tx failed OR not Acked

ESP_ERR_DPP_INVALID_ATTR

  Encountered invalid DPP Attribute

ESP_ERR_DPP_AUTH_TIMEOUT

  DPP Auth response was not received in time

ESP_ERR_DPP_INVALID_LIST

  Channel list given in esp_supp_dpp_bootstrap_gen() is not valid or too big

ESP_ERR_DPP_CONF_TIMEOUT

  DPP Configuration was not received in time

### Type Definitions

typedef enum dpp_bootstrap_type esp_supp_dpp_bootstrap_t

  Types of Bootstrap Methods for DPP.

### Enumerations

enum dpp_bootstrap_type

  Types of Bootstrap Methods for DPP.

  Values:

  enumerator DPP_BOOTSTRAP_QR_CODE

    QR Code Method

  enumerator DPP_BOOTSTRAP_PKEX

    Proof of Knowledge Method

  enumerator DPP_BOOTSTRAP_NFC_URI

    NFC URI record Method

此文档对您有帮助吗？

- 反馈已收到，谢谢！
- 如果您有其他意见，欢迎填写乐鑫文档反馈表。

- 我们重视您的反馈。
- 您可以填写乐鑫文档反馈表告诉我们如何改进该文档。