# 睡眠模式

[English]

## 概述

ESP32-C3 具有 Light-sleep 和 Deep-sleep 两种睡眠节能模式。根据应用所使用的功能，还有一些细分的子睡眠模式。关于这些睡眠模式和其子模式，参见 睡眠节能模式。另外，还可以配置一些断电选项来进一步减少功耗，请参见 断电选项 。

睡眠模式有多种唤醒源。这些唤醒源也可以组合在一起，此时任何一个唤醒源都可以触发唤醒。唤醒源 详细描述了这些唤醒源，以及配置 API。

断电选项和唤醒源的配置不是必要的，并且可以在进入睡眠模式前的任意时候进行。

最后，应用通过调用开始睡眠的 API 来使芯片进入其中一种睡眠模式，更多详情请参见 进入睡眠模式。当唤醒条件满足，芯片就会从睡眠中被唤醒。关于如何获取唤醒原因，请参见 检查睡眠唤醒原因 。关于醒来后如何处理唤醒源，请参见 禁用睡眠模式唤醒源 。

## 睡眠节能模式

在 Light-sleep 模式下，数字外设、CPU、以及大部分 RAM 都使用时钟门控，同时其供电电压降低。退出该模式后，数字外设、CPU 和 RAM 恢复运行，并且内部状态将被保留。

在 Deep-sleep 模式下，CPU、大部分 RAM、以及所有由时钟 APB_CLK 驱动的数字外设都会被断电。芯片上继续处于供电状态的部分仅包括：

> - RTC 控制器

> - RTC 高速内存

### 睡眠模式下的 Wi-Fi 和 Bluetooth 功能

在 Light-sleep 和 Deep-sleep 模式下，无线外设会被断电。因此，在进入这两种睡眠模式前，应用程序必须调用恰当的函数（`nimble_port_stop()`、`nimble_port_deinit()`、`esp_bluedroid_disable()`、`esp_bluedroid_deinit()`、`esp_bt_controller_disable()`、`esp_bt_controller_deinit()` 或 `esp_wifi_stop()`）来禁用 Wi-Fi 和 Bluetooth。在 Light-sleep 或 Deep-sleep 模式下，即使不调用这些函数也无法连接 Wi-Fi 和 Bluetooth。

如需保持 Wi-Fi 和 Bluetooth 连接，请启用 Wi-Fi 和 Bluetooth Modem-sleep 模式和自动 Light-sleep 模式（请参阅 电源管理 API）。在这两种模式下，Wi-Fi 和 Bluetooth 驱动程序发出请求时，系统将自动从睡眠中被唤醒，从而保持连接。

### 子睡眠模式

下表首行表示子睡眠模式，首列表示不同模式支持的功能。在睡眠模式下，支持更多功能的模式功耗可能更大。睡眠系统会自动选择满足用户功能需求且功耗最小的模式。

Deep-sleep：

| DSLP_ULTRA_LOW | DSLP_DEFAULT | DSLP_8MD256/
--- | --- | --- | ---
|  |  | DSLP_ADC_TSENS
ULP/触摸传感器（仅限 ESP32-S2、ESP32-S3） | Y | Y | Y
RTC IO 输入/高温下 RTC 内存 |  | Y | Y
ADC_TSEN_MONITOR |  |  | Y
8MD256 作为 RTC_SLOW_CLK 时钟源 |  |  | Y

功能：

1. RTC IO 输入/高温下 RTC 内存（试验功能）：将 RTC IO 用作输入管脚，或在高温下使用 RTC 内存。禁用上述功能，芯片可进入超低功耗模式。由 API `esp_sleep_sub_mode_config()` 配置 ESP_SLEEP_ULTRA_LOW_MODE 模式的使能与关闭。

2. ADC_TSEN_MONITOR：在 monitor 模式下使用 ADC/温度传感器（由 ULP 控制），通过 `ulp_adc_init()` 或其更高级别的 API 启用。仅适用于支持 monitor 模式的 ESP32-S2 和 ESP32-S3 芯片。

3. 8MD256 作为 RTC_SLOW_CLK 时钟源：通过 `CONFIG_RTC_CLK_SRC_INT_8MD256` 选择 8MD256 作为 RTC_SLOW_CLK 时钟源时，芯片在 Deep-sleep 模式下将自动进入该子睡眠模式.

Light-sleep：

| LSLP_DEFAULT | LSLP_ADC_TSENS | LSLP_8MD256 | LSLP_LEDC8M/
--- | --- | --- | --- | ---
|  |  |  | LSLP_XTAL_FPU
ULP/触摸传感器（仅限 ESP32-S2、ESP32-S3） | Y | Y | Y | Y
RTC IO 输入/高温下 RTC 内存 | Y | Y | Y | Y
ADC_TSEN_MONITOR |  | Y | Y | Y
8MD256 作为 RTC_SLOW_CLK 时钟源 |  |  | Y | Y
数字外设使用 8 MHz RC 时钟源 |  |  |  | Y
保持 XTAL 时钟开启 |  |  |  | Y

功能：（了解 Deep-sleep 模式，请参考前文 8MD256 和 ADC_TSEN_MONITOR 功能描述）

1. 数字外设使用 8 MHz RC 时钟源：目前，只有 LEDC 在 Light-sleep 模式下使用该时钟源。当 LEDC 选用该时钟源时，此功能将自动启用。

2. 保持 XTAL 时钟开启：在 Light-sleep 模式下保持 XTAL 时钟开启，由 `ESP_PD_DOMAIN_XTAL` 电源域控制。

ESP32-C3 不支持 ADC_TSEN_MONITOR 和 LSLP_ADC_TSENS 功能。

## 唤醒源

通过 API `esp_sleep_enable_X_wakeup` 可启用唤醒源。唤醒源在芯片被唤醒后并不会被禁用，若你不再需要某些唤醒源，可通过 API `esp_sleep_disable_wakeup_source()` 将其禁用，详见 禁用睡眠模式唤醒源。

以下是 ESP32-C3 所支持的唤醒源。

### 定时器

RTC 控制器中内嵌定时器，可用于在预定义的时间到达后唤醒芯片。时间精度为微秒，但其实际分辨率依赖于为 RTC_SLOW_CLK 所选择的时钟源。

在这种唤醒模式下，无需为睡眠模式中的 RTC 外设或内存供电。

调用 `esp_sleep_enable_timer_wakeup()` 函数可启用使用定时器唤醒睡眠模式。

### GPIO 唤醒

有两种 GPIO 唤醒 API 可供使用，分别适用于不同的睡眠场景：

1. :cpp:func:`esp_sleep_enable_gpio_wakeup` - 适用于 Light-sleep（GPIO 模块保持上电）

> 当 GPIO 模块在睡眠期间保持上电时，任何 IO 都可以用作外部输入管脚，将芯片从 Light-sleep 状态唤醒。调用 `gpio_wakeup_enable()` 函数可以将任意管脚单独配置为在高电平或低电平触发唤醒。此后，应调用 `esp_sleep_enable_gpio_wakeup()` 函数来启用此唤醒源。

> 备注

> 当启用 CONFIG_PM_POWER_DOWN_PERIPHERAL_IN_LIGHT_SLEEP 时，此 API 不可用，因为 GPIO 模块在睡眠期间会被断电。请使用 `esp_sleep_enable_gpio_wakeup_on_hp_periph_powerdown()` 替代。

2. :cpp:func:`esp_sleep_enable_gpio_wakeup_on_hp_periph_powerdown` - 适用于 Deep-sleep 和外设掉电的 Light-sleep

> 可将由 VDD3P3_RTC 电源域供电的 IO 用于芯片的 Deep-sleep 唤醒，或在外设电源域掉电时的 Light-sleep 唤醒。调用 `esp_sleep_enable_gpio_wakeup_on_hp_periph_powerdown()` 函数可以配置相应的唤醒管脚和唤醒触发电平。此函数适用于：

> - Deep-sleep 模式（始终可用）

> - 启用 CONFIG_PM_POWER_DOWN_PERIPHERAL_IN_LIGHT_SLEEP 时的 Light-sleep 模式

> 备注

> 只有由 VDD3P3_RTC 电源域供电的 GPIO（RTC IO）可以与此 API 一起使用。具体支持的管脚请参考 datasheet > IO 管脚。

备注

使用 IO 唤醒源（无论是电平模式还是边沿模式）将芯片从睡眠中唤醒时，唤醒信号必须保持（电平模式）或脉冲宽度（边沿模式）至少 3 个 RTC 慢时钟周期，唤醒逻辑才能可靠采样。一个慢时钟周期的时长取决于 CONFIG_RTC_CLK_SRC 的配置（例如 RC_SLOW @ ~136 kHz ≈ 7.4 µs/周期，XTAL32K @ 32.768 kHz ≈ 30.5 µs/周期）。该约束同样适用于 `esp_sleep_enable_gpio_wakeup()` 和 `esp_sleep_enable_gpio_wakeup_on_hp_periph_powerdown()`。

### UART 唤醒（仅适用于 Light-sleep 模式）

当 ESP32-C3 从外部设备接收 UART 输入时，通常需要在输入数据可用时唤醒芯片。UART 外设支持多种唤醒模式，可以将芯片从 Light-sleep 模式中唤醒。唤醒模式及其参数可以通过调用 `uart_wakeup_setup()` 函数进行配置。

UART 唤醒支持以下模式：

模式 0 (UART_WK_MODE_ACTIVE_THRESH) - 边沿阈值唤醒

> 当所有时钟都关闭时，此时可以通过使 RXD 翻转若干周期，当上升沿个数大于等于设定阈值时唤醒芯片。阈值可以通过 `uart_wakeup_cfg_t` 结构体中的 `rx_edge_threshold` 字段进行配置。

可调用 `esp_sleep_enable_uart_wakeup()` 函数来启用此唤醒源。

使用 UART 唤醒模式 0 之后，需要通过在 Active 模式下向 UART 传输数据或是复位整个 UART 模块，否则下一次唤醒所需的上升沿个数将减少。

### 禁用睡眠模式唤醒源

调用 API `esp_sleep_disable_wakeup_source()` 可以禁用给定唤醒源的触发器，从而禁用该唤醒源。此外，如果将参数设置为 `ESP_SLEEP_WAKEUP_ALL`，该函数可用于禁用所有触发器。

## 断电选项

应用程序可以使用 API `esp_sleep_pd_config()` 强制 RTC 外设和 RTC 内存进入特定断电模式。在 Deep-sleep 模式下，你还可以通过隔离一些 IO 来进一步降低功耗。

### RTC 外设和内存断电

默认情况下，调用函数 `esp_deep_sleep_start()` 和 `esp_light_sleep_start()` 后，所有唤醒源不需要的 RTC 电源域都会被断电。可调用函数 `esp_sleep_pd_config()` 来修改这一设置。

ESP32-C3 中只有 RTC 高速内存，因此，如果程序中的某些值被标记为 `RTC_DATA_ATTR`、`RTC_SLOW_ATTR` 或 `RTC_FAST_ATTR` 属性，那么所有这些值都将被存入 RTC 高速内存，默认情况下保持供电。如有需要，也可以使用函数 `esp_sleep_pd_config()` 对其进行修改。

### SPI Flash 进入 deep power-down 模式

为降低 Light-sleep 期间 SPI Flash 的功耗，ESP-IDF 优先推荐**采用 **Deep Power-Down（DPD）：通过启用配置项 CONFIG_ESP_SLEEP_SET_FLASH_DPD，令 SPI Flash 在供电保持开启的前提下进入器件内部的深度休眠指令状态。多数 SPI Flash 在 DPD 下电流可降至极低水平（常低于 1 µA），同时可避免反复上下电带来的唤醒延迟。

在几乎所有应用场景中，相较彻底切断 SPI Flash 供电，DPD 在安全性与功耗之间通常是更好的折中。

备注

两种方式互斥： Light-sleep 下的 SPI Flash 断电**（:ref:`CONFIG_ESP_SLEEP_POWER_DOWN_FLASH` 或通过 ``esp_sleep_pd_config`` 将 ``ESP_PD_DOMAIN_VDDSDIO`` 置为关闭）与 **DPD 不可同时使用， 在 menuconfig 中仅能在禁用 CONFIG_ESP_SLEEP_POWER_DOWN_FLASH 后再启用 CONFIG_ESP_SLEEP_SET_FLASH_DPD。

警告

使用该功能前需要查阅使用芯片所搭载的 SPI Flash 的技术手册是否支持 deep power-down 模式。

### SPI Flash 断电

默认情况下，调用函数 `esp_light_sleep_start()` 后，SPI Flash 不会 断电，因为在 sleep 过程中断电 SPI Flash 存在风险。具体而言，SPI Flash 断电需要时间，但是在此期间，系统有可能被唤醒，导致 SPI Flash 重新被上电。此时，断电尚未完成又重新上电的硬件行为有可能导致 SPI Flash 无法正常工作。

理论上讲，在 SPI Flash 完全断电后可以仅唤醒系统，然而现实情况是 SPI Flash 断电所需的时间很难预测。如果用户为 SPI Flash 供电电路添加了滤波电容，断电所需时间可能会更长。此外，即使可以预知 SPI Flash 彻底断电所需的时间，有时也不能通过设置足够长的睡眠时间来确保 SPI Flash 断电的安全（比如，突发的异步唤醒源会使得实际的睡眠时间不可控）。

警告

如果在 SPI Flash 的供电电路上添加了滤波电容，那么应当尽一切可能避免 SPI Flash 断电。

因为这些不可控的因素，ESP-IDF 很难保证 SPI Flash 断电的绝对安全。因此 ESP-IDF 不推荐用户断电 SPI Flash。对于一些功耗敏感型应用，可以通过设置 Kconfig 配置项 CONFIG_ESP_SLEEP_FLASH_LEAKAGE_WORKAROUND 来减少 Light-sleep 期间 SPI Flash 的功耗。这种方式在几乎所有场景下都要比断电 SPI Flash 更好，兼顾了安全性和功耗。

考虑到有些用户能够充分评估断电 SPI Flash 的风险，并希望通过断电 SPI Flash 来获得更低的功耗，因此 ESP-IDF 提供了两种断电 SPI Flash 的机制：

> - 设置 Kconfig 配置项 CONFIG_ESP_SLEEP_POWER_DOWN_FLASH 将使 ESP-IDF 以一个严格的条件来断电 SPI Flash。严格的条件具体指的是，RTC timer 是唯一的唤醒源 且 睡眠时间比 SPI Flash 彻底断电所需时间更长。

> - 调用函数 `esp_sleep_pd_config(ESP_PD_DOMAIN_VDDSDIO, ESP_PD_OPTION_OFF)` 将使 ESP-IDF 以一个宽松的条件来断电 SPI Flash。宽松的条件具体指的是 RTC timer 唤醒源未被使能 或 睡眠时间比 SPI Flash 彻底断电所需时间更长。

备注

- Light-sleep 模式下，ESP-IDF 没有提供保证 SPI Flash 一定会被断电的机制。

- 不管用户的配置如何，函数 `esp_deep_sleep_start()` 都会强制断电 SPI Flash

### SPI Flash 休眠策略选择建议

在休眠场景下，SPI Flash 的处理方式直接影响系统的安全性、功耗。不同应用场景对这些因素的侧重不同，因此需要选择合适的 SPI Flash 休眠策略。

#### SPI Flash 不掉电

不同 SPI Flash 的待机功耗不一致，在 ESP 系列芯片中，SPI Flash 的待机功耗通常低于 30 µA，在以下场景中，建议保持 SPI Flash 不掉电：

1. 系统对稳定性要求极高，无法接受 SPI Flash 掉电带来的任何潜在风险。

2. 休眠时间较短或不可预测，例如存在异步唤醒源（GPIO、UART 等）。

3. SPI Flash 供电电路中存在较大的滤波电容，导致 SPI Flash 实际断电时间难以估计。

在上述情况下，保持 SPI Flash 供电是最保守、也是最安全的选择，但需要注意其待机功耗相对较高 (约 10-30 µA)。

#### SPI Flash 进入 deep power-down（DPD）模式

若待机功耗仍偏高，应优先采用 Deep Power-Down（DPD），通过 CONFIG_ESP_SLEEP_SET_FLASH_DPD 降低休眠电流；功耗数据、时序及启用方式参见前文 SPI Flash 进入 deep power-down 模式。

DPD 模式适用于以下场景：

1. 需要显著降低休眠期间 SPI Flash 的功耗，但又希望避免 SPI Flash 重新上电的风险。

2. 休眠时间较短或不可预测，例如存在异步唤醒源（GPIO、UART 等）。

3. 使用的 SPI Flash 芯片明确支持 Deep Power-Down 模式。

#### SPI Flash 掉电

可以参考 SPI Flash 断电 实现在休眠中掉电 SPI Flash。在以下条件满足或经过充分评估后，可以考虑该策略：

1. 应用对极低功耗有严格要求。

2. 唤醒源可控，通常仅启用 RTC timer 唤醒源。

3. 能够确保实际睡眠时间大于 SPI Flash 彻底断电所需时间。对于 ESP 系列芯片，SPI Flash 彻底断电所需时间可能大于 300ms。如果 SPI Flash 供电电路中存在并联电容，可能需要更长的睡眠时间。

4. 如果休眠时间过短，SPI Flash 上电和下电过程所消耗的功耗可能会超过保持供电时的功耗。

5. 对 SPI Flash 供电及 IO 状态有充分控制，休眠时避免因为管脚上拉导致 SPI Flash 漏电。

由于 SPI Flash 的断电过程受硬件设计、IO 阻抗特性、供电以及环境因素影响较大，ESP-IDF 无法保证在 Light-sleep 模式下 SPI Flash 一定能够安全断电，因此该方式仅适用于风险可控且经过充分验证的场景。

### 配置 IO（仅适用于 Deep-sleep）

一些 ESP32-C3 IO 在默认情况下启用内部上拉或下拉电阻。如果这些管脚在 Deep-sleep 模式下中受外部电路驱动，电流流经这些上下拉电阻时，可能会增加电流消耗。

在 Deep-sleep 模式中：

  - 数字 GPIO (GPIO6 ~ 21) 处于高阻态。

  - RTC GPIO (GPIO0 ~ 5) 可能处于以下状态：

      - 如果未启用保持 (hold) 功能，RTC GPIO 将处于高阻态。

      - 如果启用保持功能，RTC GPIO 管脚将会在保持功能开启时处于锁存状态。

## 进入睡眠模式

应用程序通过 API `esp_light_sleep_start()` 或 `esp_deep_sleep_start()` 进入 Light-sleep 或 Deep-sleep 模式。此时，系统将按照被请求的唤醒源和断电选项配置有关的 RTC 控制器参数。

允许在未配置唤醒源的情况下进入睡眠模式。在此情况下，芯片将一直处于睡眠模式，直到从外部被复位。

备注

睡眠流程会禁用 cache，因此请求睡眠的任务其任务栈必须位于内部内存（DRAM 或 RTC fast memory）。如果任务栈位于 PSRAM 的任务请求 Light-sleep 或 Deep-sleep，将被拒绝并返回错误。

### UART 输出处理

进入睡眠前，睡眠流程会对**控制台 UART**（用于调试输出的 UART，由 CONFIG_ESP_CONSOLE_UART_NUM 选定）进行准备，以避免 APB 时钟变化或掉电导致输出乱码或未定义行为。所采用的策略可配置，会影响数据完整性、进入睡眠的时间以及功耗。

默认行为（自动模式）

若不调用 `esp_sleep_set_console_uart_handling_mode()`，则采用以下默认策略：

- Deep-sleep：始终等到控制台 UART FIFO 中的数据全部发完后再进入睡眠，确保所有调试输出被发送且不丢数据。

- Light-sleep：行为取决于 UART 所在电源域是否掉电：

    - 若 UART 保持供电（例如 HP 外设域未掉电）：在当前帧发完后挂起 UART 输出；唤醒后恢复发送，睡眠前 UART TX FIFO 中剩余数据会继续发出。

    - 若 UART 电源域掉电：睡眠流程会等到控制台 UART TX FIFO 中的数据全部发完后再进入睡眠；其他 UART 中的数据会被丢弃以更快进入睡眠。

配置控制台 UART 处理方式

可通过调用 `esp_sleep_set_console_uart_handling_mode()` 覆盖默认行为，并选择下列模式之一（参见 `esp_sleep_uart_handling_mode_t`）：

- `ESP_SLEEP_AUTO_FLUSH_SUSPEND_UART` （默认）：根据睡眠类型和电源域自动选择冲刷或挂起，如上所述。

- `ESP_SLEEP_ALWAYS_FLUSH_UART` ：进入睡眠前始终等待控制台 UART TX FIFO 中的数据全部发送完毕。适用于必须保证所有调试输出可见的场景；进入睡眠时间会更长，芯片处于 Active 状态的时间变长进而增加功耗。

- `ESP_SLEEP_ALWAYS_SUSPEND_UART` ：等待当前 UART 帧发完后挂起 UART。若 Light-sleep 期间 UART 保持供电，唤醒后会继续发送；若 UART 电源域掉电，未发送的数据将丢失。

- `ESP_SLEEP_ALWAYS_DISCARD_UART` ：丢弃控制台 UART FIFO 中所有未发送数据并立即进入睡眠。适用于追求最快进入睡眠和最低功耗、且可接受丢弃调试输出的场景。

- `ESP_SLEEP_NO_HANDLING` ：进入睡眠前不对控制台 UART 做任何处理。仅在确认 UART 状态安全时使用（例如无待发数据或已禁用控制台 UART）。

备注

睡眠流程在临界区中执行，当使用会冲刷控制台 UART 的模式（如 `ESP_SLEEP_ALWAYS_FLUSH_UART` ，或 HP 外设域掉电时的 Light-sleep/Deep-sleep 默认行为）时，请将 CONFIG_ESP_INT_WDT_TIMEOUT_MS 配置为**大于** `SOC_UART_FIFO_LEN` ×（当前波特率下发送一个字符所需时间）。否则若 TX FIFO 中积压数据过多，冲刷时间可能超过中断看门狗超时，会在进入睡眠过程中触发看门狗复位。

示例：在每次睡眠前确保所有调试输出已发出：:

    fflush(stdout);
    esp_sleep_set_console_uart_handling_mode(ESP_SLEEP_ALWAYS_FLUSH_UART);
    esp_light_sleep_start();

示例：尽量缩短进入睡眠时间并允许丢弃控制台输出：:

    esp_sleep_set_console_uart_handling_mode(ESP_SLEEP_ALWAYS_DISCARD_UART);
    esp_deep_sleep_start();

## 检查睡眠唤醒原因

`esp_sleep_get_wakeup_cause()` 函数可用于检测是何种唤醒源在睡眠期间被触发。

## 应用程序示例

- protocols/sntp 演示如何实现 Deep-sleep 模式的基本功能，周期性唤醒 ESP 模块，以从 NTP 服务器获取时间。

- wifi/power_save 演示如何通过 Wi-Fi Modem-sleep 模式和自动 Light-sleep 模式保持 Wi-Fi 连接。

- bluetooth/nimble/power_save 演示如何通过 Bluetooth Modem-sleep 模式和自动 Light-sleep 模式保持 Bluetooth 连接。

- system/deep_sleep 演示如何通过 ESP32-C3 的唤醒源，如 RTC 定时器、GPIO 等，触发 Deep-sleep 唤醒。

- system/light_sleep 演示如何使用 ESP32-C3 的唤醒源，如定时器，GPIO 等，触发 Light-sleep 唤醒。

## API 参考

### Header File

- components/esp_hw_support/include/esp_sleep.h

- This header file can be included with:

  >     #include "esp_sleep.h"

### Functions

esp_err_t esp_sleep_disable_wakeup_source(esp_sleep_source_t source)

  Disable wakeup source.

  This function is used to deactivate wake up trigger for source defined as parameter of the function.

  See docs/sleep-modes.rst for details.

  备注

  This function does not modify wake up configuration in RTC. It will be performed in esp_deep_sleep_start/esp_light_sleep_start function.

  参数:

    source -- - number of source to disable of type esp_sleep_source_t

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_STATE if trigger was not active

esp_err_t esp_sleep_enable_timer_wakeup(uint64_t time_in_us)

  Enable wakeup by timer.

  备注

  The valid `time_in_us` value depends on the bit width of the lp_timer/rtc_timer counter and the current slow clock source selection (Refer RTC clock source configuration in menuconfig). Valid values should be positive values less than RTC slow clock period * (2 ^ RTC timer bitwidth).

  参数:

    time_in_us -- time before wakeup, in microseconds

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if value is out of range.

bool esp_sleep_is_valid_wakeup_gpio(gpio_num_t gpio_num)

  Returns true if a GPIO number is valid for use as wakeup source.

  备注

  For SoCs with RTC IO capability, this can be any valid RTC IO input pin.

  参数:

    gpio_num -- Number of the GPIO to test for wakeup source capability

  返回:

    True if this GPIO number will be accepted as a sleep wakeup source.

esp_err_t esp_sleep_enable_gpio_wakeup_on_hp_periph_powerdown(uint64_t gpio_pin_mask, esp_sleep_gpio_wake_up_mode_t mode)

  Enable wakeup using specific gpio pins.

  This function enables an IO pin to wake up the chip from peripheral powerdowned sleep. (including deepsleep and peripheral powerdowned lightsleep).

  备注

  1.This function does not modify pin configuration. The pins are configured inside `esp_sleep_start`, immediately before entering sleep mode. 2.This function is also applicable to waking up the lightsleep when the peripheral power domain is powered off, see PM_POWER_DOWN_PERIPHERAL_IN_LIGHT_SLEEP in menuconfig.

  备注

  You don't need to worry about pull-up or pull-down resistors before using this function because the ESP_SLEEP_GPIO_ENABLE_INTERNAL_RESISTORS option is enabled by default. It will automatically set pull-up or pull-down resistors internally in esp_deep_sleep_start based on the wakeup mode. However, when using external pull-up or pull-down resistors, please be sure to disable the ESP_SLEEP_GPIO_ENABLE_INTERNAL_RESISTORS option, as the combination of internal and external resistors may cause interference. BTW, when you use low level to wake up the chip, we strongly recommend you to add external resistors (pull-up).

  备注

  The wakeup signal must be held (level mode) or have a pulse width (edge mode) of at least 3 RTC slow-clock cycles to be reliably sampled by the wakeup logic. The duration of one slow-clock cycle depends on `CONFIG_RTC_CLK_SRC` (e.g. RC_SLOW @ ~136 kHz ~= 7.4 us/cycle, XTAL32K @ 32.768 kHz ~= 30.5 us/cycle).

  参数:

    - gpio_pin_mask -- Bit mask of GPIO numbers which will cause wakeup. Only GPIOs which have RTC functionality (pads that powered by VDD3P3_RTC) can be used in this bit map.

    - mode -- Wakeup condition, see esp_sleep_gpio_wake_up_mode_t.

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if the mask contains any invalid wakeup pin or wakeup mode is invalid

esp_err_t esp_sleep_enable_gpio_wakeup(void)

  Enable wakeup from light sleep using GPIOs.

  Each GPIO supports wakeup function, which can be triggered on either low level or high level. This method can be used with any IO (RTC or digital), whereas external RTC wakeup is limited to RTC GPIOs. It can only be used to wakeup from light sleep though.

  To enable wakeup, first call gpio_wakeup_enable, specifying gpio number and wakeup level, for each GPIO which is used for wakeup. Then call this function to enable wakeup feature.

  备注

  1. On ESP32, GPIO wakeup source can not be used together with touch or ULP wakeup sources.

  1. If PM_POWER_DOWN_PERIPHERAL_IN_LIGHT_SLEEP is enabled (if target supported), this API is unavailable since the GPIO module is powered down during sleep. You can use `esp_sleep_enable_gpio_wakeup_on_hp_periph_powerdown` instead, or use EXT1 wakeup source by `esp_sleep_enable_ext1_wakeup_io` to achieve the same function. (Only GPIOs which have RTC functionality can be used)

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_STATE if wakeup triggers conflict

esp_err_t esp_sleep_enable_uart_wakeup(int uart_num)

  Enable wakeup from light sleep using UART.

  Use uart_wakeup_setup function to configure UART wakeup mode and parameters.

  Wakeup from light sleep takes some time, so not every character sent to the UART can be received by the application.

  备注

  1. ESP32 does not support wakeup from UART2.

  1. Wakeup mode 0(Active threshold) don't need source clock, but other modes need.

  2. If PM_POWER_DOWN_PERIPHERAL_IN_LIGHT_SLEEP is enabled (if target supported), this API is unavailable since the UART module is powered down during sleep.

  参数:

    uart_num -- UART port to wake up from

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if wakeup from given UART is not supported

esp_err_t esp_sleep_enable_bt_wakeup(void)

  Enable wakeup by bluetooth.

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_SUPPORTED if wakeup from bluetooth is not supported

esp_err_t esp_sleep_disable_bt_wakeup(void)

  Disable wakeup by bluetooth.

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_SUPPORTED if wakeup from bluetooth is not supported

esp_err_t esp_sleep_enable_usb_wakeup(void)

  Enable wakeup by High-Speed USB-OTG.

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_SUPPORTED if wakeup from USB is not supported

esp_err_t esp_sleep_disable_usb_wakeup(void)

  Disable wakeup by High-Speed USB-OTG.

  返回:

    - ESP_OK on success

    - ESP_ERR_NOT_SUPPORTED if wakeup from USB is not supported

esp_err_t esp_sleep_enable_wifi_wakeup(void)

  Enable wakeup by WiFi MAC.

  返回:

    - ESP_OK on success

esp_err_t esp_sleep_disable_wifi_wakeup(void)

  Disable wakeup by WiFi MAC.

  返回:

    - ESP_OK on success

esp_err_t esp_sleep_enable_wifi_beacon_wakeup(void)

  Enable beacon wakeup by WiFi MAC, it will wake up the system into modem state.

  返回:

    - ESP_OK on success

esp_err_t esp_sleep_disable_wifi_beacon_wakeup(void)

  Disable beacon wakeup by WiFi MAC.

  返回:

    - ESP_OK on success

uint64_t esp_sleep_get_ext1_wakeup_status(void)

  Get the bit mask of GPIOs which caused wakeup (ext1)

  If wakeup was caused by another source, this function will return 0.

  返回:

    bit mask, if GPIOn caused wakeup, BIT(n) will be set

uint64_t esp_sleep_get_gpio_wakeup_status(void)

  Get the bit mask of RTC IO which caused wakeup (GPIO wakeup source).

  If wakeup was caused by another source, this function will return 0. Each bit corresponds to an RTC IO. Use esp_sleep_wakeup_io_bit2num() to convert a bit index to GPIO number.

  返回:

    bit mask of RTC IO that caused wakeup

gpio_num_t esp_sleep_wakeup_io_bit2num(uint32_t bit)

  Convert RTC IO status bit index to GPIO number.

  Used to interpret the bit mask returned by esp_sleep_get_gpio_wakeup_status().

  参数:

    bit -- RTC IO bit index (0 to SOC_RTCIO_PIN_COUNT-1).

  返回:

    GPIO number, or GPIO_NUM_NC if bit is invalid or has no corresponding GPIO.

esp_err_t esp_sleep_pd_config(esp_sleep_pd_domain_t domain, esp_sleep_pd_option_t option)

  Configure power domain options for sleep mode.

  This function provides power domain management for sleep mode, allowing users to control which power domains remain active during sleep to maintain required functionality. The function supports:

  - Automatic power management (ESP_PD_OPTION_AUTO): Power domains are controlled automatically based on system requirements and other peripheral usage.

  - Manual power control (ESP_PD_OPTION_ON/ESP_PD_OPTION_OFF): User can force specific power domains to stay on or off during sleep.

  The management strategy uses reference counting when in manual mode, allowing multiple subsystems to request and release power domain resources safely without interfering with each other. Power domains will only change state when all users have released their requirements.

  参数:

    - domain -- power domain to configure

    - option -- power down option (ESP_PD_OPTION_OFF, ESP_PD_OPTION_ON, or ESP_PD_OPTION_AUTO)

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if either of the arguments is out of range

esp_err_t esp_deep_sleep_try_to_start(void)

  Enter deep sleep with the configured wakeup options.

  The reason for the rejection can be such as a short sleep time.

  备注

  In general, the function does not return, but if the sleep is rejected, then it returns from it.

  返回:

    - No return - If the sleep is not rejected.

    - ESP_ERR_NOT_ALLOWED Since the sleep process disables the cache, the task requesting to enter sleep must have its stack located in internal RAM. Tasks with their stacks in PSRAM are not allowed to request sleep.

    - ESP_ERR_INVALID_STATE VBAT power does not meet the requirements for entering deepsleep

    - ESP_ERR_SLEEP_REJECT sleep request is rejected(wakeup source set before the sleep request)

void esp_deep_sleep_start(void)

  Enter deep sleep with the configured wakeup options.

  备注

  The function does not do a return (no rejection). Even if wakeup source set before the sleep request it goes to deep sleep anyway.

esp_err_t esp_light_sleep_start(void)

  Enter light sleep with the configured wakeup options.

  返回:

    - ESP_OK on success (returned after wakeup)

    - ESP_ERR_NOT_ALLOWED Since the sleep process disables the cache, the task requesting to enter sleep must have its stack located in internal RAM. Tasks with their stacks in PSRAM are not allowed to request sleep.

    - ESP_ERR_SLEEP_REJECT sleep request is rejected(wakeup source set before the sleep request)

    - ESP_ERR_SLEEP_TOO_SHORT_SLEEP_DURATION after deducting the sleep flow overhead, the final sleep duration is too short to cover the minimum sleep duration of the chip, when rtc timer wakeup source enabled

esp_err_t esp_deep_sleep_try(uint64_t time_in_us)

  Enter deep-sleep mode.

  The device will automatically wake up after the deep-sleep time Upon waking up, the device calls deep sleep wake stub, and then proceeds to load application.

  Call to this function is equivalent to a call to esp_deep_sleep_enable_timer_wakeup followed by a call to esp_deep_sleep_start.

  The reason for the rejection can be such as a short sleep time.

  备注

  In general, the function does not return, but if the sleep is rejected, then it returns from it.

  参数:

    time_in_us -- deep-sleep time, unit: microsecond

  返回:

    - No return - If the sleep is not rejected.

    - ESP_ERR_SLEEP_REJECT sleep request is rejected(wakeup source set before the sleep request)

void esp_deep_sleep(uint64_t time_in_us)

  Enter deep-sleep mode.

  The device will automatically wake up after the deep-sleep time Upon waking up, the device calls deep sleep wake stub, and then proceeds to load application.

  Call to this function is equivalent to a call to esp_deep_sleep_enable_timer_wakeup followed by a call to esp_deep_sleep_start.

  备注

  The function does not do a return (no rejection).. Even if wakeup source set before the sleep request it goes to deep sleep anyway.

  参数:

    time_in_us -- deep-sleep time, unit: microsecond

esp_err_t esp_deep_sleep_register_hook(esp_deep_sleep_cb_t new_dslp_cb)

  Register a callback to be called from the deep sleep prepare.

  警告

  deepsleep callbacks should without parameters, and MUST NOT, UNDER ANY CIRCUMSTANCES, CALL A FUNCTION THAT MIGHT BLOCK.

  参数:

    new_dslp_cb -- Callback to be called

  返回:

    - ESP_OK: Callback registered to the deepsleep misc_modules_sleep_prepare

    - ESP_ERR_NO_MEM: No more hook space for register the callback

void esp_deep_sleep_deregister_hook(esp_deep_sleep_cb_t old_dslp_cb)

  Unregister an deepsleep callback.

  参数:

    old_dslp_cb -- Callback to be unregistered

esp_sleep_wakeup_cause_t esp_sleep_get_wakeup_cause(void)

  Get the wakeup source which caused wakeup from sleep.

  备注

  !!! This API will only return one wakeup source. If multiple wakeup sources wake up at the same time, the wakeup source information may be lost.

  返回:

    cause of wake up from last sleep (deep sleep or light sleep)

uint32_t esp_sleep_get_wakeup_causes(void)

  Get all wakeup sources bitmap which caused wakeup from sleep.

  返回:

    The bitmap of the wakeup sources of the last wakeup from sleep. (deep sleep or light sleep)

void esp_wake_deep_sleep(void)

  Default stub to run on wake from deep sleep.

  Allows for executing code immediately on wake from sleep, before the software bootloader or ESP-IDF app has started up.

  This function is weak-linked, so you can implement your own version to run code immediately when the chip wakes from sleep.

  See docs/deep-sleep-stub.rst for details.

void esp_set_deep_sleep_wake_stub(esp_deep_sleep_wake_stub_fn_t new_stub)

  Install a new stub at runtime to run on wake from deep sleep.

  If implementing esp_wake_deep_sleep() then it is not necessary to call this function.

  However, it is possible to call this function to substitute a different deep sleep stub. Any function used as a deep sleep stub must be marked RTC_IRAM_ATTR, and must obey the same rules given for esp_wake_deep_sleep().

void esp_set_deep_sleep_wake_stub_default_entry(void)

  Set wake stub entry to default `esp_wake_stub_entry`

esp_deep_sleep_wake_stub_fn_t esp_get_deep_sleep_wake_stub(void)

  Get current wake from deep sleep stub.

  返回:

    Return current wake from deep sleep stub, or NULL if no stub is installed.

void esp_default_wake_deep_sleep(void)

  The default esp-idf-provided esp_wake_deep_sleep() stub.

  See docs/deep-sleep-stub.rst for details.

void esp_deep_sleep_disable_rom_logging(void)

  Disable logging from the ROM code after deep sleep.

  Using LSB of RTC_STORE4.

esp_err_t esp_sleep_set_console_uart_handling_mode(esp_sleep_uart_handling_mode_t handling_mode)

  Configure how the console UART is handled when entering sleep.

  This function configures the handling behavior for the console UART (CONFIG_ESP_CONSOLE_UART_NUM) during sleep modes. The console UART is typically used for debug output, so its handling mode affects whether debug messages are preserved or discarded before sleep.

  备注

  When CONFIG_ESP_SLEEP_CACHE_SAFE_ASSERTION is enabled, the console UART will always be flushed regardless of the configured mode to ensure debug output is visible even when cache is disabled.

  参数:

    handling_mode -- Handling method, one of the following strategies:

    - ESP_SLEEP_AUTO_FLUSH_SUSPEND_UART (default): Automatically selects the appropriate strategy based on sleep type and power domain:

      - Deep sleep: Always flush to avoid data loss

      - Light sleep: Suspend if UART remains powered, flush if UART power domain is powered down

    - ESP_SLEEP_ALWAYS_FLUSH_UART: Wait for all data in TX FIFO to be fully transmitted before entering sleep. Ensures all debug output is visible but increases sleep entry time and power consumption.

    - ESP_SLEEP_ALWAYS_SUSPEND_UART: Wait for current UART frame to complete, then suspend the UART state machine. If UART remains powered during light sleep, transmission resumes after wake. If UART power domain is powered down, unsent data will be lost.

    - ESP_SLEEP_ALWAYS_DISCARD_UART: Discard all unsent data in UART FIFO and enter sleep immediately. Fastest sleep entry and lowest power, but all unsent debug output is lost.

    - ESP_SLEEP_NO_HANDLING: Do not perform any handling on the console UART before sleep. Can be used to disable the default UART handling behavior.

  返回:

    - ESP_OK on success

    - ESP_ERR_INVALID_ARG if handling_mode is not valid

    - ESP_ERR_NOT_SUPPORTED if no console UART is configured (CONFIG_ESP_CONSOLE_UART_NUM == -1)

esp_err_t esp_sleep_cpu_pd_low_init(void)

  CPU Power down low-level initialize, enable CPU power down during light sleep.

  返回:

    - ESP_OK on success

    - ESP_ERR_NO_MEM not enough retention memory

esp_err_t esp_sleep_cpu_pd_low_deinit(void)

  CPU Power down low-level deinitialize, disable CPU power down during light sleep.

  返回:

    - ESP_OK on success

    - ESP_ERR_NO_MEM not enough retention memory

esp_err_t esp_sleep_cpu_retention_init(void)

  CPU Power down initialize.

  返回:

    - ESP_OK on success

    - ESP_ERR_NO_MEM not enough retention memory

esp_err_t esp_sleep_cpu_retention_deinit(void)

  CPU Power down de-initialize.

  Release system retention memory.

  返回:

    - ESP_OK on success

void esp_sleep_config_gpio_isolate(void)

  Configure to isolate all GPIO pins in sleep state.

void esp_sleep_enable_gpio_switch(bool enable)

  Enable or disable GPIO pins status switching between slept status and waked status.

  参数:

    enable -- decide whether to switch status or not

### Macros

WAKEUP_MODE_2_INT_TYPE(mode)

ESP_PD_DOMAIN_RTC8M

### Type Definitions

typedef void (*esp_deep_sleep_cb_t)(void)

typedef esp_sleep_source_t esp_sleep_wakeup_cause_t

typedef void (*esp_deep_sleep_wake_stub_fn_t)(void)

  Function type for stub to run on wake from sleep.

### Enumerations

enum esp_sleep_gpio_wake_up_mode_t

  Logic function used for EXT1 wakeup mode.

  Values:

  enumerator ESP_GPIO_WAKEUP_GPIO_LOW
  enumerator ESP_GPIO_WAKEUP_GPIO_HIGH

enum esp_sleep_pd_domain_t

  Power domains which can be powered down in sleep mode.

  Values:

  enumerator ESP_PD_DOMAIN_XTAL

    XTAL oscillator.

  enumerator ESP_PD_DOMAIN_RC_FAST

    Internal Fast oscillator.

  enumerator ESP_PD_DOMAIN_CPU

    CPU core.

  enumerator ESP_PD_DOMAIN_VDDSDIO

    VDD_SDIO.

  enumerator ESP_PD_DOMAIN_MAX

    Number of domains.

enum esp_sleep_pd_option_t

  Power down options.

  Values:

  enumerator ESP_PD_OPTION_OFF

    Power down the power domain in sleep mode.

  enumerator ESP_PD_OPTION_ON

    Keep power domain enabled during sleep mode.

  enumerator ESP_PD_OPTION_AUTO

    Keep power domain enabled in sleep mode, if it is needed by one of the wakeup options. Otherwise power it down.

enum esp_sleep_source_t

  Sleep wakeup cause.

  Values:

  enumerator ESP_SLEEP_WAKEUP_UNDEFINED

    In case of deep sleep, reset was not caused by exit from deep sleep.

  enumerator ESP_SLEEP_WAKEUP_ALL

    Not a wakeup cause, used to disable all wakeup sources with esp_sleep_disable_wakeup_source.

  enumerator ESP_SLEEP_WAKEUP_EXT0

    Wakeup caused by external signal using RTC_IO.

  enumerator ESP_SLEEP_WAKEUP_EXT1

    Wakeup caused by external signal using RTC_CNTL.

  enumerator ESP_SLEEP_WAKEUP_TIMER

    Wakeup caused by timer.

  enumerator ESP_SLEEP_WAKEUP_TOUCHPAD

    Wakeup caused by touchpad.

  enumerator ESP_SLEEP_WAKEUP_ULP

    Wakeup caused by ULP program.

  enumerator ESP_SLEEP_WAKEUP_GPIO

    Wakeup caused by GPIO (light sleep only on ESP32, S2 and S3)

  enumerator ESP_SLEEP_WAKEUP_UART0

    Wakeup caused by UART0 (light sleep only)

  enumerator ESP_SLEEP_WAKEUP_UART
  enumerator ESP_SLEEP_WAKEUP_UART1

    Wakeup caused by UART1 (light sleep only)

  enumerator ESP_SLEEP_WAKEUP_WIFI

    Wakeup caused by WIFI (light sleep only)

  enumerator ESP_SLEEP_WAKEUP_COCPU

    Wakeup caused by COCPU int.

  enumerator ESP_SLEEP_WAKEUP_COCPU_TRAP_TRIG

    Wakeup caused by COCPU crash.

  enumerator ESP_SLEEP_WAKEUP_BT

    Wakeup caused by BT (light sleep only)

  enumerator ESP_SLEEP_WAKEUP_VAD

    Wakeup caused by VAD.

  enumerator ESP_SLEEP_WAKEUP_VBAT_UNDER_VOLT

    Wakeup caused by VDD_BAT under voltage.

  enumerator ESP_SLEEP_WAKEUP_USB

    Wakeup caused by USB HS (light sleep only)

enum esp_sleep_mode_t

  Sleep mode.

  Values:

  enumerator ESP_SLEEP_MODE_LIGHT_SLEEP

    light sleep mode

  enumerator ESP_SLEEP_MODE_DEEP_SLEEP

    deep sleep mode

enum esp_sleep_uart_handling_mode_t

  UART handling mode before entering sleep.

  These modes define how UARTs are handled when the chip enters sleep mode. The behavior affects data integrity, power consumption, and sleep entry time.

  Values:

  enumerator ESP_SLEEP_AUTO_FLUSH_SUSPEND_UART

    Automatically select flush or suspend based on sleep type and power domain configuration. For deep sleep, always flush. For light sleep, suspend if UART remains powered, flush/discard if UART power domain is powered down.

  enumerator ESP_SLEEP_ALWAYS_FLUSH_UART

    Always wait for all data in TX FIFO to be transmitted before sleep. Ensures data integrity but increases power consumption and sleep entry time.

  enumerator ESP_SLEEP_ALWAYS_SUSPEND_UART

    Suspend UART transmission after current frame completes. If UART remains powered during sleep, transmission resumes after wake. If UART power domain is powered down, unsent data will be lost.

  enumerator ESP_SLEEP_ALWAYS_DISCARD_UART

    Discard all data in TX/RX FIFOs and enter sleep immediately. Fastest sleep entry and lowest power, but all unsent data is lost.

  enumerator ESP_SLEEP_NO_HANDLING

    Do not perform any UART handling before sleep. UART state is not modified.

此文档对您有帮助吗？

- 反馈已收到，谢谢！
- 如果您有其他意见，欢迎填写乐鑫文档反馈表。

- 我们重视您的反馈。
- 您可以填写乐鑫文档反馈表告诉我们如何改进该文档。