# Compiler-Instrumented Function Tracing

[中文]

Function tracing records every function entry and exit automatically, without manual trace points. When a source file is built with the GCC flag `-finstrument-functions`, the compiler inserts a call at the start and end of each function. These calls go to hooks provided by the esp_trace component, which forward the events to the active trace encoder (for example SystemView). The events carry the raw function and call-site addresses. SystemView records them as raw addresses. Resolving the addresses to function names is done separately against the ELF file (for example with `addr2line` or a custom tool).

## Enabling Function Tracing

Enable CONFIG_ESP_TRACE_FUNCTION_TRACE. The following options control function tracing:

- CONFIG_ESP_TRACE_FUNCTION_TRACE - build the function-trace hooks and runtime.

- CONFIG_ESP_TRACE_FUNCTION_TRACE_AUTO_START - when enabled (default), recording follows the encoder's state and begins as soon as the host starts the session. When disabled, no events are emitted until the application calls `esp_trace_function_trace_start()`; an active host session alone is not enough.

Enabling the option compiles the hooks and runtime into the build. It does not add `-finstrument-functions` to any code, so on its own it produces no events. To trace a component or file, add the flag from its own `CMakeLists.txt` for the sources you want traced:

    if(CONFIG_ESP_TRACE_FUNCTION_TRACE)
        target_compile_options(${COMPONENT_LIB} PRIVATE -finstrument-functions)
    endif()

Use the GCC `-finstrument-functions-exclude-file-list` and `-finstrument-functions-exclude-function-list` flags to skip specific files or functions. Keep instrumentation scoped to your own components, and do not instrument code that runs with the flash cache disabled (IRAM ISRs, SPI flash operations).

## Decoding Function-Trace Events

After collecting a SystemView capture (see System Behavior Analysis with SEGGER SystemView), decode the function-trace events with the processing script:

    $IDF_PATH/tools/esp_app_trace/sysviewtrace_proc.py -i func -b </path/to/program.elf> -t xtensa-esp32-elf- file:///path/to/trace.svdat

The `-i func` option selects the function-trace event stream. The script uses the ELF file and toolchain prefix to resolve addresses, then prints a per-function report listing each traced function with its address, entry and exit counts, and source location.

## Application Example

- system/tracing/function_tracing demonstrates compiler-instrumented function entry/exit tracing and how to control which code is instrumented.

Was this page helpful?

- Thank you! We received your feedback.
- If you have any comments, fill in Espressif Documentation Feedback Form.

- We value your feedback.
- Let us know how we can improve this page by filling in Espressif Documentation Feedback Form.