# System

[中文]

## FreeRTOS

### IDF FreeRTOS Upgrade

The IDF FreeRTOS kernel (which is a dual-core SMP implementation of FreeRTOS) has been upgraded to be based on Vanilla FreeRTOS v10.5.1. With this upgrade, the design and implementation of IDF FreeRTOS has also been changed significantly. As a result, users should take note of the following changes to kernel behavior and API:

- When enabling single-core mode via the CONFIG_FREERTOS_UNICORE option, the kernel's behavior will now be identical to Vanilla FreeRTOS (see Single-Core Mode for more details).

- For SMP related APIs that were added by IDF FreeRTOS, checks on `xCoreID` arguments are now stricter. Providing out of range values for `xCoreID` arguments will now trigger an assert.

- The following SMP related APIs are now deprecated and replaced due to naming consistency reasons:

  > - `xTaskGetAffinity()` is deprecated, call `xTaskGetCoreID()` instead.

  > - `xTaskGetIdleTaskHandleForCPU()` is deprecated, call `xTaskGetIdleTaskHandleForCore()` instead.

  > - `xTaskGetCurrentTaskHandleForCPU()` is deprecated, call `xTaskGetCurrentTaskHandleForCore()` instead.

### Task Snapshot

The Task Snapshot API has been made private due to a lack of a practical way for the API to be used from user code (the scheduler must be halted before the API can be called).

## Panic Handler Behavior

The choice `CONFIG_ESP_SYSTEM_PANIC_GDBSTUB` in the configuration option CONFIG_ESP_SYSTEM_PANIC has been made dependent on whether the `esp_gdbstub` component is included in the build. When trimming the list of components in the build using `set(COMPONENTS main)`, `esp_gdbstub` component has to be added to this list of components to make the `CONFIG_ESP_SYSTEM_PANIC_GDBSTUB` option available.

Provide feedback about this document