IEEE 802.15.4
=============

:link_to_translation:`zh_CN:[中文]`

Receive Handle Done
-------------------

.. note::

    It is required since IDF v5.1.3 release.

User must call the function :cpp:func:`esp_ieee802154_receive_handle_done` to notify 802.15.4 driver after the received frame is handled. Otherwise the frame buffer will not be freed for future use.
